(../../boot/freeldr/freeldr/windows/winldr.c:521) trace: BootPath: 'multi(0)disk(0)rdisk(0)partition(1)\ReactOS\'
(../../boot/freeldr/freeldr/windows/wlregistry.c:101) trace:   Adding filesystem service fastfat
(../../boot/freeldr/freeldr/windows/winldr.c:535) trace: SYSTEM hive loaded with status 1
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'Boot Bus Extender'
(../../boot/freeldr/freeldr/windows/wlregistry.c:595) trace: Adding boot driver: 'multi(0)disk(0)rdisk(0)partition(1)\ReactOS\system32\drivers\acpi.sys'
(../../boot/freeldr/freeldr/windows/wlregistry.c:595) trace: Adding boot driver: 'multi(0)disk(0)rdisk(0)partition(1)\ReactOS\system32\drivers\pci.sys'
(../../boot/freeldr/freeldr/windows/wlregistry.c:673) trace:   Adding boot driver: 'multi(0)disk(0)rdisk(0)partition(1)\ReactOS\system32\drivers\usbccgp.sys'
(../../boot/freeldr/freeldr/windows/wlregistry.c:673) trace:   Adding boot driver: 'multi(0)disk(0)rdisk(0)partition(1)\ReactOS\system32\drivers\usbuhci.sys'
(../../boot/freeldr/freeldr/windows/wlregistry.c:673) trace:   Adding boot driver: 'multi(0)disk(0)rdisk(0)partition(1)\ReactOS\system32\drivers\usbohci.sys'
(../../boot/freeldr/freeldr/windows/wlregistry.c:673) trace:   Adding boot driver: 'multi(0)disk(0)rdisk(0)partition(1)\ReactOS\system32\drivers\usbehci.sys'
(../../boot/freeldr/freeldr/windows/wlregistry.c:673) trace:   Adding boot driver: 'multi(0)disk(0)rdisk(0)partition(1)\ReactOS\system32\drivers\usbhub.sys'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'System Bus Extender'
(../../boot/freeldr/freeldr/windows/wlregistry.c:595) trace: Adding boot driver: 'multi(0)disk(0)rdisk(0)partition(1)\ReactOS\system32\drivers\uniata.sys'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'SCSI Miniport'
(../../boot/freeldr/freeldr/windows/wlregistry.c:595) trace: Adding boot driver: 'multi(0)disk(0)rdisk(0)partition(1)\ReactOS\system32\drivers\buslogic.sys'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'Primary Disk'
(../../boot/freeldr/freeldr/windows/wlregistry.c:673) trace:   Adding boot driver: 'multi(0)disk(0)rdisk(0)partition(1)\ReactOS\system32\drivers\usbstor.sys'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'SCSI Class'
(../../boot/freeldr/freeldr/windows/wlregistry.c:673) trace:   Adding boot driver: 'multi(0)disk(0)rdisk(0)partition(1)\ReactOS\system32\drivers\disk.sys'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'Boot File System'
(../../boot/freeldr/freeldr/windows/wlregistry.c:673) trace:   Adding boot driver: 'multi(0)disk(0)rdisk(0)partition(1)\ReactOS\system32\drivers\ramdisk.sys'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'Base'
(../../boot/freeldr/freeldr/windows/wlregistry.c:673) trace:   Adding boot driver: 'multi(0)disk(0)rdisk(0)partition(1)\ReactOS\system32\drivers\nmidebug.sys'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'Pointer Port'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'Keyboard Port'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'Pointer Class'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'Keyboard Class'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'Debug'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'Video Init'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'Video'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'Video Save'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'File System'
(../../boot/freeldr/freeldr/windows/wlregistry.c:673) trace:   Adding boot driver: 'multi(0)disk(0)rdisk(0)partition(1)\ReactOS\system32\drivers\mup.sys'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'Event log'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'COM Infrastructure'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'NDIS'
(../../boot/freeldr/freeldr/windows/wlregistry.c:673) trace:   Adding boot driver: 'multi(0)disk(0)rdisk(0)partition(1)\ReactOS\system32\drivers\ndis.sys'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'PNP_TDI'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'TDI'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'PlugPlay'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'SpoolerGroup'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'UIGroup'
(../../boot/freeldr/freeldr/windows/wlregistry.c:524) trace: Driver group: 'Extended Base'
(../../boot/freeldr/freeldr/windows/wlregistry.c:175) trace: NLS data c_1250.nls c_852.nls l_intl.nls
(../../boot/freeldr/freeldr/windows/wlregistry.c:320) trace: AnsiFileSize: 66082
(../../boot/freeldr/freeldr/windows/wlregistry.c:344) trace: OemFileSize: 66594
(../../boot/freeldr/freeldr/windows/wlregistry.c:360) trace: LanguageFileSize: 4870
(../../boot/freeldr/freeldr/windows/wlregistry.c:181) trace: NLS data loaded with status 1
(../../boot/freeldr/freeldr/windows/winldr.c:539) trace: SYSTEM hive scanned with status 1
(../../boot/freeldr/freeldr/windows/winldr.c:563) trace: LoadAndBootWindowsCommon()
(../../boot/freeldr/freeldr/windows/winldr.c:438) trace: NTOSKRNL.EXE loaded with status 1 at 00800000
(../../boot/freeldr/freeldr/windows/winldr.c:438) trace: HAL.DLL loaded with status 1 at 0036D000
(../../boot/freeldr/freeldr/windows/winldr.c:438) trace: KDCOM.DLL loaded with status 1 at 0039A000
(../../boot/freeldr/freeldr/windows/winldr.c:307) trace: BootDriver system32\drivers\fastfat.sys DTE 00000000 RegPath: \Registry\Machine\System\CurrentControlSet\Services\fastfat
(../../boot/freeldr/freeldr/windows/winldr.c:251) trace: DriverPath: system32\drivers\, DllName: fastfat.sys, LPB
(../../boot/freeldr/freeldr/windows/winldr.c:307) trace: BootDriver system32\drivers\acpi.sys DTE 00000000 RegPath: \Registry\Machine\System\CurrentControlSet\Services\acpi
(../../boot/freeldr/freeldr/windows/winldr.c:251) trace: DriverPath: system32\drivers\, DllName: acpi.sys, LPB
(../../boot/freeldr/freeldr/windows/winldr.c:307) trace: BootDriver system32\drivers\pci.sys DTE 00000000 RegPath: \Registry\Machine\System\CurrentControlSet\Services\pciide
(../../boot/freeldr/freeldr/windows/winldr.c:251) trace: DriverPath: system32\drivers\, DllName: pci.sys, LPB
(../../boot/freeldr/freeldr/windows/winldr.c:307) trace: BootDriver system32\drivers\usbccgp.sys DTE 00000000 RegPath: \Registry\Machine\System\CurrentControlSet\Services\usbccgp
(../../boot/freeldr/freeldr/windows/winldr.c:251) trace: DriverPath: system32\drivers\, DllName: usbccgp.sys, LPB
(../../boot/freeldr/freeldr/windows/winldr.c:307) trace: BootDriver system32\drivers\usbuhci.sys DTE 00000000 RegPath: \Registry\Machine\System\CurrentControlSet\Services\usbuhci
(../../boot/freeldr/freeldr/windows/winldr.c:251) trace: DriverPath: system32\drivers\, DllName: usbuhci.sys, LPB
(../../boot/freeldr/freeldr/windows/winldr.c:307) trace: BootDriver system32\drivers\usbohci.sys DTE 00000000 RegPath: \Registry\Machine\System\CurrentControlSet\Services\usbohci
(../../boot/freeldr/freeldr/windows/winldr.c:251) trace: DriverPath: system32\drivers\, DllName: usbohci.sys, LPB
(../../boot/freeldr/freeldr/windows/winldr.c:307) trace: BootDriver system32\drivers\usbehci.sys DTE 00000000 RegPath: \Registry\Machine\System\CurrentControlSet\Services\usbehci
(../../boot/freeldr/freeldr/windows/winldr.c:251) trace: DriverPath: system32\drivers\, DllName: usbehci.sys, LPB
(../../boot/freeldr/freeldr/windows/winldr.c:307) trace: BootDriver system32\drivers\usbhub.sys DTE 00000000 RegPath: \Registry\Machine\System\CurrentControlSet\Services\usbhub
(../../boot/freeldr/freeldr/windows/winldr.c:251) trace: DriverPath: system32\drivers\, DllName: usbhub.sys, LPB
(../../boot/freeldr/freeldr/windows/winldr.c:307) trace: BootDriver system32\drivers\uniata.sys DTE 00000000 RegPath: \Registry\Machine\System\CurrentControlSet\Services\uniata
(../../boot/freeldr/freeldr/windows/winldr.c:251) trace: DriverPath: system32\drivers\, DllName: uniata.sys, LPB
(../../boot/freeldr/freeldr/windows/winldr.c:307) trace: BootDriver system32\drivers\buslogic.sys DTE 00000000 RegPath: \Registry\Machine\System\CurrentControlSet\Services\BusLogic
(../../boot/freeldr/freeldr/windows/winldr.c:251) trace: DriverPath: system32\drivers\, DllName: buslogic.sys, LPB
(../../boot/freeldr/freeldr/windows/winldr.c:307) trace: BootDriver system32\drivers\usbstor.sys DTE 00000000 RegPath: \Registry\Machine\System\CurrentControlSet\Services\usbstor
(../../boot/freeldr/freeldr/windows/winldr.c:251) trace: DriverPath: system32\drivers\, DllName: usbstor.sys, LPB
(../../boot/freeldr/freeldr/windows/winldr.c:307) trace: BootDriver system32\drivers\disk.sys DTE 00000000 RegPath: \Registry\Machine\System\CurrentControlSet\Services\Disk
(../../boot/freeldr/freeldr/windows/winldr.c:251) trace: DriverPath: system32\drivers\, DllName: disk.sys, LPB
(../../boot/freeldr/freeldr/windows/winldr.c:307) trace: BootDriver system32\drivers\ramdisk.sys DTE 00000000 RegPath: \Registry\Machine\System\CurrentControlSet\Services\RamDisk
(../../boot/freeldr/freeldr/windows/winldr.c:251) trace: DriverPath: system32\drivers\, DllName: ramdisk.sys, LPB
(../../boot/freeldr/freeldr/windows/winldr.c:307) trace: BootDriver system32\drivers\nmidebug.sys DTE 00000000 RegPath: \Registry\Machine\System\CurrentControlSet\Services\NMIDebug
(../../boot/freeldr/freeldr/windows/winldr.c:251) trace: DriverPath: system32\drivers\, DllName: nmidebug.sys, LPB
(../../boot/freeldr/freeldr/windows/winldr.c:307) trace: BootDriver system32\drivers\mup.sys DTE 00000000 RegPath: \Registry\Machine\System\CurrentControlSet\Services\Mup
(../../boot/freeldr/freeldr/windows/winldr.c:251) trace: DriverPath: system32\drivers\, DllName: mup.sys, LPB
(../../boot/freeldr/freeldr/windows/winldr.c:307) trace: BootDriver system32\drivers\ndis.sys DTE 00000000 RegPath: \Registry\Machine\System\CurrentControlSet\Services\Ndis
(../../boot/freeldr/freeldr/windows/winldr.c:251) trace: DriverPath: system32\drivers\, DllName: ndis.sys, LPB
(../../boot/freeldr/freeldr/windows/winldr.c:605) trace: Boot drivers loaded with status 1
(../../boot/freeldr/freeldr/windows/winldr.c:100) trace: ArcBoot: multi(0)disk(0)rdisk(0)partition(1)
(../../boot/freeldr/freeldr/windows/winldr.c:101) trace: SystemRoot: \ReactOS\
(../../boot/freeldr/freeldr/windows/winldr.c:102) trace: Options: /DEBUG /DEBUGPORT=COM1 /BAUDRATE=115200 /SOS
(../../boot/freeldr/freeldr/windows/conversion.c:83) trace: ConvertConfigToVA(Start 0x18C44C)
(../../boot/freeldr/freeldr/windows/conversion.c:104) trace: Device 0x18C44C class 0 type 41 id '(null)', parent 00000000
(../../boot/freeldr/freeldr/windows/conversion.c:104) trace: Device 0x18C4F4 class 3 type 12 id 'PCI BIOS', parent 8018C44C
(../../boot/freeldr/freeldr/windows/conversion.c:126) trace: Device 0x18C5BC class 3 type 12 id 'PCI', parent 8018C44C
(../../boot/freeldr/freeldr/windows/conversion.c:126) trace: Device 0x18C654 class 3 type 12 id 'APM', parent 8018C44C
(../../boot/freeldr/freeldr/windows/conversion.c:126) trace: Device 0x18C6FC class 3 type 12 id 'ISA', parent 8018C44C
(../../boot/freeldr/freeldr/windows/conversion.c:83) trace: ConvertConfigToVA(Start 0x18CAA4)
(../../boot/freeldr/freeldr/windows/conversion.c:104) trace: Device 0x18CAA4 class 4 type 13 id '(null)', parent 8018C6FC
(../../boot/freeldr/freeldr/windows/conversion.c:126) trace: Device 0x18CD94 class 4 type 13 id '(null)', parent 8018C6FC
(../../boot/freeldr/freeldr/windows/conversion.c:126) trace: Device 0x18CD3C class 4 type 17 id 'COM1', parent 8018C6FC
(../../boot/freeldr/freeldr/windows/conversion.c:126) trace: Device 0x18CF04 class 4 type 22 id '(null)', parent 8018C6FC
(../../boot/freeldr/freeldr/windows/conversion.c:83) trace: ConvertConfigToVA(Start 0x18CFB4)
(../../boot/freeldr/freeldr/windows/conversion.c:104) trace: Device 0x18CFB4 class 5 type 32 id 'PCAT_ENHANCED', parent 8018CF04
(../../boot/freeldr/freeldr/windows/conversion.c:126) trace: Device 0x18CE44 class 4 type 21 id '(null)', parent 8018C6FC
(../../boot/freeldr/freeldr/windows/conversion.c:83) trace: ConvertConfigToVA(Start 0x18D0B4)
(../../boot/freeldr/freeldr/windows/conversion.c:104) trace: Device 0x18D0B4 class 4 type 31 id 'MICROSOFT PS2 MOUSE', parent 8018CE44
(../../boot/freeldr/freeldr/windows/conversion.c:126) trace: Device 0x18D16C class 4 type 19 id 'VBE Display', parent 8018C6FC
(../../boot/freeldr/freeldr/windows/conversion.c:104) trace: Device 0x18CB44 class 5 type 25 id 'c313057f-22261df0-A', parent 8018CAA4
(../../boot/freeldr/freeldr/windows/conversion.c:126) trace: Device 0x18CC64 class 5 type 25 id 'f7794510-0a7d5d12-A', parent 8018CAA4
(../../boot/freeldr/freeldr/windows/conversion.c:126) trace: Device 0x18D1F4 class 3 type 12 id 'ACPI BIOS', parent 8018C44C
(../../boot/freeldr/freeldr/windows/conversion.c:104) trace: Device 0x18C7C4 class 5 type 39 id 'PCI Real-mode IRQ Routing Table', parent 8018C4F4
(../../boot/freeldr/freeldr/windows/winldr.c:350) trace: Loading module multi(0)disk(0)rdisk(0)partition(1)\ReactOS\AppPatch\drvmain.sdb
(../../boot/freeldr/freeldr/windows/winldr.c:216) trace: WinLdrInitializePhase1() completed
(../../boot/freeldr/freeldr/arch/i386/winldr.c:61) trace: NumPageTables = 127
(../../boot/freeldr/freeldr/arch/i386/winldr.c:260) trace: HalPageTable: 0x67D000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:244) trace: Local APIC detected at address 0xfee00000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:341) trace: *ExtendedBIOSDataArea = 0x9fc00
(../../boot/freeldr/freeldr/windows/wlmemory.c:246) trace: Got memory map with 131056 entries
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x0, PageCount=0x1, Type=6)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x0 PC=0x1 FirmwarePermanent
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x1, PageCount=0xe, Type=5)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x1 PC=0xE FirmwareTemporary
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0x1, Number: 0xE, Kernel: no
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0xf, PageCount=0x71, Type=4)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0xF PC=0x71 LoadedProgram
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0xF, Number: 0x71, Kernel: no
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x80, PageCount=0x11, Type=5)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x80 PC=0x11 FirmwareTemporary
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0x80, Number: 0x11, Kernel: no
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x91, PageCount=0x7, Type=8)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x91 PC=0x7 OsloaderStack
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0x91, Number: 0x7, Kernel: no
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x98, PageCount=0x2, Type=5)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x98 PC=0x2 FirmwareTemporary
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0x98, Number: 0x2, Kernel: no
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x9a, PageCount=0x1, Type=1)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x9A PC=0x1 SystemBlock
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0x9A, Number: 0x1, Kernel: yes
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x9b, PageCount=0x2, Type=17)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x9B PC=0x2 StartupPcrPage
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0x9B, Number: 0x2, Kernel: yes
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x9d, PageCount=0x3, Type=20)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x9D PC=0x3 MemoryData
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0x9D, Number: 0x3, Kernel: yes
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0xa0, PageCount=0x50, Type=6)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0xA0 PC=0x50 FirmwarePermanent
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0xA0, Number: 0x50, Kernel: yes
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0xf0, PageCount=0x10, Type=22)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0xF0 PC=0x10 SpecialMemory
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x100, PageCount=0x99, Type=7)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x100 PC=0x99 OsloaderHeap
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0x100, Number: 0x99, Kernel: yes
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x199, PageCount=0x1, Type=20)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x199 PC=0x1 MemoryData
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0x199, Number: 0x1, Kernel: yes
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x19a, PageCount=0x66, Type=2)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x19A PC=0x66 Free
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x200, PageCount=0x100, Type=5)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x200 PC=0x100 FirmwareTemporary
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0x200, Number: 0x100, Kernel: no
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x300, PageCount=0x49, Type=19)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x300 PC=0x49 RegistryData
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0x300, Number: 0x49, Kernel: yes
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x349, PageCount=0x24, Type=21)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x349 PC=0x24 NlsData
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0x349, Number: 0x24, Kernel: yes
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x36d, PageCount=0x2d, Type=10)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x36D PC=0x2D HalCode
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0x36D, Number: 0x2D, Kernel: yes
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x39a, PageCount=0x9, Type=9)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x39A PC=0x9 SystemCode
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0x39A, Number: 0x9, Kernel: yes
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x3a3, PageCount=0x2d8, Type=11)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x3A3 PC=0x2D8 BootDriver
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0x3A3, Number: 0x2D8, Kernel: yes
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x67b, PageCount=0x82, Type=20)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x67B PC=0x82 MemoryData
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0x67B, Number: 0x82, Kernel: yes
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x6fd, PageCount=0x7f, Type=5)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x6FD PC=0x7F FirmwareTemporary
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0x6FD, Number: 0x7F, Kernel: no
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x77c, PageCount=0x84, Type=2)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x77C PC=0x84 Free
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x800, PageCount=0x3d2, Type=9)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x800 PC=0x3D2 SystemCode
(../../boot/freeldr/freeldr/arch/i386/winldr.c:155) trace: MempSetupPaging: SP 0x800, Number: 0x3D2, Kernel: yes
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0xbd2, PageCount=0x42d, Type=2)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0xBD2 PC=0x42D Free
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0xfff, PageCount=0x1, Type=22)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0xFFF PC=0x1 SpecialMemory
(../../boot/freeldr/freeldr/windows/wlmemory.c:73) trace: MempAddMemoryBlock(BasePage=0x1000, PageCount=0x1efef, Type=2)
(../../boot/freeldr/freeldr/windows/wlmemory.c:364) trace: BP=0x1000 PC=0x1EFEF Free
(../../boot/freeldr/freeldr/windows/wlmemory.c:329) trace: MadCount: 27
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000000 PC 0001 MT 6
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000001 PC 000E MT 5
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 0000000F PC 0071 MT 4
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000080 PC 0011 MT 5
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000091 PC 0007 MT 8
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000098 PC 0002 MT 5
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 0000009A PC 0001 MT 1
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 0000009B PC 0002 MT 17
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 0000009D PC 0003 MT 20
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 000000A0 PC 0050 MT 6
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 000000F0 PC 0010 MT 22
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000100 PC 0099 MT 7
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000199 PC 0001 MT 20
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 0000019A PC 0066 MT 2
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000200 PC 0100 MT 5
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000300 PC 0049 MT 19
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000349 PC 0024 MT 21
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 0000036D PC 002D MT 10
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 0000039A PC 0009 MT 9
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 000003A3 PC 02D8 MT 11
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 0000067B PC 0082 MT 20
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 000006FD PC 007F MT 5
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 0000077C PC 0084 MT 2
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000800 PC 03D2 MT 9
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000BD2 PC 042D MT 2
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000FFF PC 0001 MT 22
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00001000 PC 1EFEF MT 2
(../../boot/freeldr/freeldr/windows/wlmemory.c:343) trace: Memory Descriptor List prepared, printing PDE
(../../boot/freeldr/freeldr/arch/i386/winldr.c:678) trace:
PDE
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0000 | 0x006FD003 0x006FE003 0x006FF003 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0008 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0010 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0018 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0020 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0028 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0030 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0038 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0040 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0048 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0050 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0058 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0060 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0068 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0070 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0078 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0080 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0088 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0090 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0098 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x00A0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x00A8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x00B0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x00B8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x00C0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x00C8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x00D0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x00D8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x00E0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x00E8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x00F0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x00F8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0100 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0108 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0110 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0118 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0120 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0128 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0130 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0138 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0140 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0148 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0150 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0158 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0160 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0168 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0170 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0178 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0180 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0188 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0190 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0198 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x01A0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x01A8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x01B0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x01B8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x01C0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x01C8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x01D0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x01D8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x01E0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x01E8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x01F0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x01F8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0200 | 0x0067E003 0x0067F003 0x00680003 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0208 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0210 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0218 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0220 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0228 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0230 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0238 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0240 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0248 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0250 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0258 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0260 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0268 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0270 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0278 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0280 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0288 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0290 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0298 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x02A0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x02A8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x02B0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x02B8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x02C0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x02C8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x02D0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x02D8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x02E0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x02E8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x02F0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x02F8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0300 | 0x0067C003 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0308 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0310 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0318 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0320 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0328 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0330 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0338 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0340 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0348 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0350 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0358 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0360 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0368 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0370 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0378 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0380 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0388 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0390 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x0398 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x03A0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x03A8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x03B0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x03B8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x03C0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x03C8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x03D0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x03D8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x03E0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x03E8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x03F0 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000
(../../boot/freeldr/freeldr/arch/i386/winldr.c:682) trace: 0x03F8 | 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x00000000 0x0067D003
(../../boot/freeldr/freeldr/arch/i386/winldr.c:424) trace: GDtIdt 0067B000, Pcr FFDFF000, Tss 0x8009D000
(../../boot/freeldr/freeldr/windows/winldr.c:633) trace: Hello from paged mode, KiSystemStartup 80905E8A, LoaderBlockVA 8009A000!
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000000 PC 0001 MT 6
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000001 PC 000E MT 5
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 0000000F PC 0071 MT 4
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000080 PC 0011 MT 5
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000091 PC 0007 MT 8
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000098 PC 0002 MT 5
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 0000009A PC 0001 MT 1
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 0000009B PC 0002 MT 17
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 0000009D PC 0003 MT 20
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 000000A0 PC 0050 MT 6
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 000000F0 PC 0010 MT 22
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000100 PC 0099 MT 7
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000199 PC 0001 MT 20
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 0000019A PC 0066 MT 2
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000200 PC 0100 MT 5
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000300 PC 0049 MT 19
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000349 PC 0024 MT 21
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 0000036D PC 002D MT 10
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 0000039A PC 0009 MT 9
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 000003A3 PC 02D8 MT 11
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 0000067B PC 0082 MT 20
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 000006FD PC 007F MT 5
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 0000077C PC 0084 MT 2
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000800 PC 03D2 MT 9
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000BD2 PC 042D MT 2
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00000FFF PC 0001 MT 22
(../../boot/freeldr/freeldr/windows/winldr.c:668) trace: BP 00001000 PC 1EFEF MT 2
(../../boot/freeldr/freeldr/windows/winldr.c:687) trace: BootDriver system32\drivers\fastfat.sys DTE 80196B4C RegPath: \Registry\Machine\System\CurrentControlSet\Services\fastfat
(../../boot/freeldr/freeldr/windows/winldr.c:687) trace: BootDriver system32\drivers\acpi.sys DTE 80196C2C RegPath: \Registry\Machine\System\CurrentControlSet\Services\acpi
(../../boot/freeldr/freeldr/windows/winldr.c:687) trace: BootDriver system32\drivers\pci.sys DTE 80196CFC RegPath: \Registry\Machine\System\CurrentControlSet\Services\pciide
(../../boot/freeldr/freeldr/windows/winldr.c:687) trace: BootDriver system32\drivers\usbccgp.sys DTE 80196DCC RegPath: \Registry\Machine\System\CurrentControlSet\Services\usbccgp
(../../boot/freeldr/freeldr/windows/winldr.c:687) trace: BootDriver system32\drivers\usbuhci.sys DTE 80196FFC RegPath: \Registry\Machine\System\CurrentControlSet\Services\usbuhci
(../../boot/freeldr/freeldr/windows/winldr.c:687) trace: BootDriver system32\drivers\usbohci.sys DTE 801970DC RegPath: \Registry\Machine\System\CurrentControlSet\Services\usbohci
(../../boot/freeldr/freeldr/windows/winldr.c:687) trace: BootDriver system32\drivers\usbehci.sys DTE 801971BC RegPath: \Registry\Machine\System\CurrentControlSet\Services\usbehci
(../../boot/freeldr/freeldr/windows/winldr.c:687) trace: BootDriver system32\drivers\usbhub.sys DTE 8019729C RegPath: \Registry\Machine\System\CurrentControlSet\Services\usbhub
(../../boot/freeldr/freeldr/windows/winldr.c:687) trace: BootDriver system32\drivers\uniata.sys DTE 8019737C RegPath: \Registry\Machine\System\CurrentControlSet\Services\uniata
(../../boot/freeldr/freeldr/windows/winldr.c:687) trace: BootDriver system32\drivers\buslogic.sys DTE 801975BC RegPath: \Registry\Machine\System\CurrentControlSet\Services\BusLogic
(../../boot/freeldr/freeldr/windows/winldr.c:687) trace: BootDriver system32\drivers\usbstor.sys DTE 8019769C RegPath: \Registry\Machine\System\CurrentControlSet\Services\usbstor
(../../boot/freeldr/freeldr/windows/winldr.c:687) trace: BootDriver system32\drivers\disk.sys DTE 8019777C RegPath: \Registry\Machine\System\CurrentControlSet\Services\Disk
(../../boot/freeldr/freeldr/windows/winldr.c:687) trace: BootDriver system32\drivers\ramdisk.sys DTE 801979A4 RegPath: \Registry\Machine\System\CurrentControlSet\Services\RamDisk
(../../boot/freeldr/freeldr/windows/winldr.c:687) trace: BootDriver system32\drivers\nmidebug.sys DTE 80197A84 RegPath: \Registry\Machine\System\CurrentControlSet\Services\NMIDebug
(../../boot/freeldr/freeldr/windows/winldr.c:687) trace: BootDriver system32\drivers\mup.sys DTE 80197B64 RegPath: \Registry\Machine\System\CurrentControlSet\Services\Mup
(../../boot/freeldr/freeldr/windows/winldr.c:687) trace: BootDriver system32\drivers\ndis.sys DTE 80197C34 RegPath: \Registry\Machine\System\CurrentControlSet\Services\Ndis
(../../boot/freeldr/freeldr/windows/winldr.c:706) trace: ArcDisk multi(0)disk(0)rdisk(0) checksum: 0xC313057F, signature: 0x22261DF0
(../../boot/freeldr/freeldr/windows/winldr.c:706) trace: ArcDisk multi(0)disk(0)rdisk(1) checksum: 0xF7794510, signature: 0xA7D5D12
(../../boot/freeldr/freeldr/windows/winldr.c:706) trace: ArcDisk multi(0)disk(0)rdisk(2) checksum: 0xC313057F, signature: 0x22261DF0
(../../boot/freeldr/freeldr/windows/winldr.c:706) trace: ArcDisk multi(0)disk(0)rdisk(3) checksum: 0xF7794510, signature: 0xA7D5D12
(../../ntoskrnl/kd/kdio.c:326) -----------------------------------------------------
(../../ntoskrnl/kd/kdio.c:327) ReactOS 0.4-SVN (Build 20120808-r57052)
(../../ntoskrnl/kd/kdio.c:329) 1 System Processor [0 MB Memory]
(../../ntoskrnl/kd/kdio.c:330) Command Line: /DEBUG /DEBUGPORT=COM1 /BAUDRATE=115200 /SOS
(../../ntoskrnl/kd/kdio.c:334) ARC Paths: multi(0)disk(0)rdisk(0)partition(1) \ multi(0)disk(0)rdisk(0)partition(1) \ReactOS\
(../../ntoskrnl/ke/i386/cpu.c:494) Supported CPU features : KF_V86_VIS KF_RDTSC KF_CR4 KF_CMOV KF_GLOBAL_PAGE KF_LARGE_PAGE KF_MTRR KF_CMPXCHG8B KF_MMX KF_WORKING_PTE KF_PAT KF_FXSR KF_FAST_SYSCALL KF_XMMI   KF_XMMI64  KF_NX_BIT
(../../ntoskrnl/ke/i386/cpu.c:801) Prefetch Cache: 64 bytes     L2 Cache: 0 bytes       L2 Cache Line: 64 bytes L2 Cache Associativity: 0
(../../hal/halx86/acpi/halacpi.c:782) ACPI Timer at: 4008h (EXT: 256)
(../../hal/halx86/acpi/halacpi.c:890) ACPI 2.0 Detected. Tables: [RSDT] [FACP]
(../../ntoskrnl/mm/ARM3/expool.c:925) EXPOOL: Pool Tracker Table at: 0xB12CA000 with 0xe01c bytes
(../../ntoskrnl/mm/ARM3/expool.c:927) EXPOOL: Big Pool Tracker Table at: 0xB12BA000 with 0x10000 bytes
(../../ntoskrnl/mm/ARM3/mminit.c:1430) HAL I/O Mapping at FFFE0000 is unsafe
(../../ntoskrnl/mm/mminit.c:262)           0x80000000 - 0x80C00000      Boot Loaded Image
(../../ntoskrnl/mm/mminit.c:266)           0xB0000000 - 0xB0301000      PFN Database
(../../ntoskrnl/mm/mminit.c:270)           0xB0301000 - 0xB12D9000      ARM3 Non Paged Pool
(../../ntoskrnl/mm/mminit.c:274)           0xBB000000 - 0xBD000000      System View Space
(../../ntoskrnl/mm/mminit.c:278)           0xBD000000 - 0xC0000000      Session Space
(../../ntoskrnl/mm/mminit.c:281)           0xC0000000 - 0xC03FFFFF      Page Tables
(../../ntoskrnl/mm/mminit.c:284)           0xC0300000 - 0xC0300FFF      Page Directories
(../../ntoskrnl/mm/mminit.c:287)           0xC0400000 - 0xC07FFFFF      Hyperspace
(../../ntoskrnl/mm/mminit.c:291)           0xE1000000 - 0xEDC00000      ARM3 Paged Pool
(../../ntoskrnl/mm/mminit.c:294)           0xEDC00000 - 0xF8BB8000      System PTE Space
(../../ntoskrnl/mm/mminit.c:297)           0xF8BB8000 - 0xFFBE0000      Non Paged Pool Expansion PTE Space
(../../ntoskrnl/mm/section.c:4865) Creating ARM3 section
ACPI Compatible Eisa/Isa HAL Detected
(../../ntoskrnl/io/pnpmgr/pnpmgr.c:3188) Firmware mapper is disabled
(../../ntoskrnl/io/pnpmgr/pnpreport.c:353) Reported device: DETECTEDInternal\ACPI_HAL (Root\ACPI_HAL\0)


ATAPI IDE MiniPort Driver (UniATA) v 0.42i2
 Parameter PrintLogo
 Parameter PrintLogo = 0x0
UniATA Init: OS should be ReactOS
UniATA Init: OS ver 4.1 (1), 1 CPU(s)
Performance calibration: dt=14995, counter=2054321
InitBadBlocks general
InitBadBlocks returned: 0xc0000034
UniataInitAtaCommands:
 Parameter SkipRaids
 Parameter SkipRaids = 0x1
 Parameter ForceSimplex
 Parameter ForceSimplex = 0x0
 Parameter LogToDisplay
 Parameter LogToDisplay = 0x0
HwInitializationDataSize = 50
set NeedPhysicalAddresses = TRUE
set AtapiAdapterControl() ptr


ATAPI IDE enum supported BusMaster Devices
 Parameter VirtualMachineType
 Parameter VirtualMachineType = 0x0
 Parameter VirtualBox
 Parameter VirtualBox = 0x0
-- BusID: 0x0:0x1:0x1
Storage Class
DevId = 269E8086 Class = 0001/0001, ProgIf 8A
 Parameter Include
 Parameter Include = 0x0
No force include, check exclude
 Parameter Exclude
 Parameter Exclude = 0x0
Default device
found, pass 0
InterruptPin = 0x0
InterruptLine = 0x0
Enabling Mem/Io spaces and busmastering...
Initial pciData.Command = 0x7
PCI_ENABLE_IO_SPACE
InterruptLine = 0x0
New pciData.Command = 0x7
PCI_ENABLE_MEMORY_SPACE
InterruptLine = 0x0
New pciData.Command = 0x7
PCI_ENABLE_BUS_MASTER
InterruptLine = 0x0
New pciData.Command = 0x7
Final pciData.Command = 0x7
Range 4 = 0xd001
count: BMListLen++
-- BusID: 0x0:0x4:0x0 - VirtualBox Guest Service
-- BusID: 0x0:0xd:0x0
Storage Class
DevId = 28298086 Class = 0001/0006, ProgIf 01
 Parameter Include
 Parameter Include = 0x0
No force include, check exclude
 Parameter Exclude
 Parameter Exclude = 0x0
Default device
found, pass 0
InterruptPin = 0x1
InterruptLine = 0x5
Enabling Mem/Io spaces and busmastering...
Initial pciData.Command = 0x7
PCI_ENABLE_IO_SPACE
InterruptLine = 0x5
New pciData.Command = 0x7
PCI_ENABLE_MEMORY_SPACE
InterruptLine = 0x5
New pciData.Command = 0x7
PCI_ENABLE_BUS_MASTER
InterruptLine = 0x5
New pciData.Command = 0x7
Final pciData.Command = 0x7
Range 0 = 0xd061
Range 1 = 0xd069
Range 2 = 0xd071
Range 3 = 0xd079
Range 4 = 0xd081
Range 5 = 0xf0804000
count: BMListLen++
-- BusID: 0x0:0x1:0x1
Storage Class
DevId = 269E8086 Class = 0001/0001, ProgIf 8A
 Parameter Include
 Parameter Include = 0x0
No force include, check exclude
 Parameter Exclude
 Parameter Exclude = 0x0
Default device
found, pass 1
InterruptPin = 0x0
InterruptLine = 0x0
Range 4 = 0xd001
found suitable device
 Parameter NativePCIMode
 Parameter NativePCIMode = 0x0
Add to BMList, AltInit 0
-- BusID: 0x0:0x4:0x0 - VirtualBox Guest Service
-- BusID: 0x0:0xd:0x0
Storage Class
DevId = 28298086 Class = 0001/0006, ProgIf 01
 Parameter Include
 Parameter Include = 0x0
No force include, check exclude
 Parameter Exclude
 Parameter Exclude = 0x0
Default device
found, pass 1
InterruptPin = 0x1
InterruptLine = 0x5
Range 0 = 0xd061
Range 1 = 0xd069
Range 2 = 0xd071
Range 3 = 0xd079
Range 4 = 0xd081
Range 5 = 0xf0804000
found suitable device
-- BusID: 0x0:0x1:0x1
Storage Class
DevId = 269E8086 Class = 0001/0001, ProgIf 8A
 Parameter Include
 Parameter Include = 0x0
No force include, check exclude
 Parameter Exclude
 Parameter Exclude = 0x0
Default device
found, pass 2
InterruptPin = 0x0
InterruptLine = 0x0
Range 4 = 0xd001
found suitable device
-- BusID: 0x0:0x4:0x0 - VirtualBox Guest Service
-- BusID: 0x0:0xd:0x0
Storage Class
DevId = 28298086 Class = 0001/0006, ProgIf 01
 Parameter Include
 Parameter Include = 0x0
No force include, check exclude
 Parameter Exclude
 Parameter Exclude = 0x0
Default device
found, pass 2
InterruptPin = 0x1
InterruptLine = 0x5
Range 0 = 0xd061
Range 1 = 0xd069
Range 2 = 0xd071
Range 3 = 0xd079
Range 4 = 0xd081
Range 5 = 0xf0804000
found suitable device
Add to BMList, AltInit 0
  BMListLen=2
adjust options for VirtualBox
 Parameter WaitBusyCount
 Parameter WaitBusyCount = 0x4e20
 Parameter WaitBusyDelay
 Parameter WaitBusyDelay = 0x96
 Parameter WaitDrqDelay
 Parameter WaitDrqDelay = 0x64
 Parameter WaitBusyLongCount
 Parameter WaitBusyLongCount = 0x4e20
 Parameter WaitBusyLongDelay
 Parameter WaitBusyLongDelay = 0xfa
 Parameter AtapiSendDisableIntr
 Parameter AtapiSendDisableIntr = 0x0
 Parameter AtapiDmaRawRead
 Parameter AtapiDmaRawRead = 0x0
 Parameter MaxIsrWait
 Parameter MaxIsrWait = 0xc8


ATAPI IDE: Look for legacy ISA-bridged PCI IDE controller (onboard)


ATAPI IDE: BMListLen 2
 Parameter IgnoreIsaCompatiblePci
 Parameter IgnoreIsaCompatiblePci = 0x0
 Parameter IgnoreIsaCompatiblePci
 Parameter IgnoreIsaCompatiblePci = 0x0
Try init channel 0, method 0
UniataFindBusMasterController: Context=0, BMListLen=2
ConfigInfo->Length 8c
AdapterInterfaceType: Isa
bm_offset 0, channel 0
AdapterInterfaceType=0x1
IoBusNumber=0x0
slotNumber=0x21
busDataRead
DevId = 269E8086 Class = 0001/0001
Storage Class
MasterDev (1)
UniataChipDetect:
HwFlags: 0x0
 Parameter ForceSimplex
 Parameter ForceSimplex = 0x0
i: 0x28
VendorID/DeviceID/Rev 0x8086/0x269e/0x0
i: 0x1f
HwFlags: 0x1000
 Parameter HwFlagsOverride
 Parameter HwFlagsOverride = 0x1000
HwFlagsOverride: 0x1000
 Parameter HwFlagsAdd
 Parameter HwFlagsAdd = 0x0
HwFlagsAdd: 0x0
HwFlags (final): 0x1000
MaxTransferMode: 0x45
 Parameter MaxTransferMode
 Parameter MaxTransferMode = 0x45
MaxTransferMode (overriden): 0x45
UniataChipDetectChannels:
MasterDev -> 1 chan
allocate 2 Luns for 1 channels
ForceSimplex = 0
HwFlags = 1000
 (0)HwFlags = 1000
 (1)HwFlags = 1000
 (2)found suitable device
HwFlags = 1000
 (3)Range 4 = 0xd001
IsBusMaster == TRUE
  AtapiGetIoRange:
  AtapiGetIoRange: rid 0x4, start 0x0, offs 0x0, len 0x8, mem 0x0
  AtapiGetIoRange: (2) 0xd000
  BusMasterAddress (base): 0xd000
AtapiReadChipConfig: devExt 0xb10612b4
AtapiReadChipConfig: dev 0x0, ph chan -1
 Parameter ForceSimplex
 Parameter ForceSimplex = 0x0
MaxTransferMode (base): 0x45
 Parameter MaxTransferMode
 Parameter MaxTransferMode = 0x45
MaxTransferMode (overriden): 0x45
 Parameter AtapiDmaZeroTransfer
 Parameter AtapiDmaZeroTransfer = 0x0
 Parameter AtapiDmaControlCmd
 Parameter AtapiDmaControlCmd = 0x0
 Parameter AtapiDmaRawRead
 Parameter AtapiDmaRawRead = 0x0
 Parameter AtapiDmaReadWrite
 Parameter AtapiDmaReadWrite = 0x1
AtapiChipInit: dev 0x0, ph chan -2
HwFlags: 0x1000
VendorID/DeviceID/Rev 0x8086/0x269e/0x0
AtapiChipInit: dev 0x0, ph chan 0
HwFlags: 0x1000
VendorID/DeviceID/Rev 0x8086/0x269e/0x0
simplexOnly = 0 (2)MasterDev (2)
1 channels & 1 irq for 1 controller
update ConfigInfo->nt4
using AtaReq sz 1000
update ConfigInfo->w2k
Reconstruct ConfigInfo
BMList[i].channel 0x0, NumberChannels 0x1, channel 0x0
de 0xb10612b4, Channel 0x0
chan = 0xb1061b30
AtapiSetupLunPtrs for channel 0 of 1, 2 luns
  Chan 0xb1061b30
  Lun 0x0
  Lun ptr 0xb12a9008
  Lun 0x1
  Lun ptr 0xb12a9310
AtapiReadChipConfig: devExt 0xb10612b4
AtapiReadChipConfig: dev 0x0, ph chan 0
 Parameter MaxTransferMode
 Parameter MaxTransferMode = 0x45
MaxTransferMode (overriden): 0x45
 Parameter ReorderEnable
 Parameter ReorderEnable = 0x1
 Parameter ReadCacheEnable
 Parameter ReadCacheEnable = 0x1
 Parameter WriteCacheEnable
 Parameter WriteCacheEnable = 0x1
 Parameter MaxTransferMode
 Parameter MaxTransferMode = 0x45
 Parameter PreferedTransferMode
 Parameter PreferedTransferMode = 0xffffffff
 Parameter ReadOnly
 Parameter ReadOnly = 0x0
 Parameter GeomType
 Parameter GeomType = 0xffffffff
 Parameter Hidden
 Parameter Hidden = 0x0
 Parameter ReadCacheEnable
 Parameter ReadCacheEnable = 0x1
 Parameter WriteCacheEnable
 Parameter WriteCacheEnable = 0x1
 Parameter MaxTransferMode
 Parameter MaxTransferMode = 0x45
 Parameter PreferedTransferMode
 Parameter PreferedTransferMode = 0xffffffff
 Parameter ReadOnly
 Parameter ReadOnly = 0x0
 Parameter GeomType
 Parameter GeomType = 0xffffffff
 Parameter Hidden
 Parameter Hidden = 0x0
set AccessRanges
Getting IO ranges
IO range 1 0x1f0
IO range 2 0x3f6
IDX_IO1 0->1f0(io)
IDX_IO2 10->3f6(io)
IDX_BM_IO 14->d000(io)
IDX_SATA_IO 19->0(io)
  AltStatus (0x50)
  Reg_0x1 (0x1f1) = 0x0
  Reg_0x2 (0x1f2) = 0x1
  Reg_0x3 (0x1f3) = 0x60
  Reg_0x4 (0x1f4) = 0x0
  Reg_0x5 (0x1f5) = 0x0
  Reg_0x6 (0x1f6) = 0xe0
  Reg_0x7 (0x1f7) = 0x50
  BM_0x0 (0xd000) = 0x0
  BM_0x1 (0xd001) = 0xff
  BM_0x2 (0xd002) = 0x60
  BM_0x3 (0xd003) = 0xff
claim Compatible controller
claim Primary
AtapiDmaAlloc: allocate tmp buffers below 4Gb
exit: init spinlock
MasterDev=0x1, NumberChannels=0x1, Isr2DevObj=0x0
Init ISR:
Unnecessary
MasterDev=0x1, NumberChannels=0x1, Isr2DevObj=0x0
return SP_RETURN_FOUND
Attempt 0 of MasterDev ok
(../../ntoskrnl/io/iomgr/iorsrce.c:882) IoReportResourceUsage is halfplemented!
AtapiHwInitialize: (base)
AtapiChipInit: dev 0xffffffff, ph chan -1
HwFlags: 0x1000
VendorID/DeviceID/Rev 0x8086/0x269e/0x0
AtapiChipInit: dev 0xffffffff, ph chan 0
HwFlags: 0x1000
VendorID/DeviceID/Rev 0x8086/0x269e/0x0
FindDevices:
AtapiDisableInterrupts_0: 0
  max_ldev 2
CheckDevice: Device 0x0
CheckDevice: reset dev
AtapiSoftReset:
  statusByte2 50:
  DMA status 0x60
  HDD at home
  HDD at home
CheckDevice: status 0x41
CheckDevice: IDE device check
IssueIdentify: Checking for IDE. Status (0x50)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xec, lba 0x20000 count 0x0 feature 0x0
IssueIdentify: IDE_STATUS_DRQ (0x58)
IssueIdentify: Status before read words 0x58
IssueIdentify: statusByte 0x58
IssueIdentify: BASE statusByte 0x58
  use 16bit IO
IssueIdentify: suck data port
IssueIdentify: statusByte 0x50
IssueIdentify: statusByte 0x50
IssueIdentify: Status after read words 0x50
Model: BVXOH RADDSI K
FW:    .1 0
S/N:   BV02d632872-baa45e 7
Pio:   0
APio:  3
SWDMA: 0
MWDMA: 0
UDMA:  4
SATA:  0
SATA support: 0, CAPs 0x0
CHS 0x2082:0x10:0x3f
NumOfSectors 0x7fffe0
SupportLba flag 0x1
MajorRevision 0x7e
UserAddressableSectors 0x800000
LBA mode
Use IDE_COMMAND_READ_NATIVE_SIZE
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xf8, lba 0x0 count 0x0 feature 0x0
  Status 0x40
NativeNumOfSectors 0x7fffff
Use IDE_COMMAND_SET_NATIVE_SIZE
Update NumOfSectors to 0x7fffff
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xf9, lba 0x7fffff count 0x0 feature 0x0
  Status 0x41
requested LunExt->GeomType=ffffffff
tmp_cylinders = 0x2082
final LunExt->opt_GeomType=2
cylinders = tmp_cylinders (0 = 0)
Geometry: C 0x2082 (0x2082)
Geometry: H 0x10 (0x10)
Geometry: S 0x3f (0x3f)
InitBadBlocks local
LunExt 0xb12a9008
S/N:VBOX_HARDDISK___________________________-VB206d2378-2ab4ae57_
IssueIdentify: Device does not interrupt on assertion of DRQ.
IssueIdentify: hard drive.
IssueIdentify: final Status on exit (0x41)
CheckDevice: Device 0x0 is IDE
CheckDevice: check status: found
CheckDevice: Device 0x1
CheckDevice: reset dev
AtapiSoftReset:
  statusByte2 41:
  DMA status 0x60
  ATAPI at home
  ATAPI at home
CheckDevice: status 0x0
CheckDevice: ATAPI signature found
IssueIdentify: Checking for ATAPI. Status (0x0)
IssueIdentify: Checking for ATAPI (2). Status (0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x1, cmd 0xa1, lba 0x20000 count 0x0 feature 0x0
IssueIdentify: IDE_STATUS_DRQ (0x58)
IssueIdentify: Status before read words 0x58
IssueIdentify: statusByte 0x58
IssueIdentify: BASE statusByte 0x58
  use 16bit IO
IssueIdentify: suck data port
IssueIdentify: statusByte 0x50
IssueIdentify: statusByte 0x50
IssueIdentify: Status after read words 0x50
Model: BVXOC -DOR M
FW:    .1 0
S/N:   BV-1100f306f
Pio:   0
APio:  3
SWDMA: 0
MWDMA: 0
UDMA:  4
SATA:  0
SATA support: 0, CAPs 0x0
InitBadBlocks local
LunExt 0xb12a9310
S/N:VBOX_CD-ROM_____________________________-VB1-01f003f6________
IssueIdentify: Device does not interrupt on assertion of DRQ.
IssueIdentify: Device is CD/Optical drive.
IssueIdentify: final Status on exit (0x50)
CheckDevice: Device 0x1 is ATAPI
CheckDevice: check status: found
FindDevices: select 0 dev to clear INTR
FindDevices: statusByte=0x41
FindDevices: select 1 dev to clear INTR
FindDevices: statusByte=0x50
FindDevices: select 0 dev on exit
AtapiEnableInterrupts_0: 1
FindDevices: returning 1
AtapiHwInitialize: lChannel 0x0, dev 0
AtapiDisableInterrupts_0: 0
AtapiHwInitialize: IDE branch
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc6, lba 0x0 count 0x80 feature 0x0
  Status 0x40
AtapiHwInitialize: Using Multiblock on Device 0. Blocks / int - 128
  Try Enable Read Cache
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xef, lba 0x0 count 0x0 feature 0xaa
  Status 0x50
  Try Enable Write Cache
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xef, lba 0x0 count 0x0 feature 0x2
  Status 0x50
  try mode 0x45
AtapiDmaInit__: Set (U)DMA on Device 0
AtapiDmaInit: deviceExtension->MaxTransferMode >= ATA_UDMA
AtapiDmaInit: LunExt->LimitedTransferMode 0x45
AtapiDmaInit: LunExt->MaxTransferMode >= ATA_UDMA   =>   0x5
Setup chip a:w:u=4:2:5
AtaSetTransferMode: Set 0x45 on Device 0/0
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xef, lba 0x0 count 0x45 feature 0x3
  Status 0x50
Using 0x45 mode
AtapiEnableInterrupts_0: 1
AtapiHwInitialize: lChannel 0x0, dev 1
AtapiDisableInterrupts_0: 0
AtapiHwInitialize: ATAPI/Changer branch
  try mode 0x45
AtapiDmaInit__: Set (U)DMA on Device 1
AtapiDmaInit: deviceExtension->MaxTransferMode >= ATA_UDMA
AtapiDmaInit: LunExt->LimitedTransferMode 0x45
AtapiDmaInit: LunExt->MaxTransferMode >= ATA_UDMA   =>   0x5
Setup chip a:w:u=4:2:5
AtaSetTransferMode: Set 0x45 on Device 0/1
AtaCommand48: cntrlr 0x0:0x0 dev 0x1, cmd 0xef, lba 0x0 count 0x45 feature 0x3
  Status 0x50
Using 0x45 mode
AtapiEnableInterrupts_0: 1
AtapiHwInitialize: (base) done
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xf88c8e2c, CDB 0xf88c8e5c, AtaReq 0xb1298000, SCmd 0x12
UniataNeedQueueing: TopLevel, qd=0
Send to device 12
TopLevel (2), srb 0xf88c8e2c
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8b98
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_INQUIRY PATH:LUN:TID = 0x0:0x0:0x0
IdeSendCommand: SCSIOP_INQUIRY ok
  HDD at home
RelativeAddressing
IdeSendCommand: REQ_STATE_TRANSFER_COMPLETE
AtapiStartIo: Srb 0xf88c8e2c complete with status 0x1
AtapiStartIo: AtapiDmaDBSync(b1061b30, f88c8e2c)
AtapiStartIo: UniataRemoveRequest(b1061b30, f88c8e2c)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan b1061b30, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x1:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
AtapiStartIo: SRB rejected
SRB_STATUS_SELECTION_TIMEOUT
AtapiStartIo: Srb 0xf88c8e2c complete with status 0xa
AtapiStartIo: AtapiDmaDBSync(0, f88c8e2c)
AtapiStartIo: UniataRemoveRequest(0, f88c8e2c)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan 0, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xf88c8e2c, CDB 0xf88c8e5c, AtaReq 0xb1298000, SCmd 0x12
UniataNeedQueueing: TopLevel, qd=0
Send to device 12
TopLevel (2), srb 0xf88c8e2c
TopLevel (3), AtaReq 0xb1298000
Try ATAPI send 12
AtapiSendCommand: req state 0x10, Action 3
AtapiSendCommand: BuildMechanismStatusSrb()
 MechanismStatusSrb 0xb1061b6c
AtapiSendCommand: AtapiSendCommand recursive
AtapiSendCommand: req state 0x20, Action 3
AtapiSendCommand: prepare..., ATAPI CMD bd (Cdb b1061b9c)
  assume IN
AtapiSendCommand: use_dma=0, Cmd bd
AtapiSendCommand: AtapiDmaReinit()
AtapiDmaReinit: !(AtaReq->Flags & REQ_FLAG_DMA_OPERATION), fall to PIO on Device 1
AtapiDmaReinit: set PIO mode on Device 1 (45 -> c)
AtapiDmaInit: deviceExtension->MaxTransferMode >= ATA_UDMA
AtapiDmaInit: LunExt->LimitedTransferMode 0x45
AtapiDmaInit: LunExt->MaxTransferMode >= ATA_UDMA   =>   0xffffffff
Setup chip a:w:u=4:-1:-1
AtaSetTransferMode: Set 0xc on Device 0/1
AtaCommand48: cntrlr 0x0:0x0 dev 0x1, cmd 0xef, lba 0x0 count 0xc feature 0x3
  Status 0x50
AtapiSendCommand: use_dma=0
AtapiSendCommand: CMD_ACTION_EXEC
AtapiSendCommand: Cdb b1061b9c Command 0xbd to TargetId 1 lun 0
AtapiSendCommand: Entered with status 0x50
AtapiSendCommand: Entry Status (0x50)
AtapiSendCommand: Poll for int. to send packet. Status (0x50)
AtapiSendCommand: status (0x58)
AtapiSendCommand: ExpectingInterrupt (0x1)
AtapiSendCommand: return SRB_STATUS_PENDING (3)
AtapiSendCommand: SRB_STATUS_PENDING (2)
AtapiStartIo: next Srb f88c8e2c
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x64
  perform generic check
  clear unexpected DMA intr
AtapiDmaDone: dev -1
  getting status...
  ATAPI status 0x58
  base status 0x58
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  dev_type ATAPI
  OldReqState = 42
  continue service interrupt
AtapiInterrupt: ATAPI Entered with status (0x58)
AtapiInterrupt: iReason 2
AtapiInterrupt: ATAPI branch
AtapiInterrupt: iReason 2
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: get R wordCount 0x4
IdeIntr: Read 0x4 words
IdeIntr: PIO Read AtaReq->DataBuffer 0xb1061b4c, srb->DataBuffer 0xb1061b4c
  status re-check 0x50
AtapiInterrupt: all transferred, AtaReq->WordsLeft == 0
AtapiInterrupt: early complete ? status 50
AtapiInterrupt: CompleteRequest, srbstatus 1
AtapiInterrupt: OriginalSrb != NULL
AtapiInterrupt: SCSIOP_MECHANISM_STATUS status 0x1
AtapiSendCommand: req state 0x50, Action 3
AtapiSendCommand: prepare..., ATAPI CMD 12 (Cdb f88c8e5c)
  assume IN
AtapiSendCommand: use_dma=0, Cmd 12
AtapiSendCommand: AtapiDmaReinit()
AtapiDmaReinit: !(AtaReq->Flags & REQ_FLAG_DMA_OPERATION), fall to PIO on Device 1
AtapiSendCommand: use_dma=0
AtapiSendCommand: CMD_ACTION_EXEC
AtapiSendCommand: Cdb f88c8e5c Command 0x12 to TargetId 1 lun 0
AtapiSendCommand: Entered with status 0x50
AtapiSendCommand: Entry Status (0x50)
AtapiSendCommand: Poll for int. to send packet. Status (0x50)
AtapiSendCommand: status (0x58)
AtapiSendCommand: ExpectingInterrupt (0x1)
AtapiSendCommand: return SRB_STATUS_PENDING (3)
AtapiInterrupt: chan->ExpectingInterrupt 1 (1)
AtapiInterrupt: send orig SRB_STATUS_PENDING (1)
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x4
  perform generic check
  clear unexpected DMA intr
AtapiDmaDone: dev -1
  getting status...
  ATAPI status 0x58
  base status 0x58
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  dev_type ATAPI
  OldReqState = 42
  continue service interrupt
AtapiInterrupt: ATAPI Entered with status (0x58)
AtapiInterrupt: iReason 2
AtapiInterrupt: ATAPI branch
AtapiInterrupt: iReason 2
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: get R wordCount 0x12
IdeIntr: Read 0x12 words
IdeIntr: PIO Read AtaReq->DataBuffer 0xf885d3e8, srb->DataBuffer 0xf885d3e8
  status re-check 0x50
AtapiInterrupt: all transferred, AtaReq->WordsLeft == 0
AtapiInterrupt: early complete ? status 50
AtapiInterrupt: CompleteRequest, srbstatus 1
AtapiInterrupt: PIO completion
AtapiInterrupt: PIO completion, wait BUSY
IdeIntr: ATAPI Read AtaReq->DataBuffer 0xf885d40c, srb->DataBuffer 0xf885d3e8, len 0x24
   Transfered 0, full size 24
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xf88c8e2c, status 1
AtapiInterrupt: RequestComplete, srb 0xf88c8e2c
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x4
  perform generic check
  clear unexpected DMA intr
AtapiDmaDone: dev -1
  getting status...
  ATAPI status 0x50
  base status 0x50
  Unexpected interrupt.
  ATAPI additional check
AtapiCheckInterrupt__: ATAPI int reason 3
AtapiInterrupt(base): Catch unexpected
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x1:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
AtapiStartIo: SRB rejected
SRB_STATUS_SELECTION_TIMEOUT
AtapiStartIo: Srb 0xf88c8e2c complete with status 0xa
AtapiStartIo: AtapiDmaDBSync(0, f88c8e2c)
AtapiStartIo: UniataRemoveRequest(0, f88c8e2c)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan 0, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x1:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
AtapiStartIo: Communication port
  INQUIRY
AtapiStartIo: Srb 0xf88c8e2c complete with status 0x1
AtapiStartIo: AtapiDmaDBSync(0, f88c8e2c)
AtapiStartIo: UniataRemoveRequest(0, f88c8e2c)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan 0, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x1:0x1:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
AtapiStartIo: SRB rejected
SRB_STATUS_SELECTION_TIMEOUT
AtapiStartIo: Srb 0xf88c8e2c complete with status 0xa
AtapiStartIo: AtapiDmaDBSync(0, f88c8e2c)
AtapiStartIo: UniataRemoveRequest(0, f88c8e2c)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan 0, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x1:0x0:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
AtapiStartIo: SRB rejected
SRB_STATUS_SELECTION_TIMEOUT
AtapiStartIo: Srb 0xf88c8e2c complete with status 0xa
AtapiStartIo: AtapiDmaDBSync(0, f88c8e2c)
AtapiStartIo: UniataRemoveRequest(0, f88c8e2c)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan 0, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
ScsiPortInitialize Status 0x0
 Parameter IgnoreIsaCompatiblePci
 Parameter IgnoreIsaCompatiblePci = 0x0
Try init channel 1, method 0
UniataFindBusMasterController: Context=0, BMListLen=2
ConfigInfo->Length 8c
AdapterInterfaceType: Isa
bm_offset 8, channel 1
AdapterInterfaceType=0x1
IoBusNumber=0x0
slotNumber=0x21
busDataRead
DevId = 269E8086 Class = 0001/0001
Storage Class
MasterDev (1)
UniataChipDetect:
HwFlags: 0x0
 Parameter ForceSimplex
 Parameter ForceSimplex = 0x0
i: 0x28
VendorID/DeviceID/Rev 0x8086/0x269e/0x0
i: 0x1f
HwFlags: 0x1000
 Parameter HwFlagsOverride
 Parameter HwFlagsOverride = 0x1000
HwFlagsOverride: 0x1000
 Parameter HwFlagsAdd
 Parameter HwFlagsAdd = 0x0
HwFlagsAdd: 0x0
HwFlags (final): 0x1000
MaxTransferMode: 0x45
 Parameter MaxTransferMode
 Parameter MaxTransferMode = 0x45
MaxTransferMode (overriden): 0x45
UniataChipDetectChannels:
MasterDev -> 1 chan
allocate 2 Luns for 1 channels
ForceSimplex = 0
HwFlags = 1000
 (0)HwFlags = 1000
 (1)HwFlags = 1000
 (2)found suitable device
HwFlags = 1000
 (3)Range 4 = 0xd001
IsBusMaster == TRUE
  AtapiGetIoRange:
  AtapiGetIoRange: rid 0x4, start 0x0, offs 0x8, len 0x8, mem 0x0
  AtapiGetIoRange: (2) 0xd008
  BusMasterAddress (base): 0xd008
AtapiReadChipConfig: devExt 0xb12977f4
AtapiReadChipConfig: dev 0x0, ph chan -1
 Parameter ForceSimplex
 Parameter ForceSimplex = 0x0
MaxTransferMode (base): 0x45
 Parameter MaxTransferMode
 Parameter MaxTransferMode = 0x45
MaxTransferMode (overriden): 0x45
 Parameter AtapiDmaZeroTransfer
 Parameter AtapiDmaZeroTransfer = 0x0
 Parameter AtapiDmaControlCmd
 Parameter AtapiDmaControlCmd = 0x0
 Parameter AtapiDmaRawRead
 Parameter AtapiDmaRawRead = 0x0
 Parameter AtapiDmaReadWrite
 Parameter AtapiDmaReadWrite = 0x1
AtapiChipInit: dev 0x0, ph chan -2
HwFlags: 0x1000
VendorID/DeviceID/Rev 0x8086/0x269e/0x0
AtapiChipInit: dev 0x0, ph chan 0
HwFlags: 0x1000
VendorID/DeviceID/Rev 0x8086/0x269e/0x0
simplexOnly = 0 (2)MasterDev (2)
1 channels & 1 irq for 1 controller
update ConfigInfo->nt4
using AtaReq sz 1000
update ConfigInfo->w2k
Reconstruct ConfigInfo
BMList[i].channel 0x1, NumberChannels 0x1, channel 0x1
de 0xb12977f4, Channel 0x1
chan = 0xb1296008
AtapiSetupLunPtrs for channel 0 of 1, 2 luns
  Chan 0xb1296008
  Lun 0x0
  Lun ptr 0xb103d008
  Lun 0x1
  Lun ptr 0xb103d310
AtapiReadChipConfig: devExt 0xb12977f4
AtapiReadChipConfig: dev 0x0, ph chan 1
 Parameter MaxTransferMode
 Parameter MaxTransferMode = 0x45
MaxTransferMode (overriden): 0x45
 Parameter ReorderEnable
 Parameter ReorderEnable = 0x1
 Parameter ReadCacheEnable
 Parameter ReadCacheEnable = 0x1
 Parameter WriteCacheEnable
 Parameter WriteCacheEnable = 0x1
 Parameter MaxTransferMode
 Parameter MaxTransferMode = 0x45
 Parameter PreferedTransferMode
 Parameter PreferedTransferMode = 0xffffffff
 Parameter ReadOnly
 Parameter ReadOnly = 0x0
 Parameter GeomType
 Parameter GeomType = 0xffffffff
 Parameter Hidden
 Parameter Hidden = 0x0
 Parameter ReadCacheEnable
 Parameter ReadCacheEnable = 0x1
 Parameter WriteCacheEnable
 Parameter WriteCacheEnable = 0x1
 Parameter MaxTransferMode
 Parameter MaxTransferMode = 0x45
 Parameter PreferedTransferMode
 Parameter PreferedTransferMode = 0xffffffff
 Parameter ReadOnly
 Parameter ReadOnly = 0x0
 Parameter GeomType
 Parameter GeomType = 0xffffffff
 Parameter Hidden
 Parameter Hidden = 0x0
set AccessRanges
cheat ScsiPort for 2nd channel, BM io-range
Getting IO ranges
IO range 1 0x170
IO range 2 0x376
IDX_IO1 0->170(io)
IDX_IO2 10->376(io)
IDX_BM_IO 14->d008(io)
IDX_SATA_IO 19->0(io)
  AltStatus (0x50)
  Reg_0x1 (0x171) = 0x0
  Reg_0x2 (0x172) = 0x1
  Reg_0x3 (0x173) = 0x1
  Reg_0x4 (0x174) = 0x0
  Reg_0x5 (0x175) = 0x0
  Reg_0x6 (0x176) = 0xe0
  Reg_0x7 (0x177) = 0x50
  BM_0x0 (0xd008) = 0x0
  BM_0x1 (0xd009) = 0xff
  BM_0x2 (0xd00a) = 0x20
  BM_0x3 (0xd00b) = 0xff
claim Compatible controller
claim Secondary
AtapiDmaAlloc: allocate tmp buffers below 4Gb
exit: init spinlock
MasterDev=0x1, NumberChannels=0x1, Isr2DevObj=0x0
Init ISR:
Unnecessary
MasterDev=0x1, NumberChannels=0x1, Isr2DevObj=0x0
return SP_RETURN_FOUND
Attempt 0 of MasterDev ok
(../../ntoskrnl/io/iomgr/iorsrce.c:882) IoReportResourceUsage is halfplemented!
AtapiHwInitialize: (base)
AtapiChipInit: dev 0xffffffff, ph chan -1
HwFlags: 0x1000
VendorID/DeviceID/Rev 0x8086/0x269e/0x0
AtapiChipInit: dev 0xffffffff, ph chan 0
HwFlags: 0x1000
VendorID/DeviceID/Rev 0x8086/0x269e/0x0
FindDevices:
AtapiDisableInterrupts_0: 0
  max_ldev 2
CheckDevice: Device 0x0
CheckDevice: reset dev
AtapiSoftReset:
  statusByte2 50:
  DMA status 0x20
  HDD at home
  HDD at home
CheckDevice: status 0x41
CheckDevice: IDE device check
IssueIdentify: Checking for IDE. Status (0x50)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xec, lba 0x20000 count 0x0 feature 0x0
IssueIdentify: IDE_STATUS_DRQ (0x58)
IssueIdentify: Status before read words 0x58
IssueIdentify: statusByte 0x58
IssueIdentify: BASE statusByte 0x58
  use 16bit IO
IssueIdentify: suck data port
IssueIdentify: statusByte 0x50
IssueIdentify: statusByte 0x50
IssueIdentify: Status after read words 0x50
Model: BVXOH RADDSI K
FW:    .1 0
S/N:   BV4d34cd6e7-35a6af b
Pio:   0
APio:  3
SWDMA: 0
MWDMA: 0
UDMA:  4
SATA:  0
SATA support: 0, CAPs 0x0
CHS 0x3fff:0x10:0x3f
NumOfSectors 0xfbfc10
NumberOfCylinders == 0x3fff
cylinders 0x4104
NumOfSectors 0xffffc0
SupportLba flag 0x1
MajorRevision 0x7e
UserAddressableSectors 0x1000000
LBA mode
Use IDE_COMMAND_READ_NATIVE_SIZE
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xf8, lba 0x0 count 0x0 feature 0x0
  Status 0x40
NativeNumOfSectors 0xffffff
Use IDE_COMMAND_SET_NATIVE_SIZE
Update NumOfSectors to 0xffffff
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xf9, lba 0xffffff count 0x0 feature 0x0
  Status 0x41
requested LunExt->GeomType=ffffffff
tmp_cylinders = 0x4104
final LunExt->opt_GeomType=2
Geometry: C 0x4104 (0x4104)
Geometry: H 0x10 (0x10)
Geometry: S 0x3f (0x3f)
InitBadBlocks local
LunExt 0xb103d008
S/N:VBOX_HARDDISK___________________________-VBd443dce6-7536afab_
IssueIdentify: Device does not interrupt on assertion of DRQ.
IssueIdentify: hard drive.
IssueIdentify: final Status on exit (0x41)
CheckDevice: Device 0x0 is IDE
CheckDevice: check status: found
CheckDevice: Device 0x1
CheckDevice: reset dev
AtapiSoftReset:
  statusByte2 41:
  DMA status 0x20
  nobody home! 0x0 != 0x55
FindDevices: select 0 dev to clear INTR
FindDevices: statusByte=0x41
FindDevices: select 1 dev to clear INTR
FindDevices: statusByte=0x0
FindDevices: select 0 dev on exit
AtapiEnableInterrupts_0: 1
FindDevices: returning 1
AtapiHwInitialize: lChannel 0x0, dev 0
AtapiDisableInterrupts_0: 0
AtapiHwInitialize: IDE branch
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc6, lba 0x0 count 0x80 feature 0x0
  Status 0x40
AtapiHwInitialize: Using Multiblock on Device 0. Blocks / int - 128
  Try Enable Read Cache
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xef, lba 0x0 count 0x0 feature 0xaa
  Status 0x50
  Try Enable Write Cache
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xef, lba 0x0 count 0x0 feature 0x2
  Status 0x50
  try mode 0x45
AtapiDmaInit__: Set (U)DMA on Device 0
AtapiDmaInit: deviceExtension->MaxTransferMode >= ATA_UDMA
AtapiDmaInit: LunExt->LimitedTransferMode 0x45
AtapiDmaInit: LunExt->MaxTransferMode >= ATA_UDMA   =>   0x5
Setup chip a:w:u=4:2:5
AtaSetTransferMode: Set 0x45 on Device 0/0
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xef, lba 0x0 count 0x45 feature 0x3
  Status 0x50
Using 0x45 mode
AtapiEnableInterrupts_0: 1
AtapiHwInitialize: lChannel 0x0, dev 1
AtapiHwInitialize: (base) done
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xf88c8e2c, CDB 0xf88c8e5c, AtaReq 0xb100c000, SCmd 0x12
UniataNeedQueueing: TopLevel, qd=0
Send to device 12
TopLevel (2), srb 0xf88c8e2c
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8b98
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_INQUIRY PATH:LUN:TID = 0x0:0x0:0x0
IdeSendCommand: SCSIOP_INQUIRY ok
  HDD at home
RelativeAddressing
IdeSendCommand: REQ_STATE_TRANSFER_COMPLETE
AtapiStartIo: Srb 0xf88c8e2c complete with status 0x1
AtapiStartIo: AtapiDmaDBSync(b1296008, f88c8e2c)
AtapiStartIo: UniataRemoveRequest(b1296008, f88c8e2c)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan b1296008, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x1:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
AtapiStartIo: SRB rejected
SRB_STATUS_SELECTION_TIMEOUT
AtapiStartIo: Srb 0xf88c8e2c complete with status 0xa
AtapiStartIo: AtapiDmaDBSync(0, f88c8e2c)
AtapiStartIo: UniataRemoveRequest(0, f88c8e2c)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan 0, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
UniataNeedQueueing: TopLevel, qd=0
Send to device 12
TopLevel (2), srb 0xf88c8e2c
TopLevel (3), AtaReq 0xb100c000
  nobody home! 0x0 != 0x55
AtapiStartIo: SRB rejected
SRB_STATUS_SELECTION_TIMEOUT
AtapiStartIo: Srb 0xf88c8e2c complete with status 0xa
AtapiStartIo: AtapiDmaDBSync(b1296008, f88c8e2c)
AtapiStartIo: UniataRemoveRequest(b1296008, f88c8e2c)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan b1296008, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x1:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
AtapiStartIo: Communication port
  INQUIRY
AtapiStartIo: Srb 0xf88c8e2c complete with status 0x1
AtapiStartIo: AtapiDmaDBSync(0, f88c8e2c)
AtapiStartIo: UniataRemoveRequest(0, f88c8e2c)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan 0, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x1:0x1:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
AtapiStartIo: SRB rejected
SRB_STATUS_SELECTION_TIMEOUT
AtapiStartIo: Srb 0xf88c8e2c complete with status 0xa
AtapiStartIo: AtapiDmaDBSync(0, f88c8e2c)
AtapiStartIo: UniataRemoveRequest(0, f88c8e2c)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan 0, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x1:0x0:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
AtapiStartIo: SRB rejected
SRB_STATUS_SELECTION_TIMEOUT
AtapiStartIo: Srb 0xf88c8e2c complete with status 0xa
AtapiStartIo: AtapiDmaDBSync(0, f88c8e2c)
AtapiStartIo: UniataRemoveRequest(0, f88c8e2c)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan 0, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
ScsiPortInitialize Status 0x0
Ok, no more retries required
!BMList[i].MasterDev


ATAPI IDE: Look for PCI IDE controller


ATAPI IDE: i 1, BMListLen 2
 Parameter IgnoreNativePci
 Parameter IgnoreNativePci = 0x0
Try init 8086 2829
(../../hal/halx86/legacy/bus/pcibus.c:719) WARNING: PCI Slot Resource Assignment is FOOBAR
UniataFindBusMasterController: Context=1, BMListLen=2
ConfigInfo->Length 8c
bm_offset 0, channel 0
AdapterInterfaceType=0x5
IoBusNumber=0x0
slotNumber=0xd
busDataRead
DevId = 28298086 Class = 0001/0006
Storage Class
UniataChipDetect:
HwFlags: 0x0
 Parameter ForceSimplex
 Parameter ForceSimplex = 0x0
i: 0x28
VendorID/DeviceID/Rev 0x8086/0x2829/0x2
i: 0x2a
HwFlags: 0x12000000
 Parameter HwFlagsOverride
 Parameter HwFlagsOverride = 0x12000000
HwFlagsOverride: 0x12000000
 Parameter HwFlagsAdd
 Parameter HwFlagsAdd = 0x0
HwFlagsAdd: 0x0
HwFlags (final): 0x12000000
MaxTransferMode: 0x48
 Parameter MaxTransferMode
 Parameter MaxTransferMode = 0x48
MaxTransferMode (overriden): 0x48
  UniataAhciDetect:
 Parameter IgnoreAhci
 Parameter IgnoreAhci = 0x0
  AtapiGetIoRange:
  AtapiGetIoRange: rid 0x5, start 0xf0804000, offs 0x0, len 0x10, mem 0x1
  AtapiGetIoRange: 0xf885d000
MemIo
  AHCI Base: 0xf885d000 MemIo 1 Proc 0
  AHCI_0x0 (0xf885d000) = 0xc8241f80
  AHCI_0x4 (0xf885d004) = 0x80000000
  AHCI_0x8 (0xf885d008) = 0x0
  AHCI_0xc (0xf885d00c) = 0x1
  AHCI_0x10 (0xf885d010) = 0x10100
  check AHCI mode, GHC 0x80000000
  AHCI CAP 0xc8241f80, CAP2 0x0
  64bit  NCQ  CCC
  AHCI PI 0x1
  CommandSlots 31
  Channels 1
  AHCI version 0x1.10 controller with 1 ports (mask 0x1) detected
  AHCI SATA Gen 2
  PM not supported -> 1 lun/chan
allocate 1 Luns for 1 channels
Intel chip config: 40
try run AHCI
ForceSimplex = 0
HwFlags = 12000000
 (0)HwFlags = 12000000
 (1)HwFlags = 12000000
 (2)found suitable device
HwFlags = 12000000
 (3)  AHCI registers layout
AtapiReadChipConfig: devExt 0xb100b7f4
AtapiReadChipConfig: dev 0x1, ph chan -1
 Parameter ForceSimplex
 Parameter ForceSimplex = 0x0
MaxTransferMode (base): 0x48
 Parameter MaxTransferMode
 Parameter MaxTransferMode = 0x48
MaxTransferMode (overriden): 0x48
 Parameter AtapiDmaZeroTransfer
 Parameter AtapiDmaZeroTransfer = 0x0
 Parameter AtapiDmaControlCmd
 Parameter AtapiDmaControlCmd = 0x0
 Parameter AtapiDmaRawRead
 Parameter AtapiDmaRawRead = 0x0
 Parameter AtapiDmaReadWrite
 Parameter AtapiDmaReadWrite = 0x1
AtapiChipInit: dev 0x1, ph chan -2
HwFlags: 0x12000000
VendorID/DeviceID/Rev 0x8086/0x2829/0x2
  UniataAhciInit:
  AHCI Base: 0xf885d000 MemIo 1 Proc 0
  AHCI_0x0 (0xf885d000) = 0xc8241f80
  AHCI_0x4 (0xf885d004) = 0x80000000
  AHCI_0x8 (0xf885d008) = 0x0
  AHCI_0xc (0xf885d00c) = 0x1
  AHCI_0x10 (0xf885d010) = 0x10100
  reset AHCI controller, GHC 0x80000000
  AHCI GHC 0x80000000
  enable AHCI mode, GHC 0x80000000
  AHCI GHC 0x80000000
  AHCI CAP 0xc8241f80
  AHCI 64bit
  AHCI 31 CMD slots
  AHCI legasy SATA
  AHCI PI 0x1
  SATA Gen 2
  chan 0, offs 0x100
AtapiSetupLunPtrs for channel 0 of 1, 1 luns
  Chan 0xb100ab30
  Lun 0x0
  Lun ptr 0xb100a008
  AtaReq 0xb1293000: cmd aligned b1293080, d=28
  ahci_cmd_ptr 0xb1293080
AtapiDmaAlloc: AHCI
AtapiDmaAlloc: CLP BASE b1291000
AtapiDmaAlloc: CLP BASE 1k-aligned b1291000
AtapiDmaAlloc: CLP Phys BASE 1f90000
UniataAhciResume: lChan 0
WriteChannelPort4 0 => ch0[14]
  AHCI CLB setup
WriteChannelPort4 1f90000 => ch0[0]
WriteChannelPort4 0 => ch0[4]
  AHCI RCV FIS setup
WriteChannelPort4 1f90400 => ch0[8]
WriteChannelPort4 0 => ch0[c]
WriteChannelPort4 10000006 => ch0[18]
UniataAhciStartFR: lChan 0
ReadChannelPort4 ch0[18] = 10000006
  CMD 0x10000006
WriteChannelPort4 10000016 => ch0[18]
UniataAhciStart: lChan 0
ReadChannelPort4 ch0[10] = 0
WriteChannelPort4 0 => ch0[10]
    SError 0x0, IS 0x0
ReadChannelPort4 ch0[18] = 10004016
  CMD 0x10004016
WriteChannelPort4 10004017 => ch0[18]
  AHCI port 0 Base: 0xf885d100 MemIo 1 Proc 0
  AHCI0_0x0 (0xf885d100) = 0x1f90000
  AHCI0_0x4 (0xf885d104) = 0x0
  AHCI0_0x8 (0xf885d108) = 0x1f90400
  AHCI0_0xc (0xf885d10c) = 0x0
  AHCI0_0x10 (0xf885d110) = 0x0
  AHCI0_0x14 (0xf885d114) = 0x0
  AHCI0_0x18 (0xf885d118) = 0x10004017
  AHCI0_0x1c (0xf885d11c) = 0x0
  AHCI0_0x20 (0xf885d120) = 0x130
  AHCI0_0x24 (0xf885d124) = 0xffffffff
  AHCI0_0x28 (0xf885d128) = 0x0
  AHCI0_0x2c (0xf885d12c) = 0x0
  AHCI0_0x30 (0xf885d130) = 0x0
  AHCI0_0x34 (0xf885d134) = 0x0
  AHCI0_0x38 (0xf885d138) = 0x0
  AHCI0_0x3c (0xf885d13c) = 0x0
simplexOnly = 0 (2)!MasterDev
update ConfigInfo->nt4
using AtaReq sz 1000
update ConfigInfo->w2k
Reconstruct ConfigInfo
set Dma32BitAddresses
BMList[i].channel 0x0, NumberChannels 0x1, channel 0x0
de 0xb100b7f4, Channel 0x0
chan = 0xb100ab30
AtapiSetupLunPtrs for channel 0 of 1, 1 luns
  Chan 0xb100ab30
  Lun 0x0
  Lun ptr 0xb100a008
  AtaReq 0xb1293000: cmd aligned b1293080, d=28
  ahci_cmd_ptr 0xb1293080
AtapiReadChipConfig: devExt 0xb100b7f4
AtapiReadChipConfig: dev 0x1, ph chan 0
 Parameter MaxTransferMode
 Parameter MaxTransferMode = 0x48
MaxTransferMode (overriden): 0x48
 Parameter ReorderEnable
 Parameter ReorderEnable = 0x1
 Parameter ReadCacheEnable
 Parameter ReadCacheEnable = 0x1
 Parameter WriteCacheEnable
 Parameter WriteCacheEnable = 0x1
 Parameter MaxTransferMode
 Parameter MaxTransferMode = 0x48
 Parameter PreferedTransferMode
 Parameter PreferedTransferMode = 0xffffffff
 Parameter ReadOnly
 Parameter ReadOnly = 0x0
 Parameter GeomType
 Parameter GeomType = 0xffffffff
 Parameter Hidden
 Parameter Hidden = 0x0
  No more setup for AHCI channel
IDX_IO1 0->0(io)
IDX_IO2 10->f885d120(mem)
IDX_BM_IO 14->0(io)
IDX_SATA_IO 19->f885d128(mem)
AtapiDmaAlloc: AHCI
  already initialized b1291000
exit: init spinlock
MasterDev=0x0, NumberChannels=0x1, Isr2DevObj=0x0
Init ISR:
Unnecessary
MasterDev=0x0, NumberChannels=0x1, Isr2DevObj=0x0
return SP_RETURN_FOUND
AtapiHwInitialize: (base)
AtapiChipInit: dev 0xffffffff, ph chan -1
HwFlags: 0x12000000
VendorID/DeviceID/Rev 0x8086/0x2829/0x2
  UniataAhciInit:
  AHCI Base: 0xf885d000 MemIo 1 Proc 0
  AHCI_0x0 (0xf885d000) = 0xc8241f80
  AHCI_0x4 (0xf885d004) = 0x80000002
  AHCI_0x8 (0xf885d008) = 0x0
  AHCI_0xc (0xf885d00c) = 0x1
  AHCI_0x10 (0xf885d010) = 0x10100
  reset AHCI controller, GHC 0x80000002
  AHCI GHC 0x80000000
  enable AHCI mode, GHC 0x80000000
  AHCI GHC 0x80000000
  AHCI CAP 0xc8241f80
  AHCI 64bit
  AHCI 31 CMD slots
  AHCI legasy SATA
  AHCI PI 0x1
  SATA Gen 2
  chan 0, offs 0x100
AtapiSetupLunPtrs for channel 0 of 1, 1 luns
  Chan 0xb100ab30
  Lun 0x0
  Lun ptr 0xb100a008
  AtaReq 0xb1293000: cmd aligned b1293080, d=28
  ahci_cmd_ptr 0xb1293080
AtapiDmaAlloc: AHCI
  already initialized b1291000
UniataAhciResume: lChan 0
WriteChannelPort4 0 => ch0[14]
  AHCI CLB setup
WriteChannelPort4 1f90000 => ch0[0]
WriteChannelPort4 0 => ch0[4]
  AHCI RCV FIS setup
WriteChannelPort4 1f90400 => ch0[8]
WriteChannelPort4 0 => ch0[c]
WriteChannelPort4 10000006 => ch0[18]
UniataAhciStartFR: lChan 0
ReadChannelPort4 ch0[18] = 10000006
  CMD 0x10000006
WriteChannelPort4 10000016 => ch0[18]
UniataAhciStart: lChan 0
ReadChannelPort4 ch0[10] = 0
WriteChannelPort4 0 => ch0[10]
    SError 0x0, IS 0x0
ReadChannelPort4 ch0[18] = 10004016
  CMD 0x10004016
WriteChannelPort4 10004017 => ch0[18]
  AHCI port 0 Base: 0xf885d100 MemIo 1 Proc 0
  AHCI0_0x0 (0xf885d100) = 0x1f90000
  AHCI0_0x4 (0xf885d104) = 0x0
  AHCI0_0x8 (0xf885d108) = 0x1f90400
  AHCI0_0xc (0xf885d10c) = 0x0
  AHCI0_0x10 (0xf885d110) = 0x0
  AHCI0_0x14 (0xf885d114) = 0x0
  AHCI0_0x18 (0xf885d118) = 0x10004017
  AHCI0_0x1c (0xf885d11c) = 0x0
  AHCI0_0x20 (0xf885d120) = 0x130
  AHCI0_0x24 (0xf885d124) = 0xffffffff
  AHCI0_0x28 (0xf885d128) = 0x0
  AHCI0_0x2c (0xf885d12c) = 0x0
  AHCI0_0x30 (0xf885d130) = 0x0
  AHCI0_0x34 (0xf885d134) = 0x0
  AHCI0_0x38 (0xf885d138) = 0x0
  AHCI0_0x3c (0xf885d13c) = 0x0
AtapiChipInit: dev 0xffffffff, ph chan 0
HwFlags: 0x12000000
VendorID/DeviceID/Rev 0x8086/0x2829/0x2
  AHCI single channel init
UniataAhciReset: lChan 0
WriteChannelPort4 0 => ch0[14]
UniataAhciHardReset: lChan 0
UniataAhciStop: lChan 0
ReadChannelPort4 ch0[18] = 10004017
WriteChannelPort4 10004016 => ch0[18]
ReadChannelPort4 ch0[18] = 10004016
  final CMD 0x10004016
UniataSataPhyEnable:
SControl 0x0
UniataSataPhyEnable: retry init 0
  SControl 00000001
UniataSataPhyEnable: retry idle 0
  SControl 00000300
UniataSataConnect:
UniataSataConnect: SStatus 00000000
  no PHY
  No devices in all LUNs
WriteChannelPort4 80400040 => ch0[14]
FindDevices:
AtapiDisableInterrupts_0: 0
WriteChannelPort4 0 => ch0[14]
  max_ldev 1
CheckDevice: Device 0x0
SStatus 0
  SATA DET <= SStatus_DET_Dev_NoPhy
AtapiEnableInterrupts_0: 1
WriteChannelPort4 fd4000ff => ch0[14]
FindDevices: returning 0 (AHCI)
AtapiHwInitialize: lChannel 0x0, dev 0
AtapiHwInitialize: (base) done
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x28298086/0x2
UniataNeedQueueing: TopLevel, qd=0
Send to device 12
TopLevel (2), srb 0xf88c8e2c
TopLevel (3), AtaReq 0xb0ff9000
SStatus 0
  SATA DET <= SStatus_DET_Dev_NoPhy
AtapiStartIo: SRB rejected
SRB_STATUS_SELECTION_TIMEOUT
AtapiStartIo: Srb 0xf88c8e2c complete with status 0xa
AtapiStartIo: AtapiDmaDBSync(b100ab30, f88c8e2c)
AtapiStartIo: UniataRemoveRequest(b100ab30, f88c8e2c)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan b100ab30, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x1:0x0:0x0
   VendorID+DeviceID/Rev 0x28298086/0x2
AtapiStartIo: Communication port
  INQUIRY
AtapiStartIo: Srb 0xf88c8e2c complete with status 0x1
AtapiStartIo: AtapiDmaDBSync(0, f88c8e2c)
AtapiStartIo: UniataRemoveRequest(0, f88c8e2c)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan 0, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x1:0x1:0x0
   VendorID+DeviceID/Rev 0x28298086/0x2
AtapiStartIo: SRB rejected
SRB_STATUS_SELECTION_TIMEOUT
AtapiStartIo: Srb 0xf88c8e2c complete with status 0xa
AtapiStartIo: AtapiDmaDBSync(0, f88c8e2c)
AtapiStartIo: UniataRemoveRequest(0, f88c8e2c)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan 0, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
ScsiPortInitialize Status 0x0
 Parameter IgnoreIsa
 Parameter IgnoreIsa = 0x0


ATAPI IDE: Look for ISA Controllers
AtapiFindController:
  assume max PIO4
allocate 2 Luns for 1 channels
AtapiSetupLunPtrs for channel 0 of 1, 2 luns
  Chan 0xb0ff8b30
  Lun 0x0
  Lun ptr 0xb128e008
  Lun 0x1
  Lun ptr 0xb128e310
AtapiReadChipConfig: devExt 0xb0ff82b4
AtapiReadChipConfig: dev 0xffffffff, ph chan -1
 Parameter ForceSimplex
 Parameter ForceSimplex = 0x0
MaxTransferMode (base): 0xc
 Parameter MaxTransferMode
 Parameter MaxTransferMode = 0xc
MaxTransferMode (overriden): 0xc
 Parameter AtapiDmaZeroTransfer
 Parameter AtapiDmaZeroTransfer = 0x0
 Parameter AtapiDmaControlCmd
 Parameter AtapiDmaControlCmd = 0x0
 Parameter AtapiDmaRawRead
 Parameter AtapiDmaRawRead = 0x0
 Parameter AtapiDmaReadWrite
 Parameter AtapiDmaReadWrite = 0x1
AtapiChipInit: dev 0xffffffff, ph chan -1
HwFlags: 0x0
VendorID/DeviceID/Rev 0x0/0x0/0x0
 Parameter PortBase
 Parameter PortBase = 0x0
 Parameter Irq
 Parameter Irq = 0x0
AtapiFindController: AtdiskPrimaryClaimed
 Parameter PortBase
 Parameter PortBase = 0x0
 Parameter Irq
 Parameter Irq = 0x0
AtapiFindController: AtdiskSecondaryClaimed
 Parameter PortBase
 Parameter PortBase = 0x0
 Parameter Irq
 Parameter Irq = 0x0
  BaseIoAddress1=1e8
  BaseIoAddress2=3ee
  AltStatus (0xff)
  Reg_0x1 (0x1e9) = 0x0
  Reg_0x2 (0x1ea) = 0x0
  Reg_0x3 (0x1eb) = 0x0
  Reg_0x4 (0x1ec) = 0x0
  Reg_0x5 (0x1ed) = 0x0
  Reg_0x6 (0x1ee) = 0x0
  Reg_0x7 (0x1ef) = 0x0
  BM_0x0 (0x0) = 0x0
  BM_0x1 (0x0) = 0x0
  BM_0x2 (0x0) = 0x0
  BM_0x3 (0x0) = 0x0
AtapiFindController: Status vs AlsStatus missmatch, abort init ?
    abort
 Parameter PortBase
 Parameter PortBase = 0x0
 Parameter Irq
 Parameter Irq = 0x0
  BaseIoAddress1=168
  BaseIoAddress2=36e
  AltStatus (0xff)
  Reg_0x1 (0x169) = 0x0
  Reg_0x2 (0x16a) = 0x0
  Reg_0x3 (0x16b) = 0x0
  Reg_0x4 (0x16c) = 0x0
  Reg_0x5 (0x16d) = 0x0
  Reg_0x6 (0x16e) = 0x0
  Reg_0x7 (0x16f) = 0x0
  BM_0x0 (0x0) = 0x0
  BM_0x1 (0x0) = 0x0
  BM_0x2 (0x0) = 0x0
  BM_0x3 (0x0) = 0x0
AtapiFindController: Status vs AlsStatus missmatch, abort init ?
    abort
AtapiFindController: return SP_RETURN_NOT_FOUND
ScsiPortInitialize Status 0xc00000c0
 Parameter IgnoreMca
 Parameter IgnoreMca = 0x0


ATAPI IDE: Look for MCA Controllers
ScsiPortInitialize Status 0xc00000c0


Leave UNIATA MiniPort DriverEntry with status 0x0
(../../ntoskrnl/io/iomgr/driver.c:1575) '\Driver\BUSLOGIC' initialization failed, status (0xc00000c0)
(../../ntoskrnl/io/iomgr/driver.c:61) Deleting driver object '\Driver\BUSLOGIC'
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xf88c9284, CDB 0xf88c92b4, AtaReq 0xb1298000, SCmd 0x1a
UniataNeedQueueing: TopLevel, qd=0
Send to device 1a
TopLevel (2), srb 0xf88c9284
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8fc0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_MODE_SENSE PATH:LUN:TID = 0x0:0x0:0x0
IdeSendCommand: REQ_STATE_TRANSFER_COMPLETE
AtapiStartIo: Srb 0xf88c9284 complete with status 0x6
AtapiStartIo: AtapiDmaDBSync(b1061b30, f88c9284)
AtapiStartIo: UniataRemoveRequest(b1061b30, f88c9284)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan b1061b30, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xf88c9284, CDB 0xf88c92b4, AtaReq 0xb1298000, SCmd 0x1a
UniataNeedQueueing: TopLevel, qd=0
Send to device 1a
TopLevel (2), srb 0xf88c9284
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8fc0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_MODE_SENSE PATH:LUN:TID = 0x0:0x0:0x0
IdeSendCommand: REQ_STATE_TRANSFER_COMPLETE
AtapiStartIo: Srb 0xf88c9284 complete with status 0x6
AtapiStartIo: AtapiDmaDBSync(b1061b30, f88c9284)
AtapiStartIo: UniataRemoveRequest(b1061b30, f88c9284)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan b1061b30, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xf88c92a8, CDB 0xf88c92d8, AtaReq 0xb1298000, SCmd 0x25
UniataNeedQueueing: TopLevel, qd=0
Send to device 25
TopLevel (2), srb 0xf88c92a8
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8fe0
** Ide: Command AtaReq 0xb1298000
** --- **
** IdeSendCommand: SCSIOP_READ_CAPACITY PATH:LUN:TID = 0x0:0x0:0x0
** IDE disk 0x0 - #sectors 0x3f, #heads 0x10, #cylinders 0x2082
IdeSendCommand: REQ_STATE_TRANSFER_COMPLETE
AtapiStartIo: Srb 0xf88c92a8 complete with status 0x1
AtapiStartIo: AtapiDmaDBSync(b1061b30, f88c92a8)
AtapiStartIo: UniataRemoveRequest(b1061b30, f88c92a8)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan b1061b30, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb1060820, CDB 0xb1060850, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb1060820
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8e78
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f885c000, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f885c000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b1060820
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb1060820, status 1
AtapiInterrupt: RequestComplete, srb 0xb1060820
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb1060820, CDB 0xb1060850, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb1060820
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8d68
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f885c000, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f885c000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b1060820
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb1060820, status 1
AtapiInterrupt: RequestComplete, srb 0xb1060820
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xf88c8ed8, CDB 0xf88c8f08, AtaReq 0xb1298000, SCmd 0x25
UniataNeedQueueing: TopLevel, qd=0
Send to device 25
TopLevel (2), srb 0xf88c8ed8
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8c10
** Ide: Command AtaReq 0xb1298000
** --- **
** IdeSendCommand: SCSIOP_READ_CAPACITY PATH:LUN:TID = 0x0:0x0:0x0
** IDE disk 0x0 - #sectors 0x3f, #heads 0x10, #cylinders 0x2082
IdeSendCommand: REQ_STATE_TRANSFER_COMPLETE
AtapiStartIo: Srb 0xf88c8ed8 complete with status 0x1
AtapiStartIo: AtapiDmaDBSync(b1061b30, f88c8ed8)
AtapiStartIo: UniataRemoveRequest(b1061b30, f88c8ed8)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan b1061b30, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb1060820, CDB 0xb1060850, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb1060820
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8dd8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f885c008, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f885c008)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b1060820
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb1060820, status 1
AtapiInterrupt: RequestComplete, srb 0xb1060820
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb1060820, CDB 0xb1060850, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb1060820
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8df0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f885c000, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f885c000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b1060820
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb1060820, status 1
AtapiInterrupt: RequestComplete, srb 0xb1060820
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xf88c9284, CDB 0xf88c92b4, AtaReq 0xb100c000, SCmd 0x1a
UniataNeedQueueing: TopLevel, qd=0
Send to device 1a
TopLevel (2), srb 0xf88c9284
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8fc0
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_MODE_SENSE PATH:LUN:TID = 0x0:0x0:0x0
IdeSendCommand: REQ_STATE_TRANSFER_COMPLETE
AtapiStartIo: Srb 0xf88c9284 complete with status 0x6
AtapiStartIo: AtapiDmaDBSync(b1296008, f88c9284)
AtapiStartIo: UniataRemoveRequest(b1296008, f88c9284)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan b1296008, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xf88c9284, CDB 0xf88c92b4, AtaReq 0xb100c000, SCmd 0x1a
UniataNeedQueueing: TopLevel, qd=0
Send to device 1a
TopLevel (2), srb 0xf88c9284
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8fc0
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_MODE_SENSE PATH:LUN:TID = 0x0:0x0:0x0
IdeSendCommand: REQ_STATE_TRANSFER_COMPLETE
AtapiStartIo: Srb 0xf88c9284 complete with status 0x6
AtapiStartIo: AtapiDmaDBSync(b1296008, f88c9284)
AtapiStartIo: UniataRemoveRequest(b1296008, f88c9284)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan b1296008, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xf88c92a8, CDB 0xf88c92d8, AtaReq 0xb100c000, SCmd 0x25
UniataNeedQueueing: TopLevel, qd=0
Send to device 25
TopLevel (2), srb 0xf88c92a8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8fe0
** Ide: Command AtaReq 0xb100c000
** --- **
** IdeSendCommand: SCSIOP_READ_CAPACITY PATH:LUN:TID = 0x0:0x0:0x0
** IDE disk 0x0 - #sectors 0x3f, #heads 0x10, #cylinders 0x4104
IdeSendCommand: REQ_STATE_TRANSFER_COMPLETE
AtapiStartIo: Srb 0xf88c92a8 complete with status 0x1
AtapiStartIo: AtapiDmaDBSync(b1296008, f88c92a8)
AtapiStartIo: UniataRemoveRequest(b1296008, f88c92a8)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan b1296008, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff8378, CDB 0xb0ff83a8, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff8378
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8e78
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f885c000, count 200, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=f885c000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff8378
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff8378, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff8378
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff8378, CDB 0xb0ff83a8, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff8378
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8d68
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f885c000, count 200, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=f885c000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff8378
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff8378, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff8378
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xf88c8ed8, CDB 0xf88c8f08, AtaReq 0xb100c000, SCmd 0x25
UniataNeedQueueing: TopLevel, qd=0
Send to device 25
TopLevel (2), srb 0xf88c8ed8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8c10
** Ide: Command AtaReq 0xb100c000
** --- **
** IdeSendCommand: SCSIOP_READ_CAPACITY PATH:LUN:TID = 0x0:0x0:0x0
** IDE disk 0x0 - #sectors 0x3f, #heads 0x10, #cylinders 0x4104
IdeSendCommand: REQ_STATE_TRANSFER_COMPLETE
AtapiStartIo: Srb 0xf88c8ed8 complete with status 0x1
AtapiStartIo: AtapiDmaDBSync(b1296008, f88c8ed8)
AtapiStartIo: UniataRemoveRequest(b1296008, f88c8ed8)
AtapiStartIo: ScsiPortNotification
AtapiStartIo: UniataGetCurRequest
AtapiStartIo: chan b1296008, Src 0
AtapiStartIo: next Srb 0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff8378, CDB 0xb0ff83a8, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff8378
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8dd8
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f885c490, count 200, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=f885c490)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff8378
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff8378, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff8378
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff8378, CDB 0xb0ff83a8, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff8378
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8df0
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f885c000, count 200, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=f885c000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff8378
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff8378, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff8378
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../drivers/bus/acpi/busmgr/bus.c:1202) Using HPET hack
(../../drivers/bus/acpi/acpienum.c:70) Detected duplicate device: PNP0C0F 0
(../../drivers/bus/acpi/acpienum.c:70) Detected duplicate device: PNP0C0F 0
(../../drivers/bus/acpi/acpienum.c:70) Detected duplicate device: PNP0C0F 0
(../../drivers/bus/acpi/buspdo.c:692) Using _BBN for bus number
(../../drivers/bus/acpi/buspdo.c:695) Found PCI root hub: 0
(../../ntoskrnl/io/pnpmgr/pnpmgr.c:4030) IRP_MN_QUERY_PNP_DEVICE_STATE failed with status 0xc00000bb
(../../drivers/bus/pci/fdo.c:571) Unknown IOCTL 0x9
(../../drivers/bus/pci/fdo.c:571) Unknown IOCTL 0x14
(../../ntoskrnl/io/pnpmgr/pnpmgr.c:4030) IRP_MN_QUERY_PNP_DEVICE_STATE failed with status 0xc00000bb
(../../ntoskrnl/mm/ARM3/sysldr.c:2959) ZwOpenFile failed with status 0xc000003a
(../../ntoskrnl/mm/ARM3/sysldr.c:2959) ZwOpenFile failed with status 0xc000003a
(../../ntoskrnl/mm/ARM3/sysldr.c:2959) ZwOpenFile failed with status 0xc000003a
(../../ntoskrnl/mm/ARM3/sysldr.c:2959) ZwOpenFile failed with status 0xc000003a
(../../ntoskrnl/mm/ARM3/sysldr.c:2959) ZwOpenFile failed with status 0xc000003a
(../../ntoskrnl/mm/ARM3/sysldr.c:2959) ZwOpenFile failed with status 0xc000003a
(../../ntoskrnl/mm/ARM3/sysldr.c:2959) ZwOpenFile failed with status 0xc000003a
(../../ntoskrnl/mm/ARM3/sysldr.c:2959) ZwOpenFile failed with status 0xc000003a
(../../ntoskrnl/mm/ARM3/sysldr.c:2959) ZwOpenFile failed with status 0xc000003a
(../../ntoskrnl/mm/ARM3/sysldr.c:2959) ZwOpenFile failed with status 0xc000003a
(../../ntoskrnl/mm/ARM3/sysldr.c:2959) ZwOpenFile failed with status 0xc000003a
(../../ntoskrnl/mm/ARM3/sysldr.c:2959) ZwOpenFile failed with status 0xc000003a
(../../ntoskrnl/mm/ARM3/sysldr.c:2959) ZwOpenFile failed with status 0xc000003a
(../../ntoskrnl/mm/ARM3/sysldr.c:2959) ZwOpenFile failed with status 0xc000003a
(../../ntoskrnl/mm/ARM3/sysldr.c:2959) ZwOpenFile failed with status 0xc000003a
(../../ntoskrnl/mm/ARM3/sysldr.c:2959) ZwOpenFile failed with status 0xc000003a
(../../ntoskrnl/mm/ARM3/sysldr.c:2959) ZwOpenFile failed with status 0xc000003a
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb1060820, CDB 0xb1060850, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb1060820
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c94d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f8858ca0, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8858ca0)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b1060820
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb1060820, status 1
AtapiInterrupt: RequestComplete, srb 0xb1060820
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb1060820, CDB 0xb1060850, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb1060820
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c93a8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f8858000, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8858000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b1060820
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb1060820, status 1
AtapiInterrupt: RequestComplete, srb 0xb1060820
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb1060820, CDB 0xb1060850, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb1060820
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c9418
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f8858290, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8858290)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b1060820
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb1060820, status 1
AtapiInterrupt: RequestComplete, srb 0xb1060820
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb1060820, CDB 0xb1060850, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb1060820
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c9530
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f8858000, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8858000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b1060820
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb1060820, status 1
AtapiInterrupt: RequestComplete, srb 0xb1060820
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb1060820, CDB 0xb1060850, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb1060820
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c95a0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f8858ca0, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8858ca0)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b1060820
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb1060820, status 1
AtapiInterrupt: RequestComplete, srb 0xb1060820
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/io/iomgr/iorsrce.c:725) Failed opening given symbolic link!
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff8378, CDB 0xb0ff83a8, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff8378
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c94d0
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f88588e0, count 200, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=f88588e0)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff8378
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff8378, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff8378
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff8378, CDB 0xb0ff83a8, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff8378
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c93a8
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f8858000, count 200, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=f8858000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff8378
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff8378, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff8378
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff8378, CDB 0xb0ff83a8, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff8378
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c9418
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f88586d8, count 200, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=f88586d8)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff8378
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff8378, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff8378
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff8378, CDB 0xb0ff83a8, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff8378
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c9530
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f8858000, count 200, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=f8858000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff8378
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff8378, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff8378
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff8378, CDB 0xb0ff83a8, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff8378
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c95a0
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f8858460, count 200, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=f8858460)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff8378
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff8378, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff8378
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8f10
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 3f, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f88585c0, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f88585c0)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8f10
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 3f, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f88585c0, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f88585c0)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8c48
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c00000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80c00000)
  get Phys(data[n=1]=80c01000)
  get Phys(data[n=2]=80c02000)
  get Phys(data[n=2]=80c03000)
  get Phys(data[n=2]=80c04000)
  get Phys(data[n=2]=80c05000)
  get Phys(data[n=2]=80c06000)
  get Phys(data[n=2]=80c07000)
  get Phys(data[n=3]=80c08000)
  get Phys(data[n=3]=80c09000)
  get Phys(data[n=3]=80c0a000)
  get Phys(data[n=3]=80c0b000)
  get Phys(data[n=3]=80c0c000)
  get Phys(data[n=3]=80c0d000)
  get Phys(data[n=3]=80c0e000)
  get Phys(data[n=3]=80c0f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8c48
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c10000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80c10000)
  get Phys(data[n=1]=80c11000)
  get Phys(data[n=1]=80c12000)
  get Phys(data[n=1]=80c13000)
  get Phys(data[n=1]=80c14000)
  get Phys(data[n=1]=80c15000)
  get Phys(data[n=1]=80c16000)
  get Phys(data[n=1]=80c17000)
  get Phys(data[n=2]=80c18000)
  get Phys(data[n=2]=80c19000)
  get Phys(data[n=2]=80c1a000)
  get Phys(data[n=2]=80c1b000)
  get Phys(data[n=2]=80c1c000)
  get Phys(data[n=2]=80c1d000)
  get Phys(data[n=2]=80c1e000)
  get Phys(data[n=2]=80c1f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xdf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0xdf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8c48
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 15f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 15f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c20000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80c20000)
  get Phys(data[n=1]=80c21000)
  get Phys(data[n=1]=80c22000)
  get Phys(data[n=1]=80c23000)
  get Phys(data[n=1]=80c24000)
  get Phys(data[n=1]=80c25000)
  get Phys(data[n=1]=80c26000)
  get Phys(data[n=1]=80c27000)
  get Phys(data[n=2]=80c28000)
  get Phys(data[n=3]=80c29000)
  get Phys(data[n=4]=80c2a000)
  get Phys(data[n=4]=80c2b000)
  get Phys(data[n=4]=80c2c000)
  get Phys(data[n=5]=80c2d000)
  get Phys(data[n=5]=80c2e000)
  get Phys(data[n=5]=80c2f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x15f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x15f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8c48
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c30000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80c30000)
  get Phys(data[n=1]=80c31000)
  get Phys(data[n=2]=80c32000)
  get Phys(data[n=2]=80c33000)
  get Phys(data[n=2]=80c34000)
  get Phys(data[n=2]=80c35000)
  get Phys(data[n=2]=80c36000)
  get Phys(data[n=2]=80c37000)
  get Phys(data[n=3]=80c38000)
  get Phys(data[n=3]=80c39000)
  get Phys(data[n=3]=80c3a000)
  get Phys(data[n=3]=80c3b000)
  get Phys(data[n=3]=80c3c000)
  get Phys(data[n=3]=80c3d000)
  get Phys(data[n=3]=80c3e000)
  get Phys(data[n=3]=80c3f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8d90
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 403f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 403f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 80c40000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80c40000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x403f, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x403f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8998
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4047, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 4047, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 80c80000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80c80000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4047, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4047 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8998
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 404f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 404f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 80cc0000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80cc0000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x404f, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x404f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8998
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1abff, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1abff, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 80cc1000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80cc1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1abff, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1abff count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8998
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1ed57, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1ed57, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 80cc2000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80cc2000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1ed57, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1ed57 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8998
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2da07, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 2da07, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 80cc3000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80cc3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2da07, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2da07 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8998
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 429cf, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 429cf, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 80cc4000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80cc4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x429cf, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x429cf count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8998
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 405f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 405f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 80d00000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80d00000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x405f, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x405f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8d50
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5f27, OrigWordsRequested 0x4000, DevSize 0x40
IdeReadWrite (REQ): Starting sector is 5f27, Number of WORDS 0x4000, DevSize 0x40
AtapiDmaSetup: mode 0x45, data f8818000, count 8000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8818000)
  get Phys(data[n=1]=f8819000)
  get Phys(data[n=2]=f881a000)
  get Phys(data[n=2]=f881b000)
  get Phys(data[n=2]=f881c000)
  get Phys(data[n=2]=f881d000)
  get Phys(data[n=2]=f881e000)
  get Phys(data[n=2]=f881f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5f27, Count 0x40(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5f27 count 0x40 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 8000, full size 8000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c90e4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5f27, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 5f27, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8857000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8857000)
  get Phys(data[n=1]=f8858000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5f27, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5f27 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\pciide.sys at F8852000 with 7 pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8c00
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5f67, OrigWordsRequested 0x7000, DevSize 0x70
IdeReadWrite (REQ): Starting sector is 5f67, Number of WORDS 0x7000, DevSize 0x70
AtapiDmaSetup: mode 0x45, data f8811000, count e000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8811000)
  get Phys(data[n=1]=f8812000)
  get Phys(data[n=1]=f8813000)
  get Phys(data[n=1]=f8814000)
  get Phys(data[n=1]=f8815000)
  get Phys(data[n=1]=f8816000)
  get Phys(data[n=1]=f8817000)
  get Phys(data[n=1]=f8818000)
  get Phys(data[n=1]=f8819000)
  get Phys(data[n=1]=f881a000)
  get Phys(data[n=1]=f881b000)
  get Phys(data[n=1]=f881c000)
  get Phys(data[n=1]=f881d000)
  get Phys(data[n=1]=f881e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5f67, Count 0x70(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5f67 count 0x70 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e000, full size e000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8f94
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5f67, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 5f67, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8850000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8850000)
  get Phys(data[n=1]=f8851000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5f67, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5f67 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\pciidex.sys at F8849000 with 9 pages
(../../drivers/bus/pci/pdo.c:1267) Enabling command flags for PCI device 0x21 on bus 0x0: [Bus master] [I/O space enable]
(../../drivers/storage/ide/pciidex/fdo.c:464) IRP_MJ_PNP / Unknown minor function 0x9
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8d50
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 500af, OrigWordsRequested 0x5800, DevSize 0x58
IdeReadWrite (REQ): Starting sector is 500af, Number of WORDS 0x5800, DevSize 0x58
AtapiDmaSetup: mode 0x45, data f8808000, count b000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8808000)
  get Phys(data[n=1]=f8809000)
  get Phys(data[n=1]=f880a000)
  get Phys(data[n=2]=f880b000)
  get Phys(data[n=2]=f880c000)
  get Phys(data[n=2]=f880d000)
  get Phys(data[n=2]=f880e000)
  get Phys(data[n=2]=f880f000)
  get Phys(data[n=2]=f8810000)
  get Phys(data[n=2]=f8811000)
  get Phys(data[n=2]=f8812000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x500af, Count 0x58(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x500af count 0x58 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered b000, full size b000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c90e4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 500af, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 500af, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8847000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8847000)
  get Phys(data[n=1]=f8848000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x500af, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x500af count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\vbemp.sys at F8841000 with 8 pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8b98
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 501cf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 501cf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8800000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8800000)
  get Phys(data[n=1]=f8801000)
  get Phys(data[n=1]=f8802000)
  get Phys(data[n=1]=f8803000)
  get Phys(data[n=1]=f8804000)
  get Phys(data[n=2]=f8805000)
  get Phys(data[n=3]=f8806000)
  get Phys(data[n=3]=f8807000)
  get Phys(data[n=3]=f8808000)
  get Phys(data[n=4]=f8809000)
  get Phys(data[n=5]=f880a000)
  get Phys(data[n=6]=f880b000)
  get Phys(data[n=6]=f880c000)
  get Phys(data[n=6]=f880d000)
  get Phys(data[n=7]=f880e000)
  get Phys(data[n=7]=f880f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x501cf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x501cf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8b98
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5024f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5024f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8810000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8810000)
  get Phys(data[n=1]=f8811000)
  get Phys(data[n=1]=f8812000)
  get Phys(data[n=2]=f8813000)
  get Phys(data[n=2]=f8814000)
  get Phys(data[n=2]=f8815000)
  get Phys(data[n=2]=f8816000)
  get Phys(data[n=2]=f8817000)
  get Phys(data[n=2]=f8818000)
  get Phys(data[n=3]=f8819000)
  get Phys(data[n=3]=f881a000)
  get Phys(data[n=3]=f881b000)
  get Phys(data[n=3]=f881c000)
  get Phys(data[n=3]=f881d000)
  get Phys(data[n=3]=f881e000)
  get Phys(data[n=3]=f881f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5024f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5024f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8b98
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 502cf, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 502cf, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data f8820000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8820000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x502cf, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x502cf count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8f94
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 501cf, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 501cf, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f883f000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f883f000)
  get Phys(data[n=1]=f8840000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x501cf, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x501cf count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\videoprt.sys at F882E000 with 13 pages
(../../drivers/bus/pci/pdo.c:1250) Assigning IRQ 11 to PCI device 0x2 on bus 0x0
(../../drivers/bus/pci/pdo.c:1267) Enabling command flags for PCI device 0x2 on bus 0x0: [Bus master] [Memory space enable]
(../../ntoskrnl/io/pnpmgr/pnpmgr.c:848) IRP_MN_QUERY_CAPABILITIES failed with status 0xc00000bb
(../../ntoskrnl/io/pnpmgr/pnpmgr.c:681) IopInitiatePnpIrp() failed (Status 0xc00000bb)
(../../ntoskrnl/io/pnpmgr/pnpmgr.c:4030) IRP_MN_QUERY_PNP_DEVICE_STATE failed with status 0xc00000bb
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8d50
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3be87, OrigWordsRequested 0x7000, DevSize 0x70
IdeReadWrite (REQ): Starting sector is 3be87, Number of WORDS 0x7000, DevSize 0x70
AtapiDmaSetup: mode 0x45, data f87ed000, count e000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87ed000)
  get Phys(data[n=1]=f87ee000)
  get Phys(data[n=1]=f87ef000)
  get Phys(data[n=1]=f87f0000)
  get Phys(data[n=1]=f87f1000)
  get Phys(data[n=1]=f87f2000)
  get Phys(data[n=1]=f87f3000)
  get Phys(data[n=1]=f87f4000)
  get Phys(data[n=1]=f87f5000)
  get Phys(data[n=1]=f87f6000)
  get Phys(data[n=1]=f87f7000)
  get Phys(data[n=2]=f87f8000)
  get Phys(data[n=2]=f87f9000)
  get Phys(data[n=2]=f87fa000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3be87, Count 0x70(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3be87 count 0x70 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e000, full size e000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c90e4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3be87, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3be87, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f882c000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f882c000)
  get Phys(data[n=1]=f882d000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3be87, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3be87 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\pcnet.sys at F8824000 with a pages
(../../drivers/network/ndis/ndis/miniport.c:2620)(NdisMRegisterMiniport) Initializing an NDIS 5.1 miniport
(../../drivers/bus/pci/pdo.c:1250) Assigning IRQ 10 to PCI device 0x3 on bus 0x0
(../../drivers/bus/pci/pdo.c:1267) Enabling command flags for PCI device 0x3 on bus 0x0: [Bus master] [Memory space enable] [I/O space enable]
(../../drivers/network/ndis/ndis/miniport.c:2845)(NdisMSetAttributesEx) Miniport attribute flags: 0x8
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8d00
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4d07, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4d07, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f87e0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87e0000)
  get Phys(data[n=1]=f87e1000)
  get Phys(data[n=1]=f87e2000)
  get Phys(data[n=2]=f87e3000)
  get Phys(data[n=2]=f87e4000)
  get Phys(data[n=2]=f87e5000)
  get Phys(data[n=2]=f87e6000)
  get Phys(data[n=2]=f87e7000)
  get Phys(data[n=2]=f87e8000)
  get Phys(data[n=2]=f87e9000)
  get Phys(data[n=2]=f87ea000)
  get Phys(data[n=2]=f87eb000)
  get Phys(data[n=2]=f87ec000)
  get Phys(data[n=2]=f87ed000)
  get Phys(data[n=2]=f87ee000)
  get Phys(data[n=2]=f87ef000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4d07, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4d07 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8d00
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4d87, OrigWordsRequested 0x6800, DevSize 0x68
IdeReadWrite (REQ): Starting sector is 4d87, Number of WORDS 0x6800, DevSize 0x68
AtapiDmaSetup: mode 0x45, data f87f0000, count d000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87f0000)
  get Phys(data[n=1]=f87f1000)
  get Phys(data[n=1]=f87f2000)
  get Phys(data[n=2]=f87f3000)
  get Phys(data[n=2]=f87f4000)
  get Phys(data[n=2]=f87f5000)
  get Phys(data[n=2]=f87f6000)
  get Phys(data[n=2]=f87f7000)
  get Phys(data[n=2]=f87f8000)
  get Phys(data[n=2]=f87f9000)
  get Phys(data[n=2]=f87fa000)
  get Phys(data[n=2]=f87fb000)
  get Phys(data[n=2]=f87fc000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4d87, Count 0x68(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4d87 count 0x68 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered d000, full size d000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c90fc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4d07, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 4d07, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f881f000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f881f000)
  get Phys(data[n=1]=f8820000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4d07, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4d07 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\i8042prt.sys at F8810000 with 11 pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8aa0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5717, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5717, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f87cf000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87cf000)
  get Phys(data[n=1]=f87d0000)
  get Phys(data[n=1]=f87d1000)
  get Phys(data[n=1]=f87d2000)
  get Phys(data[n=1]=f87d3000)
  get Phys(data[n=1]=f87d4000)
  get Phys(data[n=1]=f87d5000)
  get Phys(data[n=1]=f87d6000)
  get Phys(data[n=1]=f87d7000)
  get Phys(data[n=1]=f87d8000)
  get Phys(data[n=1]=f87d9000)
  get Phys(data[n=1]=f87da000)
  get Phys(data[n=1]=f87db000)
  get Phys(data[n=2]=f87dc000)
  get Phys(data[n=2]=f87dd000)
  get Phys(data[n=3]=f87de000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5717, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5717 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8aa0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5797, OrigWordsRequested 0x2000, DevSize 0x20
IdeReadWrite (REQ): Starting sector is 5797, Number of WORDS 0x2000, DevSize 0x20
AtapiDmaSetup: mode 0x45, data f87df000, count 4000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87df000)
  get Phys(data[n=1]=f87e0000)
  get Phys(data[n=2]=f87e1000)
  get Phys(data[n=2]=f87e2000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5797, Count 0x20(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5797 count 0x20 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 4000, full size 4000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8e9c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5717, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 5717, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f880e000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f880e000)
  get Phys(data[n=1]=f880f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5717, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5717 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\kbdclass.sys at F8805000 with b pages
(../../drivers/input/i8042prt/pnp.c:718) IRP_MJ_PNP / unknown minor function 0x9
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8aa0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b987, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3b987, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f87c4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87c4000)
  get Phys(data[n=1]=f87c5000)
  get Phys(data[n=2]=f87c6000)
  get Phys(data[n=3]=f87c7000)
  get Phys(data[n=3]=f87c8000)
  get Phys(data[n=3]=f87c9000)
  get Phys(data[n=4]=f87ca000)
  get Phys(data[n=4]=f87cb000)
  get Phys(data[n=4]=f87cc000)
  get Phys(data[n=4]=f87cd000)
  get Phys(data[n=4]=f87ce000)
  get Phys(data[n=5]=f87cf000)
  get Phys(data[n=5]=f87d0000)
  get Phys(data[n=5]=f87d1000)
  get Phys(data[n=5]=f87d2000)
  get Phys(data[n=5]=f87d3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b987, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b987 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8aa0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ba07, OrigWordsRequested 0x2000, DevSize 0x20
IdeReadWrite (REQ): Starting sector is 3ba07, Number of WORDS 0x2000, DevSize 0x20
AtapiDmaSetup: mode 0x45, data f87d4000, count 4000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87d4000)
  get Phys(data[n=1]=f87d5000)
  get Phys(data[n=1]=f87d6000)
  get Phys(data[n=1]=f87d7000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ba07, Count 0x20(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3ba07 count 0x20 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 4000, full size 4000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8e9c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b987, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3b987, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8803000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8803000)
  get Phys(data[n=1]=f8804000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b987, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b987 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\mouclass.sys at F87FA000 with b pages
(../../drivers/input/i8042prt/pnp.c:718) IRP_MJ_PNP / unknown minor function 0x9
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8d00
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3c4c7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3c4c7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f87b9000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87b9000)
  get Phys(data[n=1]=f87ba000)
  get Phys(data[n=1]=f87bb000)
  get Phys(data[n=1]=f87bc000)
  get Phys(data[n=2]=f87bd000)
  get Phys(data[n=2]=f87be000)
  get Phys(data[n=2]=f87bf000)
  get Phys(data[n=2]=f87c0000)
  get Phys(data[n=2]=f87c1000)
  get Phys(data[n=2]=f87c2000)
  get Phys(data[n=2]=f87c3000)
  get Phys(data[n=2]=f87c4000)
  get Phys(data[n=2]=f87c5000)
  get Phys(data[n=2]=f87c6000)
  get Phys(data[n=3]=f87c7000)
  get Phys(data[n=3]=f87c8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3c4c7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3c4c7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8d00
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3c547, OrigWordsRequested 0x1800, DevSize 0x18
IdeReadWrite (REQ): Starting sector is 3c547, Number of WORDS 0x1800, DevSize 0x18
AtapiDmaSetup: mode 0x45, data f87c9000, count 3000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87c9000)
  get Phys(data[n=1]=f87ca000)
  get Phys(data[n=1]=f87cb000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3c547, Count 0x18(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3c547 count 0x18 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 3000, full size 3000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c90fc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3c4c7, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3c4c7, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f87f8000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87f8000)
  get Phys(data[n=1]=f87f9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3c4c7, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3c4c7 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\serial.sys at F87EE000 with c pages
(../../ntoskrnl/io/pnpmgr/pnpres.c:614) Resource conflict: IRQ (0x4 0x4 vs. 0x4 0x4)
(../../ntoskrnl/io/pnpmgr/pnpres.c:1099) Boot resources for ACPI\PNP0501\0 cause a resource conflict!
(../../ntoskrnl/io/pnpmgr/pnpres.c:135) Satisfying port requirement with 0x3f8 (length: 0x8)
(../../ntoskrnl/io/pnpmgr/pnpres.c:384) Failed to find an available interrupt resource (0x4 to 0x4)
(../../ntoskrnl/io/pnpmgr/pnpres.c:512) Unable to satisfy preferred resource or alternates in list 0
(../../ntoskrnl/io/pnpmgr/pnpres.c:523) Out of alternate lists!
(../../ntoskrnl/io/pnpmgr/pnpres.c:1122) Failed to fixup a resource list from supplied resources for ACPI\PNP0501\0
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8d00
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b6a7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3b6a7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f87ad000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87ad000)
  get Phys(data[n=1]=f87ae000)
  get Phys(data[n=1]=f87af000)
  get Phys(data[n=1]=f87b0000)
  get Phys(data[n=2]=f87b1000)
  get Phys(data[n=2]=f87b2000)
  get Phys(data[n=2]=f87b3000)
  get Phys(data[n=2]=f87b4000)
  get Phys(data[n=2]=f87b5000)
  get Phys(data[n=2]=f87b6000)
  get Phys(data[n=2]=f87b7000)
  get Phys(data[n=2]=f87b8000)
  get Phys(data[n=2]=f87b9000)
  get Phys(data[n=2]=f87ba000)
  get Phys(data[n=2]=f87bb000)
  get Phys(data[n=2]=f87bc000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b6a7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b6a7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8d00
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b727, OrigWordsRequested 0x1800, DevSize 0x18
IdeReadWrite (REQ): Starting sector is 3b727, Number of WORDS 0x1800, DevSize 0x18
AtapiDmaSetup: mode 0x45, data f87bd000, count 3000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87bd000)
  get Phys(data[n=1]=f87be000)
  get Phys(data[n=1]=f87bf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b727, Count 0x18(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b727 count 0x18 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 3000, full size 3000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c90fc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b6a7, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3b6a7, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f87ec000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87ec000)
  get Phys(data[n=1]=f87ed000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b6a7, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b6a7 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\cmbatt.sys at F87E1000 with d pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8c18
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b55f, OrigWordsRequested 0x4800, DevSize 0x48
IdeReadWrite (REQ): Starting sector is 3b55f, Number of WORDS 0x4800, DevSize 0x48
AtapiDmaSetup: mode 0x45, data f87a0000, count 9000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87a0000)
  get Phys(data[n=1]=f87a1000)
  get Phys(data[n=1]=f87a2000)
  get Phys(data[n=1]=f87a3000)
  get Phys(data[n=2]=f87a4000)
  get Phys(data[n=2]=f87a5000)
  get Phys(data[n=2]=f87a6000)
  get Phys(data[n=2]=f87a7000)
  get Phys(data[n=2]=f87a8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b55f, Count 0x48(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b55f count 0x48 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 9000, full size 9000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8fac
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b55f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3b55f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f87df000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87df000)
  get Phys(data[n=1]=f87e0000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b55f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b55f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\battc.sys at F87DA000 with 7 pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8c18
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d5cf, OrigWordsRequested 0x4000, DevSize 0x40
IdeReadWrite (REQ): Starting sector is 3d5cf, Number of WORDS 0x4000, DevSize 0x40
AtapiDmaSetup: mode 0x45, data f8799000, count 8000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8799000)
  get Phys(data[n=1]=f879a000)
  get Phys(data[n=1]=f879b000)
  get Phys(data[n=1]=f879c000)
  get Phys(data[n=1]=f879d000)
  get Phys(data[n=1]=f879e000)
  get Phys(data[n=1]=f879f000)
  get Phys(data[n=1]=f87a0000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d5cf, Count 0x40(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d5cf count 0x40 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 8000, full size 8000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8fac
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d5cf, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3d5cf, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f87d8000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87d8000)
  get Phys(data[n=1]=f87d9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d5cf, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d5cf count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\wmilib.sys at F87D3000 with 7 pages
(../../ntoskrnl/io/pnpmgr/pnpmgr.c:464) \Driver\CMBATT->AddDevice(ACPI\ACPI0003\0) failed with status 0xc0000034
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8bd8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 407f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 407f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 80d40000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80d40000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x407f, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x407f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c91cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 43adf, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 43adf, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f8792000, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8792000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x43adf, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x43adf count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8cd4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4c6f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4c6f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8792000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8792000)
  get Phys(data[n=1]=f8793000)
  get Phys(data[n=2]=f8794000)
  get Phys(data[n=3]=f8795000)
  get Phys(data[n=4]=f8796000)
  get Phys(data[n=4]=f8797000)
  get Phys(data[n=4]=f8798000)
  get Phys(data[n=5]=f8799000)
  get Phys(data[n=5]=f879a000)
  get Phys(data[n=5]=f879b000)
  get Phys(data[n=5]=f879c000)
  get Phys(data[n=5]=f879d000)
  get Phys(data[n=6]=f879e000)
  get Phys(data[n=6]=f879f000)
  get Phys(data[n=6]=f87a0000)
  get Phys(data[n=6]=f87a1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4c6f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4c6f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8cd4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4cef, OrigWordsRequested 0x1800, DevSize 0x18
IdeReadWrite (REQ): Starting sector is 4cef, Number of WORDS 0x1800, DevSize 0x18
AtapiDmaSetup: mode 0x45, data f87a2000, count 3000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87a2000)
  get Phys(data[n=1]=f87a3000)
  get Phys(data[n=2]=f87a4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4cef, Count 0x18(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4cef count 0x18 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 3000, full size 3000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c90d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4c6f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 4c6f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f87d1000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87d1000)
  get Phys(data[n=1]=f87d2000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4c6f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4c6f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\floppy.sys at F87C1000 with 12 pages
(../../ntoskrnl/io/iomgr/driver.c:1575) '\Driver\FLOPPY' initialization failed, status (0xc000000e)
(../../ntoskrnl/io/iomgr/driver.c:61) Deleting driver object '\Driver\FLOPPY'
(../../ntoskrnl/io/iomgr/driver.c:1957) IopInitializeDriver() failed (Status c000000e)
(../../ntoskrnl/mm/ARM3/sysldr.c:935) Leaking driver: floppy.sys
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8cd4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4a0f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4a0f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f877c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f877c000)
  get Phys(data[n=1]=f877d000)
  get Phys(data[n=1]=f877e000)
  get Phys(data[n=1]=f877f000)
  get Phys(data[n=1]=f8780000)
  get Phys(data[n=2]=f8781000)
  get Phys(data[n=2]=f8782000)
  get Phys(data[n=2]=f8783000)
  get Phys(data[n=2]=f8784000)
  get Phys(data[n=2]=f8785000)
  get Phys(data[n=2]=f8786000)
  get Phys(data[n=2]=f8787000)
  get Phys(data[n=2]=f8788000)
  get Phys(data[n=2]=f8789000)
  get Phys(data[n=2]=f878a000)
  get Phys(data[n=2]=f878b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4a0f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4a0f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8cd4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4a8f, OrigWordsRequested 0x5000, DevSize 0x50
IdeReadWrite (REQ): Starting sector is 4a8f, Number of WORDS 0x5000, DevSize 0x50
AtapiDmaSetup: mode 0x45, data f878c000, count a000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f878c000)
  get Phys(data[n=1]=f878d000)
  get Phys(data[n=1]=f878e000)
  get Phys(data[n=1]=f878f000)
  get Phys(data[n=1]=f8790000)
  get Phys(data[n=2]=f8791000)
  get Phys(data[n=2]=f8792000)
  get Phys(data[n=2]=f8793000)
  get Phys(data[n=2]=f8794000)
  get Phys(data[n=2]=f8795000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4a8f, Count 0x50(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4a8f count 0x50 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a000, full size a000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c90d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4a0f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 4a0f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f87bb000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87bb000)
  get Phys(data[n=1]=f87bc000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4a0f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4a0f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\cdrom.sys at F87AE000 with f pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xf88c920c, CDB 0xf88c923c, AtaReq 0xb1298000, SCmd 0x25
UniataNeedQueueing: TopLevel, qd=0
Send to device 25
TopLevel (2), srb 0xf88c920c
TopLevel (3), AtaReq 0xb1298000
Try ATAPI send 25
AtapiSendCommand: req state 0x10, Action 3
AtapiSendCommand: prepare..., ATAPI CMD 25 (Cdb f88c923c)
  assume IN
AtapiSendCommand: use_dma=0, Cmd 25
AtapiSendCommand: AtapiDmaReinit()
AtapiDmaReinit: !(AtaReq->Flags & REQ_FLAG_DMA_OPERATION), fall to PIO on Device 1
AtapiSendCommand: use_dma=0
AtapiSendCommand: CMD_ACTION_EXEC
AtapiSendCommand: Cdb f88c923c Command 0x25 to TargetId 1 lun 0
AtapiSendCommand: Entered with status 0x50
AtapiSendCommand: Entry Status (0x50)
AtapiSendCommand: Poll for int. to send packet. Status (0x50)
AtapiSendCommand: status (0x58)
AtapiSendCommand: ExpectingInterrupt (0x1)
AtapiSendCommand: return SRB_STATUS_PENDING (3)
AtapiStartIo: next Srb f88c920c
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 3)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x4
  perform generic check
  clear unexpected DMA intr
AtapiDmaDone: dev -1
  getting status...
  ATAPI status 0x58
  base status 0x58
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  dev_type ATAPI
  OldReqState = 42
  continue service interrupt
AtapiInterrupt: ATAPI Entered with status (0x58)
AtapiInterrupt: iReason 2
AtapiInterrupt: ATAPI branch
AtapiInterrupt: iReason 2
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: get R wordCount 0x4
IdeIntr: Read 0x4 words
IdeIntr: PIO Read AtaReq->DataBuffer 0xf87ad1b8, srb->DataBuffer 0xf87ad1b8
  status re-check 0x50
AtapiInterrupt: all transferred, AtaReq->WordsLeft == 0
AtapiInterrupt: early complete ? status 50
AtapiInterrupt: CompleteRequest, srbstatus 1
AtapiInterrupt: PIO completion
AtapiInterrupt: PIO completion, wait BUSY
IdeIntr: ATAPI Read AtaReq->DataBuffer 0xf87ad1c0, srb->DataBuffer 0xf87ad1b8, len 0x8
   Transfered 0, full size 8
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xf88c920c, status 1
AtapiInterrupt: RequestComplete, srb 0xf88c920c
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x4
  perform generic check
  clear unexpected DMA intr
AtapiDmaDone: dev -1
  getting status...
  ATAPI status 0x50
  base status 0x50
  Unexpected interrupt.
  ATAPI additional check
AtapiCheckInterrupt__: ATAPI int reason 3
AtapiInterrupt(base): Catch unexpected
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xf88c9210, CDB 0xf88c9240, AtaReq 0xb1298000, SCmd 0xbd
UniataNeedQueueing: TopLevel, qd=0
Send to device bd
TopLevel (2), srb 0xf88c9210
TopLevel (3), AtaReq 0xb1298000
Try ATAPI send bd
AtapiSendCommand: req state 0x10, Action 3
AtapiSendCommand: prepare..., ATAPI CMD bd (Cdb f88c9240)
  assume IN
AtapiSendCommand: use_dma=0, Cmd bd
AtapiSendCommand: AtapiDmaReinit()
AtapiDmaReinit: !(AtaReq->Flags & REQ_FLAG_DMA_OPERATION), fall to PIO on Device 1
AtapiSendCommand: use_dma=0
AtapiSendCommand: CMD_ACTION_EXEC
AtapiSendCommand: Cdb f88c9240 Command 0xbd to TargetId 1 lun 0
AtapiSendCommand: Entered with status 0x50
AtapiSendCommand: Entry Status (0x50)
AtapiSendCommand: Poll for int. to send packet. Status (0x50)
AtapiSendCommand: status (0x58)
AtapiSendCommand: ExpectingInterrupt (0x1)
AtapiSendCommand: return SRB_STATUS_PENDING (3)
AtapiStartIo: next Srb f88c9210
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x4
  perform generic check
  clear unexpected DMA intr
AtapiDmaDone: dev -1
  getting status...
  ATAPI status 0x58
  base status 0x58
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  dev_type ATAPI
  OldReqState = 42
  continue service interrupt
AtapiInterrupt: ATAPI Entered with status (0x58)
AtapiInterrupt: iReason 2
AtapiInterrupt: ATAPI branch
AtapiInterrupt: iReason 2
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: get R wordCount 0x4
IdeIntr: Read 0x4 words
IdeIntr: PIO Read AtaReq->DataBuffer 0xf87ad1b8, srb->DataBuffer 0xf87ad1b8
  status re-check 0x50
AtapiInterrupt: all transferred, AtaReq->WordsLeft == 0
AtapiInterrupt: early complete ? status 50
AtapiInterrupt: CompleteRequest, srbstatus 1
AtapiInterrupt: PIO completion
AtapiInterrupt: PIO completion, wait BUSY
IdeIntr: ATAPI Read AtaReq->DataBuffer 0xf87ad1c0, srb->DataBuffer 0xf87ad1b8, len 0x8
   Transfered 0, full size 8
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xf88c9210, status 1
AtapiInterrupt: RequestComplete, srb 0xf88c9210
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x4
  perform generic check
  clear unexpected DMA intr
AtapiDmaDone: dev -1
  getting status...
  ATAPI status 0x50
  base status 0x50
  Unexpected interrupt.
  ATAPI additional check
AtapiCheckInterrupt__: ATAPI int reason 3
AtapiInterrupt(base): Catch unexpected
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xf88c9298, CDB 0xf88c92c8, AtaReq 0xb1298000, SCmd 0x1a
UniataNeedQueueing: TopLevel, qd=0
Send to device 1a
TopLevel (2), srb 0xf88c9298
TopLevel (3), AtaReq 0xb1298000
Try ATAPI send 1a
AtapiSendCommand: req state 0x10, Action 3
AtapiSendCommand: prepare..., ATAPI CMD 1a (Cdb f88c92c8)
  assume IN
AtapiSendCommand: use_dma=0, Cmd 1a
AtapiSendCommand: AtapiDmaReinit()
AtapiDmaReinit: !(AtaReq->Flags & REQ_FLAG_DMA_OPERATION), fall to PIO on Device 1
AtapiSendCommand: use_dma=0
AtapiSendCommand: CMD_ACTION_EXEC
AtapiSendCommand: Cdb f88c92c8 Command 0x1a to TargetId 1 lun 0
AtapiSendCommand: Entered with status 0x50
AtapiSendCommand: Entry Status (0x50)
AtapiSendCommand: Poll for int. to send packet. Status (0x50)
AtapiSendCommand: status (0x58)
AtapiSendCommand: ExpectingInterrupt (0x1)
AtapiSendCommand: return SRB_STATUS_PENDING (3)
AtapiStartIo: next Srb f88c9298
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x4
  perform generic check
  clear unexpected DMA intr
AtapiDmaDone: dev -1
  getting status...
  ATAPI status 0x41
  base status 0x41
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  dev_type ATAPI
  OldReqState = 42
  continue service interrupt
AtapiInterrupt: ATAPI Entered with status (0x41)
AtapiInterrupt: iReason 3
AtapiInterrupt: Error 0x50
  Bad Lba 0x0
  wait 10 ready after ATAPI error
  Intr on DRQ 0
AtapiInterrupt: ATAPI Error, int reason 3
Errors in PIO mode
AtapiInterrupt: Error
AtapiInterrupt: CompleteRequest, srbstatus 4
AtapiInterrupt: Error. Begin mapping...
MapError: Error register is 0x50
ATAPI: Illegal request
AtapiInterrupt: Check for underflow, AtaReq->WordsLeft a
AtapiInterrupt: RequestComplete
AtapiInterrupt: remove srb 0xf88c9298, status 4
AtapiInterrupt: RequestComplete, srb 0xf88c9298
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0f89978, CDB 0xb0f899a8, AtaReq 0xb1298000, SCmd 0x3
UniataNeedQueueing: TopLevel, qd=0
Send to device 3
TopLevel (2), srb 0xb0f89978
TopLevel (3), AtaReq 0xb1298000
Try ATAPI send 3
AtapiSendCommand: req state 0x10, Action 3
AtapiSendCommand: prepare..., ATAPI CMD 3 (Cdb b0f899a8)
  assume IN
AtapiSendCommand: SCSIOP_REQUEST_SENSE, no DMA setup
AtapiSendCommand: use_dma=0, Cmd 3
AtapiSendCommand: SCSIOP_REQUEST_SENSE -> no dma setup (2)
AtapiDmaReinit: !(AtaReq->Flags & REQ_FLAG_DMA_OPERATION), fall to PIO on Device 1
AtapiSendCommand: AtapiDmaReinit()
AtapiDmaReinit: !(AtaReq->Flags & REQ_FLAG_DMA_OPERATION), fall to PIO on Device 1
AtapiSendCommand: use_dma=0
AtapiSendCommand: CMD_ACTION_EXEC
AtapiSendCommand: Cdb b0f899a8 Command 0x3 to TargetId 1 lun 0
AtapiSendCommand: Entered with status 0x41
  continue with SCSIOP_REQUEST_SENSE
AtapiSendCommand: Entry Status (0x41)
AtapiSendCommand: Poll for int. to send packet. Status (0x41)
AtapiSendCommand: status (0x58)
AtapiSendCommand: ExpectingInterrupt (0x1)
AtapiSendCommand: return SRB_STATUS_PENDING (3)
AtapiStartIo: next Srb b0f89978
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 3)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x4
  perform generic check
  clear unexpected DMA intr
AtapiDmaDone: dev -1
  getting status...
  ATAPI status 0x58
  base status 0x58
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  dev_type ATAPI
  OldReqState = 42
  continue service interrupt
AtapiInterrupt: ATAPI Entered with status (0x58)
AtapiInterrupt: iReason 2
AtapiInterrupt: ATAPI branch
AtapiInterrupt: iReason 2
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: get R wordCount 0x9
IdeIntr: Read 0x9 words
IdeIntr: PIO Read AtaReq->DataBuffer 0xf87ac1e0, srb->DataBuffer 0xf87ac1e0
f0 00 05 00 00 00 00 0a 00 00 00 00 20 00 00 00
00 00
  status re-check 0x50
AtapiInterrupt: all transferred, AtaReq->WordsLeft == 0
AtapiInterrupt: early complete ? status 50
AtapiInterrupt: CompleteRequest, srbstatus 1
AtapiInterrupt: PIO completion
AtapiInterrupt: PIO completion, wait BUSY
IdeIntr: ATAPI Read AtaReq->DataBuffer 0xf87ac1f2, srb->DataBuffer 0xf87ac1e0, len 0x12
   Transfered 0, full size 12
AtapiInterrupt: RequestComplete
AtapiInterrupt: remove srb 0xb0f89978, status 1
AtapiInterrupt: RequestComplete, srb 0xb0f89978
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x4
  perform generic check
  clear unexpected DMA intr
AtapiDmaDone: dev -1
  getting status...
  ATAPI status 0x50
  base status 0x50
  Unexpected interrupt.
  ATAPI additional check
AtapiCheckInterrupt__: ATAPI int reason 3
AtapiInterrupt(base): Catch unexpected
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xf88c9298, CDB 0xf88c92c8, AtaReq 0xb1298000, SCmd 0x5a
UniataNeedQueueing: TopLevel, qd=0
Send to device 5a
TopLevel (2), srb 0xf88c9298
TopLevel (3), AtaReq 0xb1298000
Try ATAPI send 5a
AtapiSendCommand: req state 0x10, Action 3
AtapiSendCommand: prepare..., ATAPI CMD 5a (Cdb f88c92c8)
  assume IN
AtapiSendCommand: use_dma=0, Cmd 5a
AtapiSendCommand: AtapiDmaReinit()
AtapiDmaReinit: !(AtaReq->Flags & REQ_FLAG_DMA_OPERATION), fall to PIO on Device 1
AtapiSendCommand: use_dma=0
AtapiSendCommand: CMD_ACTION_EXEC
AtapiSendCommand: Cdb f88c92c8 Command 0x5a to TargetId 1 lun 0
AtapiSendCommand: Entered with status 0x50
AtapiSendCommand: Entry Status (0x50)
AtapiSendCommand: Poll for int. to send packet. Status (0x50)
AtapiSendCommand: status (0x58)
AtapiSendCommand: ExpectingInterrupt (0x1)
AtapiSendCommand: return SRB_STATUS_PENDING (3)
AtapiStartIo: next Srb f88c9298
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x4
  perform generic check
  clear unexpected DMA intr
AtapiDmaDone: dev -1
  getting status...
  ATAPI status 0x58
  base status 0x58
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  dev_type ATAPI
  OldReqState = 42
  continue service interrupt
AtapiInterrupt: ATAPI Entered with status (0x58)
AtapiInterrupt: iReason 2
AtapiInterrupt: ATAPI branch
AtapiInterrupt: iReason 2
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: get R wordCount 0x8
AtapiInterrupt: 12 words requested; 8 words xferred
IdeIntr: Read 0x8 words
IdeIntr: PIO Read AtaReq->DataBuffer 0xf87ad190, srb->DataBuffer 0xf87ad190
  status re-check 0x50
AtapiInterrupt: early complete + underrun ? status 50
AtapiInterrupt: CompleteRequest, srbstatus 1
AtapiInterrupt: PIO completion
AtapiInterrupt: PIO completion, wait BUSY
IdeIntr: ATAPI Read AtaReq->DataBuffer 0xf87ad1a0, srb->DataBuffer 0xf87ad190, len 0x18
AtapiInterrupt: Check for underflow, AtaReq->WordsLeft 4
   Transfered 0, full size 18
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xf88c9298, status 1
AtapiInterrupt: RequestComplete, srb 0xf88c9298
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x4
  perform generic check
  clear unexpected DMA intr
AtapiDmaDone: dev -1
  getting status...
  ATAPI status 0x50
  base status 0x50
  Unexpected interrupt.
  ATAPI additional check
AtapiCheckInterrupt__: ATAPI int reason 3
AtapiInterrupt(base): Catch unexpected
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8d3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b7a7, OrigWordsRequested 0x5800, DevSize 0x58
IdeReadWrite (REQ): Starting sector is 3b7a7, Number of WORDS 0x5800, DevSize 0x58
AtapiDmaSetup: mode 0x45, data f876d000, count b000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f876d000)
  get Phys(data[n=1]=f876e000)
  get Phys(data[n=2]=f876f000)
  get Phys(data[n=2]=f8770000)
  get Phys(data[n=2]=f8771000)
  get Phys(data[n=2]=f8772000)
  get Phys(data[n=2]=f8773000)
  get Phys(data[n=2]=f8774000)
  get Phys(data[n=2]=f8775000)
  get Phys(data[n=2]=f8776000)
  get Phys(data[n=2]=f8777000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b7a7, Count 0x58(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b7a7 count 0x58 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered b000, full size b000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c90d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b7a7, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3b7a7, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f87ac000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87ac000)
  get Phys(data[n=1]=f87ad000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b7a7, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b7a7 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\fs_rec.sys at F87A5000 with 9 pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8d3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b51f, OrigWordsRequested 0x4000, DevSize 0x40
IdeReadWrite (REQ): Starting sector is 3b51f, Number of WORDS 0x4000, DevSize 0x40
AtapiDmaSetup: mode 0x45, data f8764000, count 8000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8764000)
  get Phys(data[n=1]=f8765000)
  get Phys(data[n=1]=f8766000)
  get Phys(data[n=2]=f8767000)
  get Phys(data[n=2]=f8768000)
  get Phys(data[n=3]=f8769000)
  get Phys(data[n=4]=f876a000)
  get Phys(data[n=5]=f876b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b51f, Count 0x40(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b51f count 0x40 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 8000, full size 8000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c90d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b51f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3b51f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f87a3000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87a3000)
  get Phys(data[n=1]=f87a4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b51f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b51f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\null.sys at F879E000 with 7 pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8d3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b4d7, OrigWordsRequested 0x4800, DevSize 0x48
IdeReadWrite (REQ): Starting sector is 3b4d7, Number of WORDS 0x4800, DevSize 0x48
AtapiDmaSetup: mode 0x45, data f875d000, count 9000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f875d000)
  get Phys(data[n=1]=f875e000)
  get Phys(data[n=2]=f875f000)
  get Phys(data[n=2]=f8760000)
  get Phys(data[n=2]=f8761000)
  get Phys(data[n=2]=f8762000)
  get Phys(data[n=2]=f8763000)
  get Phys(data[n=3]=f8764000)
  get Phys(data[n=3]=f8765000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b4d7, Count 0x48(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b4d7 count 0x48 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 9000, full size 9000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c90d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b4d7, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3b4d7, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f879c000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f879c000)
  get Phys(data[n=1]=f879d000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b4d7, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b4d7 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\beep.sys at F8797000 with 7 pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8d3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 47d7, OrigWordsRequested 0x5800, DevSize 0x58
IdeReadWrite (REQ): Starting sector is 47d7, Number of WORDS 0x5800, DevSize 0x58
AtapiDmaSetup: mode 0x45, data f8756000, count b000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8756000)
  get Phys(data[n=1]=f8757000)
  get Phys(data[n=1]=f8758000)
  get Phys(data[n=1]=f8759000)
  get Phys(data[n=2]=f875a000)
  get Phys(data[n=2]=f875b000)
  get Phys(data[n=3]=f875c000)
  get Phys(data[n=3]=f875d000)
  get Phys(data[n=3]=f875e000)
  get Phys(data[n=3]=f875f000)
  get Phys(data[n=3]=f8760000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x47d7, Count 0x58(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x47d7 count 0x58 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered b000, full size b000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c90d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 47d7, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 47d7, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8795000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8795000)
  get Phys(data[n=1]=f8796000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x47d7, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x47d7 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\blue.sys at F878F000 with 8 pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8cd4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b88f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3b88f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f874e000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f874e000)
  get Phys(data[n=1]=f874f000)
  get Phys(data[n=1]=f8750000)
  get Phys(data[n=2]=f8751000)
  get Phys(data[n=2]=f8752000)
  get Phys(data[n=2]=f8753000)
  get Phys(data[n=2]=f8754000)
  get Phys(data[n=2]=f8755000)
  get Phys(data[n=2]=f8756000)
  get Phys(data[n=3]=f8757000)
  get Phys(data[n=3]=f8758000)
  get Phys(data[n=3]=f8759000)
  get Phys(data[n=3]=f875a000)
  get Phys(data[n=3]=f875b000)
  get Phys(data[n=3]=f875c000)
  get Phys(data[n=3]=f875d000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b88f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b88f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8cd4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b90f, OrigWordsRequested 0x2000, DevSize 0x20
IdeReadWrite (REQ): Starting sector is 3b90f, Number of WORDS 0x2000, DevSize 0x20
AtapiDmaSetup: mode 0x45, data f875e000, count 4000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f875e000)
  get Phys(data[n=1]=f875f000)
  get Phys(data[n=1]=f8760000)
  get Phys(data[n=1]=f8761000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b90f, Count 0x20(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b90f count 0x20 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 4000, full size 4000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c90d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b88f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3b88f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f878d000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f878d000)
  get Phys(data[n=1]=f878e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b88f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b88f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\npfs.sys at F8784000 with b pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8d3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b7ff, OrigWordsRequested 0x5000, DevSize 0x50
IdeReadWrite (REQ): Starting sector is 3b7ff, Number of WORDS 0x5000, DevSize 0x50
AtapiDmaSetup: mode 0x45, data f8743000, count a000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8743000)
  get Phys(data[n=1]=f8744000)
  get Phys(data[n=1]=f8745000)
  get Phys(data[n=1]=f8746000)
  get Phys(data[n=1]=f8747000)
  get Phys(data[n=1]=f8748000)
  get Phys(data[n=1]=f8749000)
  get Phys(data[n=1]=f874a000)
  get Phys(data[n=1]=f874b000)
  get Phys(data[n=1]=f874c000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b7ff, Count 0x50(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b7ff count 0x50 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a000, full size a000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c90d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b7ff, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3b7ff, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8782000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8782000)
  get Phys(data[n=1]=f8783000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b7ff, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b7ff count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\msfs.sys at F877D000 with 7 pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8d3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3c0cf, OrigWordsRequested 0x6800, DevSize 0x68
IdeReadWrite (REQ): Starting sector is 3c0cf, Number of WORDS 0x6800, DevSize 0x68
AtapiDmaSetup: mode 0x45, data f873c000, count d000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f873c000)
  get Phys(data[n=1]=f873d000)
  get Phys(data[n=2]=f873e000)
  get Phys(data[n=3]=f873f000)
  get Phys(data[n=3]=f8740000)
  get Phys(data[n=3]=f8741000)
  get Phys(data[n=3]=f8742000)
  get Phys(data[n=3]=f8743000)
  get Phys(data[n=3]=f8744000)
  get Phys(data[n=3]=f8745000)
  get Phys(data[n=3]=f8746000)
  get Phys(data[n=3]=f8747000)
  get Phys(data[n=3]=f8748000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3c0cf, Count 0x68(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3c0cf count 0x68 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered d000, full size d000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c90d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3c0cf, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3c0cf, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f877b000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f877b000)
  get Phys(data[n=1]=f877c000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3c0cf, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3c0cf count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\ndisuio.sys at F8773000 with a pages
(../../drivers/network/ndis/ndis/protocol.c:979)(ndisBindMiniportsToProtocol) Performing global bind for protocol 'NDISUIO'
(../../drivers/network/ndis/ndis/protocol.c:1075)(ndisBindMiniportsToProtocol) NDISUIO's BindAdapter handler returned 0x0 for \Device\{3cd326a3-11bb-4ada-8137-3927ee070294}
(../../drivers/network/ndisuio/main.c:101) NDISUIO: Loaded
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8cd4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3c137, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3c137, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8732000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8732000)
  get Phys(data[n=1]=f8733000)
  get Phys(data[n=2]=f8734000)
  get Phys(data[n=2]=f8735000)
  get Phys(data[n=3]=f8736000)
  get Phys(data[n=4]=f8737000)
  get Phys(data[n=5]=f8738000)
  get Phys(data[n=6]=f8739000)
  get Phys(data[n=6]=f873a000)
  get Phys(data[n=6]=f873b000)
  get Phys(data[n=7]=f873c000)
  get Phys(data[n=7]=f873d000)
  get Phys(data[n=7]=f873e000)
  get Phys(data[n=7]=f873f000)
  get Phys(data[n=7]=f8740000)
  get Phys(data[n=8]=f8741000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3c137, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3c137 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8cd4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3c1b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3c1b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8742000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8742000)
  get Phys(data[n=1]=f8743000)
  get Phys(data[n=1]=f8744000)
  get Phys(data[n=1]=f8745000)
  get Phys(data[n=1]=f8746000)
  get Phys(data[n=2]=f8747000)
  get Phys(data[n=2]=f8748000)
  get Phys(data[n=3]=f8749000)
  get Phys(data[n=3]=f874a000)
  get Phys(data[n=3]=f874b000)
  get Phys(data[n=3]=f874c000)
  get Phys(data[n=3]=f874d000)
  get Phys(data[n=3]=f874e000)
  get Phys(data[n=3]=f874f000)
  get Phys(data[n=3]=f8750000)
  get Phys(data[n=4]=f8751000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3c1b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3c1b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8cd4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3c237, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3c237, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8752000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8752000)
  get Phys(data[n=1]=f8753000)
  get Phys(data[n=1]=f8754000)
  get Phys(data[n=1]=f8755000)
  get Phys(data[n=1]=f8756000)
  get Phys(data[n=2]=f8757000)
  get Phys(data[n=2]=f8758000)
  get Phys(data[n=2]=f8759000)
  get Phys(data[n=2]=f875a000)
  get Phys(data[n=2]=f875b000)
  get Phys(data[n=2]=f875c000)
  get Phys(data[n=2]=f875d000)
  get Phys(data[n=2]=f875e000)
  get Phys(data[n=2]=f875f000)
  get Phys(data[n=2]=f8760000)
  get Phys(data[n=2]=f8761000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3c237, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3c237 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8cd4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3c2b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3c2b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8762000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8762000)
  get Phys(data[n=1]=f8763000)
  get Phys(data[n=1]=f8764000)
  get Phys(data[n=1]=f8765000)
  get Phys(data[n=2]=f8766000)
  get Phys(data[n=3]=f8767000)
  get Phys(data[n=3]=f8768000)
  get Phys(data[n=3]=f8769000)
  get Phys(data[n=3]=f876a000)
  get Phys(data[n=3]=f876b000)
  get Phys(data[n=3]=f876c000)
  get Phys(data[n=3]=f876d000)
  get Phys(data[n=3]=f876e000)
  get Phys(data[n=3]=f876f000)
  get Phys(data[n=3]=f8770000)
  get Phys(data[n=3]=f8771000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3c2b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3c2b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c90d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3c137, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3c137, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8771000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8771000)
  get Phys(data[n=1]=f8772000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3c137, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3c137 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\tcpip.sys at F8744000 with 2f pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c875c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3c337, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3c337, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86d8000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d8000)
  get Phys(data[n=1]=f86d9000)
  get Phys(data[n=2]=f86da000)
  get Phys(data[n=3]=f86db000)
  get Phys(data[n=3]=f86dc000)
  get Phys(data[n=3]=f86dd000)
  get Phys(data[n=3]=f86de000)
  get Phys(data[n=3]=f86df000)
  get Phys(data[n=3]=f86e0000)
  get Phys(data[n=3]=f86e1000)
  get Phys(data[n=3]=f86e2000)
  get Phys(data[n=3]=f86e3000)
  get Phys(data[n=3]=f86e4000)
  get Phys(data[n=3]=f86e5000)
  get Phys(data[n=3]=f86e6000)
  get Phys(data[n=3]=f86e7000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3c337, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3c337 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c875c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3c3b7, OrigWordsRequested 0x5000, DevSize 0x50
IdeReadWrite (REQ): Starting sector is 3c3b7, Number of WORDS 0x5000, DevSize 0x50
AtapiDmaSetup: mode 0x45, data f86e8000, count a000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86e8000)
  get Phys(data[n=1]=f86e9000)
  get Phys(data[n=2]=f86ea000)
  get Phys(data[n=3]=f86eb000)
  get Phys(data[n=4]=f86ec000)
  get Phys(data[n=5]=f86ed000)
  get Phys(data[n=5]=f86ee000)
  get Phys(data[n=5]=f86ef000)
  get Phys(data[n=6]=f86f0000)
  get Phys(data[n=6]=f86f1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3c3b7, Count 0x50(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3c3b7 count 0x50 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a000, full size a000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../drivers/network/ndis/ndis/protocol.c:986)(ndisBindMiniportsToProtocol) Performing standard bind for protocol 'TCPIP'
NDIS_STATUS_MEDIA_CONNECT
(../../drivers/network/ndis/ndis/protocol.c:1075)(ndisBindMiniportsToProtocol) TCPIP's BindAdapter handler returned 0x0 for \Device\{3cd326a3-11bb-4ada-8137-3927ee070294}
Unhandled event type: 6
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8cd4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3bcb7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3bcb7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86ff000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86ff000)
  get Phys(data[n=1]=f8700000)
  get Phys(data[n=1]=f8701000)
  get Phys(data[n=1]=f8702000)
  get Phys(data[n=1]=f8703000)
  get Phys(data[n=1]=f8704000)
  get Phys(data[n=1]=f8705000)
  get Phys(data[n=1]=f8706000)
  get Phys(data[n=1]=f8707000)
  get Phys(data[n=1]=f8708000)
  get Phys(data[n=1]=f8709000)
  get Phys(data[n=1]=f870a000)
  get Phys(data[n=2]=f870b000)
  get Phys(data[n=2]=f870c000)
  get Phys(data[n=3]=f870d000)
  get Phys(data[n=4]=f870e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3bcb7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3bcb7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8cd4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3bd37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3bd37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f870f000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f870f000)
  get Phys(data[n=1]=f8710000)
  get Phys(data[n=1]=f8711000)
  get Phys(data[n=1]=f8712000)
  get Phys(data[n=2]=f8713000)
  get Phys(data[n=2]=f8714000)
  get Phys(data[n=2]=f8715000)
  get Phys(data[n=2]=f8716000)
  get Phys(data[n=2]=f8717000)
  get Phys(data[n=3]=f8718000)
  get Phys(data[n=3]=f8719000)
  get Phys(data[n=3]=f871a000)
  get Phys(data[n=3]=f871b000)
  get Phys(data[n=3]=f871c000)
  get Phys(data[n=3]=f871d000)
  get Phys(data[n=4]=f871e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3bd37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3bd37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8cd4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3bdb7, OrigWordsRequested 0x5000, DevSize 0x50
IdeReadWrite (REQ): Starting sector is 3bdb7, Number of WORDS 0x5000, DevSize 0x50
AtapiDmaSetup: mode 0x45, data f871f000, count a000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f871f000)
  get Phys(data[n=1]=f8720000)
  get Phys(data[n=1]=f8721000)
  get Phys(data[n=1]=f8722000)
  get Phys(data[n=1]=f8723000)
  get Phys(data[n=1]=f8724000)
  get Phys(data[n=1]=f8725000)
  get Phys(data[n=1]=f8726000)
  get Phys(data[n=1]=f8727000)
  get Phys(data[n=2]=f8728000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3bdb7, Count 0x50(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3bdb7 count 0x50 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a000, full size a000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c90d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3bcb7, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3bcb7, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f873e000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f873e000)
  get Phys(data[n=1]=f873f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3bcb7, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3bcb7 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\afd.sys at F8728000 with 18 pages
(../../ntoskrnl/io/iomgr/file.c:421) Using IopParseDevice() hack. Requested invalid attributes: 1
(../../ntoskrnl/io/iomgr/file.c:421) Using IopParseDevice() hack. Requested invalid attributes: 1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb1060820, CDB 0xb1060850, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb1060820
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c95f8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f8727000, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8727000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b1060820
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb1060820, status 1
AtapiInterrupt: RequestComplete, srb 0xb1060820
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb1060820, CDB 0xb1060850, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb1060820
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c9668
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f87274d8, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f87274d8)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b1060820
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb1060820, status 1
AtapiInterrupt: RequestComplete, srb 0xb1060820
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff8378, CDB 0xb0ff83a8, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff8378
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c95f8
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f8727000, count 200, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=f8727000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff8378
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff8378, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff8378
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff8378, CDB 0xb0ff83a8, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff8378
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c9668
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 0, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 0, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f87274d8, count 200, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=f87274d8)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x0, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x0 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff8378
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff8378, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff8378
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8f50
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 61df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 61df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86e7000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86e7000)
  get Phys(data[n=1]=f86e8000)
  get Phys(data[n=1]=f86e9000)
  get Phys(data[n=1]=f86ea000)
  get Phys(data[n=1]=f86eb000)
  get Phys(data[n=1]=f86ec000)
  get Phys(data[n=1]=f86ed000)
  get Phys(data[n=1]=f86ee000)
  get Phys(data[n=1]=f86ef000)
  get Phys(data[n=2]=f86f0000)
  get Phys(data[n=2]=f86f1000)
  get Phys(data[n=2]=f86f2000)
  get Phys(data[n=2]=f86f3000)
  get Phys(data[n=2]=f86f4000)
  get Phys(data[n=2]=f86f5000)
  get Phys(data[n=3]=f86f6000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x61df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x61df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8f50
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 625f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 625f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86f7000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86f7000)
  get Phys(data[n=1]=f86f8000)
  get Phys(data[n=1]=f86f9000)
  get Phys(data[n=1]=f86fa000)
  get Phys(data[n=1]=f86fb000)
  get Phys(data[n=1]=f86fc000)
  get Phys(data[n=1]=f86fd000)
  get Phys(data[n=1]=f86fe000)
  get Phys(data[n=1]=f86ff000)
  get Phys(data[n=1]=f8700000)
  get Phys(data[n=1]=f8701000)
  get Phys(data[n=1]=f8702000)
  get Phys(data[n=1]=f8703000)
  get Phys(data[n=1]=f8704000)
  get Phys(data[n=2]=f8705000)
  get Phys(data[n=3]=f8706000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x625f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x625f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8f50
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 62df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 62df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8707000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8707000)
  get Phys(data[n=1]=f8708000)
  get Phys(data[n=1]=f8709000)
  get Phys(data[n=1]=f870a000)
  get Phys(data[n=1]=f870b000)
  get Phys(data[n=1]=f870c000)
  get Phys(data[n=1]=f870d000)
  get Phys(data[n=1]=f870e000)
  get Phys(data[n=1]=f870f000)
  get Phys(data[n=1]=f8710000)
  get Phys(data[n=1]=f8711000)
  get Phys(data[n=1]=f8712000)
  get Phys(data[n=2]=f8713000)
  get Phys(data[n=2]=f8714000)
  get Phys(data[n=3]=f8715000)
  get Phys(data[n=4]=f8716000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x62df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x62df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c8f50
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 635f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 635f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8717000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8717000)
  get Phys(data[n=1]=f8718000)
  get Phys(data[n=1]=f8719000)
  get Phys(data[n=1]=f871a000)
  get Phys(data[n=2]=f871b000)
  get Phys(data[n=2]=f871c000)
  get Phys(data[n=2]=f871d000)
  get Phys(data[n=2]=f871e000)
  get Phys(data[n=2]=f871f000)
  get Phys(data[n=3]=f8720000)
  get Phys(data[n=3]=f8721000)
  get Phys(data[n=3]=f8722000)
  get Phys(data[n=3]=f8723000)
  get Phys(data[n=3]=f8724000)
  get Phys(data[n=3]=f8725000)
  get Phys(data[n=4]=f8726000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x635f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x635f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c934c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 61df, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 61df, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8726000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8726000)
  get Phys(data[n=1]=f8727000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x61df, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x61df count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../drivers/bus/acpi/main.c:276) Fixed power button reported to power manager
(../../drivers/bus/acpi/main.c:281) Fixed sleep button reported to power manager
(../../ntoskrnl/po/events.c:267) Device capabilities: 0x3 ( POWER SLEEP )
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c9474
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 63df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 63df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80dc0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80dc0000)
  get Phys(data[n=1]=80dc1000)
  get Phys(data[n=1]=80dc2000)
  get Phys(data[n=2]=80dc3000)
  get Phys(data[n=2]=80dc4000)
  get Phys(data[n=2]=80dc5000)
  get Phys(data[n=2]=80dc6000)
  get Phys(data[n=2]=80dc7000)
  get Phys(data[n=2]=80dc8000)
  get Phys(data[n=3]=80dc9000)
  get Phys(data[n=3]=80dca000)
  get Phys(data[n=3]=80dcb000)
  get Phys(data[n=3]=80dcc000)
  get Phys(data[n=3]=80dcd000)
  get Phys(data[n=3]=80dce000)
  get Phys(data[n=3]=80dcf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x63df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x63df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c9474
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 645f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 645f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80dd0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80dd0000)
  get Phys(data[n=1]=80dd1000)
  get Phys(data[n=1]=80dd2000)
  get Phys(data[n=1]=80dd3000)
  get Phys(data[n=1]=80dd4000)
  get Phys(data[n=1]=80dd5000)
  get Phys(data[n=1]=80dd6000)
  get Phys(data[n=1]=80dd7000)
  get Phys(data[n=2]=80dd8000)
  get Phys(data[n=3]=80dd9000)
  get Phys(data[n=3]=80dda000)
  get Phys(data[n=3]=80ddb000)
  get Phys(data[n=3]=80ddc000)
  get Phys(data[n=3]=80ddd000)
  get Phys(data[n=3]=80dde000)
  get Phys(data[n=3]=80ddf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x645f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x645f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c9474
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 64df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 64df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80de0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80de0000)
  get Phys(data[n=1]=80de1000)
  get Phys(data[n=1]=80de2000)
  get Phys(data[n=1]=80de3000)
  get Phys(data[n=1]=80de4000)
  get Phys(data[n=1]=80de5000)
  get Phys(data[n=2]=80de6000)
  get Phys(data[n=2]=80de7000)
  get Phys(data[n=3]=80de8000)
  get Phys(data[n=4]=80de9000)
  get Phys(data[n=5]=80dea000)
  get Phys(data[n=5]=80deb000)
  get Phys(data[n=5]=80dec000)
  get Phys(data[n=6]=80ded000)
  get Phys(data[n=7]=80dee000)
  get Phys(data[n=7]=80def000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x64df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x64df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c9474
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 655f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 655f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80df0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80df0000)
  get Phys(data[n=1]=80df1000)
  get Phys(data[n=1]=80df2000)
  get Phys(data[n=2]=80df3000)
  get Phys(data[n=2]=80df4000)
  get Phys(data[n=2]=80df5000)
  get Phys(data[n=2]=80df6000)
  get Phys(data[n=2]=80df7000)
  get Phys(data[n=2]=80df8000)
  get Phys(data[n=3]=80df9000)
  get Phys(data[n=3]=80dfa000)
  get Phys(data[n=4]=80dfb000)
  get Phys(data[n=4]=80dfc000)
  get Phys(data[n=4]=80dfd000)
  get Phys(data[n=4]=80dfe000)
  get Phys(data[n=4]=80dff000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x655f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x655f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/mminit.c:1170) Loader pages freed: 106
(../../ntoskrnl/ex/init.c:1924) Free non-cache pages: 1e10c
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c9030
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 14bff, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 14bff, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86e7000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86e7000)
  get Phys(data[n=1]=f86e8000)
  get Phys(data[n=1]=f86e9000)
  get Phys(data[n=1]=f86ea000)
  get Phys(data[n=1]=f86eb000)
  get Phys(data[n=2]=f86ec000)
  get Phys(data[n=2]=f86ed000)
  get Phys(data[n=2]=f86ee000)
  get Phys(data[n=2]=f86ef000)
  get Phys(data[n=2]=f86f0000)
  get Phys(data[n=2]=f86f1000)
  get Phys(data[n=2]=f86f2000)
  get Phys(data[n=2]=f86f3000)
  get Phys(data[n=2]=f86f4000)
  get Phys(data[n=2]=f86f5000)
  get Phys(data[n=2]=f86f6000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x14bff, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x14bff count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c9030
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 14c7f, OrigWordsRequested 0x7400, DevSize 0x74
IdeReadWrite (REQ): Starting sector is 14c7f, Number of WORDS 0x7400, DevSize 0x74
AtapiDmaSetup: mode 0x45, data f86f7000, count e800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86f7000)
  get Phys(data[n=1]=f86f8000)
  get Phys(data[n=1]=f86f9000)
  get Phys(data[n=1]=f86fa000)
  get Phys(data[n=2]=f86fb000)
  get Phys(data[n=3]=f86fc000)
  get Phys(data[n=3]=f86fd000)
  get Phys(data[n=3]=f86fe000)
  get Phys(data[n=3]=f86ff000)
  get Phys(data[n=3]=f8700000)
  get Phys(data[n=3]=f8701000)
  get Phys(data[n=3]=f8702000)
  get Phys(data[n=3]=f8703000)
  get Phys(data[n=3]=f8704000)
  get Phys(data[n=3]=f8705000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x14c7f, Count 0x74(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x14c7f count 0x74 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e800, full size e800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c942c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 14bff, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 14bff, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8726000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8726000)
  get Phys(data[n=1]=f8727000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x14bff, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x14bff count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c00000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80c00000)
  get Phys(data[n=1]=80c01000)
  get Phys(data[n=2]=80c02000)
  get Phys(data[n=2]=80c03000)
  get Phys(data[n=2]=80c04000)
  get Phys(data[n=2]=80c05000)
  get Phys(data[n=2]=80c06000)
  get Phys(data[n=2]=80c07000)
  get Phys(data[n=3]=80c08000)
  get Phys(data[n=3]=80c09000)
  get Phys(data[n=3]=80c0a000)
  get Phys(data[n=3]=80c0b000)
  get Phys(data[n=3]=80c0c000)
  get Phys(data[n=3]=80c0d000)
  get Phys(data[n=3]=80c0e000)
  get Phys(data[n=3]=80c0f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5f, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x5f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0f31f68, CDB 0xb0f31f98, AtaReq 0xb1299018, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=1
Non-empty queue
Try IDE prepare
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb1299018
** --- **
** Ide: Command continue prep
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c10000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=80c10000)
  get Phys(data[n=1]=80c11000)
  get Phys(data[n=1]=80c12000)
  get Phys(data[n=1]=80c13000)
  get Phys(data[n=1]=80c14000)
  get Phys(data[n=1]=80c15000)
  get Phys(data[n=1]=80c16000)
  get Phys(data[n=1]=80c17000)
  get Phys(data[n=2]=80c18000)
  get Phys(data[n=2]=80c19000)
  get Phys(data[n=2]=80c1a000)
  get Phys(data[n=2]=80c1b000)
  get Phys(data[n=2]=80c1c000)
  get Phys(data[n=2]=80c1d000)
  get Phys(data[n=2]=80c1e000)
  get Phys(data[n=2]=80c1f000)
  set TERM
AtapiDmaSetup: OK
IdeSendCommand: SRB_STATUS_PENDING
AtapiStartIo: Already have 2 request(s)!
AtapiStartIo: next Srb b0f31f68
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0xb0f31f68
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0f31f68, CDB 0xb0f31f98, AtaReq 0xb1299018, SCmd 0x2a
UniataNeedQueueing: qd=1
Send to device 2a
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865664
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (ExecOnly):
IdeReadWrite: Lba 0xdf, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0xdf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0f31f68
AtapiStartIo: query PORT for next request
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0f31f68, status 1
AtapiInterrupt: RequestComplete, srb 0xb0f31f68
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 15f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 15f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c20000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80c20000)
  get Phys(data[n=1]=80c21000)
  get Phys(data[n=1]=80c22000)
  get Phys(data[n=1]=80c23000)
  get Phys(data[n=1]=80c24000)
  get Phys(data[n=1]=80c25000)
  get Phys(data[n=1]=80c26000)
  get Phys(data[n=1]=80c27000)
  get Phys(data[n=2]=80c28000)
  get Phys(data[n=3]=80c29000)
  get Phys(data[n=4]=80c2a000)
  get Phys(data[n=4]=80c2b000)
  get Phys(data[n=4]=80c2c000)
  get Phys(data[n=5]=80c2d000)
  get Phys(data[n=5]=80c2e000)
  get Phys(data[n=5]=80c2f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x15f, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x15f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c30000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80c30000)
  get Phys(data[n=1]=80c31000)
  get Phys(data[n=2]=80c32000)
  get Phys(data[n=2]=80c33000)
  get Phys(data[n=2]=80c34000)
  get Phys(data[n=2]=80c35000)
  get Phys(data[n=2]=80c36000)
  get Phys(data[n=2]=80c37000)
  get Phys(data[n=3]=80c38000)
  get Phys(data[n=3]=80c39000)
  get Phys(data[n=3]=80c3a000)
  get Phys(data[n=3]=80c3b000)
  get Phys(data[n=3]=80c3c000)
  get Phys(data[n=3]=80c3d000)
  get Phys(data[n=3]=80c3e000)
  get Phys(data[n=3]=80c3f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1df, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 204f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 204f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c00000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80c00000)
  get Phys(data[n=1]=80c01000)
  get Phys(data[n=2]=80c02000)
  get Phys(data[n=2]=80c03000)
  get Phys(data[n=2]=80c04000)
  get Phys(data[n=2]=80c05000)
  get Phys(data[n=2]=80c06000)
  get Phys(data[n=2]=80c07000)
  get Phys(data[n=3]=80c08000)
  get Phys(data[n=3]=80c09000)
  get Phys(data[n=3]=80c0a000)
  get Phys(data[n=3]=80c0b000)
  get Phys(data[n=3]=80c0c000)
  get Phys(data[n=3]=80c0d000)
  get Phys(data[n=3]=80c0e000)
  get Phys(data[n=3]=80c0f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x204f, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x204f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 20cf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 20cf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c10000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80c10000)
  get Phys(data[n=1]=80c11000)
  get Phys(data[n=1]=80c12000)
  get Phys(data[n=1]=80c13000)
  get Phys(data[n=1]=80c14000)
  get Phys(data[n=1]=80c15000)
  get Phys(data[n=1]=80c16000)
  get Phys(data[n=1]=80c17000)
  get Phys(data[n=2]=80c18000)
  get Phys(data[n=2]=80c19000)
  get Phys(data[n=2]=80c1a000)
  get Phys(data[n=2]=80c1b000)
  get Phys(data[n=2]=80c1c000)
  get Phys(data[n=2]=80c1d000)
  get Phys(data[n=2]=80c1e000)
  get Phys(data[n=2]=80c1f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x20cf, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x20cf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 214f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 214f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c20000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80c20000)
  get Phys(data[n=1]=80c21000)
  get Phys(data[n=1]=80c22000)
  get Phys(data[n=1]=80c23000)
  get Phys(data[n=1]=80c24000)
  get Phys(data[n=1]=80c25000)
  get Phys(data[n=1]=80c26000)
  get Phys(data[n=1]=80c27000)
  get Phys(data[n=2]=80c28000)
  get Phys(data[n=3]=80c29000)
  get Phys(data[n=4]=80c2a000)
  get Phys(data[n=4]=80c2b000)
  get Phys(data[n=4]=80c2c000)
  get Phys(data[n=5]=80c2d000)
  get Phys(data[n=5]=80c2e000)
  get Phys(data[n=5]=80c2f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x214f, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x214f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 21cf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 21cf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c30000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80c30000)
  get Phys(data[n=1]=80c31000)
  get Phys(data[n=2]=80c32000)
  get Phys(data[n=2]=80c33000)
  get Phys(data[n=2]=80c34000)
  get Phys(data[n=2]=80c35000)
  get Phys(data[n=2]=80c36000)
  get Phys(data[n=2]=80c37000)
  get Phys(data[n=3]=80c38000)
  get Phys(data[n=3]=80c39000)
  get Phys(data[n=3]=80c3a000)
  get Phys(data[n=3]=80c3b000)
  get Phys(data[n=3]=80c3c000)
  get Phys(data[n=3]=80c3d000)
  get Phys(data[n=3]=80c3e000)
  get Phys(data[n=3]=80c3f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x21cf, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x21cf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
WARNING:  RtlCreateTagHeap at ../../lib/rtl/heap.c:3983 is UNIMPLEMENTED!
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725e50
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4077, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 4077, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 80e40000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80e40000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4077, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4077 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725e50
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 48267, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 48267, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 80e41000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80e41000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x48267, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x48267 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725e50
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4cd87, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 4cd87, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 80e42000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80e42000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4cd87, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4cd87 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf872634c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 65f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 65f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80ec0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80ec0000)
  get Phys(data[n=1]=80ec1000)
  get Phys(data[n=1]=80ec2000)
  get Phys(data[n=1]=80ec3000)
  get Phys(data[n=2]=80ec4000)
  get Phys(data[n=2]=80ec5000)
  get Phys(data[n=3]=80ec6000)
  get Phys(data[n=3]=80ec7000)
  get Phys(data[n=4]=80ec8000)
  get Phys(data[n=5]=80ec9000)
  get Phys(data[n=6]=80eca000)
  get Phys(data[n=6]=80ecb000)
  get Phys(data[n=6]=80ecc000)
  get Phys(data[n=6]=80ecd000)
  get Phys(data[n=7]=80ece000)
  get Phys(data[n=8]=80ecf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x65f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x65f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf872634c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 6df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 6df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80ed0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80ed0000)
  get Phys(data[n=1]=80ed1000)
  get Phys(data[n=1]=80ed2000)
  get Phys(data[n=2]=80ed3000)
  get Phys(data[n=2]=80ed4000)
  get Phys(data[n=2]=80ed5000)
  get Phys(data[n=2]=80ed6000)
  get Phys(data[n=2]=80ed7000)
  get Phys(data[n=2]=80ed8000)
  get Phys(data[n=3]=80ed9000)
  get Phys(data[n=3]=80eda000)
  get Phys(data[n=4]=80edb000)
  get Phys(data[n=4]=80edc000)
  get Phys(data[n=4]=80edd000)
  get Phys(data[n=4]=80ede000)
  get Phys(data[n=4]=80edf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x6df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x6df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf872634c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 75f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 75f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80ee0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80ee0000)
  get Phys(data[n=1]=80ee1000)
  get Phys(data[n=1]=80ee2000)
  get Phys(data[n=2]=80ee3000)
  get Phys(data[n=2]=80ee4000)
  get Phys(data[n=2]=80ee5000)
  get Phys(data[n=2]=80ee6000)
  get Phys(data[n=2]=80ee7000)
  get Phys(data[n=2]=80ee8000)
  get Phys(data[n=3]=80ee9000)
  get Phys(data[n=3]=80eea000)
  get Phys(data[n=3]=80eeb000)
  get Phys(data[n=3]=80eec000)
  get Phys(data[n=3]=80eed000)
  get Phys(data[n=3]=80eee000)
  get Phys(data[n=3]=80eef000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x75f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x75f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf872634c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 7df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 7df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80ef0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80ef0000)
  get Phys(data[n=1]=80ef1000)
  get Phys(data[n=1]=80ef2000)
  get Phys(data[n=1]=80ef3000)
  get Phys(data[n=1]=80ef4000)
  get Phys(data[n=1]=80ef5000)
  get Phys(data[n=1]=80ef6000)
  get Phys(data[n=1]=80ef7000)
  get Phys(data[n=2]=80ef8000)
  get Phys(data[n=3]=80ef9000)
  get Phys(data[n=3]=80efa000)
  get Phys(data[n=3]=80efb000)
  get Phys(data[n=3]=80efc000)
  get Phys(data[n=3]=80efd000)
  get Phys(data[n=3]=80efe000)
  get Phys(data[n=3]=80eff000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x7df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x7df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf872662c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e20e7, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 1e20e7, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data 80e80000, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80e80000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e20e7, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e20e7 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726650
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e20e7, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1e20e7, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 80e80000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80e80000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e20e7, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1e20e7 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1468f, OrigWordsRequested 0x1600, DevSize 0x16
IdeReadWrite (REQ): Starting sector is 1468f, Number of WORDS 0x1600, DevSize 0x16
AtapiDmaSetup: mode 0x45, data f86d6000, count 2c00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d6000)
  get Phys(data[n=1]=f86d7000)
  get Phys(data[n=1]=f86d8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1468f, Count 0x16(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1468f count 0x16 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2c00, full size 2c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1468f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 1468f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8715000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8715000)
  get Phys(data[n=1]=f8716000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1468f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1468f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8715338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38307, OrigWordsRequested 0x3400, DevSize 0x34
IdeReadWrite (REQ): Starting sector is 38307, Number of WORDS 0x3400, DevSize 0x34
AtapiDmaSetup: mode 0x45, data f86d1000, count 6800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d1000)
  get Phys(data[n=1]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=1]=f86d4000)
  get Phys(data[n=2]=f86d5000)
  get Phys(data[n=2]=f86d6000)
  get Phys(data[n=2]=f86d7000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38307, Count 0x34(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38307 count 0x34 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 6800, full size 6800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87156cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38307, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 38307, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38307, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38307 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87155c4
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 3f, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f8711000, count 200, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3f count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87155bc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 7f, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 7f, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f8711000, count 200, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x7f, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x7f count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf871544c
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 3f, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f8711428, count 200, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=f8711428)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3f count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf871544c
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 3f, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f8711428, count 200, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=f8711428)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3f count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8715184
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 269, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 269, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80f00000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=80f00000)
  get Phys(data[n=1]=80f01000)
  get Phys(data[n=1]=80f02000)
  get Phys(data[n=2]=80f03000)
  get Phys(data[n=2]=80f04000)
  get Phys(data[n=2]=80f05000)
  get Phys(data[n=2]=80f06000)
  get Phys(data[n=2]=80f07000)
  get Phys(data[n=2]=80f08000)
  get Phys(data[n=2]=80f09000)
  get Phys(data[n=2]=80f0a000)
  get Phys(data[n=3]=80f0b000)
  get Phys(data[n=3]=80f0c000)
  get Phys(data[n=3]=80f0d000)
  get Phys(data[n=3]=80f0e000)
  get Phys(data[n=3]=80f0f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x269, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x269 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8715184
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80f10000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=80f10000)
  get Phys(data[n=1]=80f11000)
  get Phys(data[n=1]=80f12000)
  get Phys(data[n=1]=80f13000)
  get Phys(data[n=1]=80f14000)
  get Phys(data[n=1]=80f15000)
  get Phys(data[n=1]=80f16000)
  get Phys(data[n=2]=80f17000)
  get Phys(data[n=2]=80f18000)
  get Phys(data[n=2]=80f19000)
  get Phys(data[n=2]=80f1a000)
  get Phys(data[n=2]=80f1b000)
  get Phys(data[n=2]=80f1c000)
  get Phys(data[n=2]=80f1d000)
  get Phys(data[n=2]=80f1e000)
  get Phys(data[n=2]=80f1f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8715184
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 369, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 369, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80f20000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=80f20000)
  get Phys(data[n=1]=80f21000)
  get Phys(data[n=1]=80f22000)
  get Phys(data[n=1]=80f23000)
  get Phys(data[n=1]=80f24000)
  get Phys(data[n=1]=80f25000)
  get Phys(data[n=1]=80f26000)
  get Phys(data[n=2]=80f27000)
  get Phys(data[n=2]=80f28000)
  get Phys(data[n=2]=80f29000)
  get Phys(data[n=2]=80f2a000)
  get Phys(data[n=2]=80f2b000)
  get Phys(data[n=3]=80f2c000)
  get Phys(data[n=3]=80f2d000)
  get Phys(data[n=4]=80f2e000)
  get Phys(data[n=4]=80f2f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x369, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x369 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8715184
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80f30000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=80f30000)
  get Phys(data[n=1]=80f31000)
  get Phys(data[n=2]=80f32000)
  get Phys(data[n=2]=80f33000)
  get Phys(data[n=2]=80f34000)
  get Phys(data[n=2]=80f35000)
  get Phys(data[n=3]=80f36000)
  get Phys(data[n=4]=80f37000)
  get Phys(data[n=4]=80f38000)
  get Phys(data[n=4]=80f39000)
  get Phys(data[n=4]=80f3a000)
  get Phys(data[n=5]=80f3b000)
  get Phys(data[n=5]=80f3c000)
  get Phys(data[n=5]=80f3d000)
  get Phys(data[n=5]=80f3e000)
  get Phys(data[n=5]=80f3f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87152cc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 8aa07, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 8aa07, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 80f40000, count 1000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=80f40000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x8aa07, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x8aa07 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8715264
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80f80000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=80f80000)
  get Phys(data[n=1]=80f81000)
  get Phys(data[n=1]=80f82000)
  get Phys(data[n=2]=80f83000)
  get Phys(data[n=2]=80f84000)
  get Phys(data[n=2]=80f85000)
  get Phys(data[n=2]=80f86000)
  get Phys(data[n=2]=80f87000)
  get Phys(data[n=2]=80f88000)
  get Phys(data[n=2]=80f89000)
  get Phys(data[n=2]=80f8a000)
  get Phys(data[n=3]=80f8b000)
  get Phys(data[n=3]=80f8c000)
  get Phys(data[n=3]=80f8d000)
  get Phys(data[n=3]=80f8e000)
  get Phys(data[n=3]=80f8f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8715264
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80f90000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=80f90000)
  get Phys(data[n=1]=80f91000)
  get Phys(data[n=1]=80f92000)
  get Phys(data[n=1]=80f93000)
  get Phys(data[n=1]=80f94000)
  get Phys(data[n=1]=80f95000)
  get Phys(data[n=1]=80f96000)
  get Phys(data[n=2]=80f97000)
  get Phys(data[n=2]=80f98000)
  get Phys(data[n=2]=80f99000)
  get Phys(data[n=2]=80f9a000)
  get Phys(data[n=2]=80f9b000)
  get Phys(data[n=2]=80f9c000)
  get Phys(data[n=2]=80f9d000)
  get Phys(data[n=2]=80f9e000)
  get Phys(data[n=2]=80f9f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xe9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0xe9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8715264
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 169, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 169, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80fa0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=80fa0000)
  get Phys(data[n=1]=80fa1000)
  get Phys(data[n=1]=80fa2000)
  get Phys(data[n=1]=80fa3000)
  get Phys(data[n=1]=80fa4000)
  get Phys(data[n=1]=80fa5000)
  get Phys(data[n=1]=80fa6000)
  get Phys(data[n=2]=80fa7000)
  get Phys(data[n=2]=80fa8000)
  get Phys(data[n=2]=80fa9000)
  get Phys(data[n=2]=80faa000)
  get Phys(data[n=2]=80fab000)
  get Phys(data[n=3]=80fac000)
  get Phys(data[n=3]=80fad000)
  get Phys(data[n=4]=80fae000)
  get Phys(data[n=4]=80faf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x169, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x169 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8715264
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80fb0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=80fb0000)
  get Phys(data[n=1]=80fb1000)
  get Phys(data[n=2]=80fb2000)
  get Phys(data[n=2]=80fb3000)
  get Phys(data[n=2]=80fb4000)
  get Phys(data[n=2]=80fb5000)
  get Phys(data[n=3]=80fb6000)
  get Phys(data[n=4]=80fb7000)
  get Phys(data[n=4]=80fb8000)
  get Phys(data[n=4]=80fb9000)
  get Phys(data[n=4]=80fba000)
  get Phys(data[n=5]=80fbb000)
  get Phys(data[n=5]=80fbc000)
  get Phys(data[n=5]=80fbd000)
  get Phys(data[n=5]=80fbe000)
  get Phys(data[n=5]=80fbf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8715338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38307, OrigWordsRequested 0x3400, DevSize 0x34
IdeReadWrite (REQ): Starting sector is 38307, Number of WORDS 0x3400, DevSize 0x34
AtapiDmaSetup: mode 0x45, data f86d1000, count 6800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d1000)
  get Phys(data[n=1]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=2]=f86d4000)
  get Phys(data[n=2]=f86d5000)
  get Phys(data[n=2]=f86d6000)
  get Phys(data[n=2]=f86d7000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38307, Count 0x34(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38307 count 0x34 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 6800, full size 6800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87156cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38307, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 38307, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38307, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38307 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e20e7, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 1e20e7, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data 80e80000, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80e80000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e20e7, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e20e7 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726650
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e20e7, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1e20e7, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 80e80000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80e80000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e20e7, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1e20e7 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1fa8f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1fa8f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86d2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=2]=f86d4000)
  get Phys(data[n=2]=f86d5000)
  get Phys(data[n=2]=f86d6000)
  get Phys(data[n=2]=f86d7000)
  get Phys(data[n=2]=f86d8000)
  get Phys(data[n=2]=f86d9000)
  get Phys(data[n=3]=f86da000)
  get Phys(data[n=3]=f86db000)
  get Phys(data[n=3]=f86dc000)
  get Phys(data[n=3]=f86dd000)
  get Phys(data[n=3]=f86de000)
  get Phys(data[n=3]=f86df000)
  get Phys(data[n=4]=f86e0000)
  get Phys(data[n=4]=f86e1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1fa8f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1fa8f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1fb0f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1fb0f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86e2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86e2000)
  get Phys(data[n=1]=f86e3000)
  get Phys(data[n=1]=f86e4000)
  get Phys(data[n=1]=f86e5000)
  get Phys(data[n=1]=f86e6000)
  get Phys(data[n=1]=f86e7000)
  get Phys(data[n=1]=f86e8000)
  get Phys(data[n=2]=f86e9000)
  get Phys(data[n=3]=f86ea000)
  get Phys(data[n=3]=f86eb000)
  get Phys(data[n=3]=f86ec000)
  get Phys(data[n=3]=f86ed000)
  get Phys(data[n=3]=f86ee000)
  get Phys(data[n=3]=f86ef000)
  get Phys(data[n=3]=f86f0000)
  get Phys(data[n=4]=f86f1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1fb0f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1fb0f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1fb8f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1fb8f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86f2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86f2000)
  get Phys(data[n=1]=f86f3000)
  get Phys(data[n=1]=f86f4000)
  get Phys(data[n=2]=f86f5000)
  get Phys(data[n=2]=f86f6000)
  get Phys(data[n=3]=f86f7000)
  get Phys(data[n=3]=f86f8000)
  get Phys(data[n=4]=f86f9000)
  get Phys(data[n=5]=f86fa000)
  get Phys(data[n=6]=f86fb000)
  get Phys(data[n=6]=f86fc000)
  get Phys(data[n=6]=f86fd000)
  get Phys(data[n=6]=f86fe000)
  get Phys(data[n=7]=f86ff000)
  get Phys(data[n=8]=f8700000)
  get Phys(data[n=8]=f8701000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1fb8f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1fb8f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1fc0f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1fc0f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8702000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8702000)
  get Phys(data[n=1]=f8703000)
  get Phys(data[n=2]=f8704000)
  get Phys(data[n=2]=f8705000)
  get Phys(data[n=2]=f8706000)
  get Phys(data[n=2]=f8707000)
  get Phys(data[n=2]=f8708000)
  get Phys(data[n=2]=f8709000)
  get Phys(data[n=3]=f870a000)
  get Phys(data[n=3]=f870b000)
  get Phys(data[n=4]=f870c000)
  get Phys(data[n=4]=f870d000)
  get Phys(data[n=4]=f870e000)
  get Phys(data[n=4]=f870f000)
  get Phys(data[n=4]=f8710000)
  get Phys(data[n=4]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1fc0f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1fc0f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1fa8f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 1fa8f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1fa8f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1fa8f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 21a17, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 21a17, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86d2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=1]=f86d4000)
  get Phys(data[n=1]=f86d5000)
  get Phys(data[n=1]=f86d6000)
  get Phys(data[n=1]=f86d7000)
  get Phys(data[n=2]=f86d8000)
  get Phys(data[n=2]=f86d9000)
  get Phys(data[n=2]=f86da000)
  get Phys(data[n=2]=f86db000)
  get Phys(data[n=2]=f86dc000)
  get Phys(data[n=2]=f86dd000)
  get Phys(data[n=3]=f86de000)
  get Phys(data[n=3]=f86df000)
  get Phys(data[n=3]=f86e0000)
  get Phys(data[n=3]=f86e1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x21a17, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x21a17 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 21a97, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 21a97, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86e2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86e2000)
  get Phys(data[n=1]=f86e3000)
  get Phys(data[n=1]=f86e4000)
  get Phys(data[n=1]=f86e5000)
  get Phys(data[n=1]=f86e6000)
  get Phys(data[n=2]=f86e7000)
  get Phys(data[n=3]=f86e8000)
  get Phys(data[n=3]=f86e9000)
  get Phys(data[n=3]=f86ea000)
  get Phys(data[n=3]=f86eb000)
  get Phys(data[n=3]=f86ec000)
  get Phys(data[n=3]=f86ed000)
  get Phys(data[n=3]=f86ee000)
  get Phys(data[n=4]=f86ef000)
  get Phys(data[n=4]=f86f0000)
  get Phys(data[n=4]=f86f1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x21a97, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x21a97 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 21b17, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 21b17, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86f2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86f2000)
  get Phys(data[n=1]=f86f3000)
  get Phys(data[n=1]=f86f4000)
  get Phys(data[n=2]=f86f5000)
  get Phys(data[n=2]=f86f6000)
  get Phys(data[n=3]=f86f7000)
  get Phys(data[n=4]=f86f8000)
  get Phys(data[n=5]=f86f9000)
  get Phys(data[n=5]=f86fa000)
  get Phys(data[n=5]=f86fb000)
  get Phys(data[n=5]=f86fc000)
  get Phys(data[n=6]=f86fd000)
  get Phys(data[n=7]=f86fe000)
  get Phys(data[n=7]=f86ff000)
  get Phys(data[n=7]=f8700000)
  get Phys(data[n=7]=f8701000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x21b17, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x21b17 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 21b97, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 21b97, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8702000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8702000)
  get Phys(data[n=1]=f8703000)
  get Phys(data[n=1]=f8704000)
  get Phys(data[n=1]=f8705000)
  get Phys(data[n=1]=f8706000)
  get Phys(data[n=1]=f8707000)
  get Phys(data[n=2]=f8708000)
  get Phys(data[n=2]=f8709000)
  get Phys(data[n=3]=f870a000)
  get Phys(data[n=3]=f870b000)
  get Phys(data[n=3]=f870c000)
  get Phys(data[n=3]=f870d000)
  get Phys(data[n=3]=f870e000)
  get Phys(data[n=3]=f870f000)
  get Phys(data[n=3]=f8710000)
  get Phys(data[n=3]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x21b97, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x21b97 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 21a17, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 21a17, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x21a17, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x21a17 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 502d7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 502d7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86d2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=2]=f86d4000)
  get Phys(data[n=3]=f86d5000)
  get Phys(data[n=3]=f86d6000)
  get Phys(data[n=3]=f86d7000)
  get Phys(data[n=3]=f86d8000)
  get Phys(data[n=3]=f86d9000)
  get Phys(data[n=3]=f86da000)
  get Phys(data[n=4]=f86db000)
  get Phys(data[n=4]=f86dc000)
  get Phys(data[n=4]=f86dd000)
  get Phys(data[n=4]=f86de000)
  get Phys(data[n=4]=f86df000)
  get Phys(data[n=4]=f86e0000)
  get Phys(data[n=4]=f86e1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x502d7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x502d7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 50357, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 50357, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86e2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86e2000)
  get Phys(data[n=1]=f86e3000)
  get Phys(data[n=2]=f86e4000)
  get Phys(data[n=3]=f86e5000)
  get Phys(data[n=3]=f86e6000)
  get Phys(data[n=3]=f86e7000)
  get Phys(data[n=3]=f86e8000)
  get Phys(data[n=3]=f86e9000)
  get Phys(data[n=3]=f86ea000)
  get Phys(data[n=3]=f86eb000)
  get Phys(data[n=4]=f86ec000)
  get Phys(data[n=4]=f86ed000)
  get Phys(data[n=4]=f86ee000)
  get Phys(data[n=4]=f86ef000)
  get Phys(data[n=5]=f86f0000)
  get Phys(data[n=5]=f86f1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x50357, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x50357 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 503d7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 503d7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86f2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86f2000)
  get Phys(data[n=1]=f86f3000)
  get Phys(data[n=2]=f86f4000)
  get Phys(data[n=3]=f86f5000)
  get Phys(data[n=4]=f86f6000)
  get Phys(data[n=4]=f86f7000)
  get Phys(data[n=4]=f86f8000)
  get Phys(data[n=4]=f86f9000)
  get Phys(data[n=5]=f86fa000)
  get Phys(data[n=6]=f86fb000)
  get Phys(data[n=6]=f86fc000)
  get Phys(data[n=6]=f86fd000)
  get Phys(data[n=6]=f86fe000)
  get Phys(data[n=7]=f86ff000)
  get Phys(data[n=7]=f8700000)
  get Phys(data[n=7]=f8701000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x503d7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x503d7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 50457, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 50457, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8702000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8702000)
  get Phys(data[n=1]=f8703000)
  get Phys(data[n=1]=f8704000)
  get Phys(data[n=2]=f8705000)
  get Phys(data[n=2]=f8706000)
  get Phys(data[n=3]=f8707000)
  get Phys(data[n=3]=f8708000)
  get Phys(data[n=3]=f8709000)
  get Phys(data[n=3]=f870a000)
  get Phys(data[n=3]=f870b000)
  get Phys(data[n=3]=f870c000)
  get Phys(data[n=3]=f870d000)
  get Phys(data[n=3]=f870e000)
  get Phys(data[n=4]=f870f000)
  get Phys(data[n=4]=f8710000)
  get Phys(data[n=4]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x50457, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x50457 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 502d7, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 502d7, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x502d7, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x502d7 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 24b5f, OrigWordsRequested 0x8500, DevSize 0x85
IdeReadWrite (REQ): Starting sector is 24b5f, Number of WORDS 0x8500, DevSize 0x85
AtapiDmaSetup: mode 0x45, data f86d2000, count 10a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=1]=f86d4000)
  get Phys(data[n=1]=f86d5000)
  get Phys(data[n=1]=f86d6000)
  get Phys(data[n=1]=f86d7000)
  get Phys(data[n=1]=f86d8000)
  get Phys(data[n=2]=f86d9000)
  get Phys(data[n=2]=f86da000)
  get Phys(data[n=2]=f86db000)
  get Phys(data[n=2]=f86dc000)
  get Phys(data[n=2]=f86dd000)
  get Phys(data[n=2]=f86de000)
  get Phys(data[n=2]=f86df000)
  get Phys(data[n=2]=f86e0000)
  get Phys(data[n=2]=f86e1000)
  get Phys(data[n=3]=f86e2000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x24b5f, Count 0x85(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x24b5f count 0x85 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10a00, full size 10a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 24b5f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 24b5f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x24b5f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x24b5f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 25637, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 25637, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86d2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=1]=f86d4000)
  get Phys(data[n=1]=f86d5000)
  get Phys(data[n=1]=f86d6000)
  get Phys(data[n=2]=f86d7000)
  get Phys(data[n=2]=f86d8000)
  get Phys(data[n=2]=f86d9000)
  get Phys(data[n=2]=f86da000)
  get Phys(data[n=2]=f86db000)
  get Phys(data[n=2]=f86dc000)
  get Phys(data[n=2]=f86dd000)
  get Phys(data[n=2]=f86de000)
  get Phys(data[n=2]=f86df000)
  get Phys(data[n=3]=f86e0000)
  get Phys(data[n=4]=f86e1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x25637, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x25637 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 256b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 256b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86e2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86e2000)
  get Phys(data[n=1]=f86e3000)
  get Phys(data[n=1]=f86e4000)
  get Phys(data[n=1]=f86e5000)
  get Phys(data[n=1]=f86e6000)
  get Phys(data[n=1]=f86e7000)
  get Phys(data[n=2]=f86e8000)
  get Phys(data[n=2]=f86e9000)
  get Phys(data[n=2]=f86ea000)
  get Phys(data[n=2]=f86eb000)
  get Phys(data[n=3]=f86ec000)
  get Phys(data[n=3]=f86ed000)
  get Phys(data[n=4]=f86ee000)
  get Phys(data[n=4]=f86ef000)
  get Phys(data[n=5]=f86f0000)
  get Phys(data[n=6]=f86f1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x256b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x256b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 25737, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 25737, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86f2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86f2000)
  get Phys(data[n=1]=f86f3000)
  get Phys(data[n=1]=f86f4000)
  get Phys(data[n=1]=f86f5000)
  get Phys(data[n=2]=f86f6000)
  get Phys(data[n=3]=f86f7000)
  get Phys(data[n=3]=f86f8000)
  get Phys(data[n=3]=f86f9000)
  get Phys(data[n=3]=f86fa000)
  get Phys(data[n=4]=f86fb000)
  get Phys(data[n=4]=f86fc000)
  get Phys(data[n=4]=f86fd000)
  get Phys(data[n=4]=f86fe000)
  get Phys(data[n=4]=f86ff000)
  get Phys(data[n=4]=f8700000)
  get Phys(data[n=5]=f8701000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x25737, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x25737 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 257b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 257b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8702000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8702000)
  get Phys(data[n=1]=f8703000)
  get Phys(data[n=1]=f8704000)
  get Phys(data[n=1]=f8705000)
  get Phys(data[n=1]=f8706000)
  get Phys(data[n=1]=f8707000)
  get Phys(data[n=1]=f8708000)
  get Phys(data[n=1]=f8709000)
  get Phys(data[n=1]=f870a000)
  get Phys(data[n=2]=f870b000)
  get Phys(data[n=2]=f870c000)
  get Phys(data[n=2]=f870d000)
  get Phys(data[n=2]=f870e000)
  get Phys(data[n=2]=f870f000)
  get Phys(data[n=2]=f8710000)
  get Phys(data[n=3]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x257b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x257b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 25637, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 25637, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x25637, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x25637 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 26417, OrigWordsRequested 0x900, DevSize 0x9
IdeReadWrite (REQ): Starting sector is 26417, Number of WORDS 0x900, DevSize 0x9
AtapiDmaSetup: mode 0x45, data f86d2000, count 1200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x26417, Count 0x9(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x26417 count 0x9 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1200, full size 1200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 26417, OrigWordsRequested 0x900, DevSize 0x9
IdeReadWrite (REQ): Starting sector is 26417, Number of WORDS 0x900, DevSize 0x9
AtapiDmaSetup: mode 0x45, data f8710000, count 1200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x26417, Count 0x9(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x26417 count 0x9 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1200, full size 1200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 28fef, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 28fef, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86d2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=1]=f86d4000)
  get Phys(data[n=1]=f86d5000)
  get Phys(data[n=1]=f86d6000)
  get Phys(data[n=1]=f86d7000)
  get Phys(data[n=1]=f86d8000)
  get Phys(data[n=1]=f86d9000)
  get Phys(data[n=1]=f86da000)
  get Phys(data[n=1]=f86db000)
  get Phys(data[n=2]=f86dc000)
  get Phys(data[n=3]=f86dd000)
  get Phys(data[n=3]=f86de000)
  get Phys(data[n=3]=f86df000)
  get Phys(data[n=3]=f86e0000)
  get Phys(data[n=3]=f86e1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x28fef, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x28fef count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2906f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2906f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86e2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86e2000)
  get Phys(data[n=1]=f86e3000)
  get Phys(data[n=2]=f86e4000)
  get Phys(data[n=2]=f86e5000)
  get Phys(data[n=2]=f86e6000)
  get Phys(data[n=2]=f86e7000)
  get Phys(data[n=3]=f86e8000)
  get Phys(data[n=3]=f86e9000)
  get Phys(data[n=4]=f86ea000)
  get Phys(data[n=4]=f86eb000)
  get Phys(data[n=5]=f86ec000)
  get Phys(data[n=6]=f86ed000)
  get Phys(data[n=7]=f86ee000)
  get Phys(data[n=7]=f86ef000)
  get Phys(data[n=7]=f86f0000)
  get Phys(data[n=7]=f86f1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2906f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2906f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 290ef, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 290ef, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86f2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86f2000)
  get Phys(data[n=1]=f86f3000)
  get Phys(data[n=1]=f86f4000)
  get Phys(data[n=1]=f86f5000)
  get Phys(data[n=1]=f86f6000)
  get Phys(data[n=2]=f86f7000)
  get Phys(data[n=2]=f86f8000)
  get Phys(data[n=2]=f86f9000)
  get Phys(data[n=2]=f86fa000)
  get Phys(data[n=2]=f86fb000)
  get Phys(data[n=2]=f86fc000)
  get Phys(data[n=3]=f86fd000)
  get Phys(data[n=3]=f86fe000)
  get Phys(data[n=4]=f86ff000)
  get Phys(data[n=4]=f8700000)
  get Phys(data[n=4]=f8701000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x290ef, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x290ef count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2916f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2916f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8702000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8702000)
  get Phys(data[n=1]=f8703000)
  get Phys(data[n=1]=f8704000)
  get Phys(data[n=1]=f8705000)
  get Phys(data[n=1]=f8706000)
  get Phys(data[n=2]=f8707000)
  get Phys(data[n=2]=f8708000)
  get Phys(data[n=2]=f8709000)
  get Phys(data[n=2]=f870a000)
  get Phys(data[n=2]=f870b000)
  get Phys(data[n=2]=f870c000)
  get Phys(data[n=3]=f870d000)
  get Phys(data[n=3]=f870e000)
  get Phys(data[n=3]=f870f000)
  get Phys(data[n=3]=f8710000)
  get Phys(data[n=3]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2916f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2916f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 28fef, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 28fef, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x28fef, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x28fef count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2bdbf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2bdbf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86d2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=1]=f86d4000)
  get Phys(data[n=1]=f86d5000)
  get Phys(data[n=1]=f86d6000)
  get Phys(data[n=1]=f86d7000)
  get Phys(data[n=1]=f86d8000)
  get Phys(data[n=1]=f86d9000)
  get Phys(data[n=2]=f86da000)
  get Phys(data[n=3]=f86db000)
  get Phys(data[n=3]=f86dc000)
  get Phys(data[n=3]=f86dd000)
  get Phys(data[n=3]=f86de000)
  get Phys(data[n=3]=f86df000)
  get Phys(data[n=3]=f86e0000)
  get Phys(data[n=3]=f86e1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2bdbf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2bdbf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2be3f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2be3f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86e2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86e2000)
  get Phys(data[n=1]=f86e3000)
  get Phys(data[n=1]=f86e4000)
  get Phys(data[n=1]=f86e5000)
  get Phys(data[n=2]=f86e6000)
  get Phys(data[n=2]=f86e7000)
  get Phys(data[n=3]=f86e8000)
  get Phys(data[n=3]=f86e9000)
  get Phys(data[n=4]=f86ea000)
  get Phys(data[n=5]=f86eb000)
  get Phys(data[n=6]=f86ec000)
  get Phys(data[n=6]=f86ed000)
  get Phys(data[n=6]=f86ee000)
  get Phys(data[n=6]=f86ef000)
  get Phys(data[n=7]=f86f0000)
  get Phys(data[n=8]=f86f1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2be3f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2be3f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2bebf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2bebf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86f2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86f2000)
  get Phys(data[n=1]=f86f3000)
  get Phys(data[n=1]=f86f4000)
  get Phys(data[n=2]=f86f5000)
  get Phys(data[n=2]=f86f6000)
  get Phys(data[n=2]=f86f7000)
  get Phys(data[n=2]=f86f8000)
  get Phys(data[n=2]=f86f9000)
  get Phys(data[n=2]=f86fa000)
  get Phys(data[n=3]=f86fb000)
  get Phys(data[n=3]=f86fc000)
  get Phys(data[n=4]=f86fd000)
  get Phys(data[n=4]=f86fe000)
  get Phys(data[n=4]=f86ff000)
  get Phys(data[n=4]=f8700000)
  get Phys(data[n=4]=f8701000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2bebf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2bebf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2bf3f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2bf3f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8702000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8702000)
  get Phys(data[n=1]=f8703000)
  get Phys(data[n=1]=f8704000)
  get Phys(data[n=2]=f8705000)
  get Phys(data[n=2]=f8706000)
  get Phys(data[n=2]=f8707000)
  get Phys(data[n=2]=f8708000)
  get Phys(data[n=2]=f8709000)
  get Phys(data[n=2]=f870a000)
  get Phys(data[n=3]=f870b000)
  get Phys(data[n=3]=f870c000)
  get Phys(data[n=3]=f870d000)
  get Phys(data[n=3]=f870e000)
  get Phys(data[n=3]=f870f000)
  get Phys(data[n=3]=f8710000)
  get Phys(data[n=4]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2bf3f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2bf3f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2bdbf, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 2bdbf, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2bdbf, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2bdbf count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2cb8f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2cb8f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86d2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=1]=f86d4000)
  get Phys(data[n=1]=f86d5000)
  get Phys(data[n=1]=f86d6000)
  get Phys(data[n=1]=f86d7000)
  get Phys(data[n=2]=f86d8000)
  get Phys(data[n=3]=f86d9000)
  get Phys(data[n=3]=f86da000)
  get Phys(data[n=3]=f86db000)
  get Phys(data[n=3]=f86dc000)
  get Phys(data[n=3]=f86dd000)
  get Phys(data[n=3]=f86de000)
  get Phys(data[n=3]=f86df000)
  get Phys(data[n=4]=f86e0000)
  get Phys(data[n=4]=f86e1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2cb8f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2cb8f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2cc0f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2cc0f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86e2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86e2000)
  get Phys(data[n=1]=f86e3000)
  get Phys(data[n=2]=f86e4000)
  get Phys(data[n=2]=f86e5000)
  get Phys(data[n=3]=f86e6000)
  get Phys(data[n=3]=f86e7000)
  get Phys(data[n=4]=f86e8000)
  get Phys(data[n=5]=f86e9000)
  get Phys(data[n=6]=f86ea000)
  get Phys(data[n=6]=f86eb000)
  get Phys(data[n=6]=f86ec000)
  get Phys(data[n=6]=f86ed000)
  get Phys(data[n=7]=f86ee000)
  get Phys(data[n=8]=f86ef000)
  get Phys(data[n=8]=f86f0000)
  get Phys(data[n=8]=f86f1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2cc0f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2cc0f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2cc8f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2cc8f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86f2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86f2000)
  get Phys(data[n=1]=f86f3000)
  get Phys(data[n=1]=f86f4000)
  get Phys(data[n=1]=f86f5000)
  get Phys(data[n=1]=f86f6000)
  get Phys(data[n=1]=f86f7000)
  get Phys(data[n=1]=f86f8000)
  get Phys(data[n=2]=f86f9000)
  get Phys(data[n=2]=f86fa000)
  get Phys(data[n=3]=f86fb000)
  get Phys(data[n=3]=f86fc000)
  get Phys(data[n=3]=f86fd000)
  get Phys(data[n=3]=f86fe000)
  get Phys(data[n=3]=f86ff000)
  get Phys(data[n=3]=f8700000)
  get Phys(data[n=3]=f8701000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2cc8f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2cc8f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2cd0f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2cd0f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8702000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8702000)
  get Phys(data[n=1]=f8703000)
  get Phys(data[n=1]=f8704000)
  get Phys(data[n=1]=f8705000)
  get Phys(data[n=1]=f8706000)
  get Phys(data[n=1]=f8707000)
  get Phys(data[n=1]=f8708000)
  get Phys(data[n=2]=f8709000)
  get Phys(data[n=2]=f870a000)
  get Phys(data[n=2]=f870b000)
  get Phys(data[n=2]=f870c000)
  get Phys(data[n=2]=f870d000)
  get Phys(data[n=2]=f870e000)
  get Phys(data[n=3]=f870f000)
  get Phys(data[n=3]=f8710000)
  get Phys(data[n=3]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2cd0f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2cd0f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2cb8f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 2cb8f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2cb8f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2cb8f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2d73f, OrigWordsRequested 0x3c00, DevSize 0x3c
IdeReadWrite (REQ): Starting sector is 2d73f, Number of WORDS 0x3c00, DevSize 0x3c
AtapiDmaSetup: mode 0x45, data f86d2000, count 7800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=1]=f86d4000)
  get Phys(data[n=1]=f86d5000)
  get Phys(data[n=2]=f86d6000)
  get Phys(data[n=3]=f86d7000)
  get Phys(data[n=3]=f86d8000)
  get Phys(data[n=3]=f86d9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2d73f, Count 0x3c(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2d73f count 0x3c feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 7800, full size 7800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2d73f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 2d73f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2d73f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2d73f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2d8cf, OrigWordsRequested 0x2000, DevSize 0x20
IdeReadWrite (REQ): Starting sector is 2d8cf, Number of WORDS 0x2000, DevSize 0x20
AtapiDmaSetup: mode 0x45, data f86d2000, count 4000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=2]=f86d4000)
  get Phys(data[n=3]=f86d5000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2d8cf, Count 0x20(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2d8cf count 0x20 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 4000, full size 4000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2d8cf, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 2d8cf, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2d8cf, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2d8cf count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2d8ef, OrigWordsRequested 0x4d00, DevSize 0x4d
IdeReadWrite (REQ): Starting sector is 2d8ef, Number of WORDS 0x4d00, DevSize 0x4d
AtapiDmaSetup: mode 0x45, data f86d2000, count 9a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=1]=f86d4000)
  get Phys(data[n=1]=f86d5000)
  get Phys(data[n=1]=f86d6000)
  get Phys(data[n=1]=f86d7000)
  get Phys(data[n=1]=f86d8000)
  get Phys(data[n=1]=f86d9000)
  get Phys(data[n=2]=f86da000)
  get Phys(data[n=2]=f86db000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2d8ef, Count 0x4d(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2d8ef count 0x4d feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 9a00, full size 9a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2d8ef, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 2d8ef, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2d8ef, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2d8ef count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2eeff, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2eeff, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86d2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=1]=f86d4000)
  get Phys(data[n=1]=f86d5000)
  get Phys(data[n=1]=f86d6000)
  get Phys(data[n=1]=f86d7000)
  get Phys(data[n=2]=f86d8000)
  get Phys(data[n=2]=f86d9000)
  get Phys(data[n=2]=f86da000)
  get Phys(data[n=2]=f86db000)
  get Phys(data[n=3]=f86dc000)
  get Phys(data[n=3]=f86dd000)
  get Phys(data[n=4]=f86de000)
  get Phys(data[n=4]=f86df000)
  get Phys(data[n=5]=f86e0000)
  get Phys(data[n=6]=f86e1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2eeff, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2eeff count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2ef7f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2ef7f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86e2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86e2000)
  get Phys(data[n=1]=f86e3000)
  get Phys(data[n=1]=f86e4000)
  get Phys(data[n=1]=f86e5000)
  get Phys(data[n=2]=f86e6000)
  get Phys(data[n=3]=f86e7000)
  get Phys(data[n=3]=f86e8000)
  get Phys(data[n=3]=f86e9000)
  get Phys(data[n=3]=f86ea000)
  get Phys(data[n=4]=f86eb000)
  get Phys(data[n=4]=f86ec000)
  get Phys(data[n=4]=f86ed000)
  get Phys(data[n=4]=f86ee000)
  get Phys(data[n=4]=f86ef000)
  get Phys(data[n=4]=f86f0000)
  get Phys(data[n=5]=f86f1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2ef7f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2ef7f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2efff, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2efff, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86f2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86f2000)
  get Phys(data[n=1]=f86f3000)
  get Phys(data[n=1]=f86f4000)
  get Phys(data[n=1]=f86f5000)
  get Phys(data[n=1]=f86f6000)
  get Phys(data[n=1]=f86f7000)
  get Phys(data[n=1]=f86f8000)
  get Phys(data[n=1]=f86f9000)
  get Phys(data[n=1]=f86fa000)
  get Phys(data[n=2]=f86fb000)
  get Phys(data[n=2]=f86fc000)
  get Phys(data[n=2]=f86fd000)
  get Phys(data[n=2]=f86fe000)
  get Phys(data[n=2]=f86ff000)
  get Phys(data[n=2]=f8700000)
  get Phys(data[n=3]=f8701000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2efff, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2efff count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2f07f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2f07f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8702000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8702000)
  get Phys(data[n=1]=f8703000)
  get Phys(data[n=1]=f8704000)
  get Phys(data[n=1]=f8705000)
  get Phys(data[n=1]=f8706000)
  get Phys(data[n=2]=f8707000)
  get Phys(data[n=2]=f8708000)
  get Phys(data[n=2]=f8709000)
  get Phys(data[n=2]=f870a000)
  get Phys(data[n=2]=f870b000)
  get Phys(data[n=2]=f870c000)
  get Phys(data[n=2]=f870d000)
  get Phys(data[n=2]=f870e000)
  get Phys(data[n=2]=f870f000)
  get Phys(data[n=3]=f8710000)
  get Phys(data[n=4]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2f07f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2f07f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2eeff, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 2eeff, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2eeff, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2eeff count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 30b47, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 30b47, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86d2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=1]=f86d4000)
  get Phys(data[n=1]=f86d5000)
  get Phys(data[n=2]=f86d6000)
  get Phys(data[n=2]=f86d7000)
  get Phys(data[n=2]=f86d8000)
  get Phys(data[n=2]=f86d9000)
  get Phys(data[n=3]=f86da000)
  get Phys(data[n=3]=f86db000)
  get Phys(data[n=4]=f86dc000)
  get Phys(data[n=4]=f86dd000)
  get Phys(data[n=5]=f86de000)
  get Phys(data[n=6]=f86df000)
  get Phys(data[n=7]=f86e0000)
  get Phys(data[n=7]=f86e1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x30b47, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x30b47 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 30bc7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 30bc7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86e2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86e2000)
  get Phys(data[n=1]=f86e3000)
  get Phys(data[n=2]=f86e4000)
  get Phys(data[n=3]=f86e5000)
  get Phys(data[n=3]=f86e6000)
  get Phys(data[n=3]=f86e7000)
  get Phys(data[n=3]=f86e8000)
  get Phys(data[n=4]=f86e9000)
  get Phys(data[n=4]=f86ea000)
  get Phys(data[n=4]=f86eb000)
  get Phys(data[n=4]=f86ec000)
  get Phys(data[n=4]=f86ed000)
  get Phys(data[n=4]=f86ee000)
  get Phys(data[n=5]=f86ef000)
  get Phys(data[n=5]=f86f0000)
  get Phys(data[n=6]=f86f1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x30bc7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x30bc7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 30c47, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 30c47, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86f2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86f2000)
  get Phys(data[n=1]=f86f3000)
  get Phys(data[n=1]=f86f4000)
  get Phys(data[n=1]=f86f5000)
  get Phys(data[n=1]=f86f6000)
  get Phys(data[n=1]=f86f7000)
  get Phys(data[n=1]=f86f8000)
  get Phys(data[n=2]=f86f9000)
  get Phys(data[n=2]=f86fa000)
  get Phys(data[n=2]=f86fb000)
  get Phys(data[n=2]=f86fc000)
  get Phys(data[n=2]=f86fd000)
  get Phys(data[n=2]=f86fe000)
  get Phys(data[n=3]=f86ff000)
  get Phys(data[n=3]=f8700000)
  get Phys(data[n=3]=f8701000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x30c47, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x30c47 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 30cc7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 30cc7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8702000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8702000)
  get Phys(data[n=1]=f8703000)
  get Phys(data[n=1]=f8704000)
  get Phys(data[n=2]=f8705000)
  get Phys(data[n=2]=f8706000)
  get Phys(data[n=2]=f8707000)
  get Phys(data[n=2]=f8708000)
  get Phys(data[n=2]=f8709000)
  get Phys(data[n=2]=f870a000)
  get Phys(data[n=2]=f870b000)
  get Phys(data[n=2]=f870c000)
  get Phys(data[n=2]=f870d000)
  get Phys(data[n=3]=f870e000)
  get Phys(data[n=4]=f870f000)
  get Phys(data[n=4]=f8710000)
  get Phys(data[n=4]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x30cc7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x30cc7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 30b47, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 30b47, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x30b47, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x30b47 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3841f, OrigWordsRequested 0x4d00, DevSize 0x4d
IdeReadWrite (REQ): Starting sector is 3841f, Number of WORDS 0x4d00, DevSize 0x4d
AtapiDmaSetup: mode 0x45, data f86d2000, count 9a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=2]=f86d4000)
  get Phys(data[n=2]=f86d5000)
  get Phys(data[n=2]=f86d6000)
  get Phys(data[n=2]=f86d7000)
  get Phys(data[n=3]=f86d8000)
  get Phys(data[n=3]=f86d9000)
  get Phys(data[n=4]=f86da000)
  get Phys(data[n=4]=f86db000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3841f, Count 0x4d(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3841f count 0x4d feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 9a00, full size 9a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3841f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3841f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3841f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3841f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3846f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3846f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86d2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=1]=f86d4000)
  get Phys(data[n=1]=f86d5000)
  get Phys(data[n=2]=f86d6000)
  get Phys(data[n=2]=f86d7000)
  get Phys(data[n=3]=f86d8000)
  get Phys(data[n=3]=f86d9000)
  get Phys(data[n=4]=f86da000)
  get Phys(data[n=5]=f86db000)
  get Phys(data[n=6]=f86dc000)
  get Phys(data[n=6]=f86dd000)
  get Phys(data[n=6]=f86de000)
  get Phys(data[n=6]=f86df000)
  get Phys(data[n=7]=f86e0000)
  get Phys(data[n=8]=f86e1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3846f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3846f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 384ef, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 384ef, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86e2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86e2000)
  get Phys(data[n=1]=f86e3000)
  get Phys(data[n=1]=f86e4000)
  get Phys(data[n=2]=f86e5000)
  get Phys(data[n=2]=f86e6000)
  get Phys(data[n=2]=f86e7000)
  get Phys(data[n=2]=f86e8000)
  get Phys(data[n=2]=f86e9000)
  get Phys(data[n=2]=f86ea000)
  get Phys(data[n=3]=f86eb000)
  get Phys(data[n=3]=f86ec000)
  get Phys(data[n=4]=f86ed000)
  get Phys(data[n=4]=f86ee000)
  get Phys(data[n=4]=f86ef000)
  get Phys(data[n=4]=f86f0000)
  get Phys(data[n=4]=f86f1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x384ef, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x384ef count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3856f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3856f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86f2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86f2000)
  get Phys(data[n=1]=f86f3000)
  get Phys(data[n=1]=f86f4000)
  get Phys(data[n=2]=f86f5000)
  get Phys(data[n=2]=f86f6000)
  get Phys(data[n=2]=f86f7000)
  get Phys(data[n=2]=f86f8000)
  get Phys(data[n=2]=f86f9000)
  get Phys(data[n=2]=f86fa000)
  get Phys(data[n=3]=f86fb000)
  get Phys(data[n=3]=f86fc000)
  get Phys(data[n=3]=f86fd000)
  get Phys(data[n=3]=f86fe000)
  get Phys(data[n=3]=f86ff000)
  get Phys(data[n=3]=f8700000)
  get Phys(data[n=4]=f8701000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3856f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3856f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 385ef, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 385ef, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8702000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8702000)
  get Phys(data[n=1]=f8703000)
  get Phys(data[n=1]=f8704000)
  get Phys(data[n=1]=f8705000)
  get Phys(data[n=1]=f8706000)
  get Phys(data[n=1]=f8707000)
  get Phys(data[n=1]=f8708000)
  get Phys(data[n=1]=f8709000)
  get Phys(data[n=2]=f870a000)
  get Phys(data[n=3]=f870b000)
  get Phys(data[n=3]=f870c000)
  get Phys(data[n=3]=f870d000)
  get Phys(data[n=3]=f870e000)
  get Phys(data[n=3]=f870f000)
  get Phys(data[n=3]=f8710000)
  get Phys(data[n=3]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x385ef, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x385ef count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3846f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3846f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3846f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3846f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 50607, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 50607, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86d2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=2]=f86d4000)
  get Phys(data[n=2]=f86d5000)
  get Phys(data[n=3]=f86d6000)
  get Phys(data[n=3]=f86d7000)
  get Phys(data[n=4]=f86d8000)
  get Phys(data[n=5]=f86d9000)
  get Phys(data[n=6]=f86da000)
  get Phys(data[n=6]=f86db000)
  get Phys(data[n=6]=f86dc000)
  get Phys(data[n=6]=f86dd000)
  get Phys(data[n=7]=f86de000)
  get Phys(data[n=8]=f86df000)
  get Phys(data[n=8]=f86e0000)
  get Phys(data[n=8]=f86e1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x50607, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x50607 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 50687, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 50687, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86e2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86e2000)
  get Phys(data[n=1]=f86e3000)
  get Phys(data[n=1]=f86e4000)
  get Phys(data[n=1]=f86e5000)
  get Phys(data[n=1]=f86e6000)
  get Phys(data[n=1]=f86e7000)
  get Phys(data[n=1]=f86e8000)
  get Phys(data[n=2]=f86e9000)
  get Phys(data[n=2]=f86ea000)
  get Phys(data[n=3]=f86eb000)
  get Phys(data[n=3]=f86ec000)
  get Phys(data[n=3]=f86ed000)
  get Phys(data[n=3]=f86ee000)
  get Phys(data[n=3]=f86ef000)
  get Phys(data[n=3]=f86f0000)
  get Phys(data[n=3]=f86f1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x50687, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x50687 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 50707, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 50707, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86f2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86f2000)
  get Phys(data[n=1]=f86f3000)
  get Phys(data[n=1]=f86f4000)
  get Phys(data[n=1]=f86f5000)
  get Phys(data[n=1]=f86f6000)
  get Phys(data[n=1]=f86f7000)
  get Phys(data[n=1]=f86f8000)
  get Phys(data[n=2]=f86f9000)
  get Phys(data[n=2]=f86fa000)
  get Phys(data[n=2]=f86fb000)
  get Phys(data[n=2]=f86fc000)
  get Phys(data[n=2]=f86fd000)
  get Phys(data[n=2]=f86fe000)
  get Phys(data[n=3]=f86ff000)
  get Phys(data[n=3]=f8700000)
  get Phys(data[n=3]=f8701000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x50707, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x50707 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 50787, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 50787, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8702000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8702000)
  get Phys(data[n=1]=f8703000)
  get Phys(data[n=1]=f8704000)
  get Phys(data[n=1]=f8705000)
  get Phys(data[n=1]=f8706000)
  get Phys(data[n=1]=f8707000)
  get Phys(data[n=2]=f8708000)
  get Phys(data[n=3]=f8709000)
  get Phys(data[n=3]=f870a000)
  get Phys(data[n=3]=f870b000)
  get Phys(data[n=3]=f870c000)
  get Phys(data[n=3]=f870d000)
  get Phys(data[n=3]=f870e000)
  get Phys(data[n=3]=f870f000)
  get Phys(data[n=4]=f8710000)
  get Phys(data[n=4]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x50787, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x50787 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 50607, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 50607, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x50607, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x50607 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/ex/init.c:1966) Free non-cache pages: 1e096
(../../ntoskrnl/mm/ARM3/zeropage.c:50) Free non-cache pages: 1e2ef
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38ed7, OrigWordsRequested 0x5900, DevSize 0x59
IdeReadWrite (REQ): Starting sector is 38ed7, Number of WORDS 0x5900, DevSize 0x59
AtapiDmaSetup: mode 0x45, data f86d2000, count b200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=2]=f86d4000)
  get Phys(data[n=2]=f86d5000)
  get Phys(data[n=3]=f86d6000)
  get Phys(data[n=4]=f86d7000)
  get Phys(data[n=5]=f86d8000)
  get Phys(data[n=5]=f86d9000)
  get Phys(data[n=5]=f86da000)
  get Phys(data[n=5]=f86db000)
  get Phys(data[n=6]=f86dc000)
  get Phys(data[n=7]=f86dd000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38ed7, Count 0x59(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38ed7 count 0x59 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered b200, full size b200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38ed7, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 38ed7, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38ed7, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38ed7 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3a27f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3a27f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86d2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=2]=f86d4000)
  get Phys(data[n=3]=f86d5000)
  get Phys(data[n=3]=f86d6000)
  get Phys(data[n=3]=f86d7000)
  get Phys(data[n=3]=f86d8000)
  get Phys(data[n=4]=f86d9000)
  get Phys(data[n=5]=f86da000)
  get Phys(data[n=5]=f86db000)
  get Phys(data[n=5]=f86dc000)
  get Phys(data[n=5]=f86dd000)
  get Phys(data[n=6]=f86de000)
  get Phys(data[n=6]=f86df000)
  get Phys(data[n=6]=f86e0000)
  get Phys(data[n=6]=f86e1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3a27f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3a27f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3a2ff, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3a2ff, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86e2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86e2000)
  get Phys(data[n=1]=f86e3000)
  get Phys(data[n=2]=f86e4000)
  get Phys(data[n=2]=f86e5000)
  get Phys(data[n=3]=f86e6000)
  get Phys(data[n=3]=f86e7000)
  get Phys(data[n=3]=f86e8000)
  get Phys(data[n=3]=f86e9000)
  get Phys(data[n=3]=f86ea000)
  get Phys(data[n=3]=f86eb000)
  get Phys(data[n=3]=f86ec000)
  get Phys(data[n=3]=f86ed000)
  get Phys(data[n=4]=f86ee000)
  get Phys(data[n=4]=f86ef000)
  get Phys(data[n=4]=f86f0000)
  get Phys(data[n=4]=f86f1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3a2ff, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3a2ff count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3a37f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3a37f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86f2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86f2000)
  get Phys(data[n=1]=f86f3000)
  get Phys(data[n=2]=f86f4000)
  get Phys(data[n=2]=f86f5000)
  get Phys(data[n=2]=f86f6000)
  get Phys(data[n=2]=f86f7000)
  get Phys(data[n=2]=f86f8000)
  get Phys(data[n=2]=f86f9000)
  get Phys(data[n=3]=f86fa000)
  get Phys(data[n=3]=f86fb000)
  get Phys(data[n=3]=f86fc000)
  get Phys(data[n=3]=f86fd000)
  get Phys(data[n=3]=f86fe000)
  get Phys(data[n=3]=f86ff000)
  get Phys(data[n=3]=f8700000)
  get Phys(data[n=3]=f8701000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3a37f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3a37f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88657f8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4047, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 4047, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 80c80000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80c80000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4047, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x4047 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80f80000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=80f80000)
  get Phys(data[n=1]=80f81000)
  get Phys(data[n=1]=80f82000)
  get Phys(data[n=2]=80f83000)
  get Phys(data[n=2]=80f84000)
  get Phys(data[n=2]=80f85000)
  get Phys(data[n=2]=80f86000)
  get Phys(data[n=2]=80f87000)
  get Phys(data[n=2]=80f88000)
  get Phys(data[n=2]=80f89000)
  get Phys(data[n=2]=80f8a000)
  get Phys(data[n=3]=80f8b000)
  get Phys(data[n=3]=80f8c000)
  get Phys(data[n=3]=80f8d000)
  get Phys(data[n=3]=80f8e000)
  get Phys(data[n=3]=80f8f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x69, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xca, lba 0x69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5ba90, CDB 0xb0e5bac0, AtaReq 0xb100d018, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=1
Non-empty queue
Try IDE prepare
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb100d018
** --- **
** Ide: Command continue prep
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80f90000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100d070)
  get Phys(data[0]=80f90000)
  get Phys(data[n=1]=80f91000)
  get Phys(data[n=1]=80f92000)
  get Phys(data[n=1]=80f93000)
  get Phys(data[n=1]=80f94000)
  get Phys(data[n=1]=80f95000)
  get Phys(data[n=1]=80f96000)
  get Phys(data[n=2]=80f97000)
  get Phys(data[n=2]=80f98000)
  get Phys(data[n=2]=80f99000)
  get Phys(data[n=2]=80f9a000)
  get Phys(data[n=2]=80f9b000)
  get Phys(data[n=2]=80f9c000)
  get Phys(data[n=2]=80f9d000)
  get Phys(data[n=2]=80f9e000)
  get Phys(data[n=2]=80f9f000)
  set TERM
AtapiDmaSetup: OK
IdeSendCommand: SRB_STATUS_PENDING
AtapiStartIo: Already have 2 request(s)!
AtapiStartIo: next Srb b0e5ba90
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0xb0e5ba90
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5ba90, CDB 0xb0e5bac0, AtaReq 0xb100d018, SCmd 0x2a
UniataNeedQueueing: qd=1
Send to device 2a
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865664
** Ide: Command AtaReq 0xb100d018
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (ExecOnly):
IdeReadWrite: Lba 0xe9, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xca, lba 0xe9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5ba90
AtapiStartIo: query PORT for next request
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5ba90, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5ba90
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 169, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 169, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80fa0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=80fa0000)
  get Phys(data[n=1]=80fa1000)
  get Phys(data[n=1]=80fa2000)
  get Phys(data[n=1]=80fa3000)
  get Phys(data[n=1]=80fa4000)
  get Phys(data[n=1]=80fa5000)
  get Phys(data[n=1]=80fa6000)
  get Phys(data[n=2]=80fa7000)
  get Phys(data[n=2]=80fa8000)
  get Phys(data[n=2]=80fa9000)
  get Phys(data[n=2]=80faa000)
  get Phys(data[n=2]=80fab000)
  get Phys(data[n=3]=80fac000)
  get Phys(data[n=3]=80fad000)
  get Phys(data[n=4]=80fae000)
  get Phys(data[n=4]=80faf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x169, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xca, lba 0x169 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80fb0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=80fb0000)
  get Phys(data[n=1]=80fb1000)
  get Phys(data[n=2]=80fb2000)
  get Phys(data[n=2]=80fb3000)
  get Phys(data[n=2]=80fb4000)
  get Phys(data[n=2]=80fb5000)
  get Phys(data[n=3]=80fb6000)
  get Phys(data[n=4]=80fb7000)
  get Phys(data[n=4]=80fb8000)
  get Phys(data[n=4]=80fb9000)
  get Phys(data[n=4]=80fba000)
  get Phys(data[n=5]=80fbb000)
  get Phys(data[n=5]=80fbc000)
  get Phys(data[n=5]=80fbd000)
  get Phys(data[n=5]=80fbe000)
  get Phys(data[n=5]=80fbf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e9, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xca, lba 0x1e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4054, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4054, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80f80000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=80f80000)
  get Phys(data[n=1]=80f81000)
  get Phys(data[n=1]=80f82000)
  get Phys(data[n=2]=80f83000)
  get Phys(data[n=2]=80f84000)
  get Phys(data[n=2]=80f85000)
  get Phys(data[n=2]=80f86000)
  get Phys(data[n=2]=80f87000)
  get Phys(data[n=2]=80f88000)
  get Phys(data[n=2]=80f89000)
  get Phys(data[n=2]=80f8a000)
  get Phys(data[n=3]=80f8b000)
  get Phys(data[n=3]=80f8c000)
  get Phys(data[n=3]=80f8d000)
  get Phys(data[n=3]=80f8e000)
  get Phys(data[n=3]=80f8f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4054, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xca, lba 0x4054 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40d4, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 40d4, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80f90000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=80f90000)
  get Phys(data[n=1]=80f91000)
  get Phys(data[n=1]=80f92000)
  get Phys(data[n=1]=80f93000)
  get Phys(data[n=1]=80f94000)
  get Phys(data[n=1]=80f95000)
  get Phys(data[n=1]=80f96000)
  get Phys(data[n=2]=80f97000)
  get Phys(data[n=2]=80f98000)
  get Phys(data[n=2]=80f99000)
  get Phys(data[n=2]=80f9a000)
  get Phys(data[n=2]=80f9b000)
  get Phys(data[n=2]=80f9c000)
  get Phys(data[n=2]=80f9d000)
  get Phys(data[n=2]=80f9e000)
  get Phys(data[n=2]=80f9f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40d4, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xca, lba 0x40d4 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4154, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4154, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80fa0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=80fa0000)
  get Phys(data[n=1]=80fa1000)
  get Phys(data[n=1]=80fa2000)
  get Phys(data[n=1]=80fa3000)
  get Phys(data[n=1]=80fa4000)
  get Phys(data[n=1]=80fa5000)
  get Phys(data[n=1]=80fa6000)
  get Phys(data[n=2]=80fa7000)
  get Phys(data[n=2]=80fa8000)
  get Phys(data[n=2]=80fa9000)
  get Phys(data[n=2]=80faa000)
  get Phys(data[n=2]=80fab000)
  get Phys(data[n=3]=80fac000)
  get Phys(data[n=3]=80fad000)
  get Phys(data[n=4]=80fae000)
  get Phys(data[n=4]=80faf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4154, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xca, lba 0x4154 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41d4, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 41d4, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80fb0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=80fb0000)
  get Phys(data[n=1]=80fb1000)
  get Phys(data[n=2]=80fb2000)
  get Phys(data[n=2]=80fb3000)
  get Phys(data[n=2]=80fb4000)
  get Phys(data[n=2]=80fb5000)
  get Phys(data[n=3]=80fb6000)
  get Phys(data[n=4]=80fb7000)
  get Phys(data[n=4]=80fb8000)
  get Phys(data[n=4]=80fb9000)
  get Phys(data[n=4]=80fba000)
  get Phys(data[n=5]=80fbb000)
  get Phys(data[n=5]=80fbc000)
  get Phys(data[n=5]=80fbd000)
  get Phys(data[n=5]=80fbe000)
  get Phys(data[n=5]=80fbf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41d4, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xca, lba 0x41d4 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3a3ff, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3a3ff, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8702000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8702000)
  get Phys(data[n=1]=f8703000)
  get Phys(data[n=2]=f8704000)
  get Phys(data[n=2]=f8705000)
  get Phys(data[n=2]=f8706000)
  get Phys(data[n=2]=f8707000)
  get Phys(data[n=2]=f8708000)
  get Phys(data[n=2]=f8709000)
  get Phys(data[n=2]=f870a000)
  get Phys(data[n=3]=f870b000)
  get Phys(data[n=3]=f870c000)
  get Phys(data[n=3]=f870d000)
  get Phys(data[n=3]=f870e000)
  get Phys(data[n=4]=f870f000)
  get Phys(data[n=4]=f8710000)
  get Phys(data[n=5]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3a3ff, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3a3ff count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3a27f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3a27f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3a27f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3a27f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/ldr/ldrapi.c:811) NtCreateSection() failed (Status 0xc0000022)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3addf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3addf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86d2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=1]=f86d4000)
  get Phys(data[n=1]=f86d5000)
  get Phys(data[n=1]=f86d6000)
  get Phys(data[n=2]=f86d7000)
  get Phys(data[n=3]=f86d8000)
  get Phys(data[n=3]=f86d9000)
  get Phys(data[n=3]=f86da000)
  get Phys(data[n=3]=f86db000)
  get Phys(data[n=4]=f86dc000)
  get Phys(data[n=4]=f86dd000)
  get Phys(data[n=4]=f86de000)
  get Phys(data[n=4]=f86df000)
  get Phys(data[n=4]=f86e0000)
  get Phys(data[n=4]=f86e1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3addf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3addf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ae5f, OrigWordsRequested 0x5900, DevSize 0x59
IdeReadWrite (REQ): Starting sector is 3ae5f, Number of WORDS 0x5900, DevSize 0x59
AtapiDmaSetup: mode 0x45, data f86e2000, count b200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86e2000)
  get Phys(data[n=1]=f86e3000)
  get Phys(data[n=2]=f86e4000)
  get Phys(data[n=2]=f86e5000)
  get Phys(data[n=2]=f86e6000)
  get Phys(data[n=2]=f86e7000)
  get Phys(data[n=2]=f86e8000)
  get Phys(data[n=2]=f86e9000)
  get Phys(data[n=2]=f86ea000)
  get Phys(data[n=2]=f86eb000)
  get Phys(data[n=3]=f86ec000)
  get Phys(data[n=3]=f86ed000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ae5f, Count 0x59(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3ae5f count 0x59 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered b200, full size b200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3addf, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3addf, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3addf, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3addf count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 25f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 25f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81480000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81480000)
  get Phys(data[n=1]=81481000)
  get Phys(data[n=1]=81482000)
  get Phys(data[n=2]=81483000)
  get Phys(data[n=3]=81484000)
  get Phys(data[n=3]=81485000)
  get Phys(data[n=3]=81486000)
  get Phys(data[n=3]=81487000)
  get Phys(data[n=4]=81488000)
  get Phys(data[n=4]=81489000)
  get Phys(data[n=4]=8148a000)
  get Phys(data[n=4]=8148b000)
  get Phys(data[n=4]=8148c000)
  get Phys(data[n=4]=8148d000)
  get Phys(data[n=5]=8148e000)
  get Phys(data[n=5]=8148f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x25f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x25f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81490000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81490000)
  get Phys(data[n=1]=81491000)
  get Phys(data[n=1]=81492000)
  get Phys(data[n=1]=81493000)
  get Phys(data[n=1]=81494000)
  get Phys(data[n=1]=81495000)
  get Phys(data[n=1]=81496000)
  get Phys(data[n=1]=81497000)
  get Phys(data[n=2]=81498000)
  get Phys(data[n=2]=81499000)
  get Phys(data[n=2]=8149a000)
  get Phys(data[n=2]=8149b000)
  get Phys(data[n=2]=8149c000)
  get Phys(data[n=2]=8149d000)
  get Phys(data[n=3]=8149e000)
  get Phys(data[n=3]=8149f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 35f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 35f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 814a0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=814a0000)
  get Phys(data[n=1]=814a1000)
  get Phys(data[n=1]=814a2000)
  get Phys(data[n=1]=814a3000)
  get Phys(data[n=2]=814a4000)
  get Phys(data[n=2]=814a5000)
  get Phys(data[n=2]=814a6000)
  get Phys(data[n=2]=814a7000)
  get Phys(data[n=2]=814a8000)
  get Phys(data[n=2]=814a9000)
  get Phys(data[n=2]=814aa000)
  get Phys(data[n=2]=814ab000)
  get Phys(data[n=2]=814ac000)
  get Phys(data[n=3]=814ad000)
  get Phys(data[n=4]=814ae000)
  get Phys(data[n=4]=814af000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x35f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x35f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 814b0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=814b0000)
  get Phys(data[n=1]=814b1000)
  get Phys(data[n=1]=814b2000)
  get Phys(data[n=1]=814b3000)
  get Phys(data[n=1]=814b4000)
  get Phys(data[n=2]=814b5000)
  get Phys(data[n=2]=814b6000)
  get Phys(data[n=2]=814b7000)
  get Phys(data[n=2]=814b8000)
  get Phys(data[n=3]=814b9000)
  get Phys(data[n=3]=814ba000)
  get Phys(data[n=4]=814bb000)
  get Phys(data[n=4]=814bc000)
  get Phys(data[n=5]=814bd000)
  get Phys(data[n=6]=814be000)
  get Phys(data[n=7]=814bf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 45f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 45f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 814c0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=814c0000)
  get Phys(data[n=1]=814c1000)
  get Phys(data[n=1]=814c2000)
  get Phys(data[n=2]=814c3000)
  get Phys(data[n=3]=814c4000)
  get Phys(data[n=3]=814c5000)
  get Phys(data[n=3]=814c6000)
  get Phys(data[n=3]=814c7000)
  get Phys(data[n=4]=814c8000)
  get Phys(data[n=4]=814c9000)
  get Phys(data[n=4]=814ca000)
  get Phys(data[n=4]=814cb000)
  get Phys(data[n=4]=814cc000)
  get Phys(data[n=4]=814cd000)
  get Phys(data[n=5]=814ce000)
  get Phys(data[n=5]=814cf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x45f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x45f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 814d0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=814d0000)
  get Phys(data[n=1]=814d1000)
  get Phys(data[n=1]=814d2000)
  get Phys(data[n=1]=814d3000)
  get Phys(data[n=1]=814d4000)
  get Phys(data[n=1]=814d5000)
  get Phys(data[n=1]=814d6000)
  get Phys(data[n=1]=814d7000)
  get Phys(data[n=2]=814d8000)
  get Phys(data[n=2]=814d9000)
  get Phys(data[n=2]=814da000)
  get Phys(data[n=2]=814db000)
  get Phys(data[n=2]=814dc000)
  get Phys(data[n=2]=814dd000)
  get Phys(data[n=3]=814de000)
  get Phys(data[n=3]=814df000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 55f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 55f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 814e0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=814e0000)
  get Phys(data[n=1]=814e1000)
  get Phys(data[n=1]=814e2000)
  get Phys(data[n=1]=814e3000)
  get Phys(data[n=2]=814e4000)
  get Phys(data[n=2]=814e5000)
  get Phys(data[n=2]=814e6000)
  get Phys(data[n=2]=814e7000)
  get Phys(data[n=2]=814e8000)
  get Phys(data[n=2]=814e9000)
  get Phys(data[n=2]=814ea000)
  get Phys(data[n=2]=814eb000)
  get Phys(data[n=2]=814ec000)
  get Phys(data[n=3]=814ed000)
  get Phys(data[n=4]=814ee000)
  get Phys(data[n=4]=814ef000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x55f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x55f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 814f0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=814f0000)
  get Phys(data[n=1]=814f1000)
  get Phys(data[n=1]=814f2000)
  get Phys(data[n=1]=814f3000)
  get Phys(data[n=1]=814f4000)
  get Phys(data[n=2]=814f5000)
  get Phys(data[n=2]=814f6000)
  get Phys(data[n=2]=814f7000)
  get Phys(data[n=2]=814f8000)
  get Phys(data[n=3]=814f9000)
  get Phys(data[n=3]=814fa000)
  get Phys(data[n=4]=814fb000)
  get Phys(data[n=4]=814fc000)
  get Phys(data[n=5]=814fd000)
  get Phys(data[n=6]=814fe000)
  get Phys(data[n=7]=814ff000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 85f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 85f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81500000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81500000)
  get Phys(data[n=1]=81501000)
  get Phys(data[n=1]=81502000)
  get Phys(data[n=2]=81503000)
  get Phys(data[n=3]=81504000)
  get Phys(data[n=3]=81505000)
  get Phys(data[n=3]=81506000)
  get Phys(data[n=3]=81507000)
  get Phys(data[n=4]=81508000)
  get Phys(data[n=4]=81509000)
  get Phys(data[n=4]=8150a000)
  get Phys(data[n=4]=8150b000)
  get Phys(data[n=4]=8150c000)
  get Phys(data[n=4]=8150d000)
  get Phys(data[n=5]=8150e000)
  get Phys(data[n=5]=8150f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x85f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x85f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 8df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 8df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81510000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81510000)
  get Phys(data[n=1]=81511000)
  get Phys(data[n=1]=81512000)
  get Phys(data[n=1]=81513000)
  get Phys(data[n=1]=81514000)
  get Phys(data[n=1]=81515000)
  get Phys(data[n=1]=81516000)
  get Phys(data[n=1]=81517000)
  get Phys(data[n=2]=81518000)
  get Phys(data[n=2]=81519000)
  get Phys(data[n=2]=8151a000)
  get Phys(data[n=2]=8151b000)
  get Phys(data[n=2]=8151c000)
  get Phys(data[n=2]=8151d000)
  get Phys(data[n=3]=8151e000)
  get Phys(data[n=3]=8151f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x8df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x8df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 95f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 95f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81520000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81520000)
  get Phys(data[n=1]=81521000)
  get Phys(data[n=1]=81522000)
  get Phys(data[n=1]=81523000)
  get Phys(data[n=2]=81524000)
  get Phys(data[n=2]=81525000)
  get Phys(data[n=2]=81526000)
  get Phys(data[n=2]=81527000)
  get Phys(data[n=2]=81528000)
  get Phys(data[n=2]=81529000)
  get Phys(data[n=2]=8152a000)
  get Phys(data[n=2]=8152b000)
  get Phys(data[n=2]=8152c000)
  get Phys(data[n=3]=8152d000)
  get Phys(data[n=4]=8152e000)
  get Phys(data[n=4]=8152f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x95f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x95f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 9df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 9df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81530000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81530000)
  get Phys(data[n=1]=81531000)
  get Phys(data[n=1]=81532000)
  get Phys(data[n=1]=81533000)
  get Phys(data[n=1]=81534000)
  get Phys(data[n=2]=81535000)
  get Phys(data[n=2]=81536000)
  get Phys(data[n=2]=81537000)
  get Phys(data[n=2]=81538000)
  get Phys(data[n=3]=81539000)
  get Phys(data[n=3]=8153a000)
  get Phys(data[n=4]=8153b000)
  get Phys(data[n=4]=8153c000)
  get Phys(data[n=5]=8153d000)
  get Phys(data[n=6]=8153e000)
  get Phys(data[n=7]=8153f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x9df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x9df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector a5f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is a5f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81540000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81540000)
  get Phys(data[n=1]=81541000)
  get Phys(data[n=1]=81542000)
  get Phys(data[n=2]=81543000)
  get Phys(data[n=3]=81544000)
  get Phys(data[n=3]=81545000)
  get Phys(data[n=3]=81546000)
  get Phys(data[n=3]=81547000)
  get Phys(data[n=4]=81548000)
  get Phys(data[n=4]=81549000)
  get Phys(data[n=4]=8154a000)
  get Phys(data[n=4]=8154b000)
  get Phys(data[n=4]=8154c000)
  get Phys(data[n=4]=8154d000)
  get Phys(data[n=5]=8154e000)
  get Phys(data[n=5]=8154f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xa5f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0xa5f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector adf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is adf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81550000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81550000)
  get Phys(data[n=1]=81551000)
  get Phys(data[n=1]=81552000)
  get Phys(data[n=1]=81553000)
  get Phys(data[n=1]=81554000)
  get Phys(data[n=1]=81555000)
  get Phys(data[n=1]=81556000)
  get Phys(data[n=1]=81557000)
  get Phys(data[n=2]=81558000)
  get Phys(data[n=2]=81559000)
  get Phys(data[n=2]=8155a000)
  get Phys(data[n=2]=8155b000)
  get Phys(data[n=2]=8155c000)
  get Phys(data[n=2]=8155d000)
  get Phys(data[n=3]=8155e000)
  get Phys(data[n=3]=8155f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xadf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0xadf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector b5f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is b5f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81560000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81560000)
  get Phys(data[n=1]=81561000)
  get Phys(data[n=1]=81562000)
  get Phys(data[n=1]=81563000)
  get Phys(data[n=2]=81564000)
  get Phys(data[n=2]=81565000)
  get Phys(data[n=2]=81566000)
  get Phys(data[n=2]=81567000)
  get Phys(data[n=2]=81568000)
  get Phys(data[n=2]=81569000)
  get Phys(data[n=2]=8156a000)
  get Phys(data[n=2]=8156b000)
  get Phys(data[n=2]=8156c000)
  get Phys(data[n=3]=8156d000)
  get Phys(data[n=4]=8156e000)
  get Phys(data[n=4]=8156f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xb5f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0xb5f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector bdf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is bdf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81570000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81570000)
  get Phys(data[n=1]=81571000)
  get Phys(data[n=1]=81572000)
  get Phys(data[n=1]=81573000)
  get Phys(data[n=1]=81574000)
  get Phys(data[n=2]=81575000)
  get Phys(data[n=2]=81576000)
  get Phys(data[n=2]=81577000)
  get Phys(data[n=2]=81578000)
  get Phys(data[n=3]=81579000)
  get Phys(data[n=3]=8157a000)
  get Phys(data[n=4]=8157b000)
  get Phys(data[n=4]=8157c000)
  get Phys(data[n=5]=8157d000)
  get Phys(data[n=6]=8157e000)
  get Phys(data[n=7]=8157f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xbdf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0xbdf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector c5f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is c5f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81580000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81580000)
  get Phys(data[n=1]=81581000)
  get Phys(data[n=1]=81582000)
  get Phys(data[n=2]=81583000)
  get Phys(data[n=3]=81584000)
  get Phys(data[n=3]=81585000)
  get Phys(data[n=3]=81586000)
  get Phys(data[n=3]=81587000)
  get Phys(data[n=4]=81588000)
  get Phys(data[n=4]=81589000)
  get Phys(data[n=4]=8158a000)
  get Phys(data[n=4]=8158b000)
  get Phys(data[n=4]=8158c000)
  get Phys(data[n=4]=8158d000)
  get Phys(data[n=5]=8158e000)
  get Phys(data[n=5]=8158f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xc5f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0xc5f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector cdf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is cdf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81590000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81590000)
  get Phys(data[n=1]=81591000)
  get Phys(data[n=1]=81592000)
  get Phys(data[n=1]=81593000)
  get Phys(data[n=1]=81594000)
  get Phys(data[n=1]=81595000)
  get Phys(data[n=1]=81596000)
  get Phys(data[n=1]=81597000)
  get Phys(data[n=2]=81598000)
  get Phys(data[n=2]=81599000)
  get Phys(data[n=2]=8159a000)
  get Phys(data[n=2]=8159b000)
  get Phys(data[n=2]=8159c000)
  get Phys(data[n=2]=8159d000)
  get Phys(data[n=3]=8159e000)
  get Phys(data[n=3]=8159f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xcdf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0xcdf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector d5f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is d5f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 815a0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=815a0000)
  get Phys(data[n=1]=815a1000)
  get Phys(data[n=1]=815a2000)
  get Phys(data[n=1]=815a3000)
  get Phys(data[n=2]=815a4000)
  get Phys(data[n=2]=815a5000)
  get Phys(data[n=2]=815a6000)
  get Phys(data[n=2]=815a7000)
  get Phys(data[n=2]=815a8000)
  get Phys(data[n=2]=815a9000)
  get Phys(data[n=2]=815aa000)
  get Phys(data[n=2]=815ab000)
  get Phys(data[n=2]=815ac000)
  get Phys(data[n=3]=815ad000)
  get Phys(data[n=4]=815ae000)
  get Phys(data[n=4]=815af000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xd5f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0xd5f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector ddf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is ddf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 815b0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=815b0000)
  get Phys(data[n=1]=815b1000)
  get Phys(data[n=1]=815b2000)
  get Phys(data[n=1]=815b3000)
  get Phys(data[n=1]=815b4000)
  get Phys(data[n=2]=815b5000)
  get Phys(data[n=2]=815b6000)
  get Phys(data[n=2]=815b7000)
  get Phys(data[n=2]=815b8000)
  get Phys(data[n=3]=815b9000)
  get Phys(data[n=3]=815ba000)
  get Phys(data[n=4]=815bb000)
  get Phys(data[n=4]=815bc000)
  get Phys(data[n=5]=815bd000)
  get Phys(data[n=6]=815be000)
  get Phys(data[n=7]=815bf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xddf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0xddf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector e5f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is e5f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 815c0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=815c0000)
  get Phys(data[n=1]=815c1000)
  get Phys(data[n=1]=815c2000)
  get Phys(data[n=2]=815c3000)
  get Phys(data[n=3]=815c4000)
  get Phys(data[n=3]=815c5000)
  get Phys(data[n=3]=815c6000)
  get Phys(data[n=3]=815c7000)
  get Phys(data[n=4]=815c8000)
  get Phys(data[n=4]=815c9000)
  get Phys(data[n=4]=815ca000)
  get Phys(data[n=4]=815cb000)
  get Phys(data[n=4]=815cc000)
  get Phys(data[n=4]=815cd000)
  get Phys(data[n=5]=815ce000)
  get Phys(data[n=5]=815cf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xe5f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0xe5f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector edf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is edf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 815d0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=815d0000)
  get Phys(data[n=1]=815d1000)
  get Phys(data[n=1]=815d2000)
  get Phys(data[n=1]=815d3000)
  get Phys(data[n=1]=815d4000)
  get Phys(data[n=1]=815d5000)
  get Phys(data[n=1]=815d6000)
  get Phys(data[n=1]=815d7000)
  get Phys(data[n=2]=815d8000)
  get Phys(data[n=2]=815d9000)
  get Phys(data[n=2]=815da000)
  get Phys(data[n=2]=815db000)
  get Phys(data[n=2]=815dc000)
  get Phys(data[n=2]=815dd000)
  get Phys(data[n=3]=815de000)
  get Phys(data[n=3]=815df000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xedf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0xedf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector f5f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is f5f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 815e0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=815e0000)
  get Phys(data[n=1]=815e1000)
  get Phys(data[n=1]=815e2000)
  get Phys(data[n=1]=815e3000)
  get Phys(data[n=2]=815e4000)
  get Phys(data[n=2]=815e5000)
  get Phys(data[n=2]=815e6000)
  get Phys(data[n=2]=815e7000)
  get Phys(data[n=2]=815e8000)
  get Phys(data[n=2]=815e9000)
  get Phys(data[n=2]=815ea000)
  get Phys(data[n=2]=815eb000)
  get Phys(data[n=2]=815ec000)
  get Phys(data[n=3]=815ed000)
  get Phys(data[n=4]=815ee000)
  get Phys(data[n=4]=815ef000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xf5f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0xf5f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector fdf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is fdf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 815f0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=815f0000)
  get Phys(data[n=1]=815f1000)
  get Phys(data[n=1]=815f2000)
  get Phys(data[n=1]=815f3000)
  get Phys(data[n=1]=815f4000)
  get Phys(data[n=2]=815f5000)
  get Phys(data[n=2]=815f6000)
  get Phys(data[n=2]=815f7000)
  get Phys(data[n=2]=815f8000)
  get Phys(data[n=3]=815f9000)
  get Phys(data[n=3]=815fa000)
  get Phys(data[n=4]=815fb000)
  get Phys(data[n=4]=815fc000)
  get Phys(data[n=5]=815fd000)
  get Phys(data[n=6]=815fe000)
  get Phys(data[n=7]=815ff000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xfdf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0xfdf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 105f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 105f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81600000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81600000)
  get Phys(data[n=1]=81601000)
  get Phys(data[n=1]=81602000)
  get Phys(data[n=2]=81603000)
  get Phys(data[n=3]=81604000)
  get Phys(data[n=3]=81605000)
  get Phys(data[n=3]=81606000)
  get Phys(data[n=3]=81607000)
  get Phys(data[n=4]=81608000)
  get Phys(data[n=4]=81609000)
  get Phys(data[n=4]=8160a000)
  get Phys(data[n=4]=8160b000)
  get Phys(data[n=4]=8160c000)
  get Phys(data[n=4]=8160d000)
  get Phys(data[n=5]=8160e000)
  get Phys(data[n=5]=8160f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x105f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x105f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 10df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 10df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81610000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81610000)
  get Phys(data[n=1]=81611000)
  get Phys(data[n=1]=81612000)
  get Phys(data[n=1]=81613000)
  get Phys(data[n=1]=81614000)
  get Phys(data[n=1]=81615000)
  get Phys(data[n=1]=81616000)
  get Phys(data[n=1]=81617000)
  get Phys(data[n=2]=81618000)
  get Phys(data[n=2]=81619000)
  get Phys(data[n=2]=8161a000)
  get Phys(data[n=2]=8161b000)
  get Phys(data[n=2]=8161c000)
  get Phys(data[n=2]=8161d000)
  get Phys(data[n=3]=8161e000)
  get Phys(data[n=3]=8161f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x10df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x10df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 115f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 115f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81620000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81620000)
  get Phys(data[n=1]=81621000)
  get Phys(data[n=1]=81622000)
  get Phys(data[n=1]=81623000)
  get Phys(data[n=2]=81624000)
  get Phys(data[n=2]=81625000)
  get Phys(data[n=2]=81626000)
  get Phys(data[n=2]=81627000)
  get Phys(data[n=2]=81628000)
  get Phys(data[n=2]=81629000)
  get Phys(data[n=2]=8162a000)
  get Phys(data[n=2]=8162b000)
  get Phys(data[n=2]=8162c000)
  get Phys(data[n=3]=8162d000)
  get Phys(data[n=4]=8162e000)
  get Phys(data[n=4]=8162f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x115f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x115f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 11df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81630000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81630000)
  get Phys(data[n=1]=81631000)
  get Phys(data[n=1]=81632000)
  get Phys(data[n=1]=81633000)
  get Phys(data[n=1]=81634000)
  get Phys(data[n=2]=81635000)
  get Phys(data[n=2]=81636000)
  get Phys(data[n=2]=81637000)
  get Phys(data[n=2]=81638000)
  get Phys(data[n=3]=81639000)
  get Phys(data[n=3]=8163a000)
  get Phys(data[n=4]=8163b000)
  get Phys(data[n=4]=8163c000)
  get Phys(data[n=5]=8163d000)
  get Phys(data[n=6]=8163e000)
  get Phys(data[n=7]=8163f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x11df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x11df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 125f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 125f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81640000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81640000)
  get Phys(data[n=1]=81641000)
  get Phys(data[n=1]=81642000)
  get Phys(data[n=2]=81643000)
  get Phys(data[n=3]=81644000)
  get Phys(data[n=3]=81645000)
  get Phys(data[n=3]=81646000)
  get Phys(data[n=3]=81647000)
  get Phys(data[n=4]=81648000)
  get Phys(data[n=4]=81649000)
  get Phys(data[n=4]=8164a000)
  get Phys(data[n=4]=8164b000)
  get Phys(data[n=4]=8164c000)
  get Phys(data[n=4]=8164d000)
  get Phys(data[n=5]=8164e000)
  get Phys(data[n=5]=8164f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x125f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x125f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 12df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 12df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81650000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81650000)
  get Phys(data[n=1]=81651000)
  get Phys(data[n=1]=81652000)
  get Phys(data[n=1]=81653000)
  get Phys(data[n=1]=81654000)
  get Phys(data[n=1]=81655000)
  get Phys(data[n=1]=81656000)
  get Phys(data[n=1]=81657000)
  get Phys(data[n=2]=81658000)
  get Phys(data[n=2]=81659000)
  get Phys(data[n=2]=8165a000)
  get Phys(data[n=2]=8165b000)
  get Phys(data[n=2]=8165c000)
  get Phys(data[n=2]=8165d000)
  get Phys(data[n=3]=8165e000)
  get Phys(data[n=3]=8165f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x12df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x12df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 135f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 135f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81660000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81660000)
  get Phys(data[n=1]=81661000)
  get Phys(data[n=1]=81662000)
  get Phys(data[n=1]=81663000)
  get Phys(data[n=2]=81664000)
  get Phys(data[n=2]=81665000)
  get Phys(data[n=2]=81666000)
  get Phys(data[n=2]=81667000)
  get Phys(data[n=2]=81668000)
  get Phys(data[n=2]=81669000)
  get Phys(data[n=2]=8166a000)
  get Phys(data[n=2]=8166b000)
  get Phys(data[n=2]=8166c000)
  get Phys(data[n=3]=8166d000)
  get Phys(data[n=4]=8166e000)
  get Phys(data[n=4]=8166f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x135f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x135f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 13df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 13df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81670000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81670000)
  get Phys(data[n=1]=81671000)
  get Phys(data[n=1]=81672000)
  get Phys(data[n=1]=81673000)
  get Phys(data[n=1]=81674000)
  get Phys(data[n=2]=81675000)
  get Phys(data[n=2]=81676000)
  get Phys(data[n=2]=81677000)
  get Phys(data[n=2]=81678000)
  get Phys(data[n=3]=81679000)
  get Phys(data[n=3]=8167a000)
  get Phys(data[n=4]=8167b000)
  get Phys(data[n=4]=8167c000)
  get Phys(data[n=5]=8167d000)
  get Phys(data[n=6]=8167e000)
  get Phys(data[n=7]=8167f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x13df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x13df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 145f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 145f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81680000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81680000)
  get Phys(data[n=1]=81681000)
  get Phys(data[n=1]=81682000)
  get Phys(data[n=2]=81683000)
  get Phys(data[n=3]=81684000)
  get Phys(data[n=3]=81685000)
  get Phys(data[n=3]=81686000)
  get Phys(data[n=3]=81687000)
  get Phys(data[n=4]=81688000)
  get Phys(data[n=4]=81689000)
  get Phys(data[n=4]=8168a000)
  get Phys(data[n=4]=8168b000)
  get Phys(data[n=4]=8168c000)
  get Phys(data[n=4]=8168d000)
  get Phys(data[n=5]=8168e000)
  get Phys(data[n=5]=8168f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x145f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x145f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 14df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 14df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81690000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81690000)
  get Phys(data[n=1]=81691000)
  get Phys(data[n=1]=81692000)
  get Phys(data[n=1]=81693000)
  get Phys(data[n=1]=81694000)
  get Phys(data[n=1]=81695000)
  get Phys(data[n=1]=81696000)
  get Phys(data[n=1]=81697000)
  get Phys(data[n=2]=81698000)
  get Phys(data[n=2]=81699000)
  get Phys(data[n=2]=8169a000)
  get Phys(data[n=2]=8169b000)
  get Phys(data[n=2]=8169c000)
  get Phys(data[n=2]=8169d000)
  get Phys(data[n=3]=8169e000)
  get Phys(data[n=3]=8169f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x14df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x14df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 155f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 155f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 816a0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=816a0000)
  get Phys(data[n=1]=816a1000)
  get Phys(data[n=1]=816a2000)
  get Phys(data[n=1]=816a3000)
  get Phys(data[n=2]=816a4000)
  get Phys(data[n=2]=816a5000)
  get Phys(data[n=2]=816a6000)
  get Phys(data[n=2]=816a7000)
  get Phys(data[n=2]=816a8000)
  get Phys(data[n=2]=816a9000)
  get Phys(data[n=2]=816aa000)
  get Phys(data[n=2]=816ab000)
  get Phys(data[n=2]=816ac000)
  get Phys(data[n=3]=816ad000)
  get Phys(data[n=4]=816ae000)
  get Phys(data[n=4]=816af000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x155f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x155f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 15df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 15df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 816b0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=816b0000)
  get Phys(data[n=1]=816b1000)
  get Phys(data[n=1]=816b2000)
  get Phys(data[n=1]=816b3000)
  get Phys(data[n=1]=816b4000)
  get Phys(data[n=2]=816b5000)
  get Phys(data[n=2]=816b6000)
  get Phys(data[n=2]=816b7000)
  get Phys(data[n=2]=816b8000)
  get Phys(data[n=3]=816b9000)
  get Phys(data[n=3]=816ba000)
  get Phys(data[n=4]=816bb000)
  get Phys(data[n=4]=816bc000)
  get Phys(data[n=5]=816bd000)
  get Phys(data[n=6]=816be000)
  get Phys(data[n=7]=816bf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x15df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x15df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 165f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 165f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 816c0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=816c0000)
  get Phys(data[n=1]=816c1000)
  get Phys(data[n=1]=816c2000)
  get Phys(data[n=2]=816c3000)
  get Phys(data[n=3]=816c4000)
  get Phys(data[n=3]=816c5000)
  get Phys(data[n=3]=816c6000)
  get Phys(data[n=3]=816c7000)
  get Phys(data[n=4]=816c8000)
  get Phys(data[n=4]=816c9000)
  get Phys(data[n=4]=816ca000)
  get Phys(data[n=4]=816cb000)
  get Phys(data[n=4]=816cc000)
  get Phys(data[n=4]=816cd000)
  get Phys(data[n=5]=816ce000)
  get Phys(data[n=5]=816cf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x165f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x165f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 16df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 16df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 816d0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=816d0000)
  get Phys(data[n=1]=816d1000)
  get Phys(data[n=1]=816d2000)
  get Phys(data[n=1]=816d3000)
  get Phys(data[n=1]=816d4000)
  get Phys(data[n=1]=816d5000)
  get Phys(data[n=1]=816d6000)
  get Phys(data[n=1]=816d7000)
  get Phys(data[n=2]=816d8000)
  get Phys(data[n=2]=816d9000)
  get Phys(data[n=2]=816da000)
  get Phys(data[n=2]=816db000)
  get Phys(data[n=2]=816dc000)
  get Phys(data[n=2]=816dd000)
  get Phys(data[n=3]=816de000)
  get Phys(data[n=3]=816df000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x16df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x16df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 175f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 175f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 816e0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=816e0000)
  get Phys(data[n=1]=816e1000)
  get Phys(data[n=1]=816e2000)
  get Phys(data[n=1]=816e3000)
  get Phys(data[n=2]=816e4000)
  get Phys(data[n=2]=816e5000)
  get Phys(data[n=2]=816e6000)
  get Phys(data[n=2]=816e7000)
  get Phys(data[n=2]=816e8000)
  get Phys(data[n=2]=816e9000)
  get Phys(data[n=2]=816ea000)
  get Phys(data[n=2]=816eb000)
  get Phys(data[n=2]=816ec000)
  get Phys(data[n=3]=816ed000)
  get Phys(data[n=4]=816ee000)
  get Phys(data[n=4]=816ef000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x175f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x175f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 17df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 17df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 816f0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=816f0000)
  get Phys(data[n=1]=816f1000)
  get Phys(data[n=1]=816f2000)
  get Phys(data[n=1]=816f3000)
  get Phys(data[n=1]=816f4000)
  get Phys(data[n=2]=816f5000)
  get Phys(data[n=2]=816f6000)
  get Phys(data[n=2]=816f7000)
  get Phys(data[n=2]=816f8000)
  get Phys(data[n=3]=816f9000)
  get Phys(data[n=3]=816fa000)
  get Phys(data[n=4]=816fb000)
  get Phys(data[n=4]=816fc000)
  get Phys(data[n=5]=816fd000)
  get Phys(data[n=6]=816fe000)
  get Phys(data[n=7]=816ff000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x17df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x17df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 185f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 185f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81700000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81700000)
  get Phys(data[n=1]=81701000)
  get Phys(data[n=1]=81702000)
  get Phys(data[n=2]=81703000)
  get Phys(data[n=3]=81704000)
  get Phys(data[n=3]=81705000)
  get Phys(data[n=3]=81706000)
  get Phys(data[n=3]=81707000)
  get Phys(data[n=4]=81708000)
  get Phys(data[n=4]=81709000)
  get Phys(data[n=4]=8170a000)
  get Phys(data[n=4]=8170b000)
  get Phys(data[n=4]=8170c000)
  get Phys(data[n=4]=8170d000)
  get Phys(data[n=5]=8170e000)
  get Phys(data[n=5]=8170f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x185f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x185f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 18df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 18df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81710000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81710000)
  get Phys(data[n=1]=81711000)
  get Phys(data[n=1]=81712000)
  get Phys(data[n=1]=81713000)
  get Phys(data[n=1]=81714000)
  get Phys(data[n=1]=81715000)
  get Phys(data[n=1]=81716000)
  get Phys(data[n=1]=81717000)
  get Phys(data[n=2]=81718000)
  get Phys(data[n=2]=81719000)
  get Phys(data[n=2]=8171a000)
  get Phys(data[n=2]=8171b000)
  get Phys(data[n=2]=8171c000)
  get Phys(data[n=2]=8171d000)
  get Phys(data[n=3]=8171e000)
  get Phys(data[n=3]=8171f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x18df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x18df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 195f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 195f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81720000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81720000)
  get Phys(data[n=1]=81721000)
  get Phys(data[n=1]=81722000)
  get Phys(data[n=1]=81723000)
  get Phys(data[n=2]=81724000)
  get Phys(data[n=2]=81725000)
  get Phys(data[n=2]=81726000)
  get Phys(data[n=2]=81727000)
  get Phys(data[n=2]=81728000)
  get Phys(data[n=2]=81729000)
  get Phys(data[n=2]=8172a000)
  get Phys(data[n=2]=8172b000)
  get Phys(data[n=2]=8172c000)
  get Phys(data[n=3]=8172d000)
  get Phys(data[n=4]=8172e000)
  get Phys(data[n=4]=8172f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x195f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x195f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 19df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 19df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81730000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81730000)
  get Phys(data[n=1]=81731000)
  get Phys(data[n=1]=81732000)
  get Phys(data[n=1]=81733000)
  get Phys(data[n=1]=81734000)
  get Phys(data[n=2]=81735000)
  get Phys(data[n=2]=81736000)
  get Phys(data[n=2]=81737000)
  get Phys(data[n=2]=81738000)
  get Phys(data[n=3]=81739000)
  get Phys(data[n=3]=8173a000)
  get Phys(data[n=4]=8173b000)
  get Phys(data[n=4]=8173c000)
  get Phys(data[n=5]=8173d000)
  get Phys(data[n=6]=8173e000)
  get Phys(data[n=7]=8173f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x19df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x19df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1a5f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1a5f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81740000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81740000)
  get Phys(data[n=1]=81741000)
  get Phys(data[n=1]=81742000)
  get Phys(data[n=2]=81743000)
  get Phys(data[n=3]=81744000)
  get Phys(data[n=3]=81745000)
  get Phys(data[n=3]=81746000)
  get Phys(data[n=3]=81747000)
  get Phys(data[n=4]=81748000)
  get Phys(data[n=4]=81749000)
  get Phys(data[n=4]=8174a000)
  get Phys(data[n=4]=8174b000)
  get Phys(data[n=4]=8174c000)
  get Phys(data[n=4]=8174d000)
  get Phys(data[n=5]=8174e000)
  get Phys(data[n=5]=8174f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1a5f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1a5f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1adf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1adf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81750000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81750000)
  get Phys(data[n=1]=81751000)
  get Phys(data[n=1]=81752000)
  get Phys(data[n=1]=81753000)
  get Phys(data[n=1]=81754000)
  get Phys(data[n=1]=81755000)
  get Phys(data[n=1]=81756000)
  get Phys(data[n=1]=81757000)
  get Phys(data[n=2]=81758000)
  get Phys(data[n=2]=81759000)
  get Phys(data[n=2]=8175a000)
  get Phys(data[n=2]=8175b000)
  get Phys(data[n=2]=8175c000)
  get Phys(data[n=2]=8175d000)
  get Phys(data[n=3]=8175e000)
  get Phys(data[n=3]=8175f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1adf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1adf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1b5f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1b5f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81760000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81760000)
  get Phys(data[n=1]=81761000)
  get Phys(data[n=1]=81762000)
  get Phys(data[n=1]=81763000)
  get Phys(data[n=2]=81764000)
  get Phys(data[n=2]=81765000)
  get Phys(data[n=2]=81766000)
  get Phys(data[n=2]=81767000)
  get Phys(data[n=2]=81768000)
  get Phys(data[n=2]=81769000)
  get Phys(data[n=2]=8176a000)
  get Phys(data[n=2]=8176b000)
  get Phys(data[n=2]=8176c000)
  get Phys(data[n=3]=8176d000)
  get Phys(data[n=4]=8176e000)
  get Phys(data[n=4]=8176f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1b5f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1b5f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1bdf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1bdf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81770000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81770000)
  get Phys(data[n=1]=81771000)
  get Phys(data[n=1]=81772000)
  get Phys(data[n=1]=81773000)
  get Phys(data[n=1]=81774000)
  get Phys(data[n=2]=81775000)
  get Phys(data[n=2]=81776000)
  get Phys(data[n=2]=81777000)
  get Phys(data[n=2]=81778000)
  get Phys(data[n=3]=81779000)
  get Phys(data[n=3]=8177a000)
  get Phys(data[n=4]=8177b000)
  get Phys(data[n=4]=8177c000)
  get Phys(data[n=5]=8177d000)
  get Phys(data[n=6]=8177e000)
  get Phys(data[n=7]=8177f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1bdf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1bdf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1c5f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1c5f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81780000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81780000)
  get Phys(data[n=1]=81781000)
  get Phys(data[n=1]=81782000)
  get Phys(data[n=2]=81783000)
  get Phys(data[n=3]=81784000)
  get Phys(data[n=3]=81785000)
  get Phys(data[n=3]=81786000)
  get Phys(data[n=3]=81787000)
  get Phys(data[n=4]=81788000)
  get Phys(data[n=4]=81789000)
  get Phys(data[n=4]=8178a000)
  get Phys(data[n=4]=8178b000)
  get Phys(data[n=4]=8178c000)
  get Phys(data[n=4]=8178d000)
  get Phys(data[n=5]=8178e000)
  get Phys(data[n=5]=8178f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1c5f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1c5f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1cdf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1cdf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81790000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81790000)
  get Phys(data[n=1]=81791000)
  get Phys(data[n=1]=81792000)
  get Phys(data[n=1]=81793000)
  get Phys(data[n=1]=81794000)
  get Phys(data[n=1]=81795000)
  get Phys(data[n=1]=81796000)
  get Phys(data[n=1]=81797000)
  get Phys(data[n=2]=81798000)
  get Phys(data[n=2]=81799000)
  get Phys(data[n=2]=8179a000)
  get Phys(data[n=2]=8179b000)
  get Phys(data[n=2]=8179c000)
  get Phys(data[n=2]=8179d000)
  get Phys(data[n=3]=8179e000)
  get Phys(data[n=3]=8179f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1cdf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1cdf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d5f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1d5f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 817a0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=817a0000)
  get Phys(data[n=1]=817a1000)
  get Phys(data[n=1]=817a2000)
  get Phys(data[n=1]=817a3000)
  get Phys(data[n=2]=817a4000)
  get Phys(data[n=2]=817a5000)
  get Phys(data[n=2]=817a6000)
  get Phys(data[n=2]=817a7000)
  get Phys(data[n=2]=817a8000)
  get Phys(data[n=2]=817a9000)
  get Phys(data[n=2]=817aa000)
  get Phys(data[n=2]=817ab000)
  get Phys(data[n=2]=817ac000)
  get Phys(data[n=3]=817ad000)
  get Phys(data[n=4]=817ae000)
  get Phys(data[n=4]=817af000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d5f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d5f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1ddf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1ddf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 817b0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=817b0000)
  get Phys(data[n=1]=817b1000)
  get Phys(data[n=1]=817b2000)
  get Phys(data[n=1]=817b3000)
  get Phys(data[n=1]=817b4000)
  get Phys(data[n=2]=817b5000)
  get Phys(data[n=2]=817b6000)
  get Phys(data[n=2]=817b7000)
  get Phys(data[n=2]=817b8000)
  get Phys(data[n=3]=817b9000)
  get Phys(data[n=3]=817ba000)
  get Phys(data[n=4]=817bb000)
  get Phys(data[n=4]=817bc000)
  get Phys(data[n=5]=817bd000)
  get Phys(data[n=6]=817be000)
  get Phys(data[n=7]=817bf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1ddf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1ddf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e5f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1e5f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 817c0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=817c0000)
  get Phys(data[n=1]=817c1000)
  get Phys(data[n=1]=817c2000)
  get Phys(data[n=2]=817c3000)
  get Phys(data[n=3]=817c4000)
  get Phys(data[n=3]=817c5000)
  get Phys(data[n=3]=817c6000)
  get Phys(data[n=3]=817c7000)
  get Phys(data[n=4]=817c8000)
  get Phys(data[n=4]=817c9000)
  get Phys(data[n=4]=817ca000)
  get Phys(data[n=4]=817cb000)
  get Phys(data[n=4]=817cc000)
  get Phys(data[n=4]=817cd000)
  get Phys(data[n=5]=817ce000)
  get Phys(data[n=5]=817cf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e5f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e5f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1edf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1edf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 817d0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=817d0000)
  get Phys(data[n=1]=817d1000)
  get Phys(data[n=1]=817d2000)
  get Phys(data[n=1]=817d3000)
  get Phys(data[n=1]=817d4000)
  get Phys(data[n=1]=817d5000)
  get Phys(data[n=1]=817d6000)
  get Phys(data[n=1]=817d7000)
  get Phys(data[n=2]=817d8000)
  get Phys(data[n=2]=817d9000)
  get Phys(data[n=2]=817da000)
  get Phys(data[n=2]=817db000)
  get Phys(data[n=2]=817dc000)
  get Phys(data[n=2]=817dd000)
  get Phys(data[n=3]=817de000)
  get Phys(data[n=3]=817df000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1edf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1edf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1f5f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1f5f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 817e0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=817e0000)
  get Phys(data[n=1]=817e1000)
  get Phys(data[n=1]=817e2000)
  get Phys(data[n=1]=817e3000)
  get Phys(data[n=2]=817e4000)
  get Phys(data[n=2]=817e5000)
  get Phys(data[n=2]=817e6000)
  get Phys(data[n=2]=817e7000)
  get Phys(data[n=2]=817e8000)
  get Phys(data[n=2]=817e9000)
  get Phys(data[n=2]=817ea000)
  get Phys(data[n=2]=817eb000)
  get Phys(data[n=2]=817ec000)
  get Phys(data[n=3]=817ed000)
  get Phys(data[n=4]=817ee000)
  get Phys(data[n=4]=817ef000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1f5f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1f5f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1fdf, OrigWordsRequested 0x7000, DevSize 0x70
IdeReadWrite (REQ): Starting sector is 1fdf, Number of WORDS 0x7000, DevSize 0x70
AtapiDmaSetup: mode 0x45, data 817f0000, count e000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=817f0000)
  get Phys(data[n=1]=817f1000)
  get Phys(data[n=1]=817f2000)
  get Phys(data[n=1]=817f3000)
  get Phys(data[n=1]=817f4000)
  get Phys(data[n=2]=817f5000)
  get Phys(data[n=2]=817f6000)
  get Phys(data[n=2]=817f7000)
  get Phys(data[n=2]=817f8000)
  get Phys(data[n=3]=817f9000)
  get Phys(data[n=3]=817fa000)
  get Phys(data[n=4]=817fb000)
  get Phys(data[n=4]=817fc000)
  get Phys(data[n=5]=817fd000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1fdf, Count 0x70(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1fdf count 0x70 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e000, full size e000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 469, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 469, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81800000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81800000)
  get Phys(data[n=1]=81801000)
  get Phys(data[n=2]=81802000)
  get Phys(data[n=3]=81803000)
  get Phys(data[n=3]=81804000)
  get Phys(data[n=3]=81805000)
  get Phys(data[n=3]=81806000)
  get Phys(data[n=4]=81807000)
  get Phys(data[n=4]=81808000)
  get Phys(data[n=4]=81809000)
  get Phys(data[n=4]=8180a000)
  get Phys(data[n=4]=8180b000)
  get Phys(data[n=4]=8180c000)
  get Phys(data[n=5]=8180d000)
  get Phys(data[n=5]=8180e000)
  get Phys(data[n=6]=8180f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x469, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x469 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81810000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81810000)
  get Phys(data[n=1]=81811000)
  get Phys(data[n=1]=81812000)
  get Phys(data[n=1]=81813000)
  get Phys(data[n=1]=81814000)
  get Phys(data[n=1]=81815000)
  get Phys(data[n=1]=81816000)
  get Phys(data[n=2]=81817000)
  get Phys(data[n=2]=81818000)
  get Phys(data[n=2]=81819000)
  get Phys(data[n=2]=8181a000)
  get Phys(data[n=2]=8181b000)
  get Phys(data[n=2]=8181c000)
  get Phys(data[n=3]=8181d000)
  get Phys(data[n=3]=8181e000)
  get Phys(data[n=3]=8181f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x4e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 569, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 569, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81820000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81820000)
  get Phys(data[n=1]=81821000)
  get Phys(data[n=1]=81822000)
  get Phys(data[n=2]=81823000)
  get Phys(data[n=2]=81824000)
  get Phys(data[n=2]=81825000)
  get Phys(data[n=2]=81826000)
  get Phys(data[n=2]=81827000)
  get Phys(data[n=2]=81828000)
  get Phys(data[n=2]=81829000)
  get Phys(data[n=2]=8182a000)
  get Phys(data[n=2]=8182b000)
  get Phys(data[n=3]=8182c000)
  get Phys(data[n=4]=8182d000)
  get Phys(data[n=4]=8182e000)
  get Phys(data[n=4]=8182f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x569, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x569 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81830000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81830000)
  get Phys(data[n=1]=81831000)
  get Phys(data[n=1]=81832000)
  get Phys(data[n=1]=81833000)
  get Phys(data[n=2]=81834000)
  get Phys(data[n=2]=81835000)
  get Phys(data[n=2]=81836000)
  get Phys(data[n=2]=81837000)
  get Phys(data[n=3]=81838000)
  get Phys(data[n=3]=81839000)
  get Phys(data[n=4]=8183a000)
  get Phys(data[n=4]=8183b000)
  get Phys(data[n=5]=8183c000)
  get Phys(data[n=6]=8183d000)
  get Phys(data[n=7]=8183e000)
  get Phys(data[n=7]=8183f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x5e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 669, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 669, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81840000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81840000)
  get Phys(data[n=1]=81841000)
  get Phys(data[n=2]=81842000)
  get Phys(data[n=3]=81843000)
  get Phys(data[n=3]=81844000)
  get Phys(data[n=3]=81845000)
  get Phys(data[n=3]=81846000)
  get Phys(data[n=4]=81847000)
  get Phys(data[n=4]=81848000)
  get Phys(data[n=4]=81849000)
  get Phys(data[n=4]=8184a000)
  get Phys(data[n=4]=8184b000)
  get Phys(data[n=4]=8184c000)
  get Phys(data[n=5]=8184d000)
  get Phys(data[n=5]=8184e000)
  get Phys(data[n=6]=8184f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x669, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x669 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 6e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 6e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81850000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81850000)
  get Phys(data[n=1]=81851000)
  get Phys(data[n=1]=81852000)
  get Phys(data[n=1]=81853000)
  get Phys(data[n=1]=81854000)
  get Phys(data[n=1]=81855000)
  get Phys(data[n=1]=81856000)
  get Phys(data[n=2]=81857000)
  get Phys(data[n=2]=81858000)
  get Phys(data[n=2]=81859000)
  get Phys(data[n=2]=8185a000)
  get Phys(data[n=2]=8185b000)
  get Phys(data[n=2]=8185c000)
  get Phys(data[n=3]=8185d000)
  get Phys(data[n=3]=8185e000)
  get Phys(data[n=3]=8185f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x6e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x6e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 769, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 769, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81860000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81860000)
  get Phys(data[n=1]=81861000)
  get Phys(data[n=1]=81862000)
  get Phys(data[n=2]=81863000)
  get Phys(data[n=2]=81864000)
  get Phys(data[n=2]=81865000)
  get Phys(data[n=2]=81866000)
  get Phys(data[n=2]=81867000)
  get Phys(data[n=2]=81868000)
  get Phys(data[n=2]=81869000)
  get Phys(data[n=2]=8186a000)
  get Phys(data[n=2]=8186b000)
  get Phys(data[n=3]=8186c000)
  get Phys(data[n=4]=8186d000)
  get Phys(data[n=4]=8186e000)
  get Phys(data[n=4]=8186f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x769, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x769 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 7e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 7e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81870000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81870000)
  get Phys(data[n=1]=81871000)
  get Phys(data[n=1]=81872000)
  get Phys(data[n=1]=81873000)
  get Phys(data[n=2]=81874000)
  get Phys(data[n=2]=81875000)
  get Phys(data[n=2]=81876000)
  get Phys(data[n=2]=81877000)
  get Phys(data[n=3]=81878000)
  get Phys(data[n=3]=81879000)
  get Phys(data[n=4]=8187a000)
  get Phys(data[n=4]=8187b000)
  get Phys(data[n=5]=8187c000)
  get Phys(data[n=6]=8187d000)
  get Phys(data[n=7]=8187e000)
  get Phys(data[n=7]=8187f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x7e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x7e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 869, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 869, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81880000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81880000)
  get Phys(data[n=1]=81881000)
  get Phys(data[n=2]=81882000)
  get Phys(data[n=3]=81883000)
  get Phys(data[n=3]=81884000)
  get Phys(data[n=3]=81885000)
  get Phys(data[n=3]=81886000)
  get Phys(data[n=4]=81887000)
  get Phys(data[n=4]=81888000)
  get Phys(data[n=4]=81889000)
  get Phys(data[n=4]=8188a000)
  get Phys(data[n=4]=8188b000)
  get Phys(data[n=4]=8188c000)
  get Phys(data[n=5]=8188d000)
  get Phys(data[n=5]=8188e000)
  get Phys(data[n=6]=8188f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x869, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x869 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 8e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 8e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81890000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81890000)
  get Phys(data[n=1]=81891000)
  get Phys(data[n=1]=81892000)
  get Phys(data[n=1]=81893000)
  get Phys(data[n=1]=81894000)
  get Phys(data[n=1]=81895000)
  get Phys(data[n=1]=81896000)
  get Phys(data[n=2]=81897000)
  get Phys(data[n=2]=81898000)
  get Phys(data[n=2]=81899000)
  get Phys(data[n=2]=8189a000)
  get Phys(data[n=2]=8189b000)
  get Phys(data[n=2]=8189c000)
  get Phys(data[n=3]=8189d000)
  get Phys(data[n=3]=8189e000)
  get Phys(data[n=3]=8189f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x8e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x8e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 969, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 969, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 818a0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=818a0000)
  get Phys(data[n=1]=818a1000)
  get Phys(data[n=1]=818a2000)
  get Phys(data[n=2]=818a3000)
  get Phys(data[n=2]=818a4000)
  get Phys(data[n=2]=818a5000)
  get Phys(data[n=2]=818a6000)
  get Phys(data[n=2]=818a7000)
  get Phys(data[n=2]=818a8000)
  get Phys(data[n=2]=818a9000)
  get Phys(data[n=2]=818aa000)
  get Phys(data[n=2]=818ab000)
  get Phys(data[n=3]=818ac000)
  get Phys(data[n=4]=818ad000)
  get Phys(data[n=4]=818ae000)
  get Phys(data[n=4]=818af000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x969, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x969 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 9e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 9e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 818b0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=818b0000)
  get Phys(data[n=1]=818b1000)
  get Phys(data[n=1]=818b2000)
  get Phys(data[n=1]=818b3000)
  get Phys(data[n=2]=818b4000)
  get Phys(data[n=2]=818b5000)
  get Phys(data[n=2]=818b6000)
  get Phys(data[n=2]=818b7000)
  get Phys(data[n=3]=818b8000)
  get Phys(data[n=3]=818b9000)
  get Phys(data[n=4]=818ba000)
  get Phys(data[n=4]=818bb000)
  get Phys(data[n=5]=818bc000)
  get Phys(data[n=6]=818bd000)
  get Phys(data[n=7]=818be000)
  get Phys(data[n=7]=818bf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x9e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x9e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector a69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is a69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 818c0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=818c0000)
  get Phys(data[n=1]=818c1000)
  get Phys(data[n=2]=818c2000)
  get Phys(data[n=3]=818c3000)
  get Phys(data[n=3]=818c4000)
  get Phys(data[n=3]=818c5000)
  get Phys(data[n=3]=818c6000)
  get Phys(data[n=4]=818c7000)
  get Phys(data[n=4]=818c8000)
  get Phys(data[n=4]=818c9000)
  get Phys(data[n=4]=818ca000)
  get Phys(data[n=4]=818cb000)
  get Phys(data[n=4]=818cc000)
  get Phys(data[n=5]=818cd000)
  get Phys(data[n=5]=818ce000)
  get Phys(data[n=6]=818cf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xa69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0xa69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector ae9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is ae9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 818d0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=818d0000)
  get Phys(data[n=1]=818d1000)
  get Phys(data[n=1]=818d2000)
  get Phys(data[n=1]=818d3000)
  get Phys(data[n=1]=818d4000)
  get Phys(data[n=1]=818d5000)
  get Phys(data[n=1]=818d6000)
  get Phys(data[n=2]=818d7000)
  get Phys(data[n=2]=818d8000)
  get Phys(data[n=2]=818d9000)
  get Phys(data[n=2]=818da000)
  get Phys(data[n=2]=818db000)
  get Phys(data[n=2]=818dc000)
  get Phys(data[n=3]=818dd000)
  get Phys(data[n=3]=818de000)
  get Phys(data[n=3]=818df000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xae9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0xae9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector b69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is b69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 818e0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=818e0000)
  get Phys(data[n=1]=818e1000)
  get Phys(data[n=1]=818e2000)
  get Phys(data[n=2]=818e3000)
  get Phys(data[n=2]=818e4000)
  get Phys(data[n=2]=818e5000)
  get Phys(data[n=2]=818e6000)
  get Phys(data[n=2]=818e7000)
  get Phys(data[n=2]=818e8000)
  get Phys(data[n=2]=818e9000)
  get Phys(data[n=2]=818ea000)
  get Phys(data[n=2]=818eb000)
  get Phys(data[n=3]=818ec000)
  get Phys(data[n=4]=818ed000)
  get Phys(data[n=4]=818ee000)
  get Phys(data[n=4]=818ef000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xb69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0xb69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector be9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is be9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 818f0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=818f0000)
  get Phys(data[n=1]=818f1000)
  get Phys(data[n=1]=818f2000)
  get Phys(data[n=1]=818f3000)
  get Phys(data[n=2]=818f4000)
  get Phys(data[n=2]=818f5000)
  get Phys(data[n=2]=818f6000)
  get Phys(data[n=2]=818f7000)
  get Phys(data[n=3]=818f8000)
  get Phys(data[n=3]=818f9000)
  get Phys(data[n=4]=818fa000)
  get Phys(data[n=4]=818fb000)
  get Phys(data[n=5]=818fc000)
  get Phys(data[n=6]=818fd000)
  get Phys(data[n=7]=818fe000)
  get Phys(data[n=7]=818ff000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xbe9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0xbe9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector c69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is c69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81900000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81900000)
  get Phys(data[n=1]=81901000)
  get Phys(data[n=2]=81902000)
  get Phys(data[n=3]=81903000)
  get Phys(data[n=3]=81904000)
  get Phys(data[n=3]=81905000)
  get Phys(data[n=3]=81906000)
  get Phys(data[n=4]=81907000)
  get Phys(data[n=4]=81908000)
  get Phys(data[n=4]=81909000)
  get Phys(data[n=4]=8190a000)
  get Phys(data[n=4]=8190b000)
  get Phys(data[n=4]=8190c000)
  get Phys(data[n=5]=8190d000)
  get Phys(data[n=5]=8190e000)
  get Phys(data[n=6]=8190f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xc69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0xc69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector ce9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is ce9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81910000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81910000)
  get Phys(data[n=1]=81911000)
  get Phys(data[n=1]=81912000)
  get Phys(data[n=1]=81913000)
  get Phys(data[n=1]=81914000)
  get Phys(data[n=1]=81915000)
  get Phys(data[n=1]=81916000)
  get Phys(data[n=2]=81917000)
  get Phys(data[n=2]=81918000)
  get Phys(data[n=2]=81919000)
  get Phys(data[n=2]=8191a000)
  get Phys(data[n=2]=8191b000)
  get Phys(data[n=2]=8191c000)
  get Phys(data[n=3]=8191d000)
  get Phys(data[n=3]=8191e000)
  get Phys(data[n=3]=8191f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xce9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0xce9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector d69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is d69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81920000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81920000)
  get Phys(data[n=1]=81921000)
  get Phys(data[n=1]=81922000)
  get Phys(data[n=2]=81923000)
  get Phys(data[n=2]=81924000)
  get Phys(data[n=2]=81925000)
  get Phys(data[n=2]=81926000)
  get Phys(data[n=2]=81927000)
  get Phys(data[n=2]=81928000)
  get Phys(data[n=2]=81929000)
  get Phys(data[n=2]=8192a000)
  get Phys(data[n=2]=8192b000)
  get Phys(data[n=3]=8192c000)
  get Phys(data[n=4]=8192d000)
  get Phys(data[n=4]=8192e000)
  get Phys(data[n=4]=8192f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xd69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0xd69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector de9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is de9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81930000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81930000)
  get Phys(data[n=1]=81931000)
  get Phys(data[n=1]=81932000)
  get Phys(data[n=1]=81933000)
  get Phys(data[n=2]=81934000)
  get Phys(data[n=2]=81935000)
  get Phys(data[n=2]=81936000)
  get Phys(data[n=2]=81937000)
  get Phys(data[n=3]=81938000)
  get Phys(data[n=3]=81939000)
  get Phys(data[n=4]=8193a000)
  get Phys(data[n=4]=8193b000)
  get Phys(data[n=5]=8193c000)
  get Phys(data[n=6]=8193d000)
  get Phys(data[n=7]=8193e000)
  get Phys(data[n=7]=8193f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xde9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0xde9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector e69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is e69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81940000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81940000)
  get Phys(data[n=1]=81941000)
  get Phys(data[n=2]=81942000)
  get Phys(data[n=3]=81943000)
  get Phys(data[n=3]=81944000)
  get Phys(data[n=3]=81945000)
  get Phys(data[n=3]=81946000)
  get Phys(data[n=4]=81947000)
  get Phys(data[n=4]=81948000)
  get Phys(data[n=4]=81949000)
  get Phys(data[n=4]=8194a000)
  get Phys(data[n=4]=8194b000)
  get Phys(data[n=4]=8194c000)
  get Phys(data[n=5]=8194d000)
  get Phys(data[n=5]=8194e000)
  get Phys(data[n=6]=8194f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xe69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0xe69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector ee9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is ee9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81950000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81950000)
  get Phys(data[n=1]=81951000)
  get Phys(data[n=1]=81952000)
  get Phys(data[n=1]=81953000)
  get Phys(data[n=1]=81954000)
  get Phys(data[n=1]=81955000)
  get Phys(data[n=1]=81956000)
  get Phys(data[n=2]=81957000)
  get Phys(data[n=2]=81958000)
  get Phys(data[n=2]=81959000)
  get Phys(data[n=2]=8195a000)
  get Phys(data[n=2]=8195b000)
  get Phys(data[n=2]=8195c000)
  get Phys(data[n=3]=8195d000)
  get Phys(data[n=3]=8195e000)
  get Phys(data[n=3]=8195f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xee9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0xee9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector f69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is f69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81960000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81960000)
  get Phys(data[n=1]=81961000)
  get Phys(data[n=1]=81962000)
  get Phys(data[n=2]=81963000)
  get Phys(data[n=2]=81964000)
  get Phys(data[n=2]=81965000)
  get Phys(data[n=2]=81966000)
  get Phys(data[n=2]=81967000)
  get Phys(data[n=2]=81968000)
  get Phys(data[n=2]=81969000)
  get Phys(data[n=2]=8196a000)
  get Phys(data[n=2]=8196b000)
  get Phys(data[n=3]=8196c000)
  get Phys(data[n=4]=8196d000)
  get Phys(data[n=4]=8196e000)
  get Phys(data[n=4]=8196f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xf69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0xf69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector fe9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is fe9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81970000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81970000)
  get Phys(data[n=1]=81971000)
  get Phys(data[n=1]=81972000)
  get Phys(data[n=1]=81973000)
  get Phys(data[n=2]=81974000)
  get Phys(data[n=2]=81975000)
  get Phys(data[n=2]=81976000)
  get Phys(data[n=2]=81977000)
  get Phys(data[n=3]=81978000)
  get Phys(data[n=3]=81979000)
  get Phys(data[n=4]=8197a000)
  get Phys(data[n=4]=8197b000)
  get Phys(data[n=5]=8197c000)
  get Phys(data[n=6]=8197d000)
  get Phys(data[n=7]=8197e000)
  get Phys(data[n=7]=8197f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xfe9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0xfe9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1069, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1069, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81980000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81980000)
  get Phys(data[n=1]=81981000)
  get Phys(data[n=2]=81982000)
  get Phys(data[n=3]=81983000)
  get Phys(data[n=3]=81984000)
  get Phys(data[n=3]=81985000)
  get Phys(data[n=3]=81986000)
  get Phys(data[n=4]=81987000)
  get Phys(data[n=4]=81988000)
  get Phys(data[n=4]=81989000)
  get Phys(data[n=4]=8198a000)
  get Phys(data[n=4]=8198b000)
  get Phys(data[n=4]=8198c000)
  get Phys(data[n=5]=8198d000)
  get Phys(data[n=5]=8198e000)
  get Phys(data[n=6]=8198f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1069, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1069 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 10e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 10e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81990000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81990000)
  get Phys(data[n=1]=81991000)
  get Phys(data[n=1]=81992000)
  get Phys(data[n=1]=81993000)
  get Phys(data[n=1]=81994000)
  get Phys(data[n=1]=81995000)
  get Phys(data[n=1]=81996000)
  get Phys(data[n=2]=81997000)
  get Phys(data[n=2]=81998000)
  get Phys(data[n=2]=81999000)
  get Phys(data[n=2]=8199a000)
  get Phys(data[n=2]=8199b000)
  get Phys(data[n=2]=8199c000)
  get Phys(data[n=3]=8199d000)
  get Phys(data[n=3]=8199e000)
  get Phys(data[n=3]=8199f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x10e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x10e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1169, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1169, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 819a0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=819a0000)
  get Phys(data[n=1]=819a1000)
  get Phys(data[n=1]=819a2000)
  get Phys(data[n=2]=819a3000)
  get Phys(data[n=2]=819a4000)
  get Phys(data[n=2]=819a5000)
  get Phys(data[n=2]=819a6000)
  get Phys(data[n=2]=819a7000)
  get Phys(data[n=2]=819a8000)
  get Phys(data[n=2]=819a9000)
  get Phys(data[n=2]=819aa000)
  get Phys(data[n=2]=819ab000)
  get Phys(data[n=3]=819ac000)
  get Phys(data[n=4]=819ad000)
  get Phys(data[n=4]=819ae000)
  get Phys(data[n=4]=819af000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1169, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1169 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 11e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 819b0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=819b0000)
  get Phys(data[n=1]=819b1000)
  get Phys(data[n=1]=819b2000)
  get Phys(data[n=1]=819b3000)
  get Phys(data[n=2]=819b4000)
  get Phys(data[n=2]=819b5000)
  get Phys(data[n=2]=819b6000)
  get Phys(data[n=2]=819b7000)
  get Phys(data[n=3]=819b8000)
  get Phys(data[n=3]=819b9000)
  get Phys(data[n=4]=819ba000)
  get Phys(data[n=4]=819bb000)
  get Phys(data[n=5]=819bc000)
  get Phys(data[n=6]=819bd000)
  get Phys(data[n=7]=819be000)
  get Phys(data[n=7]=819bf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x11e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x11e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1269, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1269, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 819c0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=819c0000)
  get Phys(data[n=1]=819c1000)
  get Phys(data[n=2]=819c2000)
  get Phys(data[n=3]=819c3000)
  get Phys(data[n=3]=819c4000)
  get Phys(data[n=3]=819c5000)
  get Phys(data[n=3]=819c6000)
  get Phys(data[n=4]=819c7000)
  get Phys(data[n=4]=819c8000)
  get Phys(data[n=4]=819c9000)
  get Phys(data[n=4]=819ca000)
  get Phys(data[n=4]=819cb000)
  get Phys(data[n=4]=819cc000)
  get Phys(data[n=5]=819cd000)
  get Phys(data[n=5]=819ce000)
  get Phys(data[n=6]=819cf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1269, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1269 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 12e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 12e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 819d0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=819d0000)
  get Phys(data[n=1]=819d1000)
  get Phys(data[n=1]=819d2000)
  get Phys(data[n=1]=819d3000)
  get Phys(data[n=1]=819d4000)
  get Phys(data[n=1]=819d5000)
  get Phys(data[n=1]=819d6000)
  get Phys(data[n=2]=819d7000)
  get Phys(data[n=2]=819d8000)
  get Phys(data[n=2]=819d9000)
  get Phys(data[n=2]=819da000)
  get Phys(data[n=2]=819db000)
  get Phys(data[n=2]=819dc000)
  get Phys(data[n=3]=819dd000)
  get Phys(data[n=3]=819de000)
  get Phys(data[n=3]=819df000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x12e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x12e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1369, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1369, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 819e0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=819e0000)
  get Phys(data[n=1]=819e1000)
  get Phys(data[n=1]=819e2000)
  get Phys(data[n=2]=819e3000)
  get Phys(data[n=2]=819e4000)
  get Phys(data[n=2]=819e5000)
  get Phys(data[n=2]=819e6000)
  get Phys(data[n=2]=819e7000)
  get Phys(data[n=2]=819e8000)
  get Phys(data[n=2]=819e9000)
  get Phys(data[n=2]=819ea000)
  get Phys(data[n=2]=819eb000)
  get Phys(data[n=3]=819ec000)
  get Phys(data[n=4]=819ed000)
  get Phys(data[n=4]=819ee000)
  get Phys(data[n=4]=819ef000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1369, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1369 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 13e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 13e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 819f0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=819f0000)
  get Phys(data[n=1]=819f1000)
  get Phys(data[n=1]=819f2000)
  get Phys(data[n=1]=819f3000)
  get Phys(data[n=2]=819f4000)
  get Phys(data[n=2]=819f5000)
  get Phys(data[n=2]=819f6000)
  get Phys(data[n=2]=819f7000)
  get Phys(data[n=3]=819f8000)
  get Phys(data[n=3]=819f9000)
  get Phys(data[n=4]=819fa000)
  get Phys(data[n=4]=819fb000)
  get Phys(data[n=5]=819fc000)
  get Phys(data[n=6]=819fd000)
  get Phys(data[n=7]=819fe000)
  get Phys(data[n=7]=819ff000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x13e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x13e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1469, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1469, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81a00000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81a00000)
  get Phys(data[n=1]=81a01000)
  get Phys(data[n=2]=81a02000)
  get Phys(data[n=3]=81a03000)
  get Phys(data[n=3]=81a04000)
  get Phys(data[n=3]=81a05000)
  get Phys(data[n=3]=81a06000)
  get Phys(data[n=4]=81a07000)
  get Phys(data[n=4]=81a08000)
  get Phys(data[n=4]=81a09000)
  get Phys(data[n=4]=81a0a000)
  get Phys(data[n=4]=81a0b000)
  get Phys(data[n=4]=81a0c000)
  get Phys(data[n=5]=81a0d000)
  get Phys(data[n=5]=81a0e000)
  get Phys(data[n=6]=81a0f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1469, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1469 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 14e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 14e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81a10000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81a10000)
  get Phys(data[n=1]=81a11000)
  get Phys(data[n=1]=81a12000)
  get Phys(data[n=1]=81a13000)
  get Phys(data[n=1]=81a14000)
  get Phys(data[n=1]=81a15000)
  get Phys(data[n=1]=81a16000)
  get Phys(data[n=2]=81a17000)
  get Phys(data[n=2]=81a18000)
  get Phys(data[n=2]=81a19000)
  get Phys(data[n=2]=81a1a000)
  get Phys(data[n=2]=81a1b000)
  get Phys(data[n=2]=81a1c000)
  get Phys(data[n=3]=81a1d000)
  get Phys(data[n=3]=81a1e000)
  get Phys(data[n=3]=81a1f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x14e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x14e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1569, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1569, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81a20000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81a20000)
  get Phys(data[n=1]=81a21000)
  get Phys(data[n=1]=81a22000)
  get Phys(data[n=2]=81a23000)
  get Phys(data[n=2]=81a24000)
  get Phys(data[n=2]=81a25000)
  get Phys(data[n=2]=81a26000)
  get Phys(data[n=2]=81a27000)
  get Phys(data[n=2]=81a28000)
  get Phys(data[n=2]=81a29000)
  get Phys(data[n=2]=81a2a000)
  get Phys(data[n=2]=81a2b000)
  get Phys(data[n=3]=81a2c000)
  get Phys(data[n=4]=81a2d000)
  get Phys(data[n=4]=81a2e000)
  get Phys(data[n=4]=81a2f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1569, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1569 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 15e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 15e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81a30000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81a30000)
  get Phys(data[n=1]=81a31000)
  get Phys(data[n=1]=81a32000)
  get Phys(data[n=1]=81a33000)
  get Phys(data[n=2]=81a34000)
  get Phys(data[n=2]=81a35000)
  get Phys(data[n=2]=81a36000)
  get Phys(data[n=2]=81a37000)
  get Phys(data[n=3]=81a38000)
  get Phys(data[n=3]=81a39000)
  get Phys(data[n=4]=81a3a000)
  get Phys(data[n=4]=81a3b000)
  get Phys(data[n=5]=81a3c000)
  get Phys(data[n=6]=81a3d000)
  get Phys(data[n=7]=81a3e000)
  get Phys(data[n=7]=81a3f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x15e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x15e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1669, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1669, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81a40000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81a40000)
  get Phys(data[n=1]=81a41000)
  get Phys(data[n=2]=81a42000)
  get Phys(data[n=3]=81a43000)
  get Phys(data[n=3]=81a44000)
  get Phys(data[n=3]=81a45000)
  get Phys(data[n=3]=81a46000)
  get Phys(data[n=4]=81a47000)
  get Phys(data[n=4]=81a48000)
  get Phys(data[n=4]=81a49000)
  get Phys(data[n=4]=81a4a000)
  get Phys(data[n=4]=81a4b000)
  get Phys(data[n=4]=81a4c000)
  get Phys(data[n=5]=81a4d000)
  get Phys(data[n=5]=81a4e000)
  get Phys(data[n=6]=81a4f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1669, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1669 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 16e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 16e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81a50000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81a50000)
  get Phys(data[n=1]=81a51000)
  get Phys(data[n=1]=81a52000)
  get Phys(data[n=1]=81a53000)
  get Phys(data[n=1]=81a54000)
  get Phys(data[n=1]=81a55000)
  get Phys(data[n=1]=81a56000)
  get Phys(data[n=2]=81a57000)
  get Phys(data[n=2]=81a58000)
  get Phys(data[n=2]=81a59000)
  get Phys(data[n=2]=81a5a000)
  get Phys(data[n=2]=81a5b000)
  get Phys(data[n=2]=81a5c000)
  get Phys(data[n=3]=81a5d000)
  get Phys(data[n=3]=81a5e000)
  get Phys(data[n=3]=81a5f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x16e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x16e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1769, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1769, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81a60000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81a60000)
  get Phys(data[n=1]=81a61000)
  get Phys(data[n=1]=81a62000)
  get Phys(data[n=2]=81a63000)
  get Phys(data[n=2]=81a64000)
  get Phys(data[n=2]=81a65000)
  get Phys(data[n=2]=81a66000)
  get Phys(data[n=2]=81a67000)
  get Phys(data[n=2]=81a68000)
  get Phys(data[n=2]=81a69000)
  get Phys(data[n=2]=81a6a000)
  get Phys(data[n=2]=81a6b000)
  get Phys(data[n=3]=81a6c000)
  get Phys(data[n=4]=81a6d000)
  get Phys(data[n=4]=81a6e000)
  get Phys(data[n=4]=81a6f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1769, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1769 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 17e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 17e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81a70000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81a70000)
  get Phys(data[n=1]=81a71000)
  get Phys(data[n=1]=81a72000)
  get Phys(data[n=1]=81a73000)
  get Phys(data[n=2]=81a74000)
  get Phys(data[n=2]=81a75000)
  get Phys(data[n=2]=81a76000)
  get Phys(data[n=2]=81a77000)
  get Phys(data[n=3]=81a78000)
  get Phys(data[n=3]=81a79000)
  get Phys(data[n=4]=81a7a000)
  get Phys(data[n=4]=81a7b000)
  get Phys(data[n=5]=81a7c000)
  get Phys(data[n=6]=81a7d000)
  get Phys(data[n=7]=81a7e000)
  get Phys(data[n=7]=81a7f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x17e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x17e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1869, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1869, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81a80000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81a80000)
  get Phys(data[n=1]=81a81000)
  get Phys(data[n=2]=81a82000)
  get Phys(data[n=3]=81a83000)
  get Phys(data[n=3]=81a84000)
  get Phys(data[n=3]=81a85000)
  get Phys(data[n=3]=81a86000)
  get Phys(data[n=4]=81a87000)
  get Phys(data[n=4]=81a88000)
  get Phys(data[n=4]=81a89000)
  get Phys(data[n=4]=81a8a000)
  get Phys(data[n=4]=81a8b000)
  get Phys(data[n=4]=81a8c000)
  get Phys(data[n=5]=81a8d000)
  get Phys(data[n=5]=81a8e000)
  get Phys(data[n=6]=81a8f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1869, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1869 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 18e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 18e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81a90000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81a90000)
  get Phys(data[n=1]=81a91000)
  get Phys(data[n=1]=81a92000)
  get Phys(data[n=1]=81a93000)
  get Phys(data[n=1]=81a94000)
  get Phys(data[n=1]=81a95000)
  get Phys(data[n=1]=81a96000)
  get Phys(data[n=2]=81a97000)
  get Phys(data[n=2]=81a98000)
  get Phys(data[n=2]=81a99000)
  get Phys(data[n=2]=81a9a000)
  get Phys(data[n=2]=81a9b000)
  get Phys(data[n=2]=81a9c000)
  get Phys(data[n=3]=81a9d000)
  get Phys(data[n=3]=81a9e000)
  get Phys(data[n=3]=81a9f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x18e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x18e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1969, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1969, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81aa0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81aa0000)
  get Phys(data[n=1]=81aa1000)
  get Phys(data[n=1]=81aa2000)
  get Phys(data[n=2]=81aa3000)
  get Phys(data[n=2]=81aa4000)
  get Phys(data[n=2]=81aa5000)
  get Phys(data[n=2]=81aa6000)
  get Phys(data[n=2]=81aa7000)
  get Phys(data[n=2]=81aa8000)
  get Phys(data[n=2]=81aa9000)
  get Phys(data[n=2]=81aaa000)
  get Phys(data[n=2]=81aab000)
  get Phys(data[n=3]=81aac000)
  get Phys(data[n=4]=81aad000)
  get Phys(data[n=4]=81aae000)
  get Phys(data[n=4]=81aaf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1969, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1969 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 19e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 19e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81ab0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81ab0000)
  get Phys(data[n=1]=81ab1000)
  get Phys(data[n=1]=81ab2000)
  get Phys(data[n=1]=81ab3000)
  get Phys(data[n=2]=81ab4000)
  get Phys(data[n=2]=81ab5000)
  get Phys(data[n=2]=81ab6000)
  get Phys(data[n=2]=81ab7000)
  get Phys(data[n=3]=81ab8000)
  get Phys(data[n=3]=81ab9000)
  get Phys(data[n=4]=81aba000)
  get Phys(data[n=4]=81abb000)
  get Phys(data[n=5]=81abc000)
  get Phys(data[n=6]=81abd000)
  get Phys(data[n=7]=81abe000)
  get Phys(data[n=7]=81abf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x19e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x19e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1a69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1a69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81ac0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81ac0000)
  get Phys(data[n=1]=81ac1000)
  get Phys(data[n=2]=81ac2000)
  get Phys(data[n=3]=81ac3000)
  get Phys(data[n=3]=81ac4000)
  get Phys(data[n=3]=81ac5000)
  get Phys(data[n=3]=81ac6000)
  get Phys(data[n=4]=81ac7000)
  get Phys(data[n=4]=81ac8000)
  get Phys(data[n=4]=81ac9000)
  get Phys(data[n=4]=81aca000)
  get Phys(data[n=4]=81acb000)
  get Phys(data[n=4]=81acc000)
  get Phys(data[n=5]=81acd000)
  get Phys(data[n=5]=81ace000)
  get Phys(data[n=6]=81acf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1a69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1a69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1ae9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1ae9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81ad0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81ad0000)
  get Phys(data[n=1]=81ad1000)
  get Phys(data[n=1]=81ad2000)
  get Phys(data[n=1]=81ad3000)
  get Phys(data[n=1]=81ad4000)
  get Phys(data[n=1]=81ad5000)
  get Phys(data[n=1]=81ad6000)
  get Phys(data[n=2]=81ad7000)
  get Phys(data[n=2]=81ad8000)
  get Phys(data[n=2]=81ad9000)
  get Phys(data[n=2]=81ada000)
  get Phys(data[n=2]=81adb000)
  get Phys(data[n=2]=81adc000)
  get Phys(data[n=3]=81add000)
  get Phys(data[n=3]=81ade000)
  get Phys(data[n=3]=81adf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1ae9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1ae9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1b69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1b69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81ae0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81ae0000)
  get Phys(data[n=1]=81ae1000)
  get Phys(data[n=1]=81ae2000)
  get Phys(data[n=2]=81ae3000)
  get Phys(data[n=2]=81ae4000)
  get Phys(data[n=2]=81ae5000)
  get Phys(data[n=2]=81ae6000)
  get Phys(data[n=2]=81ae7000)
  get Phys(data[n=2]=81ae8000)
  get Phys(data[n=2]=81ae9000)
  get Phys(data[n=2]=81aea000)
  get Phys(data[n=2]=81aeb000)
  get Phys(data[n=3]=81aec000)
  get Phys(data[n=4]=81aed000)
  get Phys(data[n=4]=81aee000)
  get Phys(data[n=4]=81aef000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1b69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1b69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1be9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1be9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81af0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81af0000)
  get Phys(data[n=1]=81af1000)
  get Phys(data[n=1]=81af2000)
  get Phys(data[n=1]=81af3000)
  get Phys(data[n=2]=81af4000)
  get Phys(data[n=2]=81af5000)
  get Phys(data[n=2]=81af6000)
  get Phys(data[n=2]=81af7000)
  get Phys(data[n=3]=81af8000)
  get Phys(data[n=3]=81af9000)
  get Phys(data[n=4]=81afa000)
  get Phys(data[n=4]=81afb000)
  get Phys(data[n=5]=81afc000)
  get Phys(data[n=6]=81afd000)
  get Phys(data[n=7]=81afe000)
  get Phys(data[n=7]=81aff000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1be9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1be9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1c69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1c69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81b00000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81b00000)
  get Phys(data[n=1]=81b01000)
  get Phys(data[n=2]=81b02000)
  get Phys(data[n=3]=81b03000)
  get Phys(data[n=3]=81b04000)
  get Phys(data[n=3]=81b05000)
  get Phys(data[n=3]=81b06000)
  get Phys(data[n=4]=81b07000)
  get Phys(data[n=4]=81b08000)
  get Phys(data[n=4]=81b09000)
  get Phys(data[n=4]=81b0a000)
  get Phys(data[n=4]=81b0b000)
  get Phys(data[n=4]=81b0c000)
  get Phys(data[n=5]=81b0d000)
  get Phys(data[n=5]=81b0e000)
  get Phys(data[n=6]=81b0f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1c69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1c69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1ce9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1ce9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81b10000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81b10000)
  get Phys(data[n=1]=81b11000)
  get Phys(data[n=1]=81b12000)
  get Phys(data[n=1]=81b13000)
  get Phys(data[n=1]=81b14000)
  get Phys(data[n=1]=81b15000)
  get Phys(data[n=1]=81b16000)
  get Phys(data[n=2]=81b17000)
  get Phys(data[n=2]=81b18000)
  get Phys(data[n=2]=81b19000)
  get Phys(data[n=2]=81b1a000)
  get Phys(data[n=2]=81b1b000)
  get Phys(data[n=2]=81b1c000)
  get Phys(data[n=3]=81b1d000)
  get Phys(data[n=3]=81b1e000)
  get Phys(data[n=3]=81b1f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1ce9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1ce9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1d69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81b20000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81b20000)
  get Phys(data[n=1]=81b21000)
  get Phys(data[n=1]=81b22000)
  get Phys(data[n=2]=81b23000)
  get Phys(data[n=2]=81b24000)
  get Phys(data[n=2]=81b25000)
  get Phys(data[n=2]=81b26000)
  get Phys(data[n=2]=81b27000)
  get Phys(data[n=2]=81b28000)
  get Phys(data[n=2]=81b29000)
  get Phys(data[n=2]=81b2a000)
  get Phys(data[n=2]=81b2b000)
  get Phys(data[n=3]=81b2c000)
  get Phys(data[n=4]=81b2d000)
  get Phys(data[n=4]=81b2e000)
  get Phys(data[n=4]=81b2f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1d69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1de9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1de9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81b30000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81b30000)
  get Phys(data[n=1]=81b31000)
  get Phys(data[n=1]=81b32000)
  get Phys(data[n=1]=81b33000)
  get Phys(data[n=2]=81b34000)
  get Phys(data[n=2]=81b35000)
  get Phys(data[n=2]=81b36000)
  get Phys(data[n=2]=81b37000)
  get Phys(data[n=3]=81b38000)
  get Phys(data[n=3]=81b39000)
  get Phys(data[n=4]=81b3a000)
  get Phys(data[n=4]=81b3b000)
  get Phys(data[n=5]=81b3c000)
  get Phys(data[n=6]=81b3d000)
  get Phys(data[n=7]=81b3e000)
  get Phys(data[n=7]=81b3f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1de9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1de9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1e69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81b40000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81b40000)
  get Phys(data[n=1]=81b41000)
  get Phys(data[n=2]=81b42000)
  get Phys(data[n=3]=81b43000)
  get Phys(data[n=3]=81b44000)
  get Phys(data[n=3]=81b45000)
  get Phys(data[n=3]=81b46000)
  get Phys(data[n=4]=81b47000)
  get Phys(data[n=4]=81b48000)
  get Phys(data[n=4]=81b49000)
  get Phys(data[n=4]=81b4a000)
  get Phys(data[n=4]=81b4b000)
  get Phys(data[n=4]=81b4c000)
  get Phys(data[n=5]=81b4d000)
  get Phys(data[n=5]=81b4e000)
  get Phys(data[n=6]=81b4f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1e69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1ee9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1ee9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81b50000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81b50000)
  get Phys(data[n=1]=81b51000)
  get Phys(data[n=1]=81b52000)
  get Phys(data[n=1]=81b53000)
  get Phys(data[n=1]=81b54000)
  get Phys(data[n=1]=81b55000)
  get Phys(data[n=1]=81b56000)
  get Phys(data[n=2]=81b57000)
  get Phys(data[n=2]=81b58000)
  get Phys(data[n=2]=81b59000)
  get Phys(data[n=2]=81b5a000)
  get Phys(data[n=2]=81b5b000)
  get Phys(data[n=2]=81b5c000)
  get Phys(data[n=3]=81b5d000)
  get Phys(data[n=3]=81b5e000)
  get Phys(data[n=3]=81b5f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1ee9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1ee9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1f69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1f69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81b60000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81b60000)
  get Phys(data[n=1]=81b61000)
  get Phys(data[n=1]=81b62000)
  get Phys(data[n=2]=81b63000)
  get Phys(data[n=2]=81b64000)
  get Phys(data[n=2]=81b65000)
  get Phys(data[n=2]=81b66000)
  get Phys(data[n=2]=81b67000)
  get Phys(data[n=2]=81b68000)
  get Phys(data[n=2]=81b69000)
  get Phys(data[n=2]=81b6a000)
  get Phys(data[n=2]=81b6b000)
  get Phys(data[n=3]=81b6c000)
  get Phys(data[n=4]=81b6d000)
  get Phys(data[n=4]=81b6e000)
  get Phys(data[n=4]=81b6f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1f69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1f69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1fe9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1fe9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81b70000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81b70000)
  get Phys(data[n=1]=81b71000)
  get Phys(data[n=1]=81b72000)
  get Phys(data[n=1]=81b73000)
  get Phys(data[n=2]=81b74000)
  get Phys(data[n=2]=81b75000)
  get Phys(data[n=2]=81b76000)
  get Phys(data[n=2]=81b77000)
  get Phys(data[n=3]=81b78000)
  get Phys(data[n=3]=81b79000)
  get Phys(data[n=4]=81b7a000)
  get Phys(data[n=4]=81b7b000)
  get Phys(data[n=5]=81b7c000)
  get Phys(data[n=6]=81b7d000)
  get Phys(data[n=7]=81b7e000)
  get Phys(data[n=7]=81b7f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1fe9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x1fe9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2069, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2069, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81b80000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81b80000)
  get Phys(data[n=1]=81b81000)
  get Phys(data[n=2]=81b82000)
  get Phys(data[n=3]=81b83000)
  get Phys(data[n=3]=81b84000)
  get Phys(data[n=3]=81b85000)
  get Phys(data[n=3]=81b86000)
  get Phys(data[n=4]=81b87000)
  get Phys(data[n=4]=81b88000)
  get Phys(data[n=4]=81b89000)
  get Phys(data[n=4]=81b8a000)
  get Phys(data[n=4]=81b8b000)
  get Phys(data[n=4]=81b8c000)
  get Phys(data[n=5]=81b8d000)
  get Phys(data[n=5]=81b8e000)
  get Phys(data[n=6]=81b8f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2069, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2069 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 20e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 20e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81b90000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81b90000)
  get Phys(data[n=1]=81b91000)
  get Phys(data[n=1]=81b92000)
  get Phys(data[n=1]=81b93000)
  get Phys(data[n=1]=81b94000)
  get Phys(data[n=1]=81b95000)
  get Phys(data[n=1]=81b96000)
  get Phys(data[n=2]=81b97000)
  get Phys(data[n=2]=81b98000)
  get Phys(data[n=2]=81b99000)
  get Phys(data[n=2]=81b9a000)
  get Phys(data[n=2]=81b9b000)
  get Phys(data[n=2]=81b9c000)
  get Phys(data[n=3]=81b9d000)
  get Phys(data[n=3]=81b9e000)
  get Phys(data[n=3]=81b9f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x20e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x20e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2169, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2169, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81ba0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81ba0000)
  get Phys(data[n=1]=81ba1000)
  get Phys(data[n=1]=81ba2000)
  get Phys(data[n=2]=81ba3000)
  get Phys(data[n=2]=81ba4000)
  get Phys(data[n=2]=81ba5000)
  get Phys(data[n=2]=81ba6000)
  get Phys(data[n=2]=81ba7000)
  get Phys(data[n=2]=81ba8000)
  get Phys(data[n=2]=81ba9000)
  get Phys(data[n=2]=81baa000)
  get Phys(data[n=2]=81bab000)
  get Phys(data[n=3]=81bac000)
  get Phys(data[n=4]=81bad000)
  get Phys(data[n=4]=81bae000)
  get Phys(data[n=4]=81baf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2169, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2169 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 21e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 21e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81bb0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81bb0000)
  get Phys(data[n=1]=81bb1000)
  get Phys(data[n=1]=81bb2000)
  get Phys(data[n=1]=81bb3000)
  get Phys(data[n=2]=81bb4000)
  get Phys(data[n=2]=81bb5000)
  get Phys(data[n=2]=81bb6000)
  get Phys(data[n=2]=81bb7000)
  get Phys(data[n=3]=81bb8000)
  get Phys(data[n=3]=81bb9000)
  get Phys(data[n=4]=81bba000)
  get Phys(data[n=4]=81bbb000)
  get Phys(data[n=5]=81bbc000)
  get Phys(data[n=6]=81bbd000)
  get Phys(data[n=7]=81bbe000)
  get Phys(data[n=7]=81bbf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x21e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x21e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2269, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2269, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81bc0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81bc0000)
  get Phys(data[n=1]=81bc1000)
  get Phys(data[n=2]=81bc2000)
  get Phys(data[n=3]=81bc3000)
  get Phys(data[n=3]=81bc4000)
  get Phys(data[n=3]=81bc5000)
  get Phys(data[n=3]=81bc6000)
  get Phys(data[n=4]=81bc7000)
  get Phys(data[n=4]=81bc8000)
  get Phys(data[n=4]=81bc9000)
  get Phys(data[n=4]=81bca000)
  get Phys(data[n=4]=81bcb000)
  get Phys(data[n=4]=81bcc000)
  get Phys(data[n=5]=81bcd000)
  get Phys(data[n=5]=81bce000)
  get Phys(data[n=6]=81bcf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2269, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2269 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 22e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 22e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81bd0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81bd0000)
  get Phys(data[n=1]=81bd1000)
  get Phys(data[n=1]=81bd2000)
  get Phys(data[n=1]=81bd3000)
  get Phys(data[n=1]=81bd4000)
  get Phys(data[n=1]=81bd5000)
  get Phys(data[n=1]=81bd6000)
  get Phys(data[n=2]=81bd7000)
  get Phys(data[n=2]=81bd8000)
  get Phys(data[n=2]=81bd9000)
  get Phys(data[n=2]=81bda000)
  get Phys(data[n=2]=81bdb000)
  get Phys(data[n=2]=81bdc000)
  get Phys(data[n=3]=81bdd000)
  get Phys(data[n=3]=81bde000)
  get Phys(data[n=3]=81bdf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x22e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x22e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2369, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2369, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81be0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81be0000)
  get Phys(data[n=1]=81be1000)
  get Phys(data[n=1]=81be2000)
  get Phys(data[n=2]=81be3000)
  get Phys(data[n=2]=81be4000)
  get Phys(data[n=2]=81be5000)
  get Phys(data[n=2]=81be6000)
  get Phys(data[n=2]=81be7000)
  get Phys(data[n=2]=81be8000)
  get Phys(data[n=2]=81be9000)
  get Phys(data[n=2]=81bea000)
  get Phys(data[n=2]=81beb000)
  get Phys(data[n=3]=81bec000)
  get Phys(data[n=4]=81bed000)
  get Phys(data[n=4]=81bee000)
  get Phys(data[n=4]=81bef000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2369, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2369 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 23e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 23e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81bf0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81bf0000)
  get Phys(data[n=1]=81bf1000)
  get Phys(data[n=1]=81bf2000)
  get Phys(data[n=1]=81bf3000)
  get Phys(data[n=2]=81bf4000)
  get Phys(data[n=2]=81bf5000)
  get Phys(data[n=2]=81bf6000)
  get Phys(data[n=2]=81bf7000)
  get Phys(data[n=3]=81bf8000)
  get Phys(data[n=3]=81bf9000)
  get Phys(data[n=4]=81bfa000)
  get Phys(data[n=4]=81bfb000)
  get Phys(data[n=5]=81bfc000)
  get Phys(data[n=6]=81bfd000)
  get Phys(data[n=7]=81bfe000)
  get Phys(data[n=7]=81bff000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x23e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x23e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2469, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2469, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81c00000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81c00000)
  get Phys(data[n=1]=81c01000)
  get Phys(data[n=2]=81c02000)
  get Phys(data[n=2]=81c03000)
  get Phys(data[n=2]=81c04000)
  get Phys(data[n=2]=81c05000)
  get Phys(data[n=3]=81c06000)
  get Phys(data[n=3]=81c07000)
  get Phys(data[n=3]=81c08000)
  get Phys(data[n=3]=81c09000)
  get Phys(data[n=3]=81c0a000)
  get Phys(data[n=3]=81c0b000)
  get Phys(data[n=4]=81c0c000)
  get Phys(data[n=4]=81c0d000)
  get Phys(data[n=5]=81c0e000)
  get Phys(data[n=5]=81c0f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2469, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2469 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 24e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 24e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81c10000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81c10000)
  get Phys(data[n=1]=81c11000)
  get Phys(data[n=1]=81c12000)
  get Phys(data[n=1]=81c13000)
  get Phys(data[n=1]=81c14000)
  get Phys(data[n=1]=81c15000)
  get Phys(data[n=2]=81c16000)
  get Phys(data[n=2]=81c17000)
  get Phys(data[n=2]=81c18000)
  get Phys(data[n=2]=81c19000)
  get Phys(data[n=2]=81c1a000)
  get Phys(data[n=2]=81c1b000)
  get Phys(data[n=3]=81c1c000)
  get Phys(data[n=3]=81c1d000)
  get Phys(data[n=3]=81c1e000)
  get Phys(data[n=3]=81c1f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x24e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x24e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2569, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2569, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81c20000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81c20000)
  get Phys(data[n=1]=81c21000)
  get Phys(data[n=2]=81c22000)
  get Phys(data[n=2]=81c23000)
  get Phys(data[n=2]=81c24000)
  get Phys(data[n=2]=81c25000)
  get Phys(data[n=2]=81c26000)
  get Phys(data[n=2]=81c27000)
  get Phys(data[n=2]=81c28000)
  get Phys(data[n=2]=81c29000)
  get Phys(data[n=2]=81c2a000)
  get Phys(data[n=3]=81c2b000)
  get Phys(data[n=4]=81c2c000)
  get Phys(data[n=4]=81c2d000)
  get Phys(data[n=4]=81c2e000)
  get Phys(data[n=4]=81c2f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2569, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2569 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 25e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 25e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81c30000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81c30000)
  get Phys(data[n=1]=81c31000)
  get Phys(data[n=1]=81c32000)
  get Phys(data[n=2]=81c33000)
  get Phys(data[n=2]=81c34000)
  get Phys(data[n=2]=81c35000)
  get Phys(data[n=2]=81c36000)
  get Phys(data[n=3]=81c37000)
  get Phys(data[n=3]=81c38000)
  get Phys(data[n=4]=81c39000)
  get Phys(data[n=4]=81c3a000)
  get Phys(data[n=5]=81c3b000)
  get Phys(data[n=6]=81c3c000)
  get Phys(data[n=7]=81c3d000)
  get Phys(data[n=7]=81c3e000)
  get Phys(data[n=7]=81c3f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x25e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x25e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2669, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2669, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81c40000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81c40000)
  get Phys(data[n=1]=81c41000)
  get Phys(data[n=2]=81c42000)
  get Phys(data[n=2]=81c43000)
  get Phys(data[n=2]=81c44000)
  get Phys(data[n=2]=81c45000)
  get Phys(data[n=3]=81c46000)
  get Phys(data[n=3]=81c47000)
  get Phys(data[n=3]=81c48000)
  get Phys(data[n=3]=81c49000)
  get Phys(data[n=3]=81c4a000)
  get Phys(data[n=3]=81c4b000)
  get Phys(data[n=4]=81c4c000)
  get Phys(data[n=4]=81c4d000)
  get Phys(data[n=5]=81c4e000)
  get Phys(data[n=5]=81c4f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2669, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2669 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 26e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 26e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81c50000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81c50000)
  get Phys(data[n=1]=81c51000)
  get Phys(data[n=1]=81c52000)
  get Phys(data[n=1]=81c53000)
  get Phys(data[n=1]=81c54000)
  get Phys(data[n=1]=81c55000)
  get Phys(data[n=2]=81c56000)
  get Phys(data[n=2]=81c57000)
  get Phys(data[n=2]=81c58000)
  get Phys(data[n=2]=81c59000)
  get Phys(data[n=2]=81c5a000)
  get Phys(data[n=2]=81c5b000)
  get Phys(data[n=3]=81c5c000)
  get Phys(data[n=3]=81c5d000)
  get Phys(data[n=3]=81c5e000)
  get Phys(data[n=3]=81c5f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x26e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x26e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2769, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2769, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81c60000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81c60000)
  get Phys(data[n=1]=81c61000)
  get Phys(data[n=2]=81c62000)
  get Phys(data[n=2]=81c63000)
  get Phys(data[n=2]=81c64000)
  get Phys(data[n=2]=81c65000)
  get Phys(data[n=2]=81c66000)
  get Phys(data[n=2]=81c67000)
  get Phys(data[n=2]=81c68000)
  get Phys(data[n=2]=81c69000)
  get Phys(data[n=2]=81c6a000)
  get Phys(data[n=3]=81c6b000)
  get Phys(data[n=4]=81c6c000)
  get Phys(data[n=4]=81c6d000)
  get Phys(data[n=4]=81c6e000)
  get Phys(data[n=4]=81c6f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2769, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2769 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 27e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 27e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81c70000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81c70000)
  get Phys(data[n=1]=81c71000)
  get Phys(data[n=1]=81c72000)
  get Phys(data[n=2]=81c73000)
  get Phys(data[n=2]=81c74000)
  get Phys(data[n=2]=81c75000)
  get Phys(data[n=2]=81c76000)
  get Phys(data[n=3]=81c77000)
  get Phys(data[n=3]=81c78000)
  get Phys(data[n=4]=81c79000)
  get Phys(data[n=4]=81c7a000)
  get Phys(data[n=5]=81c7b000)
  get Phys(data[n=6]=81c7c000)
  get Phys(data[n=7]=81c7d000)
  get Phys(data[n=7]=81c7e000)
  get Phys(data[n=7]=81c7f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x27e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x27e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2869, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2869, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81c80000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81c80000)
  get Phys(data[n=1]=81c81000)
  get Phys(data[n=2]=81c82000)
  get Phys(data[n=2]=81c83000)
  get Phys(data[n=2]=81c84000)
  get Phys(data[n=2]=81c85000)
  get Phys(data[n=3]=81c86000)
  get Phys(data[n=3]=81c87000)
  get Phys(data[n=3]=81c88000)
  get Phys(data[n=3]=81c89000)
  get Phys(data[n=3]=81c8a000)
  get Phys(data[n=3]=81c8b000)
  get Phys(data[n=4]=81c8c000)
  get Phys(data[n=4]=81c8d000)
  get Phys(data[n=5]=81c8e000)
  get Phys(data[n=5]=81c8f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2869, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2869 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 28e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 28e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81c90000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81c90000)
  get Phys(data[n=1]=81c91000)
  get Phys(data[n=1]=81c92000)
  get Phys(data[n=1]=81c93000)
  get Phys(data[n=1]=81c94000)
  get Phys(data[n=1]=81c95000)
  get Phys(data[n=2]=81c96000)
  get Phys(data[n=2]=81c97000)
  get Phys(data[n=2]=81c98000)
  get Phys(data[n=2]=81c99000)
  get Phys(data[n=2]=81c9a000)
  get Phys(data[n=2]=81c9b000)
  get Phys(data[n=3]=81c9c000)
  get Phys(data[n=3]=81c9d000)
  get Phys(data[n=3]=81c9e000)
  get Phys(data[n=3]=81c9f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x28e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x28e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2969, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2969, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81ca0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81ca0000)
  get Phys(data[n=1]=81ca1000)
  get Phys(data[n=2]=81ca2000)
  get Phys(data[n=2]=81ca3000)
  get Phys(data[n=2]=81ca4000)
  get Phys(data[n=2]=81ca5000)
  get Phys(data[n=2]=81ca6000)
  get Phys(data[n=2]=81ca7000)
  get Phys(data[n=2]=81ca8000)
  get Phys(data[n=2]=81ca9000)
  get Phys(data[n=2]=81caa000)
  get Phys(data[n=3]=81cab000)
  get Phys(data[n=4]=81cac000)
  get Phys(data[n=4]=81cad000)
  get Phys(data[n=4]=81cae000)
  get Phys(data[n=4]=81caf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2969, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2969 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 29e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 29e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81cb0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81cb0000)
  get Phys(data[n=1]=81cb1000)
  get Phys(data[n=1]=81cb2000)
  get Phys(data[n=2]=81cb3000)
  get Phys(data[n=2]=81cb4000)
  get Phys(data[n=2]=81cb5000)
  get Phys(data[n=2]=81cb6000)
  get Phys(data[n=3]=81cb7000)
  get Phys(data[n=3]=81cb8000)
  get Phys(data[n=4]=81cb9000)
  get Phys(data[n=4]=81cba000)
  get Phys(data[n=5]=81cbb000)
  get Phys(data[n=6]=81cbc000)
  get Phys(data[n=7]=81cbd000)
  get Phys(data[n=7]=81cbe000)
  get Phys(data[n=7]=81cbf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x29e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x29e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2a69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2a69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81cc0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81cc0000)
  get Phys(data[n=1]=81cc1000)
  get Phys(data[n=2]=81cc2000)
  get Phys(data[n=2]=81cc3000)
  get Phys(data[n=2]=81cc4000)
  get Phys(data[n=2]=81cc5000)
  get Phys(data[n=3]=81cc6000)
  get Phys(data[n=3]=81cc7000)
  get Phys(data[n=3]=81cc8000)
  get Phys(data[n=3]=81cc9000)
  get Phys(data[n=3]=81cca000)
  get Phys(data[n=3]=81ccb000)
  get Phys(data[n=4]=81ccc000)
  get Phys(data[n=4]=81ccd000)
  get Phys(data[n=5]=81cce000)
  get Phys(data[n=5]=81ccf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2a69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2a69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2ae9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2ae9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81cd0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81cd0000)
  get Phys(data[n=1]=81cd1000)
  get Phys(data[n=1]=81cd2000)
  get Phys(data[n=1]=81cd3000)
  get Phys(data[n=1]=81cd4000)
  get Phys(data[n=1]=81cd5000)
  get Phys(data[n=2]=81cd6000)
  get Phys(data[n=2]=81cd7000)
  get Phys(data[n=2]=81cd8000)
  get Phys(data[n=2]=81cd9000)
  get Phys(data[n=2]=81cda000)
  get Phys(data[n=2]=81cdb000)
  get Phys(data[n=3]=81cdc000)
  get Phys(data[n=3]=81cdd000)
  get Phys(data[n=3]=81cde000)
  get Phys(data[n=3]=81cdf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2ae9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2ae9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2b69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2b69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81ce0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81ce0000)
  get Phys(data[n=1]=81ce1000)
  get Phys(data[n=2]=81ce2000)
  get Phys(data[n=2]=81ce3000)
  get Phys(data[n=2]=81ce4000)
  get Phys(data[n=2]=81ce5000)
  get Phys(data[n=2]=81ce6000)
  get Phys(data[n=2]=81ce7000)
  get Phys(data[n=2]=81ce8000)
  get Phys(data[n=2]=81ce9000)
  get Phys(data[n=2]=81cea000)
  get Phys(data[n=3]=81ceb000)
  get Phys(data[n=4]=81cec000)
  get Phys(data[n=4]=81ced000)
  get Phys(data[n=4]=81cee000)
  get Phys(data[n=4]=81cef000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2b69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2b69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2be9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2be9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81cf0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81cf0000)
  get Phys(data[n=1]=81cf1000)
  get Phys(data[n=1]=81cf2000)
  get Phys(data[n=2]=81cf3000)
  get Phys(data[n=2]=81cf4000)
  get Phys(data[n=2]=81cf5000)
  get Phys(data[n=2]=81cf6000)
  get Phys(data[n=3]=81cf7000)
  get Phys(data[n=3]=81cf8000)
  get Phys(data[n=4]=81cf9000)
  get Phys(data[n=4]=81cfa000)
  get Phys(data[n=5]=81cfb000)
  get Phys(data[n=6]=81cfc000)
  get Phys(data[n=7]=81cfd000)
  get Phys(data[n=7]=81cfe000)
  get Phys(data[n=7]=81cff000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2be9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2be9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2c69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2c69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81d00000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81d00000)
  get Phys(data[n=1]=81d01000)
  get Phys(data[n=2]=81d02000)
  get Phys(data[n=2]=81d03000)
  get Phys(data[n=2]=81d04000)
  get Phys(data[n=2]=81d05000)
  get Phys(data[n=3]=81d06000)
  get Phys(data[n=3]=81d07000)
  get Phys(data[n=3]=81d08000)
  get Phys(data[n=3]=81d09000)
  get Phys(data[n=3]=81d0a000)
  get Phys(data[n=3]=81d0b000)
  get Phys(data[n=4]=81d0c000)
  get Phys(data[n=4]=81d0d000)
  get Phys(data[n=5]=81d0e000)
  get Phys(data[n=5]=81d0f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2c69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2c69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2ce9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2ce9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81d10000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81d10000)
  get Phys(data[n=1]=81d11000)
  get Phys(data[n=1]=81d12000)
  get Phys(data[n=1]=81d13000)
  get Phys(data[n=1]=81d14000)
  get Phys(data[n=1]=81d15000)
  get Phys(data[n=2]=81d16000)
  get Phys(data[n=2]=81d17000)
  get Phys(data[n=2]=81d18000)
  get Phys(data[n=2]=81d19000)
  get Phys(data[n=2]=81d1a000)
  get Phys(data[n=2]=81d1b000)
  get Phys(data[n=3]=81d1c000)
  get Phys(data[n=3]=81d1d000)
  get Phys(data[n=3]=81d1e000)
  get Phys(data[n=3]=81d1f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2ce9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2ce9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2d69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2d69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81d20000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81d20000)
  get Phys(data[n=1]=81d21000)
  get Phys(data[n=2]=81d22000)
  get Phys(data[n=2]=81d23000)
  get Phys(data[n=2]=81d24000)
  get Phys(data[n=2]=81d25000)
  get Phys(data[n=2]=81d26000)
  get Phys(data[n=2]=81d27000)
  get Phys(data[n=2]=81d28000)
  get Phys(data[n=2]=81d29000)
  get Phys(data[n=2]=81d2a000)
  get Phys(data[n=3]=81d2b000)
  get Phys(data[n=4]=81d2c000)
  get Phys(data[n=4]=81d2d000)
  get Phys(data[n=4]=81d2e000)
  get Phys(data[n=4]=81d2f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2d69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2d69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2de9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2de9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81d30000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81d30000)
  get Phys(data[n=1]=81d31000)
  get Phys(data[n=1]=81d32000)
  get Phys(data[n=2]=81d33000)
  get Phys(data[n=2]=81d34000)
  get Phys(data[n=2]=81d35000)
  get Phys(data[n=2]=81d36000)
  get Phys(data[n=3]=81d37000)
  get Phys(data[n=3]=81d38000)
  get Phys(data[n=4]=81d39000)
  get Phys(data[n=4]=81d3a000)
  get Phys(data[n=5]=81d3b000)
  get Phys(data[n=6]=81d3c000)
  get Phys(data[n=7]=81d3d000)
  get Phys(data[n=7]=81d3e000)
  get Phys(data[n=7]=81d3f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2de9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2de9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2e69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2e69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81d40000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81d40000)
  get Phys(data[n=1]=81d41000)
  get Phys(data[n=2]=81d42000)
  get Phys(data[n=2]=81d43000)
  get Phys(data[n=2]=81d44000)
  get Phys(data[n=2]=81d45000)
  get Phys(data[n=3]=81d46000)
  get Phys(data[n=3]=81d47000)
  get Phys(data[n=3]=81d48000)
  get Phys(data[n=3]=81d49000)
  get Phys(data[n=3]=81d4a000)
  get Phys(data[n=3]=81d4b000)
  get Phys(data[n=4]=81d4c000)
  get Phys(data[n=4]=81d4d000)
  get Phys(data[n=5]=81d4e000)
  get Phys(data[n=5]=81d4f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2e69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2e69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2ee9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2ee9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81d50000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81d50000)
  get Phys(data[n=1]=81d51000)
  get Phys(data[n=1]=81d52000)
  get Phys(data[n=1]=81d53000)
  get Phys(data[n=1]=81d54000)
  get Phys(data[n=1]=81d55000)
  get Phys(data[n=2]=81d56000)
  get Phys(data[n=2]=81d57000)
  get Phys(data[n=2]=81d58000)
  get Phys(data[n=2]=81d59000)
  get Phys(data[n=2]=81d5a000)
  get Phys(data[n=2]=81d5b000)
  get Phys(data[n=3]=81d5c000)
  get Phys(data[n=3]=81d5d000)
  get Phys(data[n=3]=81d5e000)
  get Phys(data[n=3]=81d5f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2ee9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2ee9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2f69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2f69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81d60000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81d60000)
  get Phys(data[n=1]=81d61000)
  get Phys(data[n=2]=81d62000)
  get Phys(data[n=2]=81d63000)
  get Phys(data[n=2]=81d64000)
  get Phys(data[n=2]=81d65000)
  get Phys(data[n=2]=81d66000)
  get Phys(data[n=2]=81d67000)
  get Phys(data[n=2]=81d68000)
  get Phys(data[n=2]=81d69000)
  get Phys(data[n=2]=81d6a000)
  get Phys(data[n=3]=81d6b000)
  get Phys(data[n=4]=81d6c000)
  get Phys(data[n=4]=81d6d000)
  get Phys(data[n=4]=81d6e000)
  get Phys(data[n=4]=81d6f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2f69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2f69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2fe9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2fe9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81d70000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81d70000)
  get Phys(data[n=1]=81d71000)
  get Phys(data[n=1]=81d72000)
  get Phys(data[n=2]=81d73000)
  get Phys(data[n=2]=81d74000)
  get Phys(data[n=2]=81d75000)
  get Phys(data[n=2]=81d76000)
  get Phys(data[n=3]=81d77000)
  get Phys(data[n=3]=81d78000)
  get Phys(data[n=4]=81d79000)
  get Phys(data[n=4]=81d7a000)
  get Phys(data[n=5]=81d7b000)
  get Phys(data[n=6]=81d7c000)
  get Phys(data[n=7]=81d7d000)
  get Phys(data[n=7]=81d7e000)
  get Phys(data[n=7]=81d7f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2fe9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x2fe9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3069, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3069, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81d80000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81d80000)
  get Phys(data[n=1]=81d81000)
  get Phys(data[n=2]=81d82000)
  get Phys(data[n=2]=81d83000)
  get Phys(data[n=2]=81d84000)
  get Phys(data[n=2]=81d85000)
  get Phys(data[n=3]=81d86000)
  get Phys(data[n=3]=81d87000)
  get Phys(data[n=3]=81d88000)
  get Phys(data[n=3]=81d89000)
  get Phys(data[n=3]=81d8a000)
  get Phys(data[n=3]=81d8b000)
  get Phys(data[n=4]=81d8c000)
  get Phys(data[n=4]=81d8d000)
  get Phys(data[n=5]=81d8e000)
  get Phys(data[n=5]=81d8f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3069, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3069 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 30e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 30e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81d90000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81d90000)
  get Phys(data[n=1]=81d91000)
  get Phys(data[n=1]=81d92000)
  get Phys(data[n=1]=81d93000)
  get Phys(data[n=1]=81d94000)
  get Phys(data[n=1]=81d95000)
  get Phys(data[n=2]=81d96000)
  get Phys(data[n=2]=81d97000)
  get Phys(data[n=2]=81d98000)
  get Phys(data[n=2]=81d99000)
  get Phys(data[n=2]=81d9a000)
  get Phys(data[n=2]=81d9b000)
  get Phys(data[n=3]=81d9c000)
  get Phys(data[n=3]=81d9d000)
  get Phys(data[n=3]=81d9e000)
  get Phys(data[n=3]=81d9f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x30e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x30e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3169, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3169, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81da0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81da0000)
  get Phys(data[n=1]=81da1000)
  get Phys(data[n=2]=81da2000)
  get Phys(data[n=2]=81da3000)
  get Phys(data[n=2]=81da4000)
  get Phys(data[n=2]=81da5000)
  get Phys(data[n=2]=81da6000)
  get Phys(data[n=2]=81da7000)
  get Phys(data[n=2]=81da8000)
  get Phys(data[n=2]=81da9000)
  get Phys(data[n=2]=81daa000)
  get Phys(data[n=3]=81dab000)
  get Phys(data[n=4]=81dac000)
  get Phys(data[n=4]=81dad000)
  get Phys(data[n=4]=81dae000)
  get Phys(data[n=4]=81daf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3169, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3169 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 31e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 31e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81db0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81db0000)
  get Phys(data[n=1]=81db1000)
  get Phys(data[n=1]=81db2000)
  get Phys(data[n=2]=81db3000)
  get Phys(data[n=2]=81db4000)
  get Phys(data[n=2]=81db5000)
  get Phys(data[n=2]=81db6000)
  get Phys(data[n=3]=81db7000)
  get Phys(data[n=3]=81db8000)
  get Phys(data[n=4]=81db9000)
  get Phys(data[n=4]=81dba000)
  get Phys(data[n=5]=81dbb000)
  get Phys(data[n=6]=81dbc000)
  get Phys(data[n=7]=81dbd000)
  get Phys(data[n=7]=81dbe000)
  get Phys(data[n=7]=81dbf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x31e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x31e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3269, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3269, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81dc0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81dc0000)
  get Phys(data[n=1]=81dc1000)
  get Phys(data[n=2]=81dc2000)
  get Phys(data[n=2]=81dc3000)
  get Phys(data[n=2]=81dc4000)
  get Phys(data[n=2]=81dc5000)
  get Phys(data[n=3]=81dc6000)
  get Phys(data[n=3]=81dc7000)
  get Phys(data[n=3]=81dc8000)
  get Phys(data[n=3]=81dc9000)
  get Phys(data[n=3]=81dca000)
  get Phys(data[n=3]=81dcb000)
  get Phys(data[n=4]=81dcc000)
  get Phys(data[n=4]=81dcd000)
  get Phys(data[n=5]=81dce000)
  get Phys(data[n=5]=81dcf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3269, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3269 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 32e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 32e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81dd0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81dd0000)
  get Phys(data[n=1]=81dd1000)
  get Phys(data[n=1]=81dd2000)
  get Phys(data[n=1]=81dd3000)
  get Phys(data[n=1]=81dd4000)
  get Phys(data[n=1]=81dd5000)
  get Phys(data[n=2]=81dd6000)
  get Phys(data[n=2]=81dd7000)
  get Phys(data[n=2]=81dd8000)
  get Phys(data[n=2]=81dd9000)
  get Phys(data[n=2]=81dda000)
  get Phys(data[n=2]=81ddb000)
  get Phys(data[n=3]=81ddc000)
  get Phys(data[n=3]=81ddd000)
  get Phys(data[n=3]=81dde000)
  get Phys(data[n=3]=81ddf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x32e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x32e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3369, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3369, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81de0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81de0000)
  get Phys(data[n=1]=81de1000)
  get Phys(data[n=2]=81de2000)
  get Phys(data[n=2]=81de3000)
  get Phys(data[n=2]=81de4000)
  get Phys(data[n=2]=81de5000)
  get Phys(data[n=2]=81de6000)
  get Phys(data[n=2]=81de7000)
  get Phys(data[n=2]=81de8000)
  get Phys(data[n=2]=81de9000)
  get Phys(data[n=2]=81dea000)
  get Phys(data[n=3]=81deb000)
  get Phys(data[n=4]=81dec000)
  get Phys(data[n=4]=81ded000)
  get Phys(data[n=4]=81dee000)
  get Phys(data[n=4]=81def000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3369, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3369 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 33e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 33e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81df0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81df0000)
  get Phys(data[n=1]=81df1000)
  get Phys(data[n=1]=81df2000)
  get Phys(data[n=2]=81df3000)
  get Phys(data[n=2]=81df4000)
  get Phys(data[n=2]=81df5000)
  get Phys(data[n=2]=81df6000)
  get Phys(data[n=3]=81df7000)
  get Phys(data[n=3]=81df8000)
  get Phys(data[n=4]=81df9000)
  get Phys(data[n=4]=81dfa000)
  get Phys(data[n=5]=81dfb000)
  get Phys(data[n=6]=81dfc000)
  get Phys(data[n=7]=81dfd000)
  get Phys(data[n=7]=81dfe000)
  get Phys(data[n=7]=81dff000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x33e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x33e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3469, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3469, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81e00000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81e00000)
  get Phys(data[n=1]=81e01000)
  get Phys(data[n=2]=81e02000)
  get Phys(data[n=2]=81e03000)
  get Phys(data[n=2]=81e04000)
  get Phys(data[n=2]=81e05000)
  get Phys(data[n=3]=81e06000)
  get Phys(data[n=3]=81e07000)
  get Phys(data[n=3]=81e08000)
  get Phys(data[n=3]=81e09000)
  get Phys(data[n=3]=81e0a000)
  get Phys(data[n=3]=81e0b000)
  get Phys(data[n=4]=81e0c000)
  get Phys(data[n=4]=81e0d000)
  get Phys(data[n=5]=81e0e000)
  get Phys(data[n=5]=81e0f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3469, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3469 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 34e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 34e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81e10000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81e10000)
  get Phys(data[n=1]=81e11000)
  get Phys(data[n=1]=81e12000)
  get Phys(data[n=1]=81e13000)
  get Phys(data[n=1]=81e14000)
  get Phys(data[n=1]=81e15000)
  get Phys(data[n=2]=81e16000)
  get Phys(data[n=2]=81e17000)
  get Phys(data[n=2]=81e18000)
  get Phys(data[n=2]=81e19000)
  get Phys(data[n=2]=81e1a000)
  get Phys(data[n=2]=81e1b000)
  get Phys(data[n=3]=81e1c000)
  get Phys(data[n=3]=81e1d000)
  get Phys(data[n=3]=81e1e000)
  get Phys(data[n=3]=81e1f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x34e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x34e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3569, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3569, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81e20000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81e20000)
  get Phys(data[n=1]=81e21000)
  get Phys(data[n=2]=81e22000)
  get Phys(data[n=2]=81e23000)
  get Phys(data[n=2]=81e24000)
  get Phys(data[n=2]=81e25000)
  get Phys(data[n=2]=81e26000)
  get Phys(data[n=2]=81e27000)
  get Phys(data[n=2]=81e28000)
  get Phys(data[n=2]=81e29000)
  get Phys(data[n=2]=81e2a000)
  get Phys(data[n=3]=81e2b000)
  get Phys(data[n=4]=81e2c000)
  get Phys(data[n=4]=81e2d000)
  get Phys(data[n=4]=81e2e000)
  get Phys(data[n=4]=81e2f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3569, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3569 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 35e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 35e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81e30000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81e30000)
  get Phys(data[n=1]=81e31000)
  get Phys(data[n=1]=81e32000)
  get Phys(data[n=2]=81e33000)
  get Phys(data[n=2]=81e34000)
  get Phys(data[n=2]=81e35000)
  get Phys(data[n=2]=81e36000)
  get Phys(data[n=3]=81e37000)
  get Phys(data[n=3]=81e38000)
  get Phys(data[n=4]=81e39000)
  get Phys(data[n=4]=81e3a000)
  get Phys(data[n=5]=81e3b000)
  get Phys(data[n=6]=81e3c000)
  get Phys(data[n=7]=81e3d000)
  get Phys(data[n=7]=81e3e000)
  get Phys(data[n=7]=81e3f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x35e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x35e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3669, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3669, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81e40000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81e40000)
  get Phys(data[n=1]=81e41000)
  get Phys(data[n=2]=81e42000)
  get Phys(data[n=2]=81e43000)
  get Phys(data[n=2]=81e44000)
  get Phys(data[n=2]=81e45000)
  get Phys(data[n=3]=81e46000)
  get Phys(data[n=3]=81e47000)
  get Phys(data[n=3]=81e48000)
  get Phys(data[n=3]=81e49000)
  get Phys(data[n=3]=81e4a000)
  get Phys(data[n=3]=81e4b000)
  get Phys(data[n=4]=81e4c000)
  get Phys(data[n=4]=81e4d000)
  get Phys(data[n=5]=81e4e000)
  get Phys(data[n=5]=81e4f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3669, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3669 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 36e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 36e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81e50000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81e50000)
  get Phys(data[n=1]=81e51000)
  get Phys(data[n=1]=81e52000)
  get Phys(data[n=1]=81e53000)
  get Phys(data[n=1]=81e54000)
  get Phys(data[n=1]=81e55000)
  get Phys(data[n=2]=81e56000)
  get Phys(data[n=2]=81e57000)
  get Phys(data[n=2]=81e58000)
  get Phys(data[n=2]=81e59000)
  get Phys(data[n=2]=81e5a000)
  get Phys(data[n=2]=81e5b000)
  get Phys(data[n=3]=81e5c000)
  get Phys(data[n=3]=81e5d000)
  get Phys(data[n=3]=81e5e000)
  get Phys(data[n=3]=81e5f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x36e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x36e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3769, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3769, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81e60000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81e60000)
  get Phys(data[n=1]=81e61000)
  get Phys(data[n=2]=81e62000)
  get Phys(data[n=2]=81e63000)
  get Phys(data[n=2]=81e64000)
  get Phys(data[n=2]=81e65000)
  get Phys(data[n=2]=81e66000)
  get Phys(data[n=2]=81e67000)
  get Phys(data[n=2]=81e68000)
  get Phys(data[n=2]=81e69000)
  get Phys(data[n=2]=81e6a000)
  get Phys(data[n=3]=81e6b000)
  get Phys(data[n=4]=81e6c000)
  get Phys(data[n=4]=81e6d000)
  get Phys(data[n=4]=81e6e000)
  get Phys(data[n=4]=81e6f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3769, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3769 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 37e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 37e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81e70000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81e70000)
  get Phys(data[n=1]=81e71000)
  get Phys(data[n=1]=81e72000)
  get Phys(data[n=2]=81e73000)
  get Phys(data[n=2]=81e74000)
  get Phys(data[n=2]=81e75000)
  get Phys(data[n=2]=81e76000)
  get Phys(data[n=3]=81e77000)
  get Phys(data[n=3]=81e78000)
  get Phys(data[n=4]=81e79000)
  get Phys(data[n=4]=81e7a000)
  get Phys(data[n=5]=81e7b000)
  get Phys(data[n=6]=81e7c000)
  get Phys(data[n=7]=81e7d000)
  get Phys(data[n=7]=81e7e000)
  get Phys(data[n=7]=81e7f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x37e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x37e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3869, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3869, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81e80000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81e80000)
  get Phys(data[n=1]=81e81000)
  get Phys(data[n=2]=81e82000)
  get Phys(data[n=2]=81e83000)
  get Phys(data[n=2]=81e84000)
  get Phys(data[n=2]=81e85000)
  get Phys(data[n=3]=81e86000)
  get Phys(data[n=3]=81e87000)
  get Phys(data[n=3]=81e88000)
  get Phys(data[n=3]=81e89000)
  get Phys(data[n=3]=81e8a000)
  get Phys(data[n=3]=81e8b000)
  get Phys(data[n=4]=81e8c000)
  get Phys(data[n=4]=81e8d000)
  get Phys(data[n=5]=81e8e000)
  get Phys(data[n=5]=81e8f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3869, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3869 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 38e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81e90000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81e90000)
  get Phys(data[n=1]=81e91000)
  get Phys(data[n=1]=81e92000)
  get Phys(data[n=1]=81e93000)
  get Phys(data[n=1]=81e94000)
  get Phys(data[n=1]=81e95000)
  get Phys(data[n=2]=81e96000)
  get Phys(data[n=2]=81e97000)
  get Phys(data[n=2]=81e98000)
  get Phys(data[n=2]=81e99000)
  get Phys(data[n=2]=81e9a000)
  get Phys(data[n=2]=81e9b000)
  get Phys(data[n=3]=81e9c000)
  get Phys(data[n=3]=81e9d000)
  get Phys(data[n=3]=81e9e000)
  get Phys(data[n=3]=81e9f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x38e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3969, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3969, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81ea0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81ea0000)
  get Phys(data[n=1]=81ea1000)
  get Phys(data[n=2]=81ea2000)
  get Phys(data[n=2]=81ea3000)
  get Phys(data[n=2]=81ea4000)
  get Phys(data[n=2]=81ea5000)
  get Phys(data[n=2]=81ea6000)
  get Phys(data[n=2]=81ea7000)
  get Phys(data[n=2]=81ea8000)
  get Phys(data[n=2]=81ea9000)
  get Phys(data[n=2]=81eaa000)
  get Phys(data[n=3]=81eab000)
  get Phys(data[n=4]=81eac000)
  get Phys(data[n=4]=81ead000)
  get Phys(data[n=4]=81eae000)
  get Phys(data[n=4]=81eaf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3969, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3969 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 39e9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 39e9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81eb0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81eb0000)
  get Phys(data[n=1]=81eb1000)
  get Phys(data[n=1]=81eb2000)
  get Phys(data[n=2]=81eb3000)
  get Phys(data[n=2]=81eb4000)
  get Phys(data[n=2]=81eb5000)
  get Phys(data[n=2]=81eb6000)
  get Phys(data[n=3]=81eb7000)
  get Phys(data[n=3]=81eb8000)
  get Phys(data[n=4]=81eb9000)
  get Phys(data[n=4]=81eba000)
  get Phys(data[n=5]=81ebb000)
  get Phys(data[n=6]=81ebc000)
  get Phys(data[n=7]=81ebd000)
  get Phys(data[n=7]=81ebe000)
  get Phys(data[n=7]=81ebf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x39e9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x39e9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3a69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3a69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81ec0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81ec0000)
  get Phys(data[n=1]=81ec1000)
  get Phys(data[n=2]=81ec2000)
  get Phys(data[n=2]=81ec3000)
  get Phys(data[n=2]=81ec4000)
  get Phys(data[n=2]=81ec5000)
  get Phys(data[n=3]=81ec6000)
  get Phys(data[n=3]=81ec7000)
  get Phys(data[n=3]=81ec8000)
  get Phys(data[n=3]=81ec9000)
  get Phys(data[n=3]=81eca000)
  get Phys(data[n=3]=81ecb000)
  get Phys(data[n=4]=81ecc000)
  get Phys(data[n=4]=81ecd000)
  get Phys(data[n=5]=81ece000)
  get Phys(data[n=5]=81ecf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3a69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3a69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ae9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3ae9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81ed0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81ed0000)
  get Phys(data[n=1]=81ed1000)
  get Phys(data[n=1]=81ed2000)
  get Phys(data[n=1]=81ed3000)
  get Phys(data[n=1]=81ed4000)
  get Phys(data[n=1]=81ed5000)
  get Phys(data[n=2]=81ed6000)
  get Phys(data[n=2]=81ed7000)
  get Phys(data[n=2]=81ed8000)
  get Phys(data[n=2]=81ed9000)
  get Phys(data[n=2]=81eda000)
  get Phys(data[n=2]=81edb000)
  get Phys(data[n=3]=81edc000)
  get Phys(data[n=3]=81edd000)
  get Phys(data[n=3]=81ede000)
  get Phys(data[n=3]=81edf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ae9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3ae9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3b69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81ee0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81ee0000)
  get Phys(data[n=1]=81ee1000)
  get Phys(data[n=2]=81ee2000)
  get Phys(data[n=2]=81ee3000)
  get Phys(data[n=2]=81ee4000)
  get Phys(data[n=2]=81ee5000)
  get Phys(data[n=2]=81ee6000)
  get Phys(data[n=2]=81ee7000)
  get Phys(data[n=2]=81ee8000)
  get Phys(data[n=2]=81ee9000)
  get Phys(data[n=2]=81eea000)
  get Phys(data[n=3]=81eeb000)
  get Phys(data[n=4]=81eec000)
  get Phys(data[n=4]=81eed000)
  get Phys(data[n=4]=81eee000)
  get Phys(data[n=4]=81eef000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3b69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3be9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3be9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81ef0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81ef0000)
  get Phys(data[n=1]=81ef1000)
  get Phys(data[n=1]=81ef2000)
  get Phys(data[n=2]=81ef3000)
  get Phys(data[n=2]=81ef4000)
  get Phys(data[n=2]=81ef5000)
  get Phys(data[n=2]=81ef6000)
  get Phys(data[n=3]=81ef7000)
  get Phys(data[n=3]=81ef8000)
  get Phys(data[n=4]=81ef9000)
  get Phys(data[n=4]=81efa000)
  get Phys(data[n=5]=81efb000)
  get Phys(data[n=6]=81efc000)
  get Phys(data[n=7]=81efd000)
  get Phys(data[n=7]=81efe000)
  get Phys(data[n=7]=81eff000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3be9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3be9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3c69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3c69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81f00000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81f00000)
  get Phys(data[n=1]=81f01000)
  get Phys(data[n=2]=81f02000)
  get Phys(data[n=2]=81f03000)
  get Phys(data[n=2]=81f04000)
  get Phys(data[n=2]=81f05000)
  get Phys(data[n=3]=81f06000)
  get Phys(data[n=3]=81f07000)
  get Phys(data[n=3]=81f08000)
  get Phys(data[n=3]=81f09000)
  get Phys(data[n=3]=81f0a000)
  get Phys(data[n=3]=81f0b000)
  get Phys(data[n=4]=81f0c000)
  get Phys(data[n=4]=81f0d000)
  get Phys(data[n=5]=81f0e000)
  get Phys(data[n=5]=81f0f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3c69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3c69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ce9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3ce9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81f10000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81f10000)
  get Phys(data[n=1]=81f11000)
  get Phys(data[n=1]=81f12000)
  get Phys(data[n=1]=81f13000)
  get Phys(data[n=1]=81f14000)
  get Phys(data[n=1]=81f15000)
  get Phys(data[n=2]=81f16000)
  get Phys(data[n=2]=81f17000)
  get Phys(data[n=2]=81f18000)
  get Phys(data[n=2]=81f19000)
  get Phys(data[n=2]=81f1a000)
  get Phys(data[n=2]=81f1b000)
  get Phys(data[n=3]=81f1c000)
  get Phys(data[n=3]=81f1d000)
  get Phys(data[n=3]=81f1e000)
  get Phys(data[n=3]=81f1f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ce9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3ce9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3d69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81f20000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81f20000)
  get Phys(data[n=1]=81f21000)
  get Phys(data[n=2]=81f22000)
  get Phys(data[n=2]=81f23000)
  get Phys(data[n=2]=81f24000)
  get Phys(data[n=2]=81f25000)
  get Phys(data[n=2]=81f26000)
  get Phys(data[n=2]=81f27000)
  get Phys(data[n=2]=81f28000)
  get Phys(data[n=2]=81f29000)
  get Phys(data[n=2]=81f2a000)
  get Phys(data[n=3]=81f2b000)
  get Phys(data[n=4]=81f2c000)
  get Phys(data[n=4]=81f2d000)
  get Phys(data[n=4]=81f2e000)
  get Phys(data[n=4]=81f2f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3d69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3de9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3de9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81f30000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81f30000)
  get Phys(data[n=1]=81f31000)
  get Phys(data[n=1]=81f32000)
  get Phys(data[n=2]=81f33000)
  get Phys(data[n=2]=81f34000)
  get Phys(data[n=2]=81f35000)
  get Phys(data[n=2]=81f36000)
  get Phys(data[n=3]=81f37000)
  get Phys(data[n=3]=81f38000)
  get Phys(data[n=4]=81f39000)
  get Phys(data[n=4]=81f3a000)
  get Phys(data[n=5]=81f3b000)
  get Phys(data[n=6]=81f3c000)
  get Phys(data[n=7]=81f3d000)
  get Phys(data[n=7]=81f3e000)
  get Phys(data[n=7]=81f3f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3de9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3de9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81f40000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81f40000)
  get Phys(data[n=1]=81f41000)
  get Phys(data[n=2]=81f42000)
  get Phys(data[n=2]=81f43000)
  get Phys(data[n=2]=81f44000)
  get Phys(data[n=2]=81f45000)
  get Phys(data[n=3]=81f46000)
  get Phys(data[n=3]=81f47000)
  get Phys(data[n=3]=81f48000)
  get Phys(data[n=3]=81f49000)
  get Phys(data[n=3]=81f4a000)
  get Phys(data[n=3]=81f4b000)
  get Phys(data[n=4]=81f4c000)
  get Phys(data[n=4]=81f4d000)
  get Phys(data[n=5]=81f4e000)
  get Phys(data[n=5]=81f4f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3e69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ee9, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3ee9, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81f50000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81f50000)
  get Phys(data[n=1]=81f51000)
  get Phys(data[n=1]=81f52000)
  get Phys(data[n=1]=81f53000)
  get Phys(data[n=1]=81f54000)
  get Phys(data[n=1]=81f55000)
  get Phys(data[n=2]=81f56000)
  get Phys(data[n=2]=81f57000)
  get Phys(data[n=2]=81f58000)
  get Phys(data[n=2]=81f59000)
  get Phys(data[n=2]=81f5a000)
  get Phys(data[n=2]=81f5b000)
  get Phys(data[n=3]=81f5c000)
  get Phys(data[n=3]=81f5d000)
  get Phys(data[n=3]=81f5e000)
  get Phys(data[n=3]=81f5f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ee9, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3ee9 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f69, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3f69, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 81f60000, count 10000, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81f60000)
  get Phys(data[n=1]=81f61000)
  get Phys(data[n=2]=81f62000)
  get Phys(data[n=2]=81f63000)
  get Phys(data[n=2]=81f64000)
  get Phys(data[n=2]=81f65000)
  get Phys(data[n=2]=81f66000)
  get Phys(data[n=2]=81f67000)
  get Phys(data[n=2]=81f68000)
  get Phys(data[n=2]=81f69000)
  get Phys(data[n=2]=81f6a000)
  get Phys(data[n=3]=81f6b000)
  get Phys(data[n=4]=81f6c000)
  get Phys(data[n=4]=81f6d000)
  get Phys(data[n=4]=81f6e000)
  get Phys(data[n=4]=81f6f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f69, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3f69 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e5c8d8, CDB 0xb0e5c908, AtaReq 0xb100c000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e5c8d8
TopLevel (3), AtaReq 0xb100c000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87265dc
** Ide: Command AtaReq 0xb100c000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3fe9, OrigWordsRequested 0x6b00, DevSize 0x6b
IdeReadWrite (REQ): Starting sector is 3fe9, Number of WORDS 0x6b00, DevSize 0x6b
AtapiDmaSetup: mode 0x45, data 81f70000, count d600, lCh 0, dev 0
  get Phys(PRD=b100c058)
  get Phys(data[0]=81f70000)
  get Phys(data[n=1]=81f71000)
  get Phys(data[n=1]=81f72000)
  get Phys(data[n=2]=81f73000)
  get Phys(data[n=2]=81f74000)
  get Phys(data[n=2]=81f75000)
  get Phys(data[n=2]=81f76000)
  get Phys(data[n=3]=81f77000)
  get Phys(data[n=3]=81f78000)
  get Phys(data[n=4]=81f79000)
  get Phys(data[n=4]=81f7a000)
  get Phys(data[n=5]=81f7b000)
  get Phys(data[n=6]=81f7c000)
  get Phys(data[n=7]=81f7d000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3fe9, Count 0x6b(0x0)
AtaCommand48: cntrlr 0x0:0x1 dev 0x0, cmd 0xc8, lba 0x3fe9 count 0x6b feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0e5c8d8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x1, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:1, irql 0xc, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered d600, full size d600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e5c8d8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e5c8d8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e08cd8, CDB 0xb0e08d08, AtaReq 0xb1298000, SCmd 0x25
UniataNeedQueueing: TopLevel, qd=0
Send to device 25
TopLevel (2), srb 0xb0e08cd8
TopLevel (3), AtaReq 0xb1298000
Try ATAPI send 25
AtapiSendCommand: req state 0x10, Action 3
AtapiSendCommand: prepare..., ATAPI CMD 25 (Cdb b0e08d08)
  assume IN
AtapiSendCommand: use_dma=0, Cmd 25
AtapiSendCommand: AtapiDmaReinit()
AtapiDmaReinit: !(AtaReq->Flags & REQ_FLAG_DMA_OPERATION), fall to PIO on Device 1
AtapiSendCommand: use_dma=0
AtapiSendCommand: CMD_ACTION_EXEC
AtapiSendCommand: Cdb b0e08d08 Command 0x25 to TargetId 1 lun 0
AtapiSendCommand: Entered with status 0x50
AtapiSendCommand: Entry Status (0x50)
AtapiSendCommand: Poll for int. to send packet. Status (0x50)
AtapiSendCommand: status (0x58)
AtapiSendCommand: ExpectingInterrupt (0x1)
AtapiSendCommand: return SRB_STATUS_PENDING (3)
AtapiStartIo: next Srb b0e08cd8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 3)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x4
  perform generic check
  clear unexpected DMA intr
AtapiDmaDone: dev -1
  getting status...
  ATAPI status 0x58
  base status 0x58
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  dev_type ATAPI
  OldReqState = 42
  continue service interrupt
AtapiInterrupt: ATAPI Entered with status (0x58)
AtapiInterrupt: iReason 2
AtapiInterrupt: ATAPI branch
AtapiInterrupt: iReason 2
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: get R wordCount 0x4
IdeIntr: Read 0x4 words
IdeIntr: PIO Read AtaReq->DataBuffer 0xb0dfa190, srb->DataBuffer 0xb0dfa190
  status re-check 0x50
AtapiInterrupt: all transferred, AtaReq->WordsLeft == 0
AtapiInterrupt: early complete ? status 50
AtapiInterrupt: CompleteRequest, srbstatus 1
AtapiInterrupt: PIO completion
AtapiInterrupt: PIO completion, wait BUSY
IdeIntr: ATAPI Read AtaReq->DataBuffer 0xb0dfa198, srb->DataBuffer 0xb0dfa190, len 0x8
   Transfered 0, full size 8
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e08cd8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e08cd8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x4
  perform generic check
  clear unexpected DMA intr
AtapiDmaDone: dev -1
  getting status...
  ATAPI status 0x50
  base status 0x50
  Unexpected interrupt.
  ATAPI additional check
AtapiCheckInterrupt__: ATAPI int reason 3
AtapiInterrupt(base): Catch unexpected
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e08cd8, CDB 0xb0e08d08, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e08cd8
TopLevel (3), AtaReq 0xb1298000
Try ATAPI send 28
AtapiSendCommand: req state 0x10, Action 3
AtapiSendCommand: prepare..., ATAPI CMD 28 (Cdb b0e08d08)
AtapiDmaSetup: mode 0xc, data f8716000, count 800, lCh 0, dev 1
AtapiDmaSetup: Not DMA mode, assume this is just preparation
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8716000)
  set TERM
AtapiDmaSetup: OK
AtapiSendCommand: use dma
AtapiDmaSetup: already setup, 1 entries
AtapiSendCommand: use dma
AtapiSendCommand: use_dma=1, Cmd 28
  REQ_FLAG_DMA_OPERATION
AtapiSendCommand: AtapiDmaReinit()
AtapiDmaReinit: restore IO mode on Device 1
AtapiDmaInit__: Set (U)DMA on Device 1
AtapiDmaInit: deviceExtension->MaxTransferMode >= ATA_UDMA
AtapiDmaInit: LunExt->LimitedTransferMode 0x45
AtapiDmaInit: LunExt->MaxTransferMode >= ATA_UDMA   =>   0x5
Setup chip a:w:u=4:2:5
AtaSetTransferMode: Set 0x45 on Device 0/1
AtaCommand48: cntrlr 0x0:0x0 dev 0x1, cmd 0xef, lba 0x0 count 0x45 feature 0x3
  Status 0x50
AtapiSendCommand: use_dma=1
  REQ_FLAG_DMA_OPERATION
AtapiSendCommand: CMD_ACTION_EXEC
AtapiSendCommand: Cdb b0e08d08 Command 0x28 to TargetId 1 lun 0
AtapiSendCommand: Entered with status 0x50
AtapiSendCommand: Entry Status (0x50)
AtapiSendCommand: Poll for int. to send packet. Status (0x50)
AtapiSendCommand: status (0x58)
AtapiDmaStart: read on 0x0:0x1
AtapiSendCommand: ExpectingInterrupt (0x1)
AtapiSendCommand: return SRB_STATUS_PENDING (3)
AtapiStartIo: next Srb b0e08cd8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x40
  base status 0x40
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type ATAPI
  OldReqState = 42
AtapiInterrupt: ATAPI Entered with status (0x40)
AtapiInterrupt: iReason 3
AtapiInterrupt: ATAPI branch
AtapiInterrupt: iReason 3
AtapiInterrupt: i-reason=3, status=0x40
AtapiInterrupt: interruptReason = CompleteRequest
AtapiInterrupt: CompleteRequest, was DmaTransfer
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e08cd8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e08cd8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x0
  perform generic check
  getting status...
  ATAPI status 0x40
  base status 0x40
  Unexpected interrupt.
  ATAPI additional check
AtapiCheckInterrupt__: ATAPI int reason 3
AtapiInterrupt(base): set CHECK_INTR_IDLE (2)
AtapiInterrupt(base): exit with status 0x0
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8875020
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4977, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4977, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86d2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=2]=f86d4000)
  get Phys(data[n=2]=f86d5000)
  get Phys(data[n=2]=f86d6000)
  get Phys(data[n=2]=f86d7000)
  get Phys(data[n=3]=f86d8000)
  get Phys(data[n=3]=f86d9000)
  get Phys(data[n=3]=f86da000)
  get Phys(data[n=3]=f86db000)
  get Phys(data[n=3]=f86dc000)
  get Phys(data[n=3]=f86dd000)
  get Phys(data[n=4]=f86de000)
  get Phys(data[n=4]=f86df000)
  get Phys(data[n=5]=f86e0000)
  get Phys(data[n=5]=f86e1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4977, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4977 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8875020
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 49f7, OrigWordsRequested 0x1800, DevSize 0x18
IdeReadWrite (REQ): Starting sector is 49f7, Number of WORDS 0x1800, DevSize 0x18
AtapiDmaSetup: mode 0x45, data f86e2000, count 3000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86e2000)
  get Phys(data[n=1]=f86e3000)
  get Phys(data[n=1]=f86e4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x49f7, Count 0x18(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x49f7 count 0x18 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 3000, full size 3000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf887541c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4977, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 4977, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8710000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8710000)
  get Phys(data[n=1]=f8711000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4977, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4977 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\cdfs.sys at F8706000 with c pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0df8148, CDB 0xb0df8178, AtaReq 0xb1298000, SCmd 0x25
UniataNeedQueueing: TopLevel, qd=0
Send to device 25
TopLevel (2), srb 0xb0df8148
TopLevel (3), AtaReq 0xb1298000
Try ATAPI send 25
AtapiSendCommand: req state 0x10, Action 3
AtapiSendCommand: prepare..., ATAPI CMD 25 (Cdb b0df8178)
  assume IN
AtapiSendCommand: use_dma=0, Cmd 25
AtapiSendCommand: AtapiDmaReinit()
AtapiDmaReinit: !(AtaReq->Flags & REQ_FLAG_DMA_OPERATION), fall to PIO on Device 1
AtapiDmaReinit: set PIO mode on Device 1 (45 -> c)
AtapiDmaInit: deviceExtension->MaxTransferMode >= ATA_UDMA
AtapiDmaInit: LunExt->LimitedTransferMode 0x45
AtapiDmaInit: LunExt->MaxTransferMode >= ATA_UDMA   =>   0xffffffff
Setup chip a:w:u=4:-1:-1
AtaSetTransferMode: Set 0xc on Device 0/1
AtaCommand48: cntrlr 0x0:0x0 dev 0x1, cmd 0xef, lba 0x0 count 0xc feature 0x3
  Status 0x50
AtapiSendCommand: use_dma=0
AtapiSendCommand: CMD_ACTION_EXEC
AtapiSendCommand: Cdb b0df8178 Command 0x25 to TargetId 1 lun 0
AtapiSendCommand: Entered with status 0x50
AtapiSendCommand: Entry Status (0x50)
AtapiSendCommand: Poll for int. to send packet. Status (0x50)
AtapiSendCommand: status (0x58)
AtapiSendCommand: ExpectingInterrupt (0x1)
AtapiSendCommand: return SRB_STATUS_PENDING (3)
AtapiStartIo: next Srb b0df8148
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 3)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x4
  perform generic check
  clear unexpected DMA intr
AtapiDmaDone: dev -1
  getting status...
  ATAPI status 0x58
  base status 0x58
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  dev_type ATAPI
  OldReqState = 42
  continue service interrupt
AtapiInterrupt: ATAPI Entered with status (0x58)
AtapiInterrupt: iReason 2
AtapiInterrupt: ATAPI branch
AtapiInterrupt: iReason 2
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: get R wordCount 0x4
IdeIntr: Read 0x4 words
IdeIntr: PIO Read AtaReq->DataBuffer 0xb0dfa190, srb->DataBuffer 0xb0dfa190
  status re-check 0x50
AtapiInterrupt: all transferred, AtaReq->WordsLeft == 0
AtapiInterrupt: early complete ? status 50
AtapiInterrupt: CompleteRequest, srbstatus 1
AtapiInterrupt: PIO completion
AtapiInterrupt: PIO completion, wait BUSY
IdeIntr: ATAPI Read AtaReq->DataBuffer 0xb0dfa198, srb->DataBuffer 0xb0dfa190, len 0x8
   Transfered 0, full size 8
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0df8148, status 1
AtapiInterrupt: RequestComplete, srb 0xb0df8148
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x4
  perform generic check
  clear unexpected DMA intr
AtapiDmaDone: dev -1
  getting status...
  ATAPI status 0x50
  base status 0x50
  Unexpected interrupt.
  ATAPI additional check
AtapiCheckInterrupt__: ATAPI int reason 3
AtapiInterrupt(base): Catch unexpected
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e08cd8, CDB 0xb0e08d08, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e08cd8
TopLevel (3), AtaReq 0xb1298000
Try ATAPI send 28
AtapiSendCommand: req state 0x10, Action 3
AtapiSendCommand: prepare..., ATAPI CMD 28 (Cdb b0e08d08)
AtapiDmaSetup: mode 0xc, data f8716000, count 800, lCh 0, dev 1
AtapiDmaSetup: Not DMA mode, assume this is just preparation
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8716000)
  set TERM
AtapiDmaSetup: OK
AtapiSendCommand: use dma
AtapiDmaSetup: already setup, 1 entries
AtapiSendCommand: use dma
AtapiSendCommand: use_dma=1, Cmd 28
  REQ_FLAG_DMA_OPERATION
AtapiSendCommand: AtapiDmaReinit()
AtapiDmaReinit: restore IO mode on Device 1
AtapiDmaInit__: Set (U)DMA on Device 1
AtapiDmaInit: deviceExtension->MaxTransferMode >= ATA_UDMA
AtapiDmaInit: LunExt->LimitedTransferMode 0x45
AtapiDmaInit: LunExt->MaxTransferMode >= ATA_UDMA   =>   0x5
Setup chip a:w:u=4:2:5
AtaSetTransferMode: Set 0x45 on Device 0/1
AtaCommand48: cntrlr 0x0:0x0 dev 0x1, cmd 0xef, lba 0x0 count 0x45 feature 0x3
  Status 0x50
AtapiSendCommand: use_dma=1
  REQ_FLAG_DMA_OPERATION
AtapiSendCommand: CMD_ACTION_EXEC
AtapiSendCommand: Cdb b0e08d08 Command 0x28 to TargetId 1 lun 0
AtapiSendCommand: Entered with status 0x50
AtapiSendCommand: Entry Status (0x50)
AtapiSendCommand: Poll for int. to send packet. Status (0x50)
AtapiSendCommand: status (0x58)
AtapiDmaStart: read on 0x0:0x1
AtapiSendCommand: ExpectingInterrupt (0x1)
AtapiSendCommand: return SRB_STATUS_PENDING (3)
AtapiStartIo: next Srb b0e08cd8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x40
  base status 0x40
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type ATAPI
  OldReqState = 42
AtapiInterrupt: ATAPI Entered with status (0x40)
AtapiInterrupt: iReason 3
AtapiInterrupt: ATAPI branch
AtapiInterrupt: iReason 3
AtapiInterrupt: i-reason=3, status=0x40
AtapiInterrupt: interruptReason = CompleteRequest
AtapiInterrupt: CompleteRequest, was DmaTransfer
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e08cd8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e08cd8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x0
  perform generic check
  getting status...
  ATAPI status 0x40
  base status 0x40
  Unexpected interrupt.
  ATAPI additional check
AtapiCheckInterrupt__: ATAPI int reason 3
AtapiInterrupt(base): set CHECK_INTR_IDLE (2)
AtapiInterrupt(base): exit with status 0x0
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0df8148, CDB 0xb0df8178, AtaReq 0xb1298000, SCmd 0x43
UniataNeedQueueing: TopLevel, qd=0
Send to device 43
TopLevel (2), srb 0xb0df8148
TopLevel (3), AtaReq 0xb1298000
Try ATAPI send 43
AtapiSendCommand: req state 0x10, Action 3
AtapiSendCommand: prepare..., ATAPI CMD 43 (Cdb b0df8178)
  assume IN
AtapiSendCommand: use_dma=0, Cmd 43
AtapiSendCommand: AtapiDmaReinit()
AtapiDmaReinit: !(AtaReq->Flags & REQ_FLAG_DMA_OPERATION), fall to PIO on Device 1
AtapiDmaReinit: set PIO mode on Device 1 (45 -> c)
AtapiDmaInit: deviceExtension->MaxTransferMode >= ATA_UDMA
AtapiDmaInit: LunExt->LimitedTransferMode 0x45
AtapiDmaInit: LunExt->MaxTransferMode >= ATA_UDMA   =>   0xffffffff
Setup chip a:w:u=4:-1:-1
AtaSetTransferMode: Set 0xc on Device 0/1
AtaCommand48: cntrlr 0x0:0x0 dev 0x1, cmd 0xef, lba 0x0 count 0xc feature 0x3
  Status 0x50
AtapiSendCommand: use_dma=0
AtapiSendCommand: CMD_ACTION_EXEC
AtapiSendCommand: Cdb b0df8178 Command 0x43 to TargetId 1 lun 0
AtapiSendCommand: Entered with status 0x50
AtapiSendCommand: Entry Status (0x50)
AtapiSendCommand: Poll for int. to send packet. Status (0x50)
AtapiSendCommand: status (0x58)
AtapiSendCommand: ExpectingInterrupt (0x1)
AtapiSendCommand: return SRB_STATUS_PENDING (3)
AtapiStartIo: next Srb b0df8148
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x4
  perform generic check
  clear unexpected DMA intr
AtapiDmaDone: dev -1
  getting status...
  ATAPI status 0x58
  base status 0x58
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  dev_type ATAPI
  OldReqState = 42
  continue service interrupt
AtapiInterrupt: ATAPI Entered with status (0x58)
AtapiInterrupt: iReason 2
AtapiInterrupt: ATAPI branch
AtapiInterrupt: iReason 2
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: get R wordCount 0x6
IdeIntr: Read 0x6 words
IdeIntr: PIO Read AtaReq->DataBuffer 0xb0df8690, srb->DataBuffer 0xb0df8690
  status re-check 0x50
AtapiInterrupt: all transferred, AtaReq->WordsLeft == 0
AtapiInterrupt: early complete ? status 50
AtapiInterrupt: CompleteRequest, srbstatus 1
AtapiInterrupt: PIO completion
AtapiInterrupt: PIO completion, wait BUSY
IdeIntr: ATAPI Read AtaReq->DataBuffer 0xb0df869c, srb->DataBuffer 0xb0df8690, len 0xc
   Transfered 0, full size c
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0df8148, status 1
AtapiInterrupt: RequestComplete, srb 0xb0df8148
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x4
  perform generic check
  clear unexpected DMA intr
AtapiDmaDone: dev -1
  getting status...
  ATAPI status 0x50
  base status 0x50
  Unexpected interrupt.
  ATAPI additional check
AtapiCheckInterrupt__: ATAPI int reason 3
AtapiInterrupt(base): Catch unexpected
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e08cd8, CDB 0xb0e08d08, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e08cd8
TopLevel (3), AtaReq 0xb1298000
Try ATAPI send 28
AtapiSendCommand: req state 0x10, Action 3
AtapiSendCommand: prepare..., ATAPI CMD 28 (Cdb b0e08d08)
AtapiDmaSetup: mode 0xc, data f8716718, count 800, lCh 0, dev 1
AtapiDmaSetup: Not DMA mode, assume this is just preparation
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8716718)
  set TERM
AtapiDmaSetup: OK
AtapiSendCommand: use dma
AtapiDmaSetup: already setup, 1 entries
AtapiSendCommand: use dma
AtapiSendCommand: use_dma=1, Cmd 28
  REQ_FLAG_DMA_OPERATION
AtapiSendCommand: AtapiDmaReinit()
AtapiDmaReinit: restore IO mode on Device 1
AtapiDmaInit__: Set (U)DMA on Device 1
AtapiDmaInit: deviceExtension->MaxTransferMode >= ATA_UDMA
AtapiDmaInit: LunExt->LimitedTransferMode 0x45
AtapiDmaInit: LunExt->MaxTransferMode >= ATA_UDMA   =>   0x5
Setup chip a:w:u=4:2:5
AtaSetTransferMode: Set 0x45 on Device 0/1
AtaCommand48: cntrlr 0x0:0x0 dev 0x1, cmd 0xef, lba 0x0 count 0x45 feature 0x3
  Status 0x50
AtapiSendCommand: use_dma=1
  REQ_FLAG_DMA_OPERATION
AtapiSendCommand: CMD_ACTION_EXEC
AtapiSendCommand: Cdb b0e08d08 Command 0x28 to TargetId 1 lun 0
AtapiSendCommand: Entered with status 0x50
AtapiSendCommand: Entry Status (0x50)
AtapiSendCommand: Poll for int. to send packet. Status (0x50)
AtapiSendCommand: status (0x58)
AtapiDmaStart: read on 0x0:0x1
AtapiSendCommand: ExpectingInterrupt (0x1)
AtapiSendCommand: return SRB_STATUS_PENDING (3)
AtapiStartIo: next Srb b0e08cd8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x40
  base status 0x40
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type ATAPI
  OldReqState = 42
AtapiInterrupt: ATAPI Entered with status (0x40)
AtapiInterrupt: iReason 3
AtapiInterrupt: ATAPI branch
AtapiInterrupt: iReason 3
AtapiInterrupt: i-reason=3, status=0x40
AtapiInterrupt: interruptReason = CompleteRequest
AtapiInterrupt: CompleteRequest, was DmaTransfer
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e08cd8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e08cd8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x0
  perform generic check
  getting status...
  ATAPI status 0x40
  base status 0x40
  Unexpected interrupt.
  ATAPI additional check
AtapiCheckInterrupt__: ATAPI int reason 3
AtapiInterrupt(base): set CHECK_INTR_IDLE (2)
AtapiInterrupt(base): exit with status 0x0
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e08cd8, CDB 0xb0e08d08, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e08cd8
TopLevel (3), AtaReq 0xb1298000
Try ATAPI send 28
AtapiSendCommand: req state 0x10, Action 3
AtapiSendCommand: prepare..., ATAPI CMD 28 (Cdb b0e08d08)
AtapiDmaSetup: mode 0x45, data f8716718, count 800, lCh 0, dev 1
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8716718)
  set TERM
AtapiDmaSetup: OK
AtapiSendCommand: use dma
AtapiDmaSetup: already setup, 1 entries
AtapiSendCommand: use dma
AtapiSendCommand: use_dma=1, Cmd 28
  REQ_FLAG_DMA_OPERATION
AtapiSendCommand: AtapiDmaReinit()
AtapiSendCommand: use_dma=1
  REQ_FLAG_DMA_OPERATION
AtapiSendCommand: CMD_ACTION_EXEC
AtapiSendCommand: Cdb b0e08d08 Command 0x28 to TargetId 1 lun 0
AtapiSendCommand: Entered with status 0x40
AtapiSendCommand: Entry Status (0x40)
AtapiSendCommand: Poll for int. to send packet. Status (0x40)
AtapiSendCommand: status (0x58)
AtapiDmaStart: read on 0x0:0x1
AtapiSendCommand: ExpectingInterrupt (0x1)
AtapiSendCommand: return SRB_STATUS_PENDING (3)
AtapiStartIo: next Srb b0e08cd8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x40
  base status 0x40
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type ATAPI
  OldReqState = 42
AtapiInterrupt: ATAPI Entered with status (0x40)
AtapiInterrupt: iReason 3
AtapiInterrupt: ATAPI branch
AtapiInterrupt: iReason 3
AtapiInterrupt: i-reason=3, status=0x40
AtapiInterrupt: interruptReason = CompleteRequest
AtapiInterrupt: CompleteRequest, was DmaTransfer
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e08cd8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e08cd8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e08cd8, CDB 0xb0e08d08, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e08cd8
TopLevel (3), AtaReq 0xb1298000
Try ATAPI send 28
AtapiSendCommand: req state 0x10, Action 3
AtapiSendCommand: prepare..., ATAPI CMD 28 (Cdb b0e08d08)
AtapiDmaSetup: mode 0x45, data f8716718, count 800, lCh 0, dev 1
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8716718)
  set TERM
AtapiDmaSetup: OK
AtapiSendCommand: use dma
AtapiDmaSetup: already setup, 1 entries
AtapiSendCommand: use dma
AtapiSendCommand: use_dma=1, Cmd 28
  REQ_FLAG_DMA_OPERATION
AtapiSendCommand: AtapiDmaReinit()
AtapiSendCommand: use_dma=1
  REQ_FLAG_DMA_OPERATION
AtapiSendCommand: CMD_ACTION_EXEC
AtapiSendCommand: Cdb b0e08d08 Command 0x28 to TargetId 1 lun 0
AtapiSendCommand: Entered with status 0x40
AtapiSendCommand: Entry Status (0x40)
AtapiSendCommand: Poll for int. to send packet. Status (0x40)
AtapiSendCommand: status (0x58)
AtapiDmaStart: read on 0x0:0x1
AtapiSendCommand: ExpectingInterrupt (0x1)
AtapiSendCommand: return SRB_STATUS_PENDING (3)
AtapiStartIo: next Srb b0e08cd8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 3)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x40
  base status 0x40
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type ATAPI
  OldReqState = 42
AtapiInterrupt: ATAPI Entered with status (0x40)
AtapiInterrupt: iReason 3
AtapiInterrupt: ATAPI branch
AtapiInterrupt: iReason 3
AtapiInterrupt: i-reason=3, status=0x40
AtapiInterrupt: interruptReason = CompleteRequest
AtapiInterrupt: CompleteRequest, was DmaTransfer
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e08cd8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e08cd8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0e08cd8, CDB 0xb0e08d08, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0e08cd8
TopLevel (3), AtaReq 0xb1298000
Try ATAPI send 28
AtapiSendCommand: req state 0x10, Action 3
AtapiSendCommand: prepare..., ATAPI CMD 28 (Cdb b0e08d08)
AtapiDmaSetup: mode 0x45, data f8716718, count 800, lCh 0, dev 1
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8716718)
  set TERM
AtapiDmaSetup: OK
AtapiSendCommand: use dma
AtapiDmaSetup: already setup, 1 entries
AtapiSendCommand: use dma
AtapiSendCommand: use_dma=1, Cmd 28
  REQ_FLAG_DMA_OPERATION
AtapiSendCommand: AtapiDmaReinit()
AtapiSendCommand: use_dma=1
  REQ_FLAG_DMA_OPERATION
AtapiSendCommand: CMD_ACTION_EXEC
AtapiSendCommand: Cdb b0e08d08 Command 0x28 to TargetId 1 lun 0
AtapiSendCommand: Entered with status 0x40
AtapiSendCommand: Entry Status (0x40)
AtapiSendCommand: Poll for int. to send packet. Status (0x40)
AtapiSendCommand: status (0x58)
AtapiDmaStart: read on 0x0:0x1
AtapiSendCommand: ExpectingInterrupt (0x1)
AtapiSendCommand: return SRB_STATUS_PENDING (3)
AtapiStartIo: next Srb b0e08cd8
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 3)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x40
  base status 0x40
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type ATAPI
  OldReqState = 42
AtapiInterrupt: ATAPI Entered with status (0x40)
AtapiInterrupt: iReason 3
AtapiInterrupt: ATAPI branch
AtapiInterrupt: iReason 3
AtapiInterrupt: i-reason=3, status=0x40
AtapiInterrupt: interruptReason = CompleteRequest
AtapiInterrupt: CompleteRequest, was DmaTransfer
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0e08cd8, status 1
AtapiInterrupt: RequestComplete, srb 0xb0e08cd8
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x1
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0df8148, CDB 0xb0df8178, AtaReq 0xb1298000, SCmd 0x0
UniataNeedQueueing: TopLevel, qd=0
Send to device 0
TopLevel (2), srb 0xb0df8148
TopLevel (3), AtaReq 0xb1298000
Try ATAPI send 0
AtapiSendCommand: req state 0x10, Action 3
AtapiSendCommand: prepare..., ATAPI CMD 0 (Cdb b0df8178)
  assume 0-transfer
AtapiSendCommand: zero transfer, no DMA setup
AtapiSendCommand: use_dma=0, Cmd 0
AtapiSendCommand: zero transfer
AtapiSendCommand: AtapiDmaReinit() to PIO
AtapiDmaReinit: !(AtaReq->Flags & REQ_FLAG_DMA_OPERATION), fall to PIO on Device 1
AtapiDmaReinit: set PIO mode on Device 1 (45 -> c)
AtapiDmaInit: deviceExtension->MaxTransferMode >= ATA_UDMA
AtapiDmaInit: LunExt->LimitedTransferMode 0x45
AtapiDmaInit: LunExt->MaxTransferMode >= ATA_UDMA   =>   0xffffffff
Setup chip a:w:u=4:-1:-1
AtaSetTransferMode: Set 0xc on Device 0/1
AtaCommand48: cntrlr 0x0:0x0 dev 0x1, cmd 0xef, lba 0x0 count 0xc feature 0x3
  Status 0x50
AtapiSendCommand: use_dma=0
AtapiSendCommand: CMD_ACTION_EXEC
AtapiSendCommand: Cdb b0df8178 Command 0x0 to TargetId 1 lun 0
AtapiSendCommand: Entered with status 0x50
AtapiSendCommand: Entry Status (0x50)
AtapiSendCommand: Poll for int. to send packet. Status (0x50)
AtapiSendCommand: status (0x58)
AtapiSendCommand: ExpectingInterrupt (0x1)
AtapiSendCommand: return SRB_STATUS_PENDING (3)
AtapiStartIo: next Srb b0df8148
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 3)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x4
  perform generic check
  clear unexpected DMA intr
AtapiDmaDone: dev -1
  getting status...
  ATAPI status 0x40
  base status 0x40
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  dev_type ATAPI
  OldReqState = 42
  continue service interrupt
AtapiInterrupt: ATAPI Entered with status (0x40)
AtapiInterrupt: iReason 3
AtapiInterrupt: ATAPI branch
AtapiInterrupt: iReason 3
AtapiInterrupt: i-reason=3, status=0x40
AtapiInterrupt: interruptReason = CompleteRequest
AtapiInterrupt: CompleteRequest, srbstatus 1
AtapiInterrupt: PIO completion
AtapiInterrupt: PIO completion, wait BUSY
IdeIntr: ATAPI Read AtaReq->DataBuffer 0x0, srb->DataBuffer 0x0, len 0x0
   Transfered 0, full size 0
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0df8148, status 1
AtapiInterrupt: RequestComplete, srb 0xb0df8148
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = FALSE
  DMA status 0x0
  perform generic check
  getting status...
  ATAPI status 0x40
  base status 0x40
  Unexpected interrupt.
  ATAPI additional check
AtapiCheckInterrupt__: ATAPI int reason 3
AtapiInterrupt(base): set CHECK_INTR_IDLE (2)
AtapiInterrupt(base): exit with status 0x0
(../../base/system/smss2/pagefile.c:908) SMSS:PFILE: Volume `\??\E:\' (3) cannot store a paging file
Boot took 74066580982 cycles!
Interrupts: 3023 System Calls: 11700 Context Switches: 166
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87046c4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4057, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 4057, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 81f80000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81f80000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4057, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4057 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f4c1c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 52b8f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 52b8f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f86b2000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86b2000)
  get Phys(data[n=1]=f86b3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x52b8f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x52b8f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f4c1c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e2aaf, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1e2aaf, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data f86b4000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86b4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e2aaf, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e2aaf count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8704c1c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 52947, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 52947, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f86b2000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86b2000)
  get Phys(data[n=1]=f86b3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x52947, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x52947 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8704c1c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e2aa7, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1e2aa7, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data f86b4000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86b4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e2aa7, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e2aa7 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f8bb4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 52a9f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 52a9f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8671000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8671000)
  get Phys(data[n=1]=f8672000)
  get Phys(data[n=2]=f8673000)
  get Phys(data[n=2]=f8674000)
  get Phys(data[n=2]=f8675000)
  get Phys(data[n=2]=f8676000)
  get Phys(data[n=2]=f8677000)
  get Phys(data[n=2]=f8678000)
  get Phys(data[n=2]=f8679000)
  get Phys(data[n=2]=f867a000)
  get Phys(data[n=3]=f867b000)
  get Phys(data[n=4]=f867c000)
  get Phys(data[n=4]=f867d000)
  get Phys(data[n=4]=f867e000)
  get Phys(data[n=4]=f867f000)
  get Phys(data[n=4]=f8680000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x52a9f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x52a9f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f8bb4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 52b1f, OrigWordsRequested 0x7000, DevSize 0x70
IdeReadWrite (REQ): Starting sector is 52b1f, Number of WORDS 0x7000, DevSize 0x70
AtapiDmaSetup: mode 0x45, data f8681000, count e000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8681000)
  get Phys(data[n=1]=f8682000)
  get Phys(data[n=2]=f8683000)
  get Phys(data[n=2]=f8684000)
  get Phys(data[n=2]=f8685000)
  get Phys(data[n=2]=f8686000)
  get Phys(data[n=3]=f8687000)
  get Phys(data[n=3]=f8688000)
  get Phys(data[n=4]=f8689000)
  get Phys(data[n=4]=f868a000)
  get Phys(data[n=5]=f868b000)
  get Phys(data[n=6]=f868c000)
  get Phys(data[n=7]=f868d000)
  get Phys(data[n=7]=f868e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x52b1f, Count 0x70(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x52b1f count 0x70 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e000, full size e000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f8c1c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e2a7f, OrigWordsRequested 0x2800, DevSize 0x28
IdeReadWrite (REQ): Starting sector is 1e2a7f, Number of WORDS 0x2800, DevSize 0x28
AtapiDmaSetup: mode 0x45, data f868f000, count 5000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f868f000)
  get Phys(data[n=1]=f8690000)
  get Phys(data[n=2]=f8691000)
  get Phys(data[n=3]=f8692000)
  get Phys(data[n=3]=f8693000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e2a7f, Count 0x28(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e2a7f count 0x28 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 5000, full size 5000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8700bb4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 52957, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 52957, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8630000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8630000)
  get Phys(data[n=1]=f8631000)
  get Phys(data[n=1]=f8632000)
  get Phys(data[n=1]=f8633000)
  get Phys(data[n=2]=f8634000)
  get Phys(data[n=3]=f8635000)
  get Phys(data[n=3]=f8636000)
  get Phys(data[n=3]=f8637000)
  get Phys(data[n=3]=f8638000)
  get Phys(data[n=3]=f8639000)
  get Phys(data[n=3]=f863a000)
  get Phys(data[n=3]=f863b000)
  get Phys(data[n=4]=f863c000)
  get Phys(data[n=4]=f863d000)
  get Phys(data[n=4]=f863e000)
  get Phys(data[n=4]=f863f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x52957, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x52957 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8700bb4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 529d7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 529d7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8640000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8640000)
  get Phys(data[n=1]=f8641000)
  get Phys(data[n=2]=f8642000)
  get Phys(data[n=2]=f8643000)
  get Phys(data[n=3]=f8644000)
  get Phys(data[n=4]=f8645000)
  get Phys(data[n=5]=f8646000)
  get Phys(data[n=5]=f8647000)
  get Phys(data[n=5]=f8648000)
  get Phys(data[n=5]=f8649000)
  get Phys(data[n=6]=f864a000)
  get Phys(data[n=7]=f864b000)
  get Phys(data[n=7]=f864c000)
  get Phys(data[n=7]=f864d000)
  get Phys(data[n=7]=f864e000)
  get Phys(data[n=8]=f864f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x529d7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x529d7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8700bb4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 52a57, OrigWordsRequested 0x4800, DevSize 0x48
IdeReadWrite (REQ): Starting sector is 52a57, Number of WORDS 0x4800, DevSize 0x48
AtapiDmaSetup: mode 0x45, data f8650000, count 9000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8650000)
  get Phys(data[n=1]=f8651000)
  get Phys(data[n=1]=f8652000)
  get Phys(data[n=1]=f8653000)
  get Phys(data[n=1]=f8654000)
  get Phys(data[n=2]=f8655000)
  get Phys(data[n=2]=f8656000)
  get Phys(data[n=3]=f8657000)
  get Phys(data[n=3]=f8658000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x52a57, Count 0x48(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x52a57 count 0x48 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 9000, full size 9000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8700bb4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e2457, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1e2457, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8659000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8659000)
  get Phys(data[n=1]=f865a000)
  get Phys(data[n=1]=f865b000)
  get Phys(data[n=1]=f865c000)
  get Phys(data[n=1]=f865d000)
  get Phys(data[n=1]=f865e000)
  get Phys(data[n=2]=f865f000)
  get Phys(data[n=2]=f8660000)
  get Phys(data[n=2]=f8661000)
  get Phys(data[n=2]=f8662000)
  get Phys(data[n=2]=f8663000)
  get Phys(data[n=2]=f8664000)
  get Phys(data[n=3]=f8665000)
  get Phys(data[n=3]=f8666000)
  get Phys(data[n=3]=f8667000)
  get Phys(data[n=3]=f8668000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e2457, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e2457 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8700bb4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e24d7, OrigWordsRequested 0x3800, DevSize 0x38
IdeReadWrite (REQ): Starting sector is 1e24d7, Number of WORDS 0x3800, DevSize 0x38
AtapiDmaSetup: mode 0x45, data f8669000, count 7000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8669000)
  get Phys(data[n=1]=f866a000)
  get Phys(data[n=2]=f866b000)
  get Phys(data[n=2]=f866c000)
  get Phys(data[n=2]=f866d000)
  get Phys(data[n=2]=f866e000)
  get Phys(data[n=2]=f866f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e24d7, Count 0x38(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e24d7 count 0x38 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 7000, full size 7000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8700bec
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e250f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1e250f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f85c4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f85c4000)
  get Phys(data[n=1]=f85c5000)
  get Phys(data[n=1]=f85c6000)
  get Phys(data[n=1]=f85c7000)
  get Phys(data[n=1]=f85c8000)
  get Phys(data[n=2]=f85c9000)
  get Phys(data[n=2]=f85ca000)
  get Phys(data[n=2]=f85cb000)
  get Phys(data[n=2]=f85cc000)
  get Phys(data[n=2]=f85cd000)
  get Phys(data[n=2]=f85ce000)
  get Phys(data[n=2]=f85cf000)
  get Phys(data[n=2]=f85d0000)
  get Phys(data[n=2]=f85d1000)
  get Phys(data[n=3]=f85d2000)
  get Phys(data[n=4]=f85d3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e250f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e250f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8700bec
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e258f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1e258f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f85d4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f85d4000)
  get Phys(data[n=1]=f85d5000)
  get Phys(data[n=1]=f85d6000)
  get Phys(data[n=1]=f85d7000)
  get Phys(data[n=1]=f85d8000)
  get Phys(data[n=1]=f85d9000)
  get Phys(data[n=2]=f85da000)
  get Phys(data[n=2]=f85db000)
  get Phys(data[n=2]=f85dc000)
  get Phys(data[n=2]=f85dd000)
  get Phys(data[n=3]=f85de000)
  get Phys(data[n=3]=f85df000)
  get Phys(data[n=4]=f85e0000)
  get Phys(data[n=4]=f85e1000)
  get Phys(data[n=5]=f85e2000)
  get Phys(data[n=6]=f85e3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e258f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e258f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8700bec
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e260f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1e260f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f85e4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f85e4000)
  get Phys(data[n=1]=f85e5000)
  get Phys(data[n=1]=f85e6000)
  get Phys(data[n=1]=f85e7000)
  get Phys(data[n=2]=f85e8000)
  get Phys(data[n=3]=f85e9000)
  get Phys(data[n=3]=f85ea000)
  get Phys(data[n=3]=f85eb000)
  get Phys(data[n=3]=f85ec000)
  get Phys(data[n=4]=f85ed000)
  get Phys(data[n=4]=f85ee000)
  get Phys(data[n=4]=f85ef000)
  get Phys(data[n=4]=f85f0000)
  get Phys(data[n=4]=f85f1000)
  get Phys(data[n=4]=f85f2000)
  get Phys(data[n=5]=f85f3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e260f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e260f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8700bec
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e268f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1e268f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f85f4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f85f4000)
  get Phys(data[n=1]=f85f5000)
  get Phys(data[n=1]=f85f6000)
  get Phys(data[n=1]=f85f7000)
  get Phys(data[n=1]=f85f8000)
  get Phys(data[n=1]=f85f9000)
  get Phys(data[n=1]=f85fa000)
  get Phys(data[n=1]=f85fb000)
  get Phys(data[n=1]=f85fc000)
  get Phys(data[n=2]=f85fd000)
  get Phys(data[n=2]=f85fe000)
  get Phys(data[n=2]=f85ff000)
  get Phys(data[n=2]=f8600000)
  get Phys(data[n=2]=f8601000)
  get Phys(data[n=2]=f8602000)
  get Phys(data[n=3]=f8603000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e268f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e268f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8700bec
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e270f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1e270f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f85c4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f85c4000)
  get Phys(data[n=1]=f85c5000)
  get Phys(data[n=1]=f85c6000)
  get Phys(data[n=1]=f85c7000)
  get Phys(data[n=1]=f85c8000)
  get Phys(data[n=2]=f85c9000)
  get Phys(data[n=2]=f85ca000)
  get Phys(data[n=2]=f85cb000)
  get Phys(data[n=2]=f85cc000)
  get Phys(data[n=2]=f85cd000)
  get Phys(data[n=2]=f85ce000)
  get Phys(data[n=2]=f85cf000)
  get Phys(data[n=2]=f85d0000)
  get Phys(data[n=2]=f85d1000)
  get Phys(data[n=3]=f85d2000)
  get Phys(data[n=4]=f85d3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e270f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e270f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8700bec
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e278f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1e278f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f85d4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f85d4000)
  get Phys(data[n=1]=f85d5000)
  get Phys(data[n=1]=f85d6000)
  get Phys(data[n=1]=f85d7000)
  get Phys(data[n=1]=f85d8000)
  get Phys(data[n=1]=f85d9000)
  get Phys(data[n=2]=f85da000)
  get Phys(data[n=2]=f85db000)
  get Phys(data[n=2]=f85dc000)
  get Phys(data[n=2]=f85dd000)
  get Phys(data[n=3]=f85de000)
  get Phys(data[n=3]=f85df000)
  get Phys(data[n=4]=f85e0000)
  get Phys(data[n=4]=f85e1000)
  get Phys(data[n=5]=f85e2000)
  get Phys(data[n=6]=f85e3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e278f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e278f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8700bec
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e280f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1e280f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f85e4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f85e4000)
  get Phys(data[n=1]=f85e5000)
  get Phys(data[n=1]=f85e6000)
  get Phys(data[n=1]=f85e7000)
  get Phys(data[n=2]=f85e8000)
  get Phys(data[n=3]=f85e9000)
  get Phys(data[n=3]=f85ea000)
  get Phys(data[n=3]=f85eb000)
  get Phys(data[n=3]=f85ec000)
  get Phys(data[n=4]=f85ed000)
  get Phys(data[n=4]=f85ee000)
  get Phys(data[n=4]=f85ef000)
  get Phys(data[n=4]=f85f0000)
  get Phys(data[n=4]=f85f1000)
  get Phys(data[n=4]=f85f2000)
  get Phys(data[n=5]=f85f3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e280f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e280f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8700bec
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e288f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1e288f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f85f4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f85f4000)
  get Phys(data[n=1]=f85f5000)
  get Phys(data[n=1]=f85f6000)
  get Phys(data[n=1]=f85f7000)
  get Phys(data[n=1]=f85f8000)
  get Phys(data[n=1]=f85f9000)
  get Phys(data[n=1]=f85fa000)
  get Phys(data[n=1]=f85fb000)
  get Phys(data[n=1]=f85fc000)
  get Phys(data[n=2]=f85fd000)
  get Phys(data[n=2]=f85fe000)
  get Phys(data[n=2]=f85ff000)
  get Phys(data[n=2]=f8600000)
  get Phys(data[n=2]=f8601000)
  get Phys(data[n=2]=f8602000)
  get Phys(data[n=3]=f8603000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e288f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e288f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8700bec
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e290f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1e290f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f85c4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f85c4000)
  get Phys(data[n=1]=f85c5000)
  get Phys(data[n=1]=f85c6000)
  get Phys(data[n=1]=f85c7000)
  get Phys(data[n=1]=f85c8000)
  get Phys(data[n=2]=f85c9000)
  get Phys(data[n=2]=f85ca000)
  get Phys(data[n=2]=f85cb000)
  get Phys(data[n=2]=f85cc000)
  get Phys(data[n=2]=f85cd000)
  get Phys(data[n=2]=f85ce000)
  get Phys(data[n=2]=f85cf000)
  get Phys(data[n=2]=f85d0000)
  get Phys(data[n=2]=f85d1000)
  get Phys(data[n=3]=f85d2000)
  get Phys(data[n=4]=f85d3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e290f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e290f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8700bec
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e298f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1e298f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f85d4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f85d4000)
  get Phys(data[n=1]=f85d5000)
  get Phys(data[n=1]=f85d6000)
  get Phys(data[n=1]=f85d7000)
  get Phys(data[n=1]=f85d8000)
  get Phys(data[n=1]=f85d9000)
  get Phys(data[n=2]=f85da000)
  get Phys(data[n=2]=f85db000)
  get Phys(data[n=2]=f85dc000)
  get Phys(data[n=2]=f85dd000)
  get Phys(data[n=3]=f85de000)
  get Phys(data[n=3]=f85df000)
  get Phys(data[n=4]=f85e0000)
  get Phys(data[n=4]=f85e1000)
  get Phys(data[n=5]=f85e2000)
  get Phys(data[n=6]=f85e3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e298f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e298f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8700bec
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e2a0f, OrigWordsRequested 0x7000, DevSize 0x70
IdeReadWrite (REQ): Starting sector is 1e2a0f, Number of WORDS 0x7000, DevSize 0x70
AtapiDmaSetup: mode 0x45, data f85e4000, count e000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f85e4000)
  get Phys(data[n=1]=f85e5000)
  get Phys(data[n=1]=f85e6000)
  get Phys(data[n=1]=f85e7000)
  get Phys(data[n=2]=f85e8000)
  get Phys(data[n=3]=f85e9000)
  get Phys(data[n=3]=f85ea000)
  get Phys(data[n=3]=f85eb000)
  get Phys(data[n=3]=f85ec000)
  get Phys(data[n=4]=f85ed000)
  get Phys(data[n=4]=f85ee000)
  get Phys(data[n=4]=f85ef000)
  get Phys(data[n=4]=f85f0000)
  get Phys(data[n=4]=f85f1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e2a0f, Count 0x70(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e2a0f count 0x70 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e000, full size e000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/procsup.c:1969) Session 0 is ready to go: 0xBF7F0000 0xF86F0000, 1e452 0xB0DE9E00
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725fb4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5159f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5159f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86b0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86b0000)
  get Phys(data[n=1]=f86b1000)
  get Phys(data[n=1]=f86b2000)
  get Phys(data[n=1]=f86b3000)
  get Phys(data[n=2]=f86b4000)
  get Phys(data[n=2]=f86b5000)
  get Phys(data[n=2]=f86b6000)
  get Phys(data[n=2]=f86b7000)
  get Phys(data[n=2]=f86b8000)
  get Phys(data[n=2]=f86b9000)
  get Phys(data[n=3]=f86ba000)
  get Phys(data[n=3]=f86bb000)
  get Phys(data[n=3]=f86bc000)
  get Phys(data[n=3]=f86bd000)
  get Phys(data[n=3]=f86be000)
  get Phys(data[n=3]=f86bf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5159f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5159f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725fb4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5161f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5161f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86c0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86c0000)
  get Phys(data[n=1]=f86c1000)
  get Phys(data[n=1]=f86c2000)
  get Phys(data[n=1]=f86c3000)
  get Phys(data[n=1]=f86c4000)
  get Phys(data[n=1]=f86c5000)
  get Phys(data[n=1]=f86c6000)
  get Phys(data[n=1]=f86c7000)
  get Phys(data[n=1]=f86c8000)
  get Phys(data[n=2]=f86c9000)
  get Phys(data[n=3]=f86ca000)
  get Phys(data[n=3]=f86cb000)
  get Phys(data[n=3]=f86cc000)
  get Phys(data[n=3]=f86cd000)
  get Phys(data[n=3]=f86ce000)
  get Phys(data[n=3]=f86cf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5161f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5161f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725fb4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5169f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5169f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86d0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86d0000)
  get Phys(data[n=1]=f86d1000)
  get Phys(data[n=1]=f86d2000)
  get Phys(data[n=1]=f86d3000)
  get Phys(data[n=1]=f86d4000)
  get Phys(data[n=2]=f86d5000)
  get Phys(data[n=2]=f86d6000)
  get Phys(data[n=3]=f86d7000)
  get Phys(data[n=3]=f86d8000)
  get Phys(data[n=4]=f86d9000)
  get Phys(data[n=5]=f86da000)
  get Phys(data[n=6]=f86db000)
  get Phys(data[n=6]=f86dc000)
  get Phys(data[n=6]=f86dd000)
  get Phys(data[n=6]=f86de000)
  get Phys(data[n=7]=f86df000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5169f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5169f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725fb4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5171f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5171f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f86e0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86e0000)
  get Phys(data[n=1]=f86e1000)
  get Phys(data[n=1]=f86e2000)
  get Phys(data[n=1]=f86e3000)
  get Phys(data[n=2]=f86e4000)
  get Phys(data[n=2]=f86e5000)
  get Phys(data[n=2]=f86e6000)
  get Phys(data[n=2]=f86e7000)
  get Phys(data[n=2]=f86e8000)
  get Phys(data[n=2]=f86e9000)
  get Phys(data[n=3]=f86ea000)
  get Phys(data[n=3]=f86eb000)
  get Phys(data[n=4]=f86ec000)
  get Phys(data[n=4]=f86ed000)
  get Phys(data[n=4]=f86ee000)
  get Phys(data[n=4]=f86ef000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5171f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5171f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87263b0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5159f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 5159f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f86ee000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86ee000)
  get Phys(data[n=1]=f86ef000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5159f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5159f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\System32\win32k.sys at F85F5000 with fb pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87263d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5179f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5179f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 821c0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=821c0000)
  get Phys(data[n=1]=821c1000)
  get Phys(data[n=1]=821c2000)
  get Phys(data[n=1]=821c3000)
  get Phys(data[n=1]=821c4000)
  get Phys(data[n=1]=821c5000)
  get Phys(data[n=1]=821c6000)
  get Phys(data[n=2]=821c7000)
  get Phys(data[n=2]=821c8000)
  get Phys(data[n=2]=821c9000)
  get Phys(data[n=2]=821ca000)
  get Phys(data[n=2]=821cb000)
  get Phys(data[n=2]=821cc000)
  get Phys(data[n=3]=821cd000)
  get Phys(data[n=3]=821ce000)
  get Phys(data[n=3]=821cf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5179f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5179f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87263d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5181f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5181f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 821d0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=821d0000)
  get Phys(data[n=1]=821d1000)
  get Phys(data[n=1]=821d2000)
  get Phys(data[n=2]=821d3000)
  get Phys(data[n=2]=821d4000)
  get Phys(data[n=2]=821d5000)
  get Phys(data[n=2]=821d6000)
  get Phys(data[n=2]=821d7000)
  get Phys(data[n=2]=821d8000)
  get Phys(data[n=2]=821d9000)
  get Phys(data[n=2]=821da000)
  get Phys(data[n=2]=821db000)
  get Phys(data[n=3]=821dc000)
  get Phys(data[n=4]=821dd000)
  get Phys(data[n=4]=821de000)
  get Phys(data[n=4]=821df000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5181f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5181f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87263d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5189f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5189f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 821e0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=821e0000)
  get Phys(data[n=1]=821e1000)
  get Phys(data[n=1]=821e2000)
  get Phys(data[n=1]=821e3000)
  get Phys(data[n=2]=821e4000)
  get Phys(data[n=2]=821e5000)
  get Phys(data[n=2]=821e6000)
  get Phys(data[n=2]=821e7000)
  get Phys(data[n=3]=821e8000)
  get Phys(data[n=3]=821e9000)
  get Phys(data[n=4]=821ea000)
  get Phys(data[n=4]=821eb000)
  get Phys(data[n=5]=821ec000)
  get Phys(data[n=6]=821ed000)
  get Phys(data[n=7]=821ee000)
  get Phys(data[n=7]=821ef000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5189f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5189f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87263d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5191f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5191f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 821f0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=821f0000)
  get Phys(data[n=1]=821f1000)
  get Phys(data[n=2]=821f2000)
  get Phys(data[n=3]=821f3000)
  get Phys(data[n=3]=821f4000)
  get Phys(data[n=3]=821f5000)
  get Phys(data[n=3]=821f6000)
  get Phys(data[n=4]=821f7000)
  get Phys(data[n=4]=821f8000)
  get Phys(data[n=4]=821f9000)
  get Phys(data[n=4]=821fa000)
  get Phys(data[n=4]=821fb000)
  get Phys(data[n=4]=821fc000)
  get Phys(data[n=5]=821fd000)
  get Phys(data[n=5]=821fe000)
  get Phys(data[n=6]=821ff000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5191f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5191f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87263d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5199f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5199f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 82200000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82200000)
  get Phys(data[n=1]=82201000)
  get Phys(data[n=1]=82202000)
  get Phys(data[n=1]=82203000)
  get Phys(data[n=1]=82204000)
  get Phys(data[n=1]=82205000)
  get Phys(data[n=1]=82206000)
  get Phys(data[n=2]=82207000)
  get Phys(data[n=2]=82208000)
  get Phys(data[n=2]=82209000)
  get Phys(data[n=2]=8220a000)
  get Phys(data[n=2]=8220b000)
  get Phys(data[n=2]=8220c000)
  get Phys(data[n=3]=8220d000)
  get Phys(data[n=3]=8220e000)
  get Phys(data[n=3]=8220f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5199f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5199f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87263d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 51a1f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 51a1f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 82210000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82210000)
  get Phys(data[n=1]=82211000)
  get Phys(data[n=1]=82212000)
  get Phys(data[n=2]=82213000)
  get Phys(data[n=2]=82214000)
  get Phys(data[n=2]=82215000)
  get Phys(data[n=2]=82216000)
  get Phys(data[n=2]=82217000)
  get Phys(data[n=2]=82218000)
  get Phys(data[n=2]=82219000)
  get Phys(data[n=2]=8221a000)
  get Phys(data[n=2]=8221b000)
  get Phys(data[n=3]=8221c000)
  get Phys(data[n=4]=8221d000)
  get Phys(data[n=4]=8221e000)
  get Phys(data[n=4]=8221f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x51a1f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x51a1f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87263d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 51a9f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 51a9f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 82220000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82220000)
  get Phys(data[n=1]=82221000)
  get Phys(data[n=1]=82222000)
  get Phys(data[n=1]=82223000)
  get Phys(data[n=2]=82224000)
  get Phys(data[n=2]=82225000)
  get Phys(data[n=2]=82226000)
  get Phys(data[n=2]=82227000)
  get Phys(data[n=3]=82228000)
  get Phys(data[n=3]=82229000)
  get Phys(data[n=4]=8222a000)
  get Phys(data[n=4]=8222b000)
  get Phys(data[n=5]=8222c000)
  get Phys(data[n=6]=8222d000)
  get Phys(data[n=7]=8222e000)
  get Phys(data[n=7]=8222f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x51a9f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x51a9f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87263d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 51b1f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 51b1f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 82230000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82230000)
  get Phys(data[n=1]=82231000)
  get Phys(data[n=2]=82232000)
  get Phys(data[n=3]=82233000)
  get Phys(data[n=3]=82234000)
  get Phys(data[n=3]=82235000)
  get Phys(data[n=3]=82236000)
  get Phys(data[n=4]=82237000)
  get Phys(data[n=4]=82238000)
  get Phys(data[n=4]=82239000)
  get Phys(data[n=4]=8223a000)
  get Phys(data[n=4]=8223b000)
  get Phys(data[n=4]=8223c000)
  get Phys(data[n=5]=8223d000)
  get Phys(data[n=5]=8223e000)
  get Phys(data[n=6]=8223f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x51b1f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x51b1f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87263d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 51b9f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 51b9f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 82240000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82240000)
  get Phys(data[n=1]=82241000)
  get Phys(data[n=1]=82242000)
  get Phys(data[n=1]=82243000)
  get Phys(data[n=1]=82244000)
  get Phys(data[n=1]=82245000)
  get Phys(data[n=1]=82246000)
  get Phys(data[n=2]=82247000)
  get Phys(data[n=2]=82248000)
  get Phys(data[n=2]=82249000)
  get Phys(data[n=2]=8224a000)
  get Phys(data[n=2]=8224b000)
  get Phys(data[n=2]=8224c000)
  get Phys(data[n=3]=8224d000)
  get Phys(data[n=3]=8224e000)
  get Phys(data[n=3]=8224f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x51b9f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x51b9f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87263d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 51c1f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 51c1f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 82250000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82250000)
  get Phys(data[n=1]=82251000)
  get Phys(data[n=1]=82252000)
  get Phys(data[n=2]=82253000)
  get Phys(data[n=2]=82254000)
  get Phys(data[n=2]=82255000)
  get Phys(data[n=2]=82256000)
  get Phys(data[n=2]=82257000)
  get Phys(data[n=2]=82258000)
  get Phys(data[n=2]=82259000)
  get Phys(data[n=2]=8225a000)
  get Phys(data[n=2]=8225b000)
  get Phys(data[n=3]=8225c000)
  get Phys(data[n=4]=8225d000)
  get Phys(data[n=4]=8225e000)
  get Phys(data[n=4]=8225f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x51c1f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x51c1f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87263d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 51c9f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 51c9f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 82260000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82260000)
  get Phys(data[n=1]=82261000)
  get Phys(data[n=1]=82262000)
  get Phys(data[n=1]=82263000)
  get Phys(data[n=2]=82264000)
  get Phys(data[n=2]=82265000)
  get Phys(data[n=2]=82266000)
  get Phys(data[n=2]=82267000)
  get Phys(data[n=3]=82268000)
  get Phys(data[n=3]=82269000)
  get Phys(data[n=4]=8226a000)
  get Phys(data[n=4]=8226b000)
  get Phys(data[n=5]=8226c000)
  get Phys(data[n=6]=8226d000)
  get Phys(data[n=7]=8226e000)
  get Phys(data[n=7]=8226f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x51c9f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x51c9f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87263d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 51d1f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 51d1f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 82270000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82270000)
  get Phys(data[n=1]=82271000)
  get Phys(data[n=2]=82272000)
  get Phys(data[n=3]=82273000)
  get Phys(data[n=3]=82274000)
  get Phys(data[n=3]=82275000)
  get Phys(data[n=3]=82276000)
  get Phys(data[n=4]=82277000)
  get Phys(data[n=4]=82278000)
  get Phys(data[n=4]=82279000)
  get Phys(data[n=4]=8227a000)
  get Phys(data[n=4]=8227b000)
  get Phys(data[n=4]=8227c000)
  get Phys(data[n=5]=8227d000)
  get Phys(data[n=5]=8227e000)
  get Phys(data[n=6]=8227f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x51d1f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x51d1f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725e64
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4f9bf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4f9bf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f85b5000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f85b5000)
  get Phys(data[n=1]=f85b6000)
  get Phys(data[n=1]=f85b7000)
  get Phys(data[n=1]=f85b8000)
  get Phys(data[n=1]=f85b9000)
  get Phys(data[n=2]=f85ba000)
  get Phys(data[n=2]=f85bb000)
  get Phys(data[n=2]=f85bc000)
  get Phys(data[n=2]=f85bd000)
  get Phys(data[n=2]=f85be000)
  get Phys(data[n=2]=f85bf000)
  get Phys(data[n=3]=f85c0000)
  get Phys(data[n=3]=f85c1000)
  get Phys(data[n=3]=f85c2000)
  get Phys(data[n=3]=f85c3000)
  get Phys(data[n=3]=f85c4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4f9bf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4f9bf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725e64
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4fa3f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4fa3f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f85c5000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f85c5000)
  get Phys(data[n=1]=f85c6000)
  get Phys(data[n=1]=f85c7000)
  get Phys(data[n=1]=f85c8000)
  get Phys(data[n=1]=f85c9000)
  get Phys(data[n=1]=f85ca000)
  get Phys(data[n=1]=f85cb000)
  get Phys(data[n=1]=f85cc000)
  get Phys(data[n=1]=f85cd000)
  get Phys(data[n=1]=f85ce000)
  get Phys(data[n=2]=f85cf000)
  get Phys(data[n=3]=f85d0000)
  get Phys(data[n=3]=f85d1000)
  get Phys(data[n=3]=f85d2000)
  get Phys(data[n=3]=f85d3000)
  get Phys(data[n=3]=f85d4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4fa3f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4fa3f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725e64
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4fabf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4fabf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f85d5000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f85d5000)
  get Phys(data[n=1]=f85d6000)
  get Phys(data[n=2]=f85d7000)
  get Phys(data[n=2]=f85d8000)
  get Phys(data[n=2]=f85d9000)
  get Phys(data[n=2]=f85da000)
  get Phys(data[n=3]=f85db000)
  get Phys(data[n=3]=f85dc000)
  get Phys(data[n=4]=f85dd000)
  get Phys(data[n=4]=f85de000)
  get Phys(data[n=5]=f85df000)
  get Phys(data[n=6]=f85e0000)
  get Phys(data[n=7]=f85e1000)
  get Phys(data[n=7]=f85e2000)
  get Phys(data[n=7]=f85e3000)
  get Phys(data[n=7]=f85e4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4fabf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4fabf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725e64
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4fb3f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4fb3f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f85e5000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f85e5000)
  get Phys(data[n=1]=f85e6000)
  get Phys(data[n=1]=f85e7000)
  get Phys(data[n=1]=f85e8000)
  get Phys(data[n=1]=f85e9000)
  get Phys(data[n=2]=f85ea000)
  get Phys(data[n=2]=f85eb000)
  get Phys(data[n=2]=f85ec000)
  get Phys(data[n=2]=f85ed000)
  get Phys(data[n=2]=f85ee000)
  get Phys(data[n=2]=f85ef000)
  get Phys(data[n=3]=f85f0000)
  get Phys(data[n=3]=f85f1000)
  get Phys(data[n=4]=f85f2000)
  get Phys(data[n=4]=f85f3000)
  get Phys(data[n=4]=f85f4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4fb3f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4fb3f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726260
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4f9bf, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 4f9bf, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f85f3000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f85f3000)
  get Phys(data[n=1]=f85f4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4f9bf, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4f9bf count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\System32\ftfd.dll at F8594000 with 61 pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726280
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4fbbf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4fbbf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 822c0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=822c0000)
  get Phys(data[n=1]=822c1000)
  get Phys(data[n=1]=822c2000)
  get Phys(data[n=2]=822c3000)
  get Phys(data[n=2]=822c4000)
  get Phys(data[n=3]=822c5000)
  get Phys(data[n=4]=822c6000)
  get Phys(data[n=5]=822c7000)
  get Phys(data[n=5]=822c8000)
  get Phys(data[n=5]=822c9000)
  get Phys(data[n=5]=822ca000)
  get Phys(data[n=6]=822cb000)
  get Phys(data[n=7]=822cc000)
  get Phys(data[n=7]=822cd000)
  get Phys(data[n=7]=822ce000)
  get Phys(data[n=7]=822cf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4fbbf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4fbbf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726280
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4fc3f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4fc3f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 822d0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=822d0000)
  get Phys(data[n=1]=822d1000)
  get Phys(data[n=1]=822d2000)
  get Phys(data[n=1]=822d3000)
  get Phys(data[n=1]=822d4000)
  get Phys(data[n=1]=822d5000)
  get Phys(data[n=2]=822d6000)
  get Phys(data[n=2]=822d7000)
  get Phys(data[n=3]=822d8000)
  get Phys(data[n=3]=822d9000)
  get Phys(data[n=3]=822da000)
  get Phys(data[n=3]=822db000)
  get Phys(data[n=3]=822dc000)
  get Phys(data[n=3]=822dd000)
  get Phys(data[n=3]=822de000)
  get Phys(data[n=3]=822df000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4fc3f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4fc3f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726280
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4fcbf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4fcbf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 822e0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=822e0000)
  get Phys(data[n=1]=822e1000)
  get Phys(data[n=1]=822e2000)
  get Phys(data[n=1]=822e3000)
  get Phys(data[n=1]=822e4000)
  get Phys(data[n=1]=822e5000)
  get Phys(data[n=2]=822e6000)
  get Phys(data[n=2]=822e7000)
  get Phys(data[n=2]=822e8000)
  get Phys(data[n=2]=822e9000)
  get Phys(data[n=2]=822ea000)
  get Phys(data[n=2]=822eb000)
  get Phys(data[n=3]=822ec000)
  get Phys(data[n=3]=822ed000)
  get Phys(data[n=3]=822ee000)
  get Phys(data[n=3]=822ef000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4fcbf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4fcbf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726280
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4fd3f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4fd3f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 822f0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=822f0000)
  get Phys(data[n=1]=822f1000)
  get Phys(data[n=1]=822f2000)
  get Phys(data[n=1]=822f3000)
  get Phys(data[n=1]=822f4000)
  get Phys(data[n=2]=822f5000)
  get Phys(data[n=3]=822f6000)
  get Phys(data[n=3]=822f7000)
  get Phys(data[n=3]=822f8000)
  get Phys(data[n=3]=822f9000)
  get Phys(data[n=3]=822fa000)
  get Phys(data[n=3]=822fb000)
  get Phys(data[n=3]=822fc000)
  get Phys(data[n=4]=822fd000)
  get Phys(data[n=4]=822fe000)
  get Phys(data[n=4]=822ff000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4fd3f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4fd3f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87258ec
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4fdbf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4fdbf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f84d2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f84d2000)
  get Phys(data[n=1]=f84d3000)
  get Phys(data[n=1]=f84d4000)
  get Phys(data[n=1]=f84d5000)
  get Phys(data[n=1]=f84d6000)
  get Phys(data[n=1]=f84d7000)
  get Phys(data[n=2]=f84d8000)
  get Phys(data[n=2]=f84d9000)
  get Phys(data[n=2]=f84da000)
  get Phys(data[n=2]=f84db000)
  get Phys(data[n=2]=f84dc000)
  get Phys(data[n=2]=f84dd000)
  get Phys(data[n=3]=f84de000)
  get Phys(data[n=3]=f84df000)
  get Phys(data[n=3]=f84e0000)
  get Phys(data[n=3]=f84e1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4fdbf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4fdbf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87258ec
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4fe3f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4fe3f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f84e2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f84e2000)
  get Phys(data[n=1]=f84e3000)
  get Phys(data[n=1]=f84e4000)
  get Phys(data[n=1]=f84e5000)
  get Phys(data[n=1]=f84e6000)
  get Phys(data[n=2]=f84e7000)
  get Phys(data[n=3]=f84e8000)
  get Phys(data[n=3]=f84e9000)
  get Phys(data[n=3]=f84ea000)
  get Phys(data[n=3]=f84eb000)
  get Phys(data[n=3]=f84ec000)
  get Phys(data[n=3]=f84ed000)
  get Phys(data[n=3]=f84ee000)
  get Phys(data[n=4]=f84ef000)
  get Phys(data[n=4]=f84f0000)
  get Phys(data[n=4]=f84f1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4fe3f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4fe3f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87258ec
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4febf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4febf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f84f2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f84f2000)
  get Phys(data[n=1]=f84f3000)
  get Phys(data[n=1]=f84f4000)
  get Phys(data[n=2]=f84f5000)
  get Phys(data[n=2]=f84f6000)
  get Phys(data[n=3]=f84f7000)
  get Phys(data[n=4]=f84f8000)
  get Phys(data[n=5]=f84f9000)
  get Phys(data[n=5]=f84fa000)
  get Phys(data[n=5]=f84fb000)
  get Phys(data[n=5]=f84fc000)
  get Phys(data[n=6]=f84fd000)
  get Phys(data[n=7]=f84fe000)
  get Phys(data[n=7]=f84ff000)
  get Phys(data[n=7]=f8500000)
  get Phys(data[n=7]=f8501000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4febf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4febf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87258ec
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4ff3f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4ff3f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8502000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8502000)
  get Phys(data[n=1]=f8503000)
  get Phys(data[n=1]=f8504000)
  get Phys(data[n=1]=f8505000)
  get Phys(data[n=1]=f8506000)
  get Phys(data[n=1]=f8507000)
  get Phys(data[n=2]=f8508000)
  get Phys(data[n=2]=f8509000)
  get Phys(data[n=3]=f850a000)
  get Phys(data[n=3]=f850b000)
  get Phys(data[n=3]=f850c000)
  get Phys(data[n=3]=f850d000)
  get Phys(data[n=3]=f850e000)
  get Phys(data[n=3]=f850f000)
  get Phys(data[n=3]=f8510000)
  get Phys(data[n=3]=f8511000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4ff3f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4ff3f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87258ec
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4ffbf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4ffbf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f84d2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f84d2000)
  get Phys(data[n=1]=f84d3000)
  get Phys(data[n=1]=f84d4000)
  get Phys(data[n=1]=f84d5000)
  get Phys(data[n=1]=f84d6000)
  get Phys(data[n=1]=f84d7000)
  get Phys(data[n=2]=f84d8000)
  get Phys(data[n=2]=f84d9000)
  get Phys(data[n=2]=f84da000)
  get Phys(data[n=2]=f84db000)
  get Phys(data[n=2]=f84dc000)
  get Phys(data[n=2]=f84dd000)
  get Phys(data[n=3]=f84de000)
  get Phys(data[n=3]=f84df000)
  get Phys(data[n=3]=f84e0000)
  get Phys(data[n=3]=f84e1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4ffbf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4ffbf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87258ec
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5003f, OrigWordsRequested 0x6c00, DevSize 0x6c
IdeReadWrite (REQ): Starting sector is 5003f, Number of WORDS 0x6c00, DevSize 0x6c
AtapiDmaSetup: mode 0x45, data f84e2000, count d800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f84e2000)
  get Phys(data[n=1]=f84e3000)
  get Phys(data[n=1]=f84e4000)
  get Phys(data[n=1]=f84e5000)
  get Phys(data[n=1]=f84e6000)
  get Phys(data[n=2]=f84e7000)
  get Phys(data[n=3]=f84e8000)
  get Phys(data[n=3]=f84e9000)
  get Phys(data[n=3]=f84ea000)
  get Phys(data[n=3]=f84eb000)
  get Phys(data[n=3]=f84ec000)
  get Phys(data[n=3]=f84ed000)
  get Phys(data[n=3]=f84ee000)
  get Phys(data[n=4]=f84ef000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5003f, Count 0x6c(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5003f count 0x6c feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered d800, full size d800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 51d9f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 51d9f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f841c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f841c000)
  get Phys(data[n=1]=f841d000)
  get Phys(data[n=1]=f841e000)
  get Phys(data[n=1]=f841f000)
  get Phys(data[n=1]=f8420000)
  get Phys(data[n=1]=f8421000)
  get Phys(data[n=2]=f8422000)
  get Phys(data[n=2]=f8423000)
  get Phys(data[n=2]=f8424000)
  get Phys(data[n=2]=f8425000)
  get Phys(data[n=2]=f8426000)
  get Phys(data[n=2]=f8427000)
  get Phys(data[n=3]=f8428000)
  get Phys(data[n=3]=f8429000)
  get Phys(data[n=3]=f842a000)
  get Phys(data[n=3]=f842b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x51d9f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x51d9f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 51e1f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 51e1f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f842c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f842c000)
  get Phys(data[n=1]=f842d000)
  get Phys(data[n=1]=f842e000)
  get Phys(data[n=1]=f842f000)
  get Phys(data[n=1]=f8430000)
  get Phys(data[n=2]=f8431000)
  get Phys(data[n=3]=f8432000)
  get Phys(data[n=3]=f8433000)
  get Phys(data[n=3]=f8434000)
  get Phys(data[n=3]=f8435000)
  get Phys(data[n=3]=f8436000)
  get Phys(data[n=3]=f8437000)
  get Phys(data[n=3]=f8438000)
  get Phys(data[n=4]=f8439000)
  get Phys(data[n=4]=f843a000)
  get Phys(data[n=4]=f843b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x51e1f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x51e1f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 51e9f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 51e9f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f843c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f843c000)
  get Phys(data[n=1]=f843d000)
  get Phys(data[n=1]=f843e000)
  get Phys(data[n=2]=f843f000)
  get Phys(data[n=2]=f8440000)
  get Phys(data[n=3]=f8441000)
  get Phys(data[n=4]=f8442000)
  get Phys(data[n=5]=f8443000)
  get Phys(data[n=5]=f8444000)
  get Phys(data[n=5]=f8445000)
  get Phys(data[n=5]=f8446000)
  get Phys(data[n=6]=f8447000)
  get Phys(data[n=7]=f8448000)
  get Phys(data[n=7]=f8449000)
  get Phys(data[n=7]=f844a000)
  get Phys(data[n=7]=f844b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x51e9f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x51e9f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 51f1f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 51f1f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f844c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f844c000)
  get Phys(data[n=1]=f844d000)
  get Phys(data[n=1]=f844e000)
  get Phys(data[n=1]=f844f000)
  get Phys(data[n=1]=f8450000)
  get Phys(data[n=1]=f8451000)
  get Phys(data[n=2]=f8452000)
  get Phys(data[n=2]=f8453000)
  get Phys(data[n=3]=f8454000)
  get Phys(data[n=3]=f8455000)
  get Phys(data[n=3]=f8456000)
  get Phys(data[n=3]=f8457000)
  get Phys(data[n=3]=f8458000)
  get Phys(data[n=3]=f8459000)
  get Phys(data[n=3]=f845a000)
  get Phys(data[n=3]=f845b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x51f1f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x51f1f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 51f9f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 51f9f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f841c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f841c000)
  get Phys(data[n=1]=f841d000)
  get Phys(data[n=1]=f841e000)
  get Phys(data[n=1]=f841f000)
  get Phys(data[n=1]=f8420000)
  get Phys(data[n=1]=f8421000)
  get Phys(data[n=2]=f8422000)
  get Phys(data[n=2]=f8423000)
  get Phys(data[n=2]=f8424000)
  get Phys(data[n=2]=f8425000)
  get Phys(data[n=2]=f8426000)
  get Phys(data[n=2]=f8427000)
  get Phys(data[n=3]=f8428000)
  get Phys(data[n=3]=f8429000)
  get Phys(data[n=3]=f842a000)
  get Phys(data[n=3]=f842b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x51f9f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x51f9f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5201f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5201f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f842c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f842c000)
  get Phys(data[n=1]=f842d000)
  get Phys(data[n=1]=f842e000)
  get Phys(data[n=1]=f842f000)
  get Phys(data[n=1]=f8430000)
  get Phys(data[n=2]=f8431000)
  get Phys(data[n=3]=f8432000)
  get Phys(data[n=3]=f8433000)
  get Phys(data[n=3]=f8434000)
  get Phys(data[n=3]=f8435000)
  get Phys(data[n=3]=f8436000)
  get Phys(data[n=3]=f8437000)
  get Phys(data[n=3]=f8438000)
  get Phys(data[n=4]=f8439000)
  get Phys(data[n=4]=f843a000)
  get Phys(data[n=4]=f843b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5201f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5201f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5209f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5209f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f843c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f843c000)
  get Phys(data[n=1]=f843d000)
  get Phys(data[n=1]=f843e000)
  get Phys(data[n=2]=f843f000)
  get Phys(data[n=2]=f8440000)
  get Phys(data[n=3]=f8441000)
  get Phys(data[n=4]=f8442000)
  get Phys(data[n=5]=f8443000)
  get Phys(data[n=5]=f8444000)
  get Phys(data[n=5]=f8445000)
  get Phys(data[n=5]=f8446000)
  get Phys(data[n=6]=f8447000)
  get Phys(data[n=7]=f8448000)
  get Phys(data[n=7]=f8449000)
  get Phys(data[n=7]=f844a000)
  get Phys(data[n=7]=f844b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5209f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5209f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5211f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5211f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f844c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f844c000)
  get Phys(data[n=1]=f844d000)
  get Phys(data[n=1]=f844e000)
  get Phys(data[n=1]=f844f000)
  get Phys(data[n=1]=f8450000)
  get Phys(data[n=1]=f8451000)
  get Phys(data[n=2]=f8452000)
  get Phys(data[n=2]=f8453000)
  get Phys(data[n=3]=f8454000)
  get Phys(data[n=3]=f8455000)
  get Phys(data[n=3]=f8456000)
  get Phys(data[n=3]=f8457000)
  get Phys(data[n=3]=f8458000)
  get Phys(data[n=3]=f8459000)
  get Phys(data[n=3]=f845a000)
  get Phys(data[n=3]=f845b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5211f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5211f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5219f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5219f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f841c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f841c000)
  get Phys(data[n=1]=f841d000)
  get Phys(data[n=1]=f841e000)
  get Phys(data[n=1]=f841f000)
  get Phys(data[n=1]=f8420000)
  get Phys(data[n=1]=f8421000)
  get Phys(data[n=2]=f8422000)
  get Phys(data[n=2]=f8423000)
  get Phys(data[n=2]=f8424000)
  get Phys(data[n=2]=f8425000)
  get Phys(data[n=2]=f8426000)
  get Phys(data[n=2]=f8427000)
  get Phys(data[n=3]=f8428000)
  get Phys(data[n=3]=f8429000)
  get Phys(data[n=3]=f842a000)
  get Phys(data[n=3]=f842b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5219f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5219f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5221f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5221f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f842c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f842c000)
  get Phys(data[n=1]=f842d000)
  get Phys(data[n=1]=f842e000)
  get Phys(data[n=1]=f842f000)
  get Phys(data[n=1]=f8430000)
  get Phys(data[n=2]=f8431000)
  get Phys(data[n=3]=f8432000)
  get Phys(data[n=3]=f8433000)
  get Phys(data[n=3]=f8434000)
  get Phys(data[n=3]=f8435000)
  get Phys(data[n=3]=f8436000)
  get Phys(data[n=3]=f8437000)
  get Phys(data[n=3]=f8438000)
  get Phys(data[n=4]=f8439000)
  get Phys(data[n=4]=f843a000)
  get Phys(data[n=4]=f843b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5221f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5221f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5229f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5229f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f843c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f843c000)
  get Phys(data[n=1]=f843d000)
  get Phys(data[n=1]=f843e000)
  get Phys(data[n=2]=f843f000)
  get Phys(data[n=2]=f8440000)
  get Phys(data[n=3]=f8441000)
  get Phys(data[n=4]=f8442000)
  get Phys(data[n=5]=f8443000)
  get Phys(data[n=5]=f8444000)
  get Phys(data[n=5]=f8445000)
  get Phys(data[n=5]=f8446000)
  get Phys(data[n=6]=f8447000)
  get Phys(data[n=7]=f8448000)
  get Phys(data[n=7]=f8449000)
  get Phys(data[n=7]=f844a000)
  get Phys(data[n=7]=f844b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5229f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5229f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5231f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5231f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f844c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f844c000)
  get Phys(data[n=1]=f844d000)
  get Phys(data[n=1]=f844e000)
  get Phys(data[n=1]=f844f000)
  get Phys(data[n=1]=f8450000)
  get Phys(data[n=1]=f8451000)
  get Phys(data[n=2]=f8452000)
  get Phys(data[n=2]=f8453000)
  get Phys(data[n=3]=f8454000)
  get Phys(data[n=3]=f8455000)
  get Phys(data[n=3]=f8456000)
  get Phys(data[n=3]=f8457000)
  get Phys(data[n=3]=f8458000)
  get Phys(data[n=3]=f8459000)
  get Phys(data[n=3]=f845a000)
  get Phys(data[n=3]=f845b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5231f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5231f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5239f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5239f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f841c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f841c000)
  get Phys(data[n=1]=f841d000)
  get Phys(data[n=1]=f841e000)
  get Phys(data[n=1]=f841f000)
  get Phys(data[n=1]=f8420000)
  get Phys(data[n=1]=f8421000)
  get Phys(data[n=2]=f8422000)
  get Phys(data[n=2]=f8423000)
  get Phys(data[n=2]=f8424000)
  get Phys(data[n=2]=f8425000)
  get Phys(data[n=2]=f8426000)
  get Phys(data[n=2]=f8427000)
  get Phys(data[n=3]=f8428000)
  get Phys(data[n=3]=f8429000)
  get Phys(data[n=3]=f842a000)
  get Phys(data[n=3]=f842b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5239f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5239f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5241f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5241f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f842c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f842c000)
  get Phys(data[n=1]=f842d000)
  get Phys(data[n=1]=f842e000)
  get Phys(data[n=1]=f842f000)
  get Phys(data[n=1]=f8430000)
  get Phys(data[n=2]=f8431000)
  get Phys(data[n=3]=f8432000)
  get Phys(data[n=3]=f8433000)
  get Phys(data[n=3]=f8434000)
  get Phys(data[n=3]=f8435000)
  get Phys(data[n=3]=f8436000)
  get Phys(data[n=3]=f8437000)
  get Phys(data[n=3]=f8438000)
  get Phys(data[n=4]=f8439000)
  get Phys(data[n=4]=f843a000)
  get Phys(data[n=4]=f843b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5241f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5241f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5249f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5249f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f843c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f843c000)
  get Phys(data[n=1]=f843d000)
  get Phys(data[n=1]=f843e000)
  get Phys(data[n=2]=f843f000)
  get Phys(data[n=2]=f8440000)
  get Phys(data[n=3]=f8441000)
  get Phys(data[n=4]=f8442000)
  get Phys(data[n=5]=f8443000)
  get Phys(data[n=5]=f8444000)
  get Phys(data[n=5]=f8445000)
  get Phys(data[n=5]=f8446000)
  get Phys(data[n=6]=f8447000)
  get Phys(data[n=7]=f8448000)
  get Phys(data[n=7]=f8449000)
  get Phys(data[n=7]=f844a000)
  get Phys(data[n=7]=f844b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5249f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5249f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5251f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5251f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f844c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f844c000)
  get Phys(data[n=1]=f844d000)
  get Phys(data[n=1]=f844e000)
  get Phys(data[n=1]=f844f000)
  get Phys(data[n=1]=f8450000)
  get Phys(data[n=1]=f8451000)
  get Phys(data[n=2]=f8452000)
  get Phys(data[n=2]=f8453000)
  get Phys(data[n=3]=f8454000)
  get Phys(data[n=3]=f8455000)
  get Phys(data[n=3]=f8456000)
  get Phys(data[n=3]=f8457000)
  get Phys(data[n=3]=f8458000)
  get Phys(data[n=3]=f8459000)
  get Phys(data[n=3]=f845a000)
  get Phys(data[n=3]=f845b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5251f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5251f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5259f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5259f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f841c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f841c000)
  get Phys(data[n=1]=f841d000)
  get Phys(data[n=1]=f841e000)
  get Phys(data[n=1]=f841f000)
  get Phys(data[n=1]=f8420000)
  get Phys(data[n=1]=f8421000)
  get Phys(data[n=2]=f8422000)
  get Phys(data[n=2]=f8423000)
  get Phys(data[n=2]=f8424000)
  get Phys(data[n=2]=f8425000)
  get Phys(data[n=2]=f8426000)
  get Phys(data[n=2]=f8427000)
  get Phys(data[n=3]=f8428000)
  get Phys(data[n=3]=f8429000)
  get Phys(data[n=3]=f842a000)
  get Phys(data[n=3]=f842b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5259f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5259f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5261f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5261f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f842c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f842c000)
  get Phys(data[n=1]=f842d000)
  get Phys(data[n=1]=f842e000)
  get Phys(data[n=1]=f842f000)
  get Phys(data[n=1]=f8430000)
  get Phys(data[n=2]=f8431000)
  get Phys(data[n=3]=f8432000)
  get Phys(data[n=3]=f8433000)
  get Phys(data[n=3]=f8434000)
  get Phys(data[n=3]=f8435000)
  get Phys(data[n=3]=f8436000)
  get Phys(data[n=3]=f8437000)
  get Phys(data[n=3]=f8438000)
  get Phys(data[n=4]=f8439000)
  get Phys(data[n=4]=f843a000)
  get Phys(data[n=4]=f843b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5261f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5261f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5269f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5269f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f843c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f843c000)
  get Phys(data[n=1]=f843d000)
  get Phys(data[n=1]=f843e000)
  get Phys(data[n=2]=f843f000)
  get Phys(data[n=2]=f8440000)
  get Phys(data[n=3]=f8441000)
  get Phys(data[n=4]=f8442000)
  get Phys(data[n=5]=f8443000)
  get Phys(data[n=5]=f8444000)
  get Phys(data[n=5]=f8445000)
  get Phys(data[n=5]=f8446000)
  get Phys(data[n=6]=f8447000)
  get Phys(data[n=7]=f8448000)
  get Phys(data[n=7]=f8449000)
  get Phys(data[n=7]=f844a000)
  get Phys(data[n=7]=f844b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5269f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5269f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725a3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5271f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 5271f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data f844c000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f844c000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5271f, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x5271f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726028
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 406f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 406f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 823c3000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=823c3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x406f, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x406f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d60f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3d60f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=1]=f8557000)
  get Phys(data[n=1]=f8558000)
  get Phys(data[n=2]=f8559000)
  get Phys(data[n=2]=f855a000)
  get Phys(data[n=2]=f855b000)
  get Phys(data[n=2]=f855c000)
  get Phys(data[n=3]=f855d000)
  get Phys(data[n=3]=f855e000)
  get Phys(data[n=4]=f855f000)
  get Phys(data[n=4]=f8560000)
  get Phys(data[n=5]=f8561000)
  get Phys(data[n=6]=f8562000)
  get Phys(data[n=7]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d60f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d60f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d68f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3d68f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=2]=f8567000)
  get Phys(data[n=3]=f8568000)
  get Phys(data[n=3]=f8569000)
  get Phys(data[n=3]=f856a000)
  get Phys(data[n=3]=f856b000)
  get Phys(data[n=4]=f856c000)
  get Phys(data[n=4]=f856d000)
  get Phys(data[n=4]=f856e000)
  get Phys(data[n=4]=f856f000)
  get Phys(data[n=4]=f8570000)
  get Phys(data[n=4]=f8571000)
  get Phys(data[n=5]=f8572000)
  get Phys(data[n=5]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d68f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d68f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d70f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3d70f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8574000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=1]=f8576000)
  get Phys(data[n=1]=f8577000)
  get Phys(data[n=1]=f8578000)
  get Phys(data[n=1]=f8579000)
  get Phys(data[n=1]=f857a000)
  get Phys(data[n=1]=f857b000)
  get Phys(data[n=2]=f857c000)
  get Phys(data[n=2]=f857d000)
  get Phys(data[n=2]=f857e000)
  get Phys(data[n=2]=f857f000)
  get Phys(data[n=2]=f8580000)
  get Phys(data[n=2]=f8581000)
  get Phys(data[n=3]=f8582000)
  get Phys(data[n=3]=f8583000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d70f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d70f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d78f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3d78f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8584000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8584000)
  get Phys(data[n=1]=f8585000)
  get Phys(data[n=1]=f8586000)
  get Phys(data[n=1]=f8587000)
  get Phys(data[n=2]=f8588000)
  get Phys(data[n=2]=f8589000)
  get Phys(data[n=2]=f858a000)
  get Phys(data[n=2]=f858b000)
  get Phys(data[n=2]=f858c000)
  get Phys(data[n=2]=f858d000)
  get Phys(data[n=2]=f858e000)
  get Phys(data[n=2]=f858f000)
  get Phys(data[n=2]=f8590000)
  get Phys(data[n=3]=f8591000)
  get Phys(data[n=4]=f8592000)
  get Phys(data[n=4]=f8593000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d78f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d78f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3da0f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3da0f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 824f3000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=824f3000)
  get Phys(data[n=1]=824f4000)
  get Phys(data[n=1]=824f5000)
  get Phys(data[n=1]=824f6000)
  get Phys(data[n=1]=824f7000)
  get Phys(data[n=2]=824f8000)
  get Phys(data[n=2]=824f9000)
  get Phys(data[n=2]=824fa000)
  get Phys(data[n=2]=824fb000)
  get Phys(data[n=3]=824fc000)
  get Phys(data[n=3]=824fd000)
  get Phys(data[n=4]=824fe000)
  get Phys(data[n=4]=824ff000)
  get Phys(data[n=5]=82500000)
  get Phys(data[n=6]=82501000)
  get Phys(data[n=7]=82502000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3da0f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3da0f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3da8f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3da8f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 82503000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82503000)
  get Phys(data[n=1]=82504000)
  get Phys(data[n=1]=82505000)
  get Phys(data[n=2]=82506000)
  get Phys(data[n=3]=82507000)
  get Phys(data[n=3]=82508000)
  get Phys(data[n=3]=82509000)
  get Phys(data[n=3]=8250a000)
  get Phys(data[n=4]=8250b000)
  get Phys(data[n=4]=8250c000)
  get Phys(data[n=4]=8250d000)
  get Phys(data[n=4]=8250e000)
  get Phys(data[n=4]=8250f000)
  get Phys(data[n=4]=82510000)
  get Phys(data[n=5]=82511000)
  get Phys(data[n=5]=82512000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3da8f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3da8f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3db0f, OrigWordsRequested 0x7f00, DevSize 0x7f
IdeReadWrite (REQ): Starting sector is 3db0f, Number of WORDS 0x7f00, DevSize 0x7f
AtapiDmaSetup: mode 0x45, data 82513000, count fe00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82513000)
  get Phys(data[n=1]=82514000)
  get Phys(data[n=1]=82515000)
  get Phys(data[n=1]=82516000)
  get Phys(data[n=1]=82517000)
  get Phys(data[n=1]=82518000)
  get Phys(data[n=1]=82519000)
  get Phys(data[n=1]=8251a000)
  get Phys(data[n=2]=8251b000)
  get Phys(data[n=2]=8251c000)
  get Phys(data[n=2]=8251d000)
  get Phys(data[n=2]=8251e000)
  get Phys(data[n=2]=8251f000)
  get Phys(data[n=2]=82520000)
  get Phys(data[n=3]=82521000)
  get Phys(data[n=3]=82522000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3db0f, Count 0x7f(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3db0f count 0x7f feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered fe00, full size fe00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3db8f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3db8f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=2]=f8556000)
  get Phys(data[n=2]=f8557000)
  get Phys(data[n=3]=f8558000)
  get Phys(data[n=3]=f8559000)
  get Phys(data[n=4]=f855a000)
  get Phys(data[n=5]=f855b000)
  get Phys(data[n=6]=f855c000)
  get Phys(data[n=6]=f855d000)
  get Phys(data[n=6]=f855e000)
  get Phys(data[n=6]=f855f000)
  get Phys(data[n=7]=f8560000)
  get Phys(data[n=8]=f8561000)
  get Phys(data[n=8]=f8562000)
  get Phys(data[n=8]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3db8f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3db8f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3dc0f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3dc0f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=1]=f8567000)
  get Phys(data[n=1]=f8568000)
  get Phys(data[n=1]=f8569000)
  get Phys(data[n=1]=f856a000)
  get Phys(data[n=2]=f856b000)
  get Phys(data[n=2]=f856c000)
  get Phys(data[n=3]=f856d000)
  get Phys(data[n=3]=f856e000)
  get Phys(data[n=3]=f856f000)
  get Phys(data[n=3]=f8570000)
  get Phys(data[n=3]=f8571000)
  get Phys(data[n=3]=f8572000)
  get Phys(data[n=3]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3dc0f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3dc0f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3dc8f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3dc8f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8574000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=1]=f8576000)
  get Phys(data[n=1]=f8577000)
  get Phys(data[n=1]=f8578000)
  get Phys(data[n=1]=f8579000)
  get Phys(data[n=1]=f857a000)
  get Phys(data[n=2]=f857b000)
  get Phys(data[n=2]=f857c000)
  get Phys(data[n=2]=f857d000)
  get Phys(data[n=2]=f857e000)
  get Phys(data[n=2]=f857f000)
  get Phys(data[n=2]=f8580000)
  get Phys(data[n=3]=f8581000)
  get Phys(data[n=3]=f8582000)
  get Phys(data[n=3]=f8583000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3dc8f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3dc8f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3dd0f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3dd0f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8584000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8584000)
  get Phys(data[n=1]=f8585000)
  get Phys(data[n=1]=f8586000)
  get Phys(data[n=1]=f8587000)
  get Phys(data[n=1]=f8588000)
  get Phys(data[n=1]=f8589000)
  get Phys(data[n=2]=f858a000)
  get Phys(data[n=3]=f858b000)
  get Phys(data[n=3]=f858c000)
  get Phys(data[n=3]=f858d000)
  get Phys(data[n=3]=f858e000)
  get Phys(data[n=3]=f858f000)
  get Phys(data[n=3]=f8590000)
  get Phys(data[n=3]=f8591000)
  get Phys(data[n=4]=f8592000)
  get Phys(data[n=4]=f8593000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3dd0f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3dd0f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3df8f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3df8f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 82618000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82618000)
  get Phys(data[n=1]=82619000)
  get Phys(data[n=2]=8261a000)
  get Phys(data[n=2]=8261b000)
  get Phys(data[n=3]=8261c000)
  get Phys(data[n=3]=8261d000)
  get Phys(data[n=4]=8261e000)
  get Phys(data[n=5]=8261f000)
  get Phys(data[n=6]=82620000)
  get Phys(data[n=6]=82621000)
  get Phys(data[n=6]=82622000)
  get Phys(data[n=6]=82623000)
  get Phys(data[n=7]=82624000)
  get Phys(data[n=8]=82625000)
  get Phys(data[n=8]=82626000)
  get Phys(data[n=8]=82627000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3df8f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3df8f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e00f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e00f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 82628000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82628000)
  get Phys(data[n=1]=82629000)
  get Phys(data[n=1]=8262a000)
  get Phys(data[n=1]=8262b000)
  get Phys(data[n=1]=8262c000)
  get Phys(data[n=1]=8262d000)
  get Phys(data[n=1]=8262e000)
  get Phys(data[n=2]=8262f000)
  get Phys(data[n=2]=82630000)
  get Phys(data[n=3]=82631000)
  get Phys(data[n=3]=82632000)
  get Phys(data[n=3]=82633000)
  get Phys(data[n=3]=82634000)
  get Phys(data[n=3]=82635000)
  get Phys(data[n=3]=82636000)
  get Phys(data[n=3]=82637000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e00f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e00f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e08f, OrigWordsRequested 0x2200, DevSize 0x22
IdeReadWrite (REQ): Starting sector is 3e08f, Number of WORDS 0x2200, DevSize 0x22
AtapiDmaSetup: mode 0x45, data 82638000, count 4400, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82638000)
  get Phys(data[n=1]=82639000)
  get Phys(data[n=1]=8263a000)
  get Phys(data[n=1]=8263b000)
  get Phys(data[n=1]=8263c000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e08f, Count 0x22(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e08f count 0x22 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 4400, full size 4400
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e0b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e0b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=1]=f8557000)
  get Phys(data[n=1]=f8558000)
  get Phys(data[n=2]=f8559000)
  get Phys(data[n=3]=f855a000)
  get Phys(data[n=3]=f855b000)
  get Phys(data[n=3]=f855c000)
  get Phys(data[n=3]=f855d000)
  get Phys(data[n=4]=f855e000)
  get Phys(data[n=4]=f855f000)
  get Phys(data[n=4]=f8560000)
  get Phys(data[n=4]=f8561000)
  get Phys(data[n=4]=f8562000)
  get Phys(data[n=4]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e0b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e0b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e137, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e137, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=2]=f8566000)
  get Phys(data[n=2]=f8567000)
  get Phys(data[n=2]=f8568000)
  get Phys(data[n=2]=f8569000)
  get Phys(data[n=2]=f856a000)
  get Phys(data[n=2]=f856b000)
  get Phys(data[n=2]=f856c000)
  get Phys(data[n=2]=f856d000)
  get Phys(data[n=3]=f856e000)
  get Phys(data[n=3]=f856f000)
  get Phys(data[n=3]=f8570000)
  get Phys(data[n=3]=f8571000)
  get Phys(data[n=3]=f8572000)
  get Phys(data[n=3]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e137, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e137 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e1b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e1b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8574000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=1]=f8576000)
  get Phys(data[n=1]=f8577000)
  get Phys(data[n=1]=f8578000)
  get Phys(data[n=1]=f8579000)
  get Phys(data[n=2]=f857a000)
  get Phys(data[n=2]=f857b000)
  get Phys(data[n=2]=f857c000)
  get Phys(data[n=2]=f857d000)
  get Phys(data[n=2]=f857e000)
  get Phys(data[n=2]=f857f000)
  get Phys(data[n=2]=f8580000)
  get Phys(data[n=2]=f8581000)
  get Phys(data[n=2]=f8582000)
  get Phys(data[n=3]=f8583000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e1b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e1b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e237, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e237, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8584000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8584000)
  get Phys(data[n=1]=f8585000)
  get Phys(data[n=1]=f8586000)
  get Phys(data[n=1]=f8587000)
  get Phys(data[n=1]=f8588000)
  get Phys(data[n=1]=f8589000)
  get Phys(data[n=1]=f858a000)
  get Phys(data[n=2]=f858b000)
  get Phys(data[n=2]=f858c000)
  get Phys(data[n=2]=f858d000)
  get Phys(data[n=2]=f858e000)
  get Phys(data[n=3]=f858f000)
  get Phys(data[n=3]=f8590000)
  get Phys(data[n=4]=f8591000)
  get Phys(data[n=4]=f8592000)
  get Phys(data[n=5]=f8593000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e237, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e237 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e2b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e2b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 8272e000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=8272e000)
  get Phys(data[n=1]=8272f000)
  get Phys(data[n=1]=82730000)
  get Phys(data[n=1]=82731000)
  get Phys(data[n=1]=82732000)
  get Phys(data[n=2]=82733000)
  get Phys(data[n=3]=82734000)
  get Phys(data[n=3]=82735000)
  get Phys(data[n=3]=82736000)
  get Phys(data[n=3]=82737000)
  get Phys(data[n=4]=82738000)
  get Phys(data[n=4]=82739000)
  get Phys(data[n=4]=8273a000)
  get Phys(data[n=4]=8273b000)
  get Phys(data[n=4]=8273c000)
  get Phys(data[n=4]=8273d000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e2b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e2b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e337, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e337, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 8273e000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=8273e000)
  get Phys(data[n=1]=8273f000)
  get Phys(data[n=2]=82740000)
  get Phys(data[n=2]=82741000)
  get Phys(data[n=2]=82742000)
  get Phys(data[n=2]=82743000)
  get Phys(data[n=2]=82744000)
  get Phys(data[n=2]=82745000)
  get Phys(data[n=2]=82746000)
  get Phys(data[n=2]=82747000)
  get Phys(data[n=3]=82748000)
  get Phys(data[n=3]=82749000)
  get Phys(data[n=3]=8274a000)
  get Phys(data[n=3]=8274b000)
  get Phys(data[n=3]=8274c000)
  get Phys(data[n=3]=8274d000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e337, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e337 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e3b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e3b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 8274e000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=8274e000)
  get Phys(data[n=1]=8274f000)
  get Phys(data[n=1]=82750000)
  get Phys(data[n=1]=82751000)
  get Phys(data[n=1]=82752000)
  get Phys(data[n=1]=82753000)
  get Phys(data[n=2]=82754000)
  get Phys(data[n=2]=82755000)
  get Phys(data[n=2]=82756000)
  get Phys(data[n=2]=82757000)
  get Phys(data[n=2]=82758000)
  get Phys(data[n=2]=82759000)
  get Phys(data[n=2]=8275a000)
  get Phys(data[n=2]=8275b000)
  get Phys(data[n=2]=8275c000)
  get Phys(data[n=3]=8275d000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e3b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e3b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e437, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e437, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 8275e000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=8275e000)
  get Phys(data[n=1]=8275f000)
  get Phys(data[n=1]=82760000)
  get Phys(data[n=1]=82761000)
  get Phys(data[n=1]=82762000)
  get Phys(data[n=1]=82763000)
  get Phys(data[n=1]=82764000)
  get Phys(data[n=2]=82765000)
  get Phys(data[n=2]=82766000)
  get Phys(data[n=2]=82767000)
  get Phys(data[n=2]=82768000)
  get Phys(data[n=3]=82769000)
  get Phys(data[n=3]=8276a000)
  get Phys(data[n=4]=8276b000)
  get Phys(data[n=4]=8276c000)
  get Phys(data[n=5]=8276d000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e437, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e437 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725fe0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e4b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e4b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 8276e000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=8276e000)
  get Phys(data[n=1]=8276f000)
  get Phys(data[n=1]=82770000)
  get Phys(data[n=1]=82771000)
  get Phys(data[n=1]=82772000)
  get Phys(data[n=2]=82773000)
  get Phys(data[n=3]=82774000)
  get Phys(data[n=3]=82775000)
  get Phys(data[n=3]=82776000)
  get Phys(data[n=3]=82777000)
  get Phys(data[n=4]=82778000)
  get Phys(data[n=4]=82779000)
  get Phys(data[n=4]=8277a000)
  get Phys(data[n=4]=8277b000)
  get Phys(data[n=4]=8277c000)
  get Phys(data[n=4]=8277d000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e4b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e4b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725fe0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e537, OrigWordsRequested 0x2a00, DevSize 0x2a
IdeReadWrite (REQ): Starting sector is 3e537, Number of WORDS 0x2a00, DevSize 0x2a
AtapiDmaSetup: mode 0x45, data 8277e000, count 5400, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=8277e000)
  get Phys(data[n=1]=8277f000)
  get Phys(data[n=2]=82780000)
  get Phys(data[n=2]=82781000)
  get Phys(data[n=2]=82782000)
  get Phys(data[n=2]=82783000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e537, Count 0x2a(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e537 count 0x2a feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 5400, full size 5400
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e567, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e567, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=1]=f8557000)
  get Phys(data[n=2]=f8558000)
  get Phys(data[n=2]=f8559000)
  get Phys(data[n=2]=f855a000)
  get Phys(data[n=2]=f855b000)
  get Phys(data[n=2]=f855c000)
  get Phys(data[n=2]=f855d000)
  get Phys(data[n=3]=f855e000)
  get Phys(data[n=3]=f855f000)
  get Phys(data[n=4]=f8560000)
  get Phys(data[n=4]=f8561000)
  get Phys(data[n=4]=f8562000)
  get Phys(data[n=4]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e567, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e567 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e5e7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e5e7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=1]=f8567000)
  get Phys(data[n=2]=f8568000)
  get Phys(data[n=2]=f8569000)
  get Phys(data[n=2]=f856a000)
  get Phys(data[n=2]=f856b000)
  get Phys(data[n=2]=f856c000)
  get Phys(data[n=2]=f856d000)
  get Phys(data[n=3]=f856e000)
  get Phys(data[n=3]=f856f000)
  get Phys(data[n=3]=f8570000)
  get Phys(data[n=3]=f8571000)
  get Phys(data[n=3]=f8572000)
  get Phys(data[n=3]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e5e7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e5e7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e667, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e667, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8574000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=1]=f8576000)
  get Phys(data[n=1]=f8577000)
  get Phys(data[n=1]=f8578000)
  get Phys(data[n=1]=f8579000)
  get Phys(data[n=1]=f857a000)
  get Phys(data[n=1]=f857b000)
  get Phys(data[n=1]=f857c000)
  get Phys(data[n=2]=f857d000)
  get Phys(data[n=3]=f857e000)
  get Phys(data[n=3]=f857f000)
  get Phys(data[n=3]=f8580000)
  get Phys(data[n=3]=f8581000)
  get Phys(data[n=3]=f8582000)
  get Phys(data[n=3]=f8583000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e667, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e667 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e6e7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e6e7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8584000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8584000)
  get Phys(data[n=1]=f8585000)
  get Phys(data[n=1]=f8586000)
  get Phys(data[n=1]=f8587000)
  get Phys(data[n=1]=f8588000)
  get Phys(data[n=2]=f8589000)
  get Phys(data[n=2]=f858a000)
  get Phys(data[n=3]=f858b000)
  get Phys(data[n=3]=f858c000)
  get Phys(data[n=4]=f858d000)
  get Phys(data[n=5]=f858e000)
  get Phys(data[n=6]=f858f000)
  get Phys(data[n=6]=f8590000)
  get Phys(data[n=6]=f8591000)
  get Phys(data[n=6]=f8592000)
  get Phys(data[n=7]=f8593000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e6e7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e6e7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e767, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e767, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 82884000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82884000)
  get Phys(data[n=1]=82885000)
  get Phys(data[n=1]=82886000)
  get Phys(data[n=2]=82887000)
  get Phys(data[n=2]=82888000)
  get Phys(data[n=2]=82889000)
  get Phys(data[n=2]=8288a000)
  get Phys(data[n=2]=8288b000)
  get Phys(data[n=2]=8288c000)
  get Phys(data[n=3]=8288d000)
  get Phys(data[n=3]=8288e000)
  get Phys(data[n=4]=8288f000)
  get Phys(data[n=4]=82890000)
  get Phys(data[n=4]=82891000)
  get Phys(data[n=4]=82892000)
  get Phys(data[n=4]=82893000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e767, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e767 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e7e7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e7e7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 82894000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82894000)
  get Phys(data[n=1]=82895000)
  get Phys(data[n=1]=82896000)
  get Phys(data[n=2]=82897000)
  get Phys(data[n=2]=82898000)
  get Phys(data[n=2]=82899000)
  get Phys(data[n=2]=8289a000)
  get Phys(data[n=2]=8289b000)
  get Phys(data[n=2]=8289c000)
  get Phys(data[n=3]=8289d000)
  get Phys(data[n=3]=8289e000)
  get Phys(data[n=3]=8289f000)
  get Phys(data[n=3]=828a0000)
  get Phys(data[n=3]=828a1000)
  get Phys(data[n=3]=828a2000)
  get Phys(data[n=4]=828a3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e7e7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e7e7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e867, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e867, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 828a4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=828a4000)
  get Phys(data[n=1]=828a5000)
  get Phys(data[n=1]=828a6000)
  get Phys(data[n=1]=828a7000)
  get Phys(data[n=1]=828a8000)
  get Phys(data[n=1]=828a9000)
  get Phys(data[n=1]=828aa000)
  get Phys(data[n=1]=828ab000)
  get Phys(data[n=2]=828ac000)
  get Phys(data[n=3]=828ad000)
  get Phys(data[n=3]=828ae000)
  get Phys(data[n=3]=828af000)
  get Phys(data[n=3]=828b0000)
  get Phys(data[n=3]=828b1000)
  get Phys(data[n=3]=828b2000)
  get Phys(data[n=3]=828b3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e867, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e867 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e8e7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e8e7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 828b4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=828b4000)
  get Phys(data[n=1]=828b5000)
  get Phys(data[n=1]=828b6000)
  get Phys(data[n=1]=828b7000)
  get Phys(data[n=2]=828b8000)
  get Phys(data[n=2]=828b9000)
  get Phys(data[n=3]=828ba000)
  get Phys(data[n=3]=828bb000)
  get Phys(data[n=4]=828bc000)
  get Phys(data[n=5]=828bd000)
  get Phys(data[n=6]=828be000)
  get Phys(data[n=6]=828bf000)
  get Phys(data[n=6]=828c0000)
  get Phys(data[n=6]=828c1000)
  get Phys(data[n=7]=828c2000)
  get Phys(data[n=8]=828c3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e8e7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e8e7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725fe0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e967, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3e967, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 828c4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=828c4000)
  get Phys(data[n=1]=828c5000)
  get Phys(data[n=1]=828c6000)
  get Phys(data[n=2]=828c7000)
  get Phys(data[n=2]=828c8000)
  get Phys(data[n=2]=828c9000)
  get Phys(data[n=2]=828ca000)
  get Phys(data[n=2]=828cb000)
  get Phys(data[n=2]=828cc000)
  get Phys(data[n=3]=828cd000)
  get Phys(data[n=3]=828ce000)
  get Phys(data[n=4]=828cf000)
  get Phys(data[n=4]=828d0000)
  get Phys(data[n=4]=828d1000)
  get Phys(data[n=4]=828d2000)
  get Phys(data[n=4]=828d3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e967, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e967 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725fe0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3e9e7, OrigWordsRequested 0x2b00, DevSize 0x2b
IdeReadWrite (REQ): Starting sector is 3e9e7, Number of WORDS 0x2b00, DevSize 0x2b
AtapiDmaSetup: mode 0x45, data 828d4000, count 5600, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=828d4000)
  get Phys(data[n=1]=828d5000)
  get Phys(data[n=1]=828d6000)
  get Phys(data[n=2]=828d7000)
  get Phys(data[n=2]=828d8000)
  get Phys(data[n=2]=828d9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3e9e7, Count 0x2b(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3e9e7 count 0x2b feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 5600, full size 5600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ea17, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3ea17, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=2]=f8556000)
  get Phys(data[n=2]=f8557000)
  get Phys(data[n=3]=f8558000)
  get Phys(data[n=3]=f8559000)
  get Phys(data[n=3]=f855a000)
  get Phys(data[n=3]=f855b000)
  get Phys(data[n=3]=f855c000)
  get Phys(data[n=3]=f855d000)
  get Phys(data[n=3]=f855e000)
  get Phys(data[n=3]=f855f000)
  get Phys(data[n=4]=f8560000)
  get Phys(data[n=4]=f8561000)
  get Phys(data[n=4]=f8562000)
  get Phys(data[n=4]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ea17, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3ea17 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ea97, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3ea97, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=2]=f8566000)
  get Phys(data[n=2]=f8567000)
  get Phys(data[n=2]=f8568000)
  get Phys(data[n=2]=f8569000)
  get Phys(data[n=2]=f856a000)
  get Phys(data[n=2]=f856b000)
  get Phys(data[n=3]=f856c000)
  get Phys(data[n=3]=f856d000)
  get Phys(data[n=3]=f856e000)
  get Phys(data[n=3]=f856f000)
  get Phys(data[n=3]=f8570000)
  get Phys(data[n=3]=f8571000)
  get Phys(data[n=3]=f8572000)
  get Phys(data[n=3]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ea97, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3ea97 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3eb17, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3eb17, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8574000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=2]=f8576000)
  get Phys(data[n=2]=f8577000)
  get Phys(data[n=2]=f8578000)
  get Phys(data[n=2]=f8579000)
  get Phys(data[n=2]=f857a000)
  get Phys(data[n=2]=f857b000)
  get Phys(data[n=2]=f857c000)
  get Phys(data[n=3]=f857d000)
  get Phys(data[n=3]=f857e000)
  get Phys(data[n=3]=f857f000)
  get Phys(data[n=3]=f8580000)
  get Phys(data[n=4]=f8581000)
  get Phys(data[n=4]=f8582000)
  get Phys(data[n=5]=f8583000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3eb17, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3eb17 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3eb97, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3eb97, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8584000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8584000)
  get Phys(data[n=1]=f8585000)
  get Phys(data[n=2]=f8586000)
  get Phys(data[n=3]=f8587000)
  get Phys(data[n=3]=f8588000)
  get Phys(data[n=3]=f8589000)
  get Phys(data[n=3]=f858a000)
  get Phys(data[n=4]=f858b000)
  get Phys(data[n=5]=f858c000)
  get Phys(data[n=5]=f858d000)
  get Phys(data[n=5]=f858e000)
  get Phys(data[n=5]=f858f000)
  get Phys(data[n=6]=f8590000)
  get Phys(data[n=6]=f8591000)
  get Phys(data[n=6]=f8592000)
  get Phys(data[n=6]=f8593000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3eb97, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3eb97 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ec17, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3ec17, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 82996000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82996000)
  get Phys(data[n=1]=82997000)
  get Phys(data[n=2]=82998000)
  get Phys(data[n=2]=82999000)
  get Phys(data[n=3]=8299a000)
  get Phys(data[n=3]=8299b000)
  get Phys(data[n=3]=8299c000)
  get Phys(data[n=3]=8299d000)
  get Phys(data[n=3]=8299e000)
  get Phys(data[n=3]=8299f000)
  get Phys(data[n=3]=829a0000)
  get Phys(data[n=3]=829a1000)
  get Phys(data[n=4]=829a2000)
  get Phys(data[n=4]=829a3000)
  get Phys(data[n=4]=829a4000)
  get Phys(data[n=4]=829a5000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ec17, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3ec17 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ec97, OrigWordsRequested 0xc00, DevSize 0xc
IdeReadWrite (REQ): Starting sector is 3ec97, Number of WORDS 0xc00, DevSize 0xc
AtapiDmaSetup: mode 0x45, data 829a6000, count 1800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=829a6000)
  get Phys(data[n=1]=829a7000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ec97, Count 0xc(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3ec97 count 0xc feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1800, full size 1800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3eca7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3eca7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=1]=f8557000)
  get Phys(data[n=1]=f8558000)
  get Phys(data[n=1]=f8559000)
  get Phys(data[n=1]=f855a000)
  get Phys(data[n=1]=f855b000)
  get Phys(data[n=1]=f855c000)
  get Phys(data[n=2]=f855d000)
  get Phys(data[n=2]=f855e000)
  get Phys(data[n=2]=f855f000)
  get Phys(data[n=2]=f8560000)
  get Phys(data[n=2]=f8561000)
  get Phys(data[n=2]=f8562000)
  get Phys(data[n=3]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3eca7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3eca7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ed27, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3ed27, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=1]=f8567000)
  get Phys(data[n=1]=f8568000)
  get Phys(data[n=2]=f8569000)
  get Phys(data[n=2]=f856a000)
  get Phys(data[n=2]=f856b000)
  get Phys(data[n=2]=f856c000)
  get Phys(data[n=2]=f856d000)
  get Phys(data[n=2]=f856e000)
  get Phys(data[n=2]=f856f000)
  get Phys(data[n=2]=f8570000)
  get Phys(data[n=2]=f8571000)
  get Phys(data[n=3]=f8572000)
  get Phys(data[n=4]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ed27, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3ed27 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3eda7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3eda7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8574000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=1]=f8576000)
  get Phys(data[n=1]=f8577000)
  get Phys(data[n=1]=f8578000)
  get Phys(data[n=1]=f8579000)
  get Phys(data[n=2]=f857a000)
  get Phys(data[n=2]=f857b000)
  get Phys(data[n=2]=f857c000)
  get Phys(data[n=2]=f857d000)
  get Phys(data[n=3]=f857e000)
  get Phys(data[n=3]=f857f000)
  get Phys(data[n=4]=f8580000)
  get Phys(data[n=4]=f8581000)
  get Phys(data[n=5]=f8582000)
  get Phys(data[n=6]=f8583000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3eda7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3eda7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ee27, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3ee27, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8584000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8584000)
  get Phys(data[n=1]=f8585000)
  get Phys(data[n=1]=f8586000)
  get Phys(data[n=1]=f8587000)
  get Phys(data[n=2]=f8588000)
  get Phys(data[n=3]=f8589000)
  get Phys(data[n=3]=f858a000)
  get Phys(data[n=3]=f858b000)
  get Phys(data[n=3]=f858c000)
  get Phys(data[n=4]=f858d000)
  get Phys(data[n=4]=f858e000)
  get Phys(data[n=4]=f858f000)
  get Phys(data[n=4]=f8590000)
  get Phys(data[n=4]=f8591000)
  get Phys(data[n=4]=f8592000)
  get Phys(data[n=5]=f8593000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ee27, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3ee27 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726048
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3eea7, OrigWordsRequested 0x6500, DevSize 0x65
IdeReadWrite (REQ): Starting sector is 3eea7, Number of WORDS 0x6500, DevSize 0x65
AtapiDmaSetup: mode 0x45, data 82a63000, count ca00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82a63000)
  get Phys(data[n=1]=82a64000)
  get Phys(data[n=1]=82a65000)
  get Phys(data[n=1]=82a66000)
  get Phys(data[n=1]=82a67000)
  get Phys(data[n=1]=82a68000)
  get Phys(data[n=1]=82a69000)
  get Phys(data[n=1]=82a6a000)
  get Phys(data[n=1]=82a6b000)
  get Phys(data[n=2]=82a6c000)
  get Phys(data[n=2]=82a6d000)
  get Phys(data[n=2]=82a6e000)
  get Phys(data[n=2]=82a6f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3eea7, Count 0x65(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3eea7 count 0x65 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered ca00, full size ca00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ef0f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3ef0f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=1]=f8557000)
  get Phys(data[n=1]=f8558000)
  get Phys(data[n=1]=f8559000)
  get Phys(data[n=2]=f855a000)
  get Phys(data[n=2]=f855b000)
  get Phys(data[n=2]=f855c000)
  get Phys(data[n=2]=f855d000)
  get Phys(data[n=2]=f855e000)
  get Phys(data[n=2]=f855f000)
  get Phys(data[n=3]=f8560000)
  get Phys(data[n=3]=f8561000)
  get Phys(data[n=3]=f8562000)
  get Phys(data[n=3]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ef0f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3ef0f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ef8f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3ef8f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=2]=f8566000)
  get Phys(data[n=2]=f8567000)
  get Phys(data[n=2]=f8568000)
  get Phys(data[n=2]=f8569000)
  get Phys(data[n=2]=f856a000)
  get Phys(data[n=2]=f856b000)
  get Phys(data[n=2]=f856c000)
  get Phys(data[n=2]=f856d000)
  get Phys(data[n=2]=f856e000)
  get Phys(data[n=3]=f856f000)
  get Phys(data[n=4]=f8570000)
  get Phys(data[n=4]=f8571000)
  get Phys(data[n=4]=f8572000)
  get Phys(data[n=4]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ef8f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3ef8f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f00f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3f00f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8574000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=1]=f8576000)
  get Phys(data[n=2]=f8577000)
  get Phys(data[n=2]=f8578000)
  get Phys(data[n=2]=f8579000)
  get Phys(data[n=2]=f857a000)
  get Phys(data[n=3]=f857b000)
  get Phys(data[n=3]=f857c000)
  get Phys(data[n=4]=f857d000)
  get Phys(data[n=4]=f857e000)
  get Phys(data[n=5]=f857f000)
  get Phys(data[n=6]=f8580000)
  get Phys(data[n=7]=f8581000)
  get Phys(data[n=7]=f8582000)
  get Phys(data[n=7]=f8583000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f00f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f00f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f08f, OrigWordsRequested 0x4d00, DevSize 0x4d
IdeReadWrite (REQ): Starting sector is 3f08f, Number of WORDS 0x4d00, DevSize 0x4d
AtapiDmaSetup: mode 0x45, data f8584000, count 9a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8584000)
  get Phys(data[n=1]=f8585000)
  get Phys(data[n=2]=f8586000)
  get Phys(data[n=2]=f8587000)
  get Phys(data[n=2]=f8588000)
  get Phys(data[n=2]=f8589000)
  get Phys(data[n=3]=f858a000)
  get Phys(data[n=3]=f858b000)
  get Phys(data[n=3]=f858c000)
  get Phys(data[n=3]=f858d000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f08f, Count 0x4d(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f08f count 0x4d feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 9a00, full size 9a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f0df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3f0df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=2]=f8557000)
  get Phys(data[n=2]=f8558000)
  get Phys(data[n=2]=f8559000)
  get Phys(data[n=2]=f855a000)
  get Phys(data[n=2]=f855b000)
  get Phys(data[n=2]=f855c000)
  get Phys(data[n=3]=f855d000)
  get Phys(data[n=3]=f855e000)
  get Phys(data[n=3]=f855f000)
  get Phys(data[n=3]=f8560000)
  get Phys(data[n=3]=f8561000)
  get Phys(data[n=3]=f8562000)
  get Phys(data[n=4]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f0df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f0df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f15f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3f15f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=1]=f8567000)
  get Phys(data[n=1]=f8568000)
  get Phys(data[n=1]=f8569000)
  get Phys(data[n=1]=f856a000)
  get Phys(data[n=1]=f856b000)
  get Phys(data[n=2]=f856c000)
  get Phys(data[n=3]=f856d000)
  get Phys(data[n=3]=f856e000)
  get Phys(data[n=3]=f856f000)
  get Phys(data[n=3]=f8570000)
  get Phys(data[n=3]=f8571000)
  get Phys(data[n=3]=f8572000)
  get Phys(data[n=3]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f15f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f15f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f1df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3f1df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8574000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=1]=f8576000)
  get Phys(data[n=1]=f8577000)
  get Phys(data[n=2]=f8578000)
  get Phys(data[n=2]=f8579000)
  get Phys(data[n=3]=f857a000)
  get Phys(data[n=3]=f857b000)
  get Phys(data[n=4]=f857c000)
  get Phys(data[n=5]=f857d000)
  get Phys(data[n=6]=f857e000)
  get Phys(data[n=6]=f857f000)
  get Phys(data[n=6]=f8580000)
  get Phys(data[n=6]=f8581000)
  get Phys(data[n=7]=f8582000)
  get Phys(data[n=8]=f8583000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f1df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f1df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f25f, OrigWordsRequested 0x5900, DevSize 0x59
IdeReadWrite (REQ): Starting sector is 3f25f, Number of WORDS 0x5900, DevSize 0x59
AtapiDmaSetup: mode 0x45, data f8584000, count b200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8584000)
  get Phys(data[n=1]=f8585000)
  get Phys(data[n=1]=f8586000)
  get Phys(data[n=2]=f8587000)
  get Phys(data[n=2]=f8588000)
  get Phys(data[n=2]=f8589000)
  get Phys(data[n=2]=f858a000)
  get Phys(data[n=2]=f858b000)
  get Phys(data[n=2]=f858c000)
  get Phys(data[n=3]=f858d000)
  get Phys(data[n=3]=f858e000)
  get Phys(data[n=4]=f858f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f25f, Count 0x59(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f25f count 0x59 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered b200, full size b200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f2bf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3f2bf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=1]=f8557000)
  get Phys(data[n=1]=f8558000)
  get Phys(data[n=1]=f8559000)
  get Phys(data[n=2]=f855a000)
  get Phys(data[n=2]=f855b000)
  get Phys(data[n=2]=f855c000)
  get Phys(data[n=2]=f855d000)
  get Phys(data[n=2]=f855e000)
  get Phys(data[n=2]=f855f000)
  get Phys(data[n=3]=f8560000)
  get Phys(data[n=3]=f8561000)
  get Phys(data[n=3]=f8562000)
  get Phys(data[n=3]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f2bf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f2bf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f33f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3f33f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=1]=f8567000)
  get Phys(data[n=1]=f8568000)
  get Phys(data[n=2]=f8569000)
  get Phys(data[n=3]=f856a000)
  get Phys(data[n=3]=f856b000)
  get Phys(data[n=3]=f856c000)
  get Phys(data[n=3]=f856d000)
  get Phys(data[n=3]=f856e000)
  get Phys(data[n=3]=f856f000)
  get Phys(data[n=3]=f8570000)
  get Phys(data[n=4]=f8571000)
  get Phys(data[n=4]=f8572000)
  get Phys(data[n=4]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f33f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f33f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f3bf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3f3bf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8574000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=1]=f8576000)
  get Phys(data[n=2]=f8577000)
  get Phys(data[n=2]=f8578000)
  get Phys(data[n=3]=f8579000)
  get Phys(data[n=4]=f857a000)
  get Phys(data[n=5]=f857b000)
  get Phys(data[n=5]=f857c000)
  get Phys(data[n=5]=f857d000)
  get Phys(data[n=5]=f857e000)
  get Phys(data[n=6]=f857f000)
  get Phys(data[n=7]=f8580000)
  get Phys(data[n=7]=f8581000)
  get Phys(data[n=7]=f8582000)
  get Phys(data[n=7]=f8583000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f3bf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f3bf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f43f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3f43f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8584000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8584000)
  get Phys(data[n=1]=f8585000)
  get Phys(data[n=1]=f8586000)
  get Phys(data[n=1]=f8587000)
  get Phys(data[n=1]=f8588000)
  get Phys(data[n=1]=f8589000)
  get Phys(data[n=2]=f858a000)
  get Phys(data[n=2]=f858b000)
  get Phys(data[n=3]=f858c000)
  get Phys(data[n=3]=f858d000)
  get Phys(data[n=3]=f858e000)
  get Phys(data[n=3]=f858f000)
  get Phys(data[n=3]=f8590000)
  get Phys(data[n=3]=f8591000)
  get Phys(data[n=3]=f8592000)
  get Phys(data[n=3]=f8593000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f43f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f43f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f4bf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3f4bf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 82c32000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82c32000)
  get Phys(data[n=1]=82c33000)
  get Phys(data[n=1]=82c34000)
  get Phys(data[n=1]=82c35000)
  get Phys(data[n=1]=82c36000)
  get Phys(data[n=2]=82c37000)
  get Phys(data[n=2]=82c38000)
  get Phys(data[n=2]=82c39000)
  get Phys(data[n=2]=82c3a000)
  get Phys(data[n=2]=82c3b000)
  get Phys(data[n=2]=82c3c000)
  get Phys(data[n=3]=82c3d000)
  get Phys(data[n=3]=82c3e000)
  get Phys(data[n=3]=82c3f000)
  get Phys(data[n=3]=82c40000)
  get Phys(data[n=3]=82c41000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f4bf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f4bf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f53f, OrigWordsRequested 0x4600, DevSize 0x46
IdeReadWrite (REQ): Starting sector is 3f53f, Number of WORDS 0x4600, DevSize 0x46
AtapiDmaSetup: mode 0x45, data 82c42000, count 8c00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82c42000)
  get Phys(data[n=1]=82c43000)
  get Phys(data[n=1]=82c44000)
  get Phys(data[n=1]=82c45000)
  get Phys(data[n=2]=82c46000)
  get Phys(data[n=3]=82c47000)
  get Phys(data[n=3]=82c48000)
  get Phys(data[n=3]=82c49000)
  get Phys(data[n=3]=82c4a000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f53f, Count 0x46(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f53f count 0x46 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 8c00, full size 8c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f587, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3f587, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=1]=f8557000)
  get Phys(data[n=1]=f8558000)
  get Phys(data[n=1]=f8559000)
  get Phys(data[n=1]=f855a000)
  get Phys(data[n=2]=f855b000)
  get Phys(data[n=2]=f855c000)
  get Phys(data[n=2]=f855d000)
  get Phys(data[n=2]=f855e000)
  get Phys(data[n=2]=f855f000)
  get Phys(data[n=2]=f8560000)
  get Phys(data[n=2]=f8561000)
  get Phys(data[n=2]=f8562000)
  get Phys(data[n=2]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f587, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f587 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f607, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3f607, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=1]=f8567000)
  get Phys(data[n=1]=f8568000)
  get Phys(data[n=1]=f8569000)
  get Phys(data[n=1]=f856a000)
  get Phys(data[n=1]=f856b000)
  get Phys(data[n=2]=f856c000)
  get Phys(data[n=2]=f856d000)
  get Phys(data[n=2]=f856e000)
  get Phys(data[n=2]=f856f000)
  get Phys(data[n=3]=f8570000)
  get Phys(data[n=3]=f8571000)
  get Phys(data[n=4]=f8572000)
  get Phys(data[n=4]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f607, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f607 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f687, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3f687, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8574000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=2]=f8576000)
  get Phys(data[n=2]=f8577000)
  get Phys(data[n=2]=f8578000)
  get Phys(data[n=2]=f8579000)
  get Phys(data[n=3]=f857a000)
  get Phys(data[n=4]=f857b000)
  get Phys(data[n=4]=f857c000)
  get Phys(data[n=4]=f857d000)
  get Phys(data[n=4]=f857e000)
  get Phys(data[n=5]=f857f000)
  get Phys(data[n=5]=f8580000)
  get Phys(data[n=5]=f8581000)
  get Phys(data[n=5]=f8582000)
  get Phys(data[n=5]=f8583000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f687, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f687 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f707, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3f707, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8584000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8584000)
  get Phys(data[n=1]=f8585000)
  get Phys(data[n=1]=f8586000)
  get Phys(data[n=2]=f8587000)
  get Phys(data[n=2]=f8588000)
  get Phys(data[n=2]=f8589000)
  get Phys(data[n=2]=f858a000)
  get Phys(data[n=2]=f858b000)
  get Phys(data[n=2]=f858c000)
  get Phys(data[n=2]=f858d000)
  get Phys(data[n=2]=f858e000)
  get Phys(data[n=3]=f858f000)
  get Phys(data[n=3]=f8590000)
  get Phys(data[n=3]=f8591000)
  get Phys(data[n=3]=f8592000)
  get Phys(data[n=3]=f8593000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f707, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f707 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f787, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3f787, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 82d06000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82d06000)
  get Phys(data[n=1]=82d07000)
  get Phys(data[n=1]=82d08000)
  get Phys(data[n=1]=82d09000)
  get Phys(data[n=1]=82d0a000)
  get Phys(data[n=1]=82d0b000)
  get Phys(data[n=2]=82d0c000)
  get Phys(data[n=2]=82d0d000)
  get Phys(data[n=2]=82d0e000)
  get Phys(data[n=2]=82d0f000)
  get Phys(data[n=2]=82d10000)
  get Phys(data[n=2]=82d11000)
  get Phys(data[n=2]=82d12000)
  get Phys(data[n=2]=82d13000)
  get Phys(data[n=2]=82d14000)
  get Phys(data[n=3]=82d15000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f787, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f787 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725ff0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f807, OrigWordsRequested 0x1b00, DevSize 0x1b
IdeReadWrite (REQ): Starting sector is 3f807, Number of WORDS 0x1b00, DevSize 0x1b
AtapiDmaSetup: mode 0x45, data 82d16000, count 3600, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82d16000)
  get Phys(data[n=1]=82d17000)
  get Phys(data[n=1]=82d18000)
  get Phys(data[n=1]=82d19000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f807, Count 0x1b(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f807 count 0x1b feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 3600, full size 3600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f827, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3f827, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=2]=f8556000)
  get Phys(data[n=2]=f8557000)
  get Phys(data[n=2]=f8558000)
  get Phys(data[n=2]=f8559000)
  get Phys(data[n=2]=f855a000)
  get Phys(data[n=2]=f855b000)
  get Phys(data[n=2]=f855c000)
  get Phys(data[n=2]=f855d000)
  get Phys(data[n=2]=f855e000)
  get Phys(data[n=3]=f855f000)
  get Phys(data[n=4]=f8560000)
  get Phys(data[n=4]=f8561000)
  get Phys(data[n=4]=f8562000)
  get Phys(data[n=4]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f827, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f827 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f8a7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3f8a7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=2]=f8567000)
  get Phys(data[n=2]=f8568000)
  get Phys(data[n=2]=f8569000)
  get Phys(data[n=2]=f856a000)
  get Phys(data[n=3]=f856b000)
  get Phys(data[n=3]=f856c000)
  get Phys(data[n=4]=f856d000)
  get Phys(data[n=4]=f856e000)
  get Phys(data[n=5]=f856f000)
  get Phys(data[n=6]=f8570000)
  get Phys(data[n=7]=f8571000)
  get Phys(data[n=7]=f8572000)
  get Phys(data[n=7]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f8a7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f8a7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f927, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3f927, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8574000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=2]=f8576000)
  get Phys(data[n=2]=f8577000)
  get Phys(data[n=2]=f8578000)
  get Phys(data[n=2]=f8579000)
  get Phys(data[n=3]=f857a000)
  get Phys(data[n=3]=f857b000)
  get Phys(data[n=3]=f857c000)
  get Phys(data[n=3]=f857d000)
  get Phys(data[n=3]=f857e000)
  get Phys(data[n=3]=f857f000)
  get Phys(data[n=4]=f8580000)
  get Phys(data[n=4]=f8581000)
  get Phys(data[n=5]=f8582000)
  get Phys(data[n=5]=f8583000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f927, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f927 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3f9a7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3f9a7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8584000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8584000)
  get Phys(data[n=1]=f8585000)
  get Phys(data[n=1]=f8586000)
  get Phys(data[n=1]=f8587000)
  get Phys(data[n=1]=f8588000)
  get Phys(data[n=1]=f8589000)
  get Phys(data[n=2]=f858a000)
  get Phys(data[n=2]=f858b000)
  get Phys(data[n=2]=f858c000)
  get Phys(data[n=2]=f858d000)
  get Phys(data[n=2]=f858e000)
  get Phys(data[n=2]=f858f000)
  get Phys(data[n=3]=f8590000)
  get Phys(data[n=3]=f8591000)
  get Phys(data[n=3]=f8592000)
  get Phys(data[n=3]=f8593000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3f9a7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3f9a7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725fe0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3fa27, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3fa27, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 82dd8000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82dd8000)
  get Phys(data[n=1]=82dd9000)
  get Phys(data[n=1]=82dda000)
  get Phys(data[n=1]=82ddb000)
  get Phys(data[n=1]=82ddc000)
  get Phys(data[n=1]=82ddd000)
  get Phys(data[n=1]=82dde000)
  get Phys(data[n=1]=82ddf000)
  get Phys(data[n=1]=82de0000)
  get Phys(data[n=1]=82de1000)
  get Phys(data[n=2]=82de2000)
  get Phys(data[n=3]=82de3000)
  get Phys(data[n=3]=82de4000)
  get Phys(data[n=3]=82de5000)
  get Phys(data[n=3]=82de6000)
  get Phys(data[n=3]=82de7000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3fa27, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3fa27 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725fe0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3faa7, OrigWordsRequested 0x900, DevSize 0x9
IdeReadWrite (REQ): Starting sector is 3faa7, Number of WORDS 0x900, DevSize 0x9
AtapiDmaSetup: mode 0x45, data 82de8000, count 1200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82de8000)
  get Phys(data[n=1]=82de9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3faa7, Count 0x9(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3faa7 count 0x9 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1200, full size 1200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3fab7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3fab7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=1]=f8557000)
  get Phys(data[n=1]=f8558000)
  get Phys(data[n=1]=f8559000)
  get Phys(data[n=2]=f855a000)
  get Phys(data[n=3]=f855b000)
  get Phys(data[n=3]=f855c000)
  get Phys(data[n=3]=f855d000)
  get Phys(data[n=3]=f855e000)
  get Phys(data[n=3]=f855f000)
  get Phys(data[n=3]=f8560000)
  get Phys(data[n=3]=f8561000)
  get Phys(data[n=4]=f8562000)
  get Phys(data[n=4]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3fab7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3fab7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3fb37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3fb37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=2]=f8566000)
  get Phys(data[n=2]=f8567000)
  get Phys(data[n=3]=f8568000)
  get Phys(data[n=3]=f8569000)
  get Phys(data[n=4]=f856a000)
  get Phys(data[n=5]=f856b000)
  get Phys(data[n=6]=f856c000)
  get Phys(data[n=6]=f856d000)
  get Phys(data[n=6]=f856e000)
  get Phys(data[n=6]=f856f000)
  get Phys(data[n=7]=f8570000)
  get Phys(data[n=8]=f8571000)
  get Phys(data[n=8]=f8572000)
  get Phys(data[n=8]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3fb37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3fb37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3fbb7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3fbb7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8574000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=1]=f8576000)
  get Phys(data[n=1]=f8577000)
  get Phys(data[n=1]=f8578000)
  get Phys(data[n=1]=f8579000)
  get Phys(data[n=1]=f857a000)
  get Phys(data[n=2]=f857b000)
  get Phys(data[n=2]=f857c000)
  get Phys(data[n=3]=f857d000)
  get Phys(data[n=3]=f857e000)
  get Phys(data[n=3]=f857f000)
  get Phys(data[n=3]=f8580000)
  get Phys(data[n=3]=f8581000)
  get Phys(data[n=3]=f8582000)
  get Phys(data[n=3]=f8583000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3fbb7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3fbb7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3fc37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3fc37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8584000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8584000)
  get Phys(data[n=1]=f8585000)
  get Phys(data[n=1]=f8586000)
  get Phys(data[n=1]=f8587000)
  get Phys(data[n=1]=f8588000)
  get Phys(data[n=1]=f8589000)
  get Phys(data[n=1]=f858a000)
  get Phys(data[n=2]=f858b000)
  get Phys(data[n=2]=f858c000)
  get Phys(data[n=2]=f858d000)
  get Phys(data[n=2]=f858e000)
  get Phys(data[n=2]=f858f000)
  get Phys(data[n=2]=f8590000)
  get Phys(data[n=3]=f8591000)
  get Phys(data[n=3]=f8592000)
  get Phys(data[n=3]=f8593000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3fc37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3fc37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725fe0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3fcb7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3fcb7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 82eab000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82eab000)
  get Phys(data[n=1]=82eac000)
  get Phys(data[n=1]=82ead000)
  get Phys(data[n=1]=82eae000)
  get Phys(data[n=1]=82eaf000)
  get Phys(data[n=2]=82eb0000)
  get Phys(data[n=3]=82eb1000)
  get Phys(data[n=3]=82eb2000)
  get Phys(data[n=3]=82eb3000)
  get Phys(data[n=3]=82eb4000)
  get Phys(data[n=3]=82eb5000)
  get Phys(data[n=3]=82eb6000)
  get Phys(data[n=3]=82eb7000)
  get Phys(data[n=4]=82eb8000)
  get Phys(data[n=4]=82eb9000)
  get Phys(data[n=4]=82eba000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3fcb7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3fcb7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8725fe0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3fd37, OrigWordsRequested 0x1600, DevSize 0x16
IdeReadWrite (REQ): Starting sector is 3fd37, Number of WORDS 0x1600, DevSize 0x16
AtapiDmaSetup: mode 0x45, data 82ebb000, count 2c00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82ebb000)
  get Phys(data[n=1]=82ebc000)
  get Phys(data[n=1]=82ebd000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3fd37, Count 0x16(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3fd37 count 0x16 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2c00, full size 2c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3fd4f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3fd4f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=2]=f8556000)
  get Phys(data[n=2]=f8557000)
  get Phys(data[n=2]=f8558000)
  get Phys(data[n=2]=f8559000)
  get Phys(data[n=2]=f855a000)
  get Phys(data[n=2]=f855b000)
  get Phys(data[n=2]=f855c000)
  get Phys(data[n=3]=f855d000)
  get Phys(data[n=3]=f855e000)
  get Phys(data[n=3]=f855f000)
  get Phys(data[n=3]=f8560000)
  get Phys(data[n=4]=f8561000)
  get Phys(data[n=4]=f8562000)
  get Phys(data[n=5]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3fd4f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3fd4f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3fdcf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3fdcf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=2]=f8566000)
  get Phys(data[n=3]=f8567000)
  get Phys(data[n=3]=f8568000)
  get Phys(data[n=3]=f8569000)
  get Phys(data[n=3]=f856a000)
  get Phys(data[n=4]=f856b000)
  get Phys(data[n=5]=f856c000)
  get Phys(data[n=5]=f856d000)
  get Phys(data[n=5]=f856e000)
  get Phys(data[n=5]=f856f000)
  get Phys(data[n=6]=f8570000)
  get Phys(data[n=6]=f8571000)
  get Phys(data[n=6]=f8572000)
  get Phys(data[n=6]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3fdcf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3fdcf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3fe4f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3fe4f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8574000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=2]=f8576000)
  get Phys(data[n=2]=f8577000)
  get Phys(data[n=3]=f8578000)
  get Phys(data[n=3]=f8579000)
  get Phys(data[n=3]=f857a000)
  get Phys(data[n=3]=f857b000)
  get Phys(data[n=3]=f857c000)
  get Phys(data[n=3]=f857d000)
  get Phys(data[n=3]=f857e000)
  get Phys(data[n=3]=f857f000)
  get Phys(data[n=4]=f8580000)
  get Phys(data[n=4]=f8581000)
  get Phys(data[n=4]=f8582000)
  get Phys(data[n=4]=f8583000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3fe4f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3fe4f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3fecf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3fecf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8584000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8584000)
  get Phys(data[n=1]=f8585000)
  get Phys(data[n=2]=f8586000)
  get Phys(data[n=2]=f8587000)
  get Phys(data[n=2]=f8588000)
  get Phys(data[n=2]=f8589000)
  get Phys(data[n=2]=f858a000)
  get Phys(data[n=2]=f858b000)
  get Phys(data[n=3]=f858c000)
  get Phys(data[n=3]=f858d000)
  get Phys(data[n=3]=f858e000)
  get Phys(data[n=3]=f858f000)
  get Phys(data[n=3]=f8590000)
  get Phys(data[n=3]=f8591000)
  get Phys(data[n=3]=f8592000)
  get Phys(data[n=3]=f8593000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3fecf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3fecf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726008
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ff4f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3ff4f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 82f7f000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82f7f000)
  get Phys(data[n=1]=82f80000)
  get Phys(data[n=1]=82f81000)
  get Phys(data[n=1]=82f82000)
  get Phys(data[n=1]=82f83000)
  get Phys(data[n=1]=82f84000)
  get Phys(data[n=1]=82f85000)
  get Phys(data[n=1]=82f86000)
  get Phys(data[n=2]=82f87000)
  get Phys(data[n=2]=82f88000)
  get Phys(data[n=2]=82f89000)
  get Phys(data[n=2]=82f8a000)
  get Phys(data[n=3]=82f8b000)
  get Phys(data[n=3]=82f8c000)
  get Phys(data[n=4]=82f8d000)
  get Phys(data[n=4]=82f8e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ff4f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3ff4f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726008
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ffcf, OrigWordsRequested 0x2000, DevSize 0x20
IdeReadWrite (REQ): Starting sector is 3ffcf, Number of WORDS 0x2000, DevSize 0x20
AtapiDmaSetup: mode 0x45, data 82f8f000, count 4000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=82f8f000)
  get Phys(data[n=1]=82f90000)
  get Phys(data[n=2]=82f91000)
  get Phys(data[n=2]=82f92000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ffcf, Count 0x20(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3ffcf count 0x20 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 4000, full size 4000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ffef, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3ffef, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=1]=f8557000)
  get Phys(data[n=2]=f8558000)
  get Phys(data[n=2]=f8559000)
  get Phys(data[n=2]=f855a000)
  get Phys(data[n=2]=f855b000)
  get Phys(data[n=3]=f855c000)
  get Phys(data[n=3]=f855d000)
  get Phys(data[n=4]=f855e000)
  get Phys(data[n=4]=f855f000)
  get Phys(data[n=5]=f8560000)
  get Phys(data[n=6]=f8561000)
  get Phys(data[n=7]=f8562000)
  get Phys(data[n=7]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ffef, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3ffef count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4006f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4006f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=2]=f8566000)
  get Phys(data[n=3]=f8567000)
  get Phys(data[n=3]=f8568000)
  get Phys(data[n=3]=f8569000)
  get Phys(data[n=3]=f856a000)
  get Phys(data[n=4]=f856b000)
  get Phys(data[n=4]=f856c000)
  get Phys(data[n=4]=f856d000)
  get Phys(data[n=4]=f856e000)
  get Phys(data[n=4]=f856f000)
  get Phys(data[n=4]=f8570000)
  get Phys(data[n=5]=f8571000)
  get Phys(data[n=5]=f8572000)
  get Phys(data[n=6]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4006f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4006f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 400ef, OrigWordsRequested 0x5400, DevSize 0x54
IdeReadWrite (REQ): Starting sector is 400ef, Number of WORDS 0x5400, DevSize 0x54
AtapiDmaSetup: mode 0x45, data f8574000, count a800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=1]=f8576000)
  get Phys(data[n=1]=f8577000)
  get Phys(data[n=1]=f8578000)
  get Phys(data[n=1]=f8579000)
  get Phys(data[n=1]=f857a000)
  get Phys(data[n=2]=f857b000)
  get Phys(data[n=2]=f857c000)
  get Phys(data[n=2]=f857d000)
  get Phys(data[n=2]=f857e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x400ef, Count 0x54(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x400ef count 0x54 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a800, full size a800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40147, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 40147, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=2]=f8557000)
  get Phys(data[n=2]=f8558000)
  get Phys(data[n=3]=f8559000)
  get Phys(data[n=3]=f855a000)
  get Phys(data[n=4]=f855b000)
  get Phys(data[n=5]=f855c000)
  get Phys(data[n=6]=f855d000)
  get Phys(data[n=6]=f855e000)
  get Phys(data[n=6]=f855f000)
  get Phys(data[n=6]=f8560000)
  get Phys(data[n=7]=f8561000)
  get Phys(data[n=8]=f8562000)
  get Phys(data[n=8]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40147, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40147 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 401c7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 401c7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=2]=f8566000)
  get Phys(data[n=2]=f8567000)
  get Phys(data[n=2]=f8568000)
  get Phys(data[n=2]=f8569000)
  get Phys(data[n=2]=f856a000)
  get Phys(data[n=2]=f856b000)
  get Phys(data[n=3]=f856c000)
  get Phys(data[n=3]=f856d000)
  get Phys(data[n=4]=f856e000)
  get Phys(data[n=4]=f856f000)
  get Phys(data[n=4]=f8570000)
  get Phys(data[n=4]=f8571000)
  get Phys(data[n=4]=f8572000)
  get Phys(data[n=4]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x401c7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x401c7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40247, OrigWordsRequested 0x4c00, DevSize 0x4c
IdeReadWrite (REQ): Starting sector is 40247, Number of WORDS 0x4c00, DevSize 0x4c
AtapiDmaSetup: mode 0x45, data f8574000, count 9800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=2]=f8576000)
  get Phys(data[n=2]=f8577000)
  get Phys(data[n=2]=f8578000)
  get Phys(data[n=2]=f8579000)
  get Phys(data[n=2]=f857a000)
  get Phys(data[n=2]=f857b000)
  get Phys(data[n=3]=f857c000)
  get Phys(data[n=3]=f857d000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40247, Count 0x4c(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40247 count 0x4c feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 9800, full size 9800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40297, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 40297, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=2]=f8556000)
  get Phys(data[n=2]=f8557000)
  get Phys(data[n=3]=f8558000)
  get Phys(data[n=4]=f8559000)
  get Phys(data[n=5]=f855a000)
  get Phys(data[n=5]=f855b000)
  get Phys(data[n=5]=f855c000)
  get Phys(data[n=5]=f855d000)
  get Phys(data[n=6]=f855e000)
  get Phys(data[n=7]=f855f000)
  get Phys(data[n=7]=f8560000)
  get Phys(data[n=7]=f8561000)
  get Phys(data[n=7]=f8562000)
  get Phys(data[n=8]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40297, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40297 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40317, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 40317, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=1]=f8567000)
  get Phys(data[n=1]=f8568000)
  get Phys(data[n=2]=f8569000)
  get Phys(data[n=2]=f856a000)
  get Phys(data[n=3]=f856b000)
  get Phys(data[n=3]=f856c000)
  get Phys(data[n=3]=f856d000)
  get Phys(data[n=3]=f856e000)
  get Phys(data[n=3]=f856f000)
  get Phys(data[n=3]=f8570000)
  get Phys(data[n=3]=f8571000)
  get Phys(data[n=3]=f8572000)
  get Phys(data[n=4]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40317, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40317 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40397, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 40397, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8574000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=1]=f8576000)
  get Phys(data[n=1]=f8577000)
  get Phys(data[n=1]=f8578000)
  get Phys(data[n=2]=f8579000)
  get Phys(data[n=2]=f857a000)
  get Phys(data[n=2]=f857b000)
  get Phys(data[n=2]=f857c000)
  get Phys(data[n=2]=f857d000)
  get Phys(data[n=2]=f857e000)
  get Phys(data[n=3]=f857f000)
  get Phys(data[n=3]=f8580000)
  get Phys(data[n=3]=f8581000)
  get Phys(data[n=3]=f8582000)
  get Phys(data[n=3]=f8583000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40397, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40397 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40417, OrigWordsRequested 0x1700, DevSize 0x17
IdeReadWrite (REQ): Starting sector is 40417, Number of WORDS 0x1700, DevSize 0x17
AtapiDmaSetup: mode 0x45, data f8584000, count 2e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8584000)
  get Phys(data[n=1]=f8585000)
  get Phys(data[n=1]=f8586000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40417, Count 0x17(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40417 count 0x17 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2e00, full size 2e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4042f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4042f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=2]=f8556000)
  get Phys(data[n=3]=f8557000)
  get Phys(data[n=3]=f8558000)
  get Phys(data[n=3]=f8559000)
  get Phys(data[n=3]=f855a000)
  get Phys(data[n=4]=f855b000)
  get Phys(data[n=5]=f855c000)
  get Phys(data[n=5]=f855d000)
  get Phys(data[n=5]=f855e000)
  get Phys(data[n=5]=f855f000)
  get Phys(data[n=6]=f8560000)
  get Phys(data[n=6]=f8561000)
  get Phys(data[n=6]=f8562000)
  get Phys(data[n=6]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4042f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4042f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 404af, OrigWordsRequested 0x4e00, DevSize 0x4e
IdeReadWrite (REQ): Starting sector is 404af, Number of WORDS 0x4e00, DevSize 0x4e
AtapiDmaSetup: mode 0x45, data f8564000, count 9c00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=2]=f8566000)
  get Phys(data[n=2]=f8567000)
  get Phys(data[n=3]=f8568000)
  get Phys(data[n=3]=f8569000)
  get Phys(data[n=3]=f856a000)
  get Phys(data[n=3]=f856b000)
  get Phys(data[n=3]=f856c000)
  get Phys(data[n=3]=f856d000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x404af, Count 0x4e(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x404af count 0x4e feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 9c00, full size 9c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 404ff, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 404ff, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=2]=f8556000)
  get Phys(data[n=2]=f8557000)
  get Phys(data[n=2]=f8558000)
  get Phys(data[n=2]=f8559000)
  get Phys(data[n=3]=f855a000)
  get Phys(data[n=4]=f855b000)
  get Phys(data[n=4]=f855c000)
  get Phys(data[n=4]=f855d000)
  get Phys(data[n=4]=f855e000)
  get Phys(data[n=5]=f855f000)
  get Phys(data[n=5]=f8560000)
  get Phys(data[n=5]=f8561000)
  get Phys(data[n=5]=f8562000)
  get Phys(data[n=5]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x404ff, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x404ff count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4057f, OrigWordsRequested 0x6800, DevSize 0x68
IdeReadWrite (REQ): Starting sector is 4057f, Number of WORDS 0x6800, DevSize 0x68
AtapiDmaSetup: mode 0x45, data f8564000, count d000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=2]=f8567000)
  get Phys(data[n=2]=f8568000)
  get Phys(data[n=2]=f8569000)
  get Phys(data[n=2]=f856a000)
  get Phys(data[n=2]=f856b000)
  get Phys(data[n=2]=f856c000)
  get Phys(data[n=2]=f856d000)
  get Phys(data[n=2]=f856e000)
  get Phys(data[n=3]=f856f000)
  get Phys(data[n=3]=f8570000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4057f, Count 0x68(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4057f count 0x68 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered d000, full size d000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 405e7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 405e7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=1]=f8557000)
  get Phys(data[n=2]=f8558000)
  get Phys(data[n=3]=f8559000)
  get Phys(data[n=3]=f855a000)
  get Phys(data[n=3]=f855b000)
  get Phys(data[n=3]=f855c000)
  get Phys(data[n=4]=f855d000)
  get Phys(data[n=4]=f855e000)
  get Phys(data[n=4]=f855f000)
  get Phys(data[n=4]=f8560000)
  get Phys(data[n=4]=f8561000)
  get Phys(data[n=4]=f8562000)
  get Phys(data[n=5]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x405e7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x405e7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40667, OrigWordsRequested 0x7300, DevSize 0x73
IdeReadWrite (REQ): Starting sector is 40667, Number of WORDS 0x7300, DevSize 0x73
AtapiDmaSetup: mode 0x45, data f8564000, count e600, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=1]=f8567000)
  get Phys(data[n=1]=f8568000)
  get Phys(data[n=1]=f8569000)
  get Phys(data[n=1]=f856a000)
  get Phys(data[n=1]=f856b000)
  get Phys(data[n=1]=f856c000)
  get Phys(data[n=2]=f856d000)
  get Phys(data[n=2]=f856e000)
  get Phys(data[n=2]=f856f000)
  get Phys(data[n=2]=f8570000)
  get Phys(data[n=2]=f8571000)
  get Phys(data[n=2]=f8572000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40667, Count 0x73(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40667 count 0x73 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e600, full size e600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 406df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 406df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=2]=f8557000)
  get Phys(data[n=3]=f8558000)
  get Phys(data[n=3]=f8559000)
  get Phys(data[n=3]=f855a000)
  get Phys(data[n=3]=f855b000)
  get Phys(data[n=4]=f855c000)
  get Phys(data[n=4]=f855d000)
  get Phys(data[n=4]=f855e000)
  get Phys(data[n=4]=f855f000)
  get Phys(data[n=4]=f8560000)
  get Phys(data[n=4]=f8561000)
  get Phys(data[n=5]=f8562000)
  get Phys(data[n=5]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x406df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x406df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4075f, OrigWordsRequested 0x5400, DevSize 0x54
IdeReadWrite (REQ): Starting sector is 4075f, Number of WORDS 0x5400, DevSize 0x54
AtapiDmaSetup: mode 0x45, data f8564000, count a800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=1]=f8567000)
  get Phys(data[n=1]=f8568000)
  get Phys(data[n=1]=f8569000)
  get Phys(data[n=1]=f856a000)
  get Phys(data[n=1]=f856b000)
  get Phys(data[n=2]=f856c000)
  get Phys(data[n=2]=f856d000)
  get Phys(data[n=2]=f856e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4075f, Count 0x54(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4075f count 0x54 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a800, full size a800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 407b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 407b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=2]=f8556000)
  get Phys(data[n=3]=f8557000)
  get Phys(data[n=3]=f8558000)
  get Phys(data[n=3]=f8559000)
  get Phys(data[n=3]=f855a000)
  get Phys(data[n=4]=f855b000)
  get Phys(data[n=4]=f855c000)
  get Phys(data[n=4]=f855d000)
  get Phys(data[n=4]=f855e000)
  get Phys(data[n=4]=f855f000)
  get Phys(data[n=4]=f8560000)
  get Phys(data[n=5]=f8561000)
  get Phys(data[n=5]=f8562000)
  get Phys(data[n=6]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x407b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x407b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40837, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 40837, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=1]=f8567000)
  get Phys(data[n=1]=f8568000)
  get Phys(data[n=1]=f8569000)
  get Phys(data[n=1]=f856a000)
  get Phys(data[n=2]=f856b000)
  get Phys(data[n=2]=f856c000)
  get Phys(data[n=2]=f856d000)
  get Phys(data[n=2]=f856e000)
  get Phys(data[n=2]=f856f000)
  get Phys(data[n=2]=f8570000)
  get Phys(data[n=3]=f8571000)
  get Phys(data[n=3]=f8572000)
  get Phys(data[n=3]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40837, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40837 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 408b7, OrigWordsRequested 0xb00, DevSize 0xb
IdeReadWrite (REQ): Starting sector is 408b7, Number of WORDS 0xb00, DevSize 0xb
AtapiDmaSetup: mode 0x45, data f8574000, count 1600, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x408b7, Count 0xb(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x408b7 count 0xb feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1600, full size 1600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 408c7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 408c7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=1]=f8557000)
  get Phys(data[n=1]=f8558000)
  get Phys(data[n=2]=f8559000)
  get Phys(data[n=2]=f855a000)
  get Phys(data[n=2]=f855b000)
  get Phys(data[n=2]=f855c000)
  get Phys(data[n=2]=f855d000)
  get Phys(data[n=2]=f855e000)
  get Phys(data[n=3]=f855f000)
  get Phys(data[n=3]=f8560000)
  get Phys(data[n=4]=f8561000)
  get Phys(data[n=4]=f8562000)
  get Phys(data[n=4]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x408c7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x408c7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40947, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 40947, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=1]=f8567000)
  get Phys(data[n=1]=f8568000)
  get Phys(data[n=2]=f8569000)
  get Phys(data[n=2]=f856a000)
  get Phys(data[n=2]=f856b000)
  get Phys(data[n=2]=f856c000)
  get Phys(data[n=2]=f856d000)
  get Phys(data[n=2]=f856e000)
  get Phys(data[n=3]=f856f000)
  get Phys(data[n=3]=f8570000)
  get Phys(data[n=3]=f8571000)
  get Phys(data[n=3]=f8572000)
  get Phys(data[n=3]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40947, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40947 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 409c7, OrigWordsRequested 0x700, DevSize 0x7
IdeReadWrite (REQ): Starting sector is 409c7, Number of WORDS 0x700, DevSize 0x7
AtapiDmaSetup: mode 0x45, data f8574000, count e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x409c7, Count 0x7(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x409c7 count 0x7 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e00, full size e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 409cf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 409cf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=2]=f8557000)
  get Phys(data[n=2]=f8558000)
  get Phys(data[n=2]=f8559000)
  get Phys(data[n=2]=f855a000)
  get Phys(data[n=2]=f855b000)
  get Phys(data[n=2]=f855c000)
  get Phys(data[n=3]=f855d000)
  get Phys(data[n=3]=f855e000)
  get Phys(data[n=4]=f855f000)
  get Phys(data[n=4]=f8560000)
  get Phys(data[n=4]=f8561000)
  get Phys(data[n=4]=f8562000)
  get Phys(data[n=4]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x409cf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x409cf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40a4f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 40a4f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=2]=f8567000)
  get Phys(data[n=2]=f8568000)
  get Phys(data[n=2]=f8569000)
  get Phys(data[n=2]=f856a000)
  get Phys(data[n=2]=f856b000)
  get Phys(data[n=2]=f856c000)
  get Phys(data[n=3]=f856d000)
  get Phys(data[n=3]=f856e000)
  get Phys(data[n=3]=f856f000)
  get Phys(data[n=3]=f8570000)
  get Phys(data[n=3]=f8571000)
  get Phys(data[n=3]=f8572000)
  get Phys(data[n=4]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40a4f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40a4f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40acf, OrigWordsRequested 0x3c00, DevSize 0x3c
IdeReadWrite (REQ): Starting sector is 40acf, Number of WORDS 0x3c00, DevSize 0x3c
AtapiDmaSetup: mode 0x45, data f8574000, count 7800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=1]=f8576000)
  get Phys(data[n=1]=f8577000)
  get Phys(data[n=1]=f8578000)
  get Phys(data[n=1]=f8579000)
  get Phys(data[n=1]=f857a000)
  get Phys(data[n=1]=f857b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40acf, Count 0x3c(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40acf count 0x3c feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 7800, full size 7800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40b0f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 40b0f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=2]=f8556000)
  get Phys(data[n=2]=f8557000)
  get Phys(data[n=2]=f8558000)
  get Phys(data[n=2]=f8559000)
  get Phys(data[n=2]=f855a000)
  get Phys(data[n=2]=f855b000)
  get Phys(data[n=3]=f855c000)
  get Phys(data[n=3]=f855d000)
  get Phys(data[n=4]=f855e000)
  get Phys(data[n=4]=f855f000)
  get Phys(data[n=4]=f8560000)
  get Phys(data[n=4]=f8561000)
  get Phys(data[n=4]=f8562000)
  get Phys(data[n=4]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40b0f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40b0f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40b8f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 40b8f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=2]=f8566000)
  get Phys(data[n=2]=f8567000)
  get Phys(data[n=2]=f8568000)
  get Phys(data[n=2]=f8569000)
  get Phys(data[n=2]=f856a000)
  get Phys(data[n=2]=f856b000)
  get Phys(data[n=3]=f856c000)
  get Phys(data[n=3]=f856d000)
  get Phys(data[n=3]=f856e000)
  get Phys(data[n=3]=f856f000)
  get Phys(data[n=3]=f8570000)
  get Phys(data[n=3]=f8571000)
  get Phys(data[n=4]=f8572000)
  get Phys(data[n=4]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40b8f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40b8f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40c0f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 40c0f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8574000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40c0f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40c0f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40c1f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 40c1f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=1]=f8557000)
  get Phys(data[n=1]=f8558000)
  get Phys(data[n=2]=f8559000)
  get Phys(data[n=2]=f855a000)
  get Phys(data[n=3]=f855b000)
  get Phys(data[n=3]=f855c000)
  get Phys(data[n=3]=f855d000)
  get Phys(data[n=3]=f855e000)
  get Phys(data[n=3]=f855f000)
  get Phys(data[n=3]=f8560000)
  get Phys(data[n=3]=f8561000)
  get Phys(data[n=3]=f8562000)
  get Phys(data[n=4]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40c1f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40c1f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40c9f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 40c9f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=1]=f8567000)
  get Phys(data[n=1]=f8568000)
  get Phys(data[n=2]=f8569000)
  get Phys(data[n=2]=f856a000)
  get Phys(data[n=2]=f856b000)
  get Phys(data[n=2]=f856c000)
  get Phys(data[n=2]=f856d000)
  get Phys(data[n=2]=f856e000)
  get Phys(data[n=3]=f856f000)
  get Phys(data[n=3]=f8570000)
  get Phys(data[n=3]=f8571000)
  get Phys(data[n=3]=f8572000)
  get Phys(data[n=3]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40c9f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40c9f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40d1f, OrigWordsRequested 0x1f00, DevSize 0x1f
IdeReadWrite (REQ): Starting sector is 40d1f, Number of WORDS 0x1f00, DevSize 0x1f
AtapiDmaSetup: mode 0x45, data f8574000, count 3e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=1]=f8576000)
  get Phys(data[n=1]=f8577000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40d1f, Count 0x1f(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40d1f count 0x1f feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 3e00, full size 3e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40d3f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 40d3f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=1]=f8557000)
  get Phys(data[n=2]=f8558000)
  get Phys(data[n=2]=f8559000)
  get Phys(data[n=3]=f855a000)
  get Phys(data[n=3]=f855b000)
  get Phys(data[n=3]=f855c000)
  get Phys(data[n=3]=f855d000)
  get Phys(data[n=3]=f855e000)
  get Phys(data[n=3]=f855f000)
  get Phys(data[n=3]=f8560000)
  get Phys(data[n=3]=f8561000)
  get Phys(data[n=4]=f8562000)
  get Phys(data[n=4]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40d3f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40d3f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40dbf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 40dbf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=1]=f8567000)
  get Phys(data[n=2]=f8568000)
  get Phys(data[n=2]=f8569000)
  get Phys(data[n=2]=f856a000)
  get Phys(data[n=2]=f856b000)
  get Phys(data[n=2]=f856c000)
  get Phys(data[n=2]=f856d000)
  get Phys(data[n=3]=f856e000)
  get Phys(data[n=3]=f856f000)
  get Phys(data[n=3]=f8570000)
  get Phys(data[n=3]=f8571000)
  get Phys(data[n=3]=f8572000)
  get Phys(data[n=3]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40dbf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40dbf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40e3f, OrigWordsRequested 0x2600, DevSize 0x26
IdeReadWrite (REQ): Starting sector is 40e3f, Number of WORDS 0x2600, DevSize 0x26
AtapiDmaSetup: mode 0x45, data f8574000, count 4c00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=1]=f8576000)
  get Phys(data[n=2]=f8577000)
  get Phys(data[n=3]=f8578000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40e3f, Count 0x26(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40e3f count 0x26 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 4c00, full size 4c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40e67, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 40e67, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=2]=f8556000)
  get Phys(data[n=2]=f8557000)
  get Phys(data[n=3]=f8558000)
  get Phys(data[n=3]=f8559000)
  get Phys(data[n=3]=f855a000)
  get Phys(data[n=3]=f855b000)
  get Phys(data[n=3]=f855c000)
  get Phys(data[n=3]=f855d000)
  get Phys(data[n=3]=f855e000)
  get Phys(data[n=3]=f855f000)
  get Phys(data[n=4]=f8560000)
  get Phys(data[n=4]=f8561000)
  get Phys(data[n=4]=f8562000)
  get Phys(data[n=4]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40e67, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40e67 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40ee7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 40ee7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=2]=f8566000)
  get Phys(data[n=2]=f8567000)
  get Phys(data[n=2]=f8568000)
  get Phys(data[n=2]=f8569000)
  get Phys(data[n=2]=f856a000)
  get Phys(data[n=2]=f856b000)
  get Phys(data[n=3]=f856c000)
  get Phys(data[n=3]=f856d000)
  get Phys(data[n=3]=f856e000)
  get Phys(data[n=3]=f856f000)
  get Phys(data[n=3]=f8570000)
  get Phys(data[n=3]=f8571000)
  get Phys(data[n=3]=f8572000)
  get Phys(data[n=3]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40ee7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40ee7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40f67, OrigWordsRequested 0x1a00, DevSize 0x1a
IdeReadWrite (REQ): Starting sector is 40f67, Number of WORDS 0x1a00, DevSize 0x1a
AtapiDmaSetup: mode 0x45, data f8574000, count 3400, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=2]=f8576000)
  get Phys(data[n=2]=f8577000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40f67, Count 0x1a(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40f67 count 0x1a feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 3400, full size 3400
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 40f87, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 40f87, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=2]=f8556000)
  get Phys(data[n=2]=f8557000)
  get Phys(data[n=2]=f8558000)
  get Phys(data[n=2]=f8559000)
  get Phys(data[n=2]=f855a000)
  get Phys(data[n=2]=f855b000)
  get Phys(data[n=2]=f855c000)
  get Phys(data[n=2]=f855d000)
  get Phys(data[n=3]=f855e000)
  get Phys(data[n=3]=f855f000)
  get Phys(data[n=3]=f8560000)
  get Phys(data[n=3]=f8561000)
  get Phys(data[n=3]=f8562000)
  get Phys(data[n=3]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x40f87, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x40f87 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41007, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 41007, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=1]=f8567000)
  get Phys(data[n=1]=f8568000)
  get Phys(data[n=1]=f8569000)
  get Phys(data[n=2]=f856a000)
  get Phys(data[n=2]=f856b000)
  get Phys(data[n=2]=f856c000)
  get Phys(data[n=2]=f856d000)
  get Phys(data[n=2]=f856e000)
  get Phys(data[n=2]=f856f000)
  get Phys(data[n=2]=f8570000)
  get Phys(data[n=2]=f8571000)
  get Phys(data[n=2]=f8572000)
  get Phys(data[n=3]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41007, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41007 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41087, OrigWordsRequested 0x2900, DevSize 0x29
IdeReadWrite (REQ): Starting sector is 41087, Number of WORDS 0x2900, DevSize 0x29
AtapiDmaSetup: mode 0x45, data f8574000, count 5200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=1]=f8576000)
  get Phys(data[n=1]=f8577000)
  get Phys(data[n=1]=f8578000)
  get Phys(data[n=1]=f8579000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41087, Count 0x29(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41087 count 0x29 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 5200, full size 5200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87260e8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 410b7, OrigWordsRequested 0x3800, DevSize 0x38
IdeReadWrite (REQ): Starting sector is 410b7, Number of WORDS 0x3800, DevSize 0x38
AtapiDmaSetup: mode 0x45, data f8554000, count 7000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=1]=f8557000)
  get Phys(data[n=1]=f8558000)
  get Phys(data[n=1]=f8559000)
  get Phys(data[n=1]=f855a000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x410b7, Count 0x38(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x410b7 count 0x38 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 7000, full size 7000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87260e8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 410ef, OrigWordsRequested 0x3300, DevSize 0x33
IdeReadWrite (REQ): Starting sector is 410ef, Number of WORDS 0x3300, DevSize 0x33
AtapiDmaSetup: mode 0x45, data f8554000, count 6600, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=1]=f8557000)
  get Phys(data[n=1]=f8558000)
  get Phys(data[n=1]=f8559000)
  get Phys(data[n=1]=f855a000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x410ef, Count 0x33(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x410ef count 0x33 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 6600, full size 6600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41127, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 41127, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=1]=f8557000)
  get Phys(data[n=1]=f8558000)
  get Phys(data[n=2]=f8559000)
  get Phys(data[n=2]=f855a000)
  get Phys(data[n=2]=f855b000)
  get Phys(data[n=2]=f855c000)
  get Phys(data[n=2]=f855d000)
  get Phys(data[n=2]=f855e000)
  get Phys(data[n=3]=f855f000)
  get Phys(data[n=3]=f8560000)
  get Phys(data[n=3]=f8561000)
  get Phys(data[n=3]=f8562000)
  get Phys(data[n=3]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41127, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41127 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 411a7, OrigWordsRequested 0x3a00, DevSize 0x3a
IdeReadWrite (REQ): Starting sector is 411a7, Number of WORDS 0x3a00, DevSize 0x3a
AtapiDmaSetup: mode 0x45, data f8564000, count 7400, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=1]=f8567000)
  get Phys(data[n=1]=f8568000)
  get Phys(data[n=1]=f8569000)
  get Phys(data[n=1]=f856a000)
  get Phys(data[n=1]=f856b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x411a7, Count 0x3a(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x411a7 count 0x3a feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 7400, full size 7400
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 411e7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 411e7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=1]=f8557000)
  get Phys(data[n=1]=f8558000)
  get Phys(data[n=1]=f8559000)
  get Phys(data[n=2]=f855a000)
  get Phys(data[n=2]=f855b000)
  get Phys(data[n=2]=f855c000)
  get Phys(data[n=2]=f855d000)
  get Phys(data[n=2]=f855e000)
  get Phys(data[n=2]=f855f000)
  get Phys(data[n=3]=f8560000)
  get Phys(data[n=3]=f8561000)
  get Phys(data[n=3]=f8562000)
  get Phys(data[n=3]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x411e7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x411e7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726080
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41267, OrigWordsRequested 0x2900, DevSize 0x29
IdeReadWrite (REQ): Starting sector is 41267, Number of WORDS 0x2900, DevSize 0x29
AtapiDmaSetup: mode 0x45, data f8564000, count 5200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=1]=f8567000)
  get Phys(data[n=1]=f8568000)
  get Phys(data[n=2]=f8569000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41267, Count 0x29(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41267 count 0x29 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 5200, full size 5200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8726338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4f857, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 4f857, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8554000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4f857, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4f857 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4f857, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 4f857, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8700000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8700000)
  get Phys(data[n=1]=f8701000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4f857, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4f857 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f92d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4f867, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4f867, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=1]=f8557000)
  get Phys(data[n=1]=f8558000)
  get Phys(data[n=1]=f8559000)
  get Phys(data[n=2]=f855a000)
  get Phys(data[n=3]=f855b000)
  get Phys(data[n=3]=f855c000)
  get Phys(data[n=3]=f855d000)
  get Phys(data[n=3]=f855e000)
  get Phys(data[n=3]=f855f000)
  get Phys(data[n=3]=f8560000)
  get Phys(data[n=3]=f8561000)
  get Phys(data[n=4]=f8562000)
  get Phys(data[n=4]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4f867, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4f867 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f92d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4f8e7, OrigWordsRequested 0x3c00, DevSize 0x3c
IdeReadWrite (REQ): Starting sector is 4f8e7, Number of WORDS 0x3c00, DevSize 0x3c
AtapiDmaSetup: mode 0x45, data f8564000, count 7800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=2]=f8566000)
  get Phys(data[n=2]=f8567000)
  get Phys(data[n=3]=f8568000)
  get Phys(data[n=3]=f8569000)
  get Phys(data[n=4]=f856a000)
  get Phys(data[n=5]=f856b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4f8e7, Count 0x3c(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4f8e7 count 0x3c feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 7800, full size 7800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4f867, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 4f867, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8700000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8700000)
  get Phys(data[n=1]=f8701000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4f867, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4f867 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../subsystems/win32/csrss/csrsrv/init.c:750) Fake basesrv init
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f92d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 51167, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 51167, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=1]=f8556000)
  get Phys(data[n=2]=f8557000)
  get Phys(data[n=2]=f8558000)
  get Phys(data[n=2]=f8559000)
  get Phys(data[n=2]=f855a000)
  get Phys(data[n=2]=f855b000)
  get Phys(data[n=2]=f855c000)
  get Phys(data[n=3]=f855d000)
  get Phys(data[n=3]=f855e000)
  get Phys(data[n=3]=f855f000)
  get Phys(data[n=3]=f8560000)
  get Phys(data[n=3]=f8561000)
  get Phys(data[n=3]=f8562000)
  get Phys(data[n=4]=f8563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x51167, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x51167 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f92d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 511e7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 511e7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8564000)
  get Phys(data[n=1]=f8565000)
  get Phys(data[n=1]=f8566000)
  get Phys(data[n=1]=f8567000)
  get Phys(data[n=1]=f8568000)
  get Phys(data[n=1]=f8569000)
  get Phys(data[n=1]=f856a000)
  get Phys(data[n=1]=f856b000)
  get Phys(data[n=2]=f856c000)
  get Phys(data[n=3]=f856d000)
  get Phys(data[n=3]=f856e000)
  get Phys(data[n=3]=f856f000)
  get Phys(data[n=3]=f8570000)
  get Phys(data[n=3]=f8571000)
  get Phys(data[n=3]=f8572000)
  get Phys(data[n=3]=f8573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x511e7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x511e7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f92d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 51267, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 51267, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8574000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8574000)
  get Phys(data[n=1]=f8575000)
  get Phys(data[n=2]=f8576000)
  get Phys(data[n=2]=f8577000)
  get Phys(data[n=3]=f8578000)
  get Phys(data[n=3]=f8579000)
  get Phys(data[n=4]=f857a000)
  get Phys(data[n=4]=f857b000)
  get Phys(data[n=5]=f857c000)
  get Phys(data[n=6]=f857d000)
  get Phys(data[n=7]=f857e000)
  get Phys(data[n=7]=f857f000)
  get Phys(data[n=7]=f8580000)
  get Phys(data[n=7]=f8581000)
  get Phys(data[n=8]=f8582000)
  get Phys(data[n=9]=f8583000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x51267, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x51267 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f92d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 512e7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 512e7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8584000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8584000)
  get Phys(data[n=1]=f8585000)
  get Phys(data[n=1]=f8586000)
  get Phys(data[n=2]=f8587000)
  get Phys(data[n=2]=f8588000)
  get Phys(data[n=2]=f8589000)
  get Phys(data[n=2]=f858a000)
  get Phys(data[n=3]=f858b000)
  get Phys(data[n=3]=f858c000)
  get Phys(data[n=4]=f858d000)
  get Phys(data[n=4]=f858e000)
  get Phys(data[n=5]=f858f000)
  get Phys(data[n=5]=f8590000)
  get Phys(data[n=5]=f8591000)
  get Phys(data[n=5]=f8592000)
  get Phys(data[n=5]=f8593000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x512e7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x512e7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 51167, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 51167, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8700000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8700000)
  get Phys(data[n=1]=f8701000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x51167, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x51167 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1fc8f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1fc8f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 83794000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=83794000)
  get Phys(data[n=1]=83795000)
  get Phys(data[n=1]=83796000)
  get Phys(data[n=1]=83797000)
  get Phys(data[n=1]=83798000)
  get Phys(data[n=1]=83799000)
  get Phys(data[n=1]=8379a000)
  get Phys(data[n=2]=8379b000)
  get Phys(data[n=2]=8379c000)
  get Phys(data[n=2]=8379d000)
  get Phys(data[n=2]=8379e000)
  get Phys(data[n=2]=8379f000)
  get Phys(data[n=2]=837a0000)
  get Phys(data[n=2]=837a1000)
  get Phys(data[n=2]=837a2000)
  get Phys(data[n=2]=837a3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1fc8f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1fc8f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1fd0f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1fd0f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 837a4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=837a4000)
  get Phys(data[n=1]=837a5000)
  get Phys(data[n=1]=837a6000)
  get Phys(data[n=1]=837a7000)
  get Phys(data[n=1]=837a8000)
  get Phys(data[n=1]=837a9000)
  get Phys(data[n=1]=837aa000)
  get Phys(data[n=1]=837ab000)
  get Phys(data[n=2]=837ac000)
  get Phys(data[n=2]=837ad000)
  get Phys(data[n=3]=837ae000)
  get Phys(data[n=3]=837af000)
  get Phys(data[n=4]=837b0000)
  get Phys(data[n=4]=837b1000)
  get Phys(data[n=5]=837b2000)
  get Phys(data[n=5]=837b3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1fd0f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1fd0f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1fd8f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1fd8f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 837b4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=837b4000)
  get Phys(data[n=1]=837b5000)
  get Phys(data[n=2]=837b6000)
  get Phys(data[n=2]=837b7000)
  get Phys(data[n=2]=837b8000)
  get Phys(data[n=2]=837b9000)
  get Phys(data[n=3]=837ba000)
  get Phys(data[n=4]=837bb000)
  get Phys(data[n=4]=837bc000)
  get Phys(data[n=4]=837bd000)
  get Phys(data[n=4]=837be000)
  get Phys(data[n=5]=837bf000)
  get Phys(data[n=5]=837c0000)
  get Phys(data[n=5]=837c1000)
  get Phys(data[n=5]=837c2000)
  get Phys(data[n=5]=837c3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1fd8f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1fd8f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1fe0f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1fe0f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 837c4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=837c4000)
  get Phys(data[n=1]=837c5000)
  get Phys(data[n=1]=837c6000)
  get Phys(data[n=2]=837c7000)
  get Phys(data[n=2]=837c8000)
  get Phys(data[n=2]=837c9000)
  get Phys(data[n=2]=837ca000)
  get Phys(data[n=2]=837cb000)
  get Phys(data[n=2]=837cc000)
  get Phys(data[n=2]=837cd000)
  get Phys(data[n=2]=837ce000)
  get Phys(data[n=3]=837cf000)
  get Phys(data[n=3]=837d0000)
  get Phys(data[n=3]=837d1000)
  get Phys(data[n=3]=837d2000)
  get Phys(data[n=3]=837d3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1fe0f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1fe0f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 25837, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 25837, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 837d4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=837d4000)
  get Phys(data[n=1]=837d5000)
  get Phys(data[n=1]=837d6000)
  get Phys(data[n=2]=837d7000)
  get Phys(data[n=2]=837d8000)
  get Phys(data[n=2]=837d9000)
  get Phys(data[n=2]=837da000)
  get Phys(data[n=2]=837db000)
  get Phys(data[n=2]=837dc000)
  get Phys(data[n=2]=837dd000)
  get Phys(data[n=2]=837de000)
  get Phys(data[n=2]=837df000)
  get Phys(data[n=3]=837e0000)
  get Phys(data[n=4]=837e1000)
  get Phys(data[n=4]=837e2000)
  get Phys(data[n=4]=837e3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x25837, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x25837 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 258b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 258b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 837e4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=837e4000)
  get Phys(data[n=1]=837e5000)
  get Phys(data[n=1]=837e6000)
  get Phys(data[n=1]=837e7000)
  get Phys(data[n=2]=837e8000)
  get Phys(data[n=2]=837e9000)
  get Phys(data[n=3]=837ea000)
  get Phys(data[n=3]=837eb000)
  get Phys(data[n=4]=837ec000)
  get Phys(data[n=4]=837ed000)
  get Phys(data[n=5]=837ee000)
  get Phys(data[n=5]=837ef000)
  get Phys(data[n=6]=837f0000)
  get Phys(data[n=7]=837f1000)
  get Phys(data[n=8]=837f2000)
  get Phys(data[n=8]=837f3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x258b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x258b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 25937, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 25937, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 837f4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=837f4000)
  get Phys(data[n=1]=837f5000)
  get Phys(data[n=2]=837f6000)
  get Phys(data[n=3]=837f7000)
  get Phys(data[n=3]=837f8000)
  get Phys(data[n=3]=837f9000)
  get Phys(data[n=3]=837fa000)
  get Phys(data[n=4]=837fb000)
  get Phys(data[n=4]=837fc000)
  get Phys(data[n=4]=837fd000)
  get Phys(data[n=4]=837fe000)
  get Phys(data[n=4]=837ff000)
  get Phys(data[n=5]=83800000)
  get Phys(data[n=6]=83801000)
  get Phys(data[n=7]=83802000)
  get Phys(data[n=7]=83803000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x25937, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x25937 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 259b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 259b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 83804000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=83804000)
  get Phys(data[n=1]=83805000)
  get Phys(data[n=1]=83806000)
  get Phys(data[n=1]=83807000)
  get Phys(data[n=1]=83808000)
  get Phys(data[n=1]=83809000)
  get Phys(data[n=2]=8380a000)
  get Phys(data[n=2]=8380b000)
  get Phys(data[n=2]=8380c000)
  get Phys(data[n=2]=8380d000)
  get Phys(data[n=2]=8380e000)
  get Phys(data[n=2]=8380f000)
  get Phys(data[n=3]=83810000)
  get Phys(data[n=3]=83811000)
  get Phys(data[n=3]=83812000)
  get Phys(data[n=3]=83813000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x259b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x259b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f9338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2dbd7, OrigWordsRequested 0x6000, DevSize 0x60
IdeReadWrite (REQ): Starting sector is 2dbd7, Number of WORDS 0x6000, DevSize 0x60
AtapiDmaSetup: mode 0x45, data f8554000, count c000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8554000)
  get Phys(data[n=1]=f8555000)
  get Phys(data[n=2]=f8556000)
  get Phys(data[n=2]=f8557000)
  get Phys(data[n=3]=f8558000)
  get Phys(data[n=3]=f8559000)
  get Phys(data[n=4]=f855a000)
  get Phys(data[n=5]=f855b000)
  get Phys(data[n=6]=f855c000)
  get Phys(data[n=6]=f855d000)
  get Phys(data[n=6]=f855e000)
  get Phys(data[n=6]=f855f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2dbd7, Count 0x60(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2dbd7 count 0x60 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered c000, full size c000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2dbd7, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 2dbd7, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8700000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8700000)
  get Phys(data[n=1]=f8701000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2dbd7, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2dbd7 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 50807, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 50807, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 83854000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=83854000)
  get Phys(data[n=1]=83855000)
  get Phys(data[n=2]=83856000)
  get Phys(data[n=2]=83857000)
  get Phys(data[n=2]=83858000)
  get Phys(data[n=2]=83859000)
  get Phys(data[n=3]=8385a000)
  get Phys(data[n=3]=8385b000)
  get Phys(data[n=3]=8385c000)
  get Phys(data[n=3]=8385d000)
  get Phys(data[n=3]=8385e000)
  get Phys(data[n=3]=8385f000)
  get Phys(data[n=4]=83860000)
  get Phys(data[n=5]=83861000)
  get Phys(data[n=6]=83862000)
  get Phys(data[n=6]=83863000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x50807, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x50807 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 50887, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 50887, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 83864000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=83864000)
  get Phys(data[n=1]=83865000)
  get Phys(data[n=1]=83866000)
  get Phys(data[n=1]=83867000)
  get Phys(data[n=1]=83868000)
  get Phys(data[n=1]=83869000)
  get Phys(data[n=2]=8386a000)
  get Phys(data[n=2]=8386b000)
  get Phys(data[n=2]=8386c000)
  get Phys(data[n=2]=8386d000)
  get Phys(data[n=2]=8386e000)
  get Phys(data[n=2]=8386f000)
  get Phys(data[n=3]=83870000)
  get Phys(data[n=3]=83871000)
  get Phys(data[n=3]=83872000)
  get Phys(data[n=3]=83873000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x50887, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x50887 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 50907, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 50907, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 83874000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=83874000)
  get Phys(data[n=1]=83875000)
  get Phys(data[n=2]=83876000)
  get Phys(data[n=2]=83877000)
  get Phys(data[n=2]=83878000)
  get Phys(data[n=2]=83879000)
  get Phys(data[n=2]=8387a000)
  get Phys(data[n=2]=8387b000)
  get Phys(data[n=2]=8387c000)
  get Phys(data[n=2]=8387d000)
  get Phys(data[n=2]=8387e000)
  get Phys(data[n=3]=8387f000)
  get Phys(data[n=4]=83880000)
  get Phys(data[n=4]=83881000)
  get Phys(data[n=4]=83882000)
  get Phys(data[n=4]=83883000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x50907, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x50907 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 50987, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 50987, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 83884000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=83884000)
  get Phys(data[n=1]=83885000)
  get Phys(data[n=1]=83886000)
  get Phys(data[n=2]=83887000)
  get Phys(data[n=2]=83888000)
  get Phys(data[n=3]=83889000)
  get Phys(data[n=3]=8388a000)
  get Phys(data[n=4]=8388b000)
  get Phys(data[n=4]=8388c000)
  get Phys(data[n=5]=8388d000)
  get Phys(data[n=5]=8388e000)
  get Phys(data[n=6]=8388f000)
  get Phys(data[n=7]=83890000)
  get Phys(data[n=8]=83891000)
  get Phys(data[n=8]=83892000)
  get Phys(data[n=8]=83893000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x50987, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x50987 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../dll/ntdll/csr/connect.c:371) Next-GEN CSRSS support
(../../win32ss/user/ntuser/sysparams.c:1571) err: UserSystemParametersInfo called without active windowstation.
(../../win32ss/user/ntuser/winsta.c:208) err: Invalid window station handle
(../../win32ss/user/ntuser/ntuser.c:161) err: Enter NtUserInitialize(0, 00000000, 00000000)
(../../win32ss/user/ntuser/display.c:79) err: InitDisplayDriver(\Device\Video0, \Registry\Machine\System\CurrentControlSet\Hardware Profiles\Current\System\CurrentControlSet\Services\VBE\Device0);
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8592848
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4f927, OrigWordsRequested 0x2200, DevSize 0x22
IdeReadWrite (REQ): Starting sector is 4f927, Number of WORDS 0x2200, DevSize 0x22
AtapiDmaSetup: mode 0x45, data f8544000, count 4400, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8544000)
  get Phys(data[n=1]=f8545000)
  get Phys(data[n=1]=f8546000)
  get Phys(data[n=2]=f8547000)
  get Phys(data[n=2]=f8548000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4f927, Count 0x22(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4f927 count 0x22 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 4400, full size 4400
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8592bdc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4f927, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 4f927, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8700000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8700000)
  get Phys(data[n=1]=f8701000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4f927, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4f927 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\System32\framebuf.dll at F857C000 with 8 pages
err:(../../win32ss/user/user32/misc/dllmain.c:353) GetConnected
(../../win32ss/user/ntuser/hook.c:1089) err: Kill Thread Hooks pti 0xb0be0600 pdo 0x0
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 14dbf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 14dbf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f852c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f852c000)
  get Phys(data[n=1]=f852d000)
  get Phys(data[n=2]=f852e000)
  get Phys(data[n=2]=f852f000)
  get Phys(data[n=2]=f8530000)
  get Phys(data[n=2]=f8531000)
  get Phys(data[n=2]=f8532000)
  get Phys(data[n=2]=f8533000)
  get Phys(data[n=2]=f8534000)
  get Phys(data[n=2]=f8535000)
  get Phys(data[n=2]=f8536000)
  get Phys(data[n=3]=f8537000)
  get Phys(data[n=4]=f8538000)
  get Phys(data[n=4]=f8539000)
  get Phys(data[n=4]=f853a000)
  get Phys(data[n=4]=f853b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x14dbf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x14dbf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 14e3f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 14e3f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f853c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f853c000)
  get Phys(data[n=1]=f853d000)
  get Phys(data[n=1]=f853e000)
  get Phys(data[n=2]=f853f000)
  get Phys(data[n=2]=f8540000)
  get Phys(data[n=3]=f8541000)
  get Phys(data[n=3]=f8542000)
  get Phys(data[n=4]=f8543000)
  get Phys(data[n=4]=f8544000)
  get Phys(data[n=5]=f8545000)
  get Phys(data[n=5]=f8546000)
  get Phys(data[n=6]=f8547000)
  get Phys(data[n=7]=f8548000)
  get Phys(data[n=8]=f8549000)
  get Phys(data[n=8]=f854a000)
  get Phys(data[n=8]=f854b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x14e3f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x14e3f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87262d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 14ebf, OrigWordsRequested 0x1900, DevSize 0x19
IdeReadWrite (REQ): Starting sector is 14ebf, Number of WORDS 0x1900, DevSize 0x19
AtapiDmaSetup: mode 0x45, data f854c000, count 3200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f854c000)
  get Phys(data[n=1]=f854d000)
  get Phys(data[n=2]=f854e000)
  get Phys(data[n=2]=f854f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x14ebf, Count 0x19(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x14ebf count 0x19 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 3200, full size 3200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87266cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 14dbf, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 14dbf, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8700000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8700000)
  get Phys(data[n=1]=f8701000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x14dbf, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x14dbf count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f92d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3896f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3896f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f852c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f852c000)
  get Phys(data[n=1]=f852d000)
  get Phys(data[n=1]=f852e000)
  get Phys(data[n=2]=f852f000)
  get Phys(data[n=2]=f8530000)
  get Phys(data[n=3]=f8531000)
  get Phys(data[n=3]=f8532000)
  get Phys(data[n=4]=f8533000)
  get Phys(data[n=4]=f8534000)
  get Phys(data[n=5]=f8535000)
  get Phys(data[n=5]=f8536000)
  get Phys(data[n=6]=f8537000)
  get Phys(data[n=7]=f8538000)
  get Phys(data[n=8]=f8539000)
  get Phys(data[n=8]=f853a000)
  get Phys(data[n=8]=f853b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3896f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3896f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f92d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 389ef, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 389ef, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f853c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f853c000)
  get Phys(data[n=1]=f853d000)
  get Phys(data[n=2]=f853e000)
  get Phys(data[n=2]=f853f000)
  get Phys(data[n=2]=f8540000)
  get Phys(data[n=2]=f8541000)
  get Phys(data[n=3]=f8542000)
  get Phys(data[n=3]=f8543000)
  get Phys(data[n=3]=f8544000)
  get Phys(data[n=3]=f8545000)
  get Phys(data[n=3]=f8546000)
  get Phys(data[n=3]=f8547000)
  get Phys(data[n=4]=f8548000)
  get Phys(data[n=4]=f8549000)
  get Phys(data[n=5]=f854a000)
  get Phys(data[n=5]=f854b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x389ef, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x389ef count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f92d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38a6f, OrigWordsRequested 0x4800, DevSize 0x48
IdeReadWrite (REQ): Starting sector is 38a6f, Number of WORDS 0x4800, DevSize 0x48
AtapiDmaSetup: mode 0x45, data f854c000, count 9000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f854c000)
  get Phys(data[n=1]=f854d000)
  get Phys(data[n=1]=f854e000)
  get Phys(data[n=1]=f854f000)
  get Phys(data[n=1]=f8550000)
  get Phys(data[n=1]=f8551000)
  get Phys(data[n=2]=f8552000)
  get Phys(data[n=2]=f8553000)
  get Phys(data[n=2]=f8554000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38a6f, Count 0x48(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38a6f count 0x48 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 9000, full size 9000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3896f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3896f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f86ff000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86ff000)
  get Phys(data[n=1]=f8700000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3896f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3896f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../win32ss/user/ntuser/sysparams.c:1571) err: UserSystemParametersInfo called without active windowstation.
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 50c07, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 50c07, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 83d14000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=83d14000)
  get Phys(data[n=1]=83d15000)
  get Phys(data[n=2]=83d16000)
  get Phys(data[n=2]=83d17000)
  get Phys(data[n=2]=83d18000)
  get Phys(data[n=2]=83d19000)
  get Phys(data[n=3]=83d1a000)
  get Phys(data[n=4]=83d1b000)
  get Phys(data[n=4]=83d1c000)
  get Phys(data[n=4]=83d1d000)
  get Phys(data[n=5]=83d1e000)
  get Phys(data[n=5]=83d1f000)
  get Phys(data[n=6]=83d20000)
  get Phys(data[n=6]=83d21000)
  get Phys(data[n=6]=83d22000)
  get Phys(data[n=6]=83d23000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x50c07, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x50c07 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 50c87, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 50c87, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 83d24000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=83d24000)
  get Phys(data[n=1]=83d25000)
  get Phys(data[n=1]=83d26000)
  get Phys(data[n=1]=83d27000)
  get Phys(data[n=1]=83d28000)
  get Phys(data[n=2]=83d29000)
  get Phys(data[n=3]=83d2a000)
  get Phys(data[n=3]=83d2b000)
  get Phys(data[n=3]=83d2c000)
  get Phys(data[n=3]=83d2d000)
  get Phys(data[n=3]=83d2e000)
  get Phys(data[n=3]=83d2f000)
  get Phys(data[n=3]=83d30000)
  get Phys(data[n=4]=83d31000)
  get Phys(data[n=4]=83d32000)
  get Phys(data[n=5]=83d33000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x50c87, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x50c87 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 50d07, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 50d07, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 83d34000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=83d34000)
  get Phys(data[n=1]=83d35000)
  get Phys(data[n=1]=83d36000)
  get Phys(data[n=2]=83d37000)
  get Phys(data[n=2]=83d38000)
  get Phys(data[n=3]=83d39000)
  get Phys(data[n=4]=83d3a000)
  get Phys(data[n=5]=83d3b000)
  get Phys(data[n=5]=83d3c000)
  get Phys(data[n=5]=83d3d000)
  get Phys(data[n=5]=83d3e000)
  get Phys(data[n=6]=83d3f000)
  get Phys(data[n=7]=83d40000)
  get Phys(data[n=7]=83d41000)
  get Phys(data[n=7]=83d42000)
  get Phys(data[n=7]=83d43000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x50d07, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x50d07 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 50d87, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 50d87, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 83d44000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=83d44000)
  get Phys(data[n=1]=83d45000)
  get Phys(data[n=1]=83d46000)
  get Phys(data[n=1]=83d47000)
  get Phys(data[n=1]=83d48000)
  get Phys(data[n=1]=83d49000)
  get Phys(data[n=2]=83d4a000)
  get Phys(data[n=2]=83d4b000)
  get Phys(data[n=3]=83d4c000)
  get Phys(data[n=3]=83d4d000)
  get Phys(data[n=3]=83d4e000)
  get Phys(data[n=3]=83d4f000)
  get Phys(data[n=3]=83d50000)
  get Phys(data[n=3]=83d51000)
  get Phys(data[n=3]=83d52000)
  get Phys(data[n=3]=83d53000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x50d87, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x50d87 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 50a07, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 50a07, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 83d54000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=83d54000)
  get Phys(data[n=1]=83d55000)
  get Phys(data[n=1]=83d56000)
  get Phys(data[n=1]=83d57000)
  get Phys(data[n=2]=83d58000)
  get Phys(data[n=3]=83d59000)
  get Phys(data[n=3]=83d5a000)
  get Phys(data[n=3]=83d5b000)
  get Phys(data[n=4]=83d5c000)
  get Phys(data[n=4]=83d5d000)
  get Phys(data[n=5]=83d5e000)
  get Phys(data[n=5]=83d5f000)
  get Phys(data[n=5]=83d60000)
  get Phys(data[n=5]=83d61000)
  get Phys(data[n=5]=83d62000)
  get Phys(data[n=5]=83d63000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x50a07, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x50a07 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 50a87, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 50a87, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 83d64000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=83d64000)
  get Phys(data[n=1]=83d65000)
  get Phys(data[n=1]=83d66000)
  get Phys(data[n=2]=83d67000)
  get Phys(data[n=3]=83d68000)
  get Phys(data[n=3]=83d69000)
  get Phys(data[n=3]=83d6a000)
  get Phys(data[n=3]=83d6b000)
  get Phys(data[n=3]=83d6c000)
  get Phys(data[n=3]=83d6d000)
  get Phys(data[n=3]=83d6e000)
  get Phys(data[n=4]=83d6f000)
  get Phys(data[n=4]=83d70000)
  get Phys(data[n=5]=83d71000)
  get Phys(data[n=5]=83d72000)
  get Phys(data[n=6]=83d73000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x50a87, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x50a87 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 50b07, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 50b07, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 83d74000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=83d74000)
  get Phys(data[n=1]=83d75000)
  get Phys(data[n=1]=83d76000)
  get Phys(data[n=2]=83d77000)
  get Phys(data[n=3]=83d78000)
  get Phys(data[n=4]=83d79000)
  get Phys(data[n=4]=83d7a000)
  get Phys(data[n=4]=83d7b000)
  get Phys(data[n=4]=83d7c000)
  get Phys(data[n=5]=83d7d000)
  get Phys(data[n=6]=83d7e000)
  get Phys(data[n=6]=83d7f000)
  get Phys(data[n=6]=83d80000)
  get Phys(data[n=6]=83d81000)
  get Phys(data[n=7]=83d82000)
  get Phys(data[n=7]=83d83000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x50b07, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x50b07 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 50b87, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 50b87, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 83d84000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=83d84000)
  get Phys(data[n=1]=83d85000)
  get Phys(data[n=1]=83d86000)
  get Phys(data[n=1]=83d87000)
  get Phys(data[n=2]=83d88000)
  get Phys(data[n=2]=83d89000)
  get Phys(data[n=3]=83d8a000)
  get Phys(data[n=3]=83d8b000)
  get Phys(data[n=3]=83d8c000)
  get Phys(data[n=3]=83d8d000)
  get Phys(data[n=3]=83d8e000)
  get Phys(data[n=3]=83d8f000)
  get Phys(data[n=3]=83d90000)
  get Phys(data[n=3]=83d91000)
  get Phys(data[n=4]=83d92000)
  get Phys(data[n=4]=83d93000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x50b87, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x50b87 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3aa9f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3aa9f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f851c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f851c000)
  get Phys(data[n=1]=f851d000)
  get Phys(data[n=2]=f851e000)
  get Phys(data[n=3]=f851f000)
  get Phys(data[n=3]=f8520000)
  get Phys(data[n=4]=f8521000)
  get Phys(data[n=4]=f8522000)
  get Phys(data[n=4]=f8523000)
  get Phys(data[n=4]=f8524000)
  get Phys(data[n=4]=f8525000)
  get Phys(data[n=4]=f8526000)
  get Phys(data[n=4]=f8527000)
  get Phys(data[n=4]=f8528000)
  get Phys(data[n=4]=f8529000)
  get Phys(data[n=5]=f852a000)
  get Phys(data[n=6]=f852b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3aa9f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3aa9f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ab1f, OrigWordsRequested 0x3300, DevSize 0x33
IdeReadWrite (REQ): Starting sector is 3ab1f, Number of WORDS 0x3300, DevSize 0x33
AtapiDmaSetup: mode 0x45, data f852c000, count 6600, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f852c000)
  get Phys(data[n=1]=f852d000)
  get Phys(data[n=1]=f852e000)
  get Phys(data[n=1]=f852f000)
  get Phys(data[n=1]=f8530000)
  get Phys(data[n=1]=f8531000)
  get Phys(data[n=2]=f8532000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ab1f, Count 0x33(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3ab1f count 0x33 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 6600, full size 6600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3aa9f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3aa9f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f86ff000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86ff000)
  get Phys(data[n=1]=f8700000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3aa9f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3aa9f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 371ff, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 371ff, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f851c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f851c000)
  get Phys(data[n=1]=f851d000)
  get Phys(data[n=1]=f851e000)
  get Phys(data[n=1]=f851f000)
  get Phys(data[n=1]=f8520000)
  get Phys(data[n=1]=f8521000)
  get Phys(data[n=1]=f8522000)
  get Phys(data[n=1]=f8523000)
  get Phys(data[n=1]=f8524000)
  get Phys(data[n=2]=f8525000)
  get Phys(data[n=3]=f8526000)
  get Phys(data[n=3]=f8527000)
  get Phys(data[n=3]=f8528000)
  get Phys(data[n=3]=f8529000)
  get Phys(data[n=3]=f852a000)
  get Phys(data[n=3]=f852b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x371ff, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x371ff count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3727f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3727f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f852c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f852c000)
  get Phys(data[n=1]=f852d000)
  get Phys(data[n=1]=f852e000)
  get Phys(data[n=2]=f852f000)
  get Phys(data[n=2]=f8530000)
  get Phys(data[n=3]=f8531000)
  get Phys(data[n=3]=f8532000)
  get Phys(data[n=4]=f8533000)
  get Phys(data[n=4]=f8534000)
  get Phys(data[n=5]=f8535000)
  get Phys(data[n=6]=f8536000)
  get Phys(data[n=7]=f8537000)
  get Phys(data[n=7]=f8538000)
  get Phys(data[n=7]=f8539000)
  get Phys(data[n=7]=f853a000)
  get Phys(data[n=8]=f853b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3727f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3727f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 372ff, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 372ff, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f853c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f853c000)
  get Phys(data[n=1]=f853d000)
  get Phys(data[n=1]=f853e000)
  get Phys(data[n=1]=f853f000)
  get Phys(data[n=2]=f8540000)
  get Phys(data[n=2]=f8541000)
  get Phys(data[n=2]=f8542000)
  get Phys(data[n=2]=f8543000)
  get Phys(data[n=2]=f8544000)
  get Phys(data[n=2]=f8545000)
  get Phys(data[n=3]=f8546000)
  get Phys(data[n=3]=f8547000)
  get Phys(data[n=4]=f8548000)
  get Phys(data[n=4]=f8549000)
  get Phys(data[n=4]=f854a000)
  get Phys(data[n=4]=f854b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x372ff, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x372ff count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3737f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3737f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f854c000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f854c000)
  get Phys(data[n=1]=f854d000)
  get Phys(data[n=1]=f854e000)
  get Phys(data[n=1]=f854f000)
  get Phys(data[n=2]=f8550000)
  get Phys(data[n=2]=f8551000)
  get Phys(data[n=2]=f8552000)
  get Phys(data[n=2]=f8553000)
  get Phys(data[n=2]=f8554000)
  get Phys(data[n=2]=f8555000)
  get Phys(data[n=3]=f8556000)
  get Phys(data[n=3]=f8557000)
  get Phys(data[n=3]=f8558000)
  get Phys(data[n=3]=f8559000)
  get Phys(data[n=4]=f855a000)
  get Phys(data[n=4]=f855b000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3737f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3737f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 371ff, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 371ff, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f86ff000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86ff000)
  get Phys(data[n=1]=f8700000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x371ff, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x371ff count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf85928a8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e7df, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 1e7df, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8317000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8317000)
  get Phys(data[n=1]=f8318000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e7df, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e7df count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8592c3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e7df, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 1e7df, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f86ff000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86ff000)
  get Phys(data[n=1]=f8700000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e7df, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e7df count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\System32\kbdpl1.dll at F834F000 with 8 pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8593260
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 25a37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 25a37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84614000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84614000)
  get Phys(data[n=1]=84615000)
  get Phys(data[n=1]=84616000)
  get Phys(data[n=2]=84617000)
  get Phys(data[n=2]=84618000)
  get Phys(data[n=2]=84619000)
  get Phys(data[n=2]=8461a000)
  get Phys(data[n=2]=8461b000)
  get Phys(data[n=2]=8461c000)
  get Phys(data[n=2]=8461d000)
  get Phys(data[n=2]=8461e000)
  get Phys(data[n=3]=8461f000)
  get Phys(data[n=3]=84620000)
  get Phys(data[n=3]=84621000)
  get Phys(data[n=3]=84622000)
  get Phys(data[n=3]=84623000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x25a37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x25a37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8593260
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 25ab7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 25ab7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84624000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84624000)
  get Phys(data[n=1]=84625000)
  get Phys(data[n=1]=84626000)
  get Phys(data[n=1]=84627000)
  get Phys(data[n=1]=84628000)
  get Phys(data[n=2]=84629000)
  get Phys(data[n=2]=8462a000)
  get Phys(data[n=3]=8462b000)
  get Phys(data[n=3]=8462c000)
  get Phys(data[n=3]=8462d000)
  get Phys(data[n=3]=8462e000)
  get Phys(data[n=3]=8462f000)
  get Phys(data[n=3]=84630000)
  get Phys(data[n=3]=84631000)
  get Phys(data[n=3]=84632000)
  get Phys(data[n=3]=84633000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x25ab7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x25ab7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8593260
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 25b37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 25b37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84634000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84634000)
  get Phys(data[n=1]=84635000)
  get Phys(data[n=1]=84636000)
  get Phys(data[n=1]=84637000)
  get Phys(data[n=1]=84638000)
  get Phys(data[n=1]=84639000)
  get Phys(data[n=1]=8463a000)
  get Phys(data[n=1]=8463b000)
  get Phys(data[n=2]=8463c000)
  get Phys(data[n=2]=8463d000)
  get Phys(data[n=3]=8463e000)
  get Phys(data[n=3]=8463f000)
  get Phys(data[n=4]=84640000)
  get Phys(data[n=4]=84641000)
  get Phys(data[n=5]=84642000)
  get Phys(data[n=5]=84643000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x25b37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x25b37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8593260
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 25bb7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 25bb7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84644000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84644000)
  get Phys(data[n=1]=84645000)
  get Phys(data[n=2]=84646000)
  get Phys(data[n=2]=84647000)
  get Phys(data[n=2]=84648000)
  get Phys(data[n=2]=84649000)
  get Phys(data[n=3]=8464a000)
  get Phys(data[n=3]=8464b000)
  get Phys(data[n=3]=8464c000)
  get Phys(data[n=4]=8464d000)
  get Phys(data[n=4]=8464e000)
  get Phys(data[n=5]=8464f000)
  get Phys(data[n=5]=84650000)
  get Phys(data[n=5]=84651000)
  get Phys(data[n=5]=84652000)
  get Phys(data[n=5]=84653000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x25bb7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x25bb7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf85928a8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e7cf, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 1e7cf, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f830f000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f830f000)
  get Phys(data[n=1]=f8310000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e7cf, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e7cf count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8592c3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e7cf, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 1e7cf, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f86ff000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86ff000)
  get Phys(data[n=1]=f8700000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e7cf, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e7cf count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\System32\kbdpl.dll at F8347000 with 8 pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf85928a8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e947, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 1e947, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8307000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8307000)
  get Phys(data[n=1]=f8308000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e947, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e947 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8592c3c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e947, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 1e947, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f86ff000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86ff000)
  get Phys(data[n=1]=f8700000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e947, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e947 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\System32\kbdus.dll at F833F000 with 8 pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf85932d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 14acf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 14acf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f82ff000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ff000)
  get Phys(data[n=1]=f8300000)
  get Phys(data[n=1]=f8301000)
  get Phys(data[n=2]=f8302000)
  get Phys(data[n=2]=f8303000)
  get Phys(data[n=3]=f8304000)
  get Phys(data[n=3]=f8305000)
  get Phys(data[n=4]=f8306000)
  get Phys(data[n=5]=f8307000)
  get Phys(data[n=6]=f8308000)
  get Phys(data[n=6]=f8309000)
  get Phys(data[n=6]=f830a000)
  get Phys(data[n=6]=f830b000)
  get Phys(data[n=7]=f830c000)
  get Phys(data[n=7]=f830d000)
  get Phys(data[n=7]=f830e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x14acf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x14acf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf85932d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 14b4f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 14b4f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f830f000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f830f000)
  get Phys(data[n=1]=f8310000)
  get Phys(data[n=2]=f8311000)
  get Phys(data[n=2]=f8312000)
  get Phys(data[n=3]=f8313000)
  get Phys(data[n=3]=f8314000)
  get Phys(data[n=3]=f8315000)
  get Phys(data[n=3]=f8316000)
  get Phys(data[n=4]=f8317000)
  get Phys(data[n=4]=f8318000)
  get Phys(data[n=5]=f8319000)
  get Phys(data[n=5]=f831a000)
  get Phys(data[n=5]=f831b000)
  get Phys(data[n=5]=f831c000)
  get Phys(data[n=5]=f831d000)
  get Phys(data[n=5]=f831e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x14b4f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x14b4f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf85932d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 14bcf, OrigWordsRequested 0x2900, DevSize 0x29
IdeReadWrite (REQ): Starting sector is 14bcf, Number of WORDS 0x2900, DevSize 0x29
AtapiDmaSetup: mode 0x45, data f831f000, count 5200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f831f000)
  get Phys(data[n=1]=f8320000)
  get Phys(data[n=2]=f8321000)
  get Phys(data[n=2]=f8322000)
  get Phys(data[n=2]=f8323000)
  get Phys(data[n=2]=f8324000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x14bcf, Count 0x29(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x14bcf count 0x29 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 5200, full size 5200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf85936cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 14acf, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 14acf, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f86ff000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86ff000)
  get Phys(data[n=1]=f8700000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x14acf, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x14acf count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8593338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1485f, OrigWordsRequested 0x3900, DevSize 0x39
IdeReadWrite (REQ): Starting sector is 1485f, Number of WORDS 0x3900, DevSize 0x39
AtapiDmaSetup: mode 0x45, data f82ff000, count 7200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ff000)
  get Phys(data[n=1]=f8300000)
  get Phys(data[n=2]=f8301000)
  get Phys(data[n=3]=f8302000)
  get Phys(data[n=4]=f8303000)
  get Phys(data[n=4]=f8304000)
  get Phys(data[n=4]=f8305000)
  get Phys(data[n=4]=f8306000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1485f, Count 0x39(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1485f count 0x39 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 7200, full size 7200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf85936cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1485f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 1485f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f86fe000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f86fe000)
  get Phys(data[n=1]=f86ff000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1485f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1485f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f92d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 26347, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 26347, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f82be000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82be000)
  get Phys(data[n=1]=f82bf000)
  get Phys(data[n=2]=f82c0000)
  get Phys(data[n=2]=f82c1000)
  get Phys(data[n=2]=f82c2000)
  get Phys(data[n=2]=f82c3000)
  get Phys(data[n=2]=f82c4000)
  get Phys(data[n=2]=f82c5000)
  get Phys(data[n=3]=f82c6000)
  get Phys(data[n=3]=f82c7000)
  get Phys(data[n=3]=f82c8000)
  get Phys(data[n=3]=f82c9000)
  get Phys(data[n=3]=f82ca000)
  get Phys(data[n=4]=f82cb000)
  get Phys(data[n=5]=f82cc000)
  get Phys(data[n=5]=f82cd000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x26347, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x26347 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f92d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 263c7, OrigWordsRequested 0x5000, DevSize 0x50
IdeReadWrite (REQ): Starting sector is 263c7, Number of WORDS 0x5000, DevSize 0x50
AtapiDmaSetup: mode 0x45, data f82ce000, count a000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ce000)
  get Phys(data[n=1]=f82cf000)
  get Phys(data[n=1]=f82d0000)
  get Phys(data[n=2]=f82d1000)
  get Phys(data[n=3]=f82d2000)
  get Phys(data[n=3]=f82d3000)
  get Phys(data[n=3]=f82d4000)
  get Phys(data[n=3]=f82d5000)
  get Phys(data[n=4]=f82d6000)
  get Phys(data[n=4]=f82d7000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x263c7, Count 0x50(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x263c7 count 0x50 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a000, full size a000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 26347, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 26347, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f82fd000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82fd000)
  get Phys(data[n=1]=f82fe000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x26347, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x26347 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf85932d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2730f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2730f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f82ff000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ff000)
  get Phys(data[n=1]=f8300000)
  get Phys(data[n=2]=f8301000)
  get Phys(data[n=2]=f8302000)
  get Phys(data[n=2]=f8303000)
  get Phys(data[n=2]=f8304000)
  get Phys(data[n=2]=f8305000)
  get Phys(data[n=2]=f8306000)
  get Phys(data[n=2]=f8307000)
  get Phys(data[n=2]=f8308000)
  get Phys(data[n=3]=f8309000)
  get Phys(data[n=3]=f830a000)
  get Phys(data[n=3]=f830b000)
  get Phys(data[n=3]=f830c000)
  get Phys(data[n=3]=f830d000)
  get Phys(data[n=3]=f830e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2730f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2730f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf85932d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2738f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2738f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f830f000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f830f000)
  get Phys(data[n=1]=f8310000)
  get Phys(data[n=1]=f8311000)
  get Phys(data[n=1]=f8312000)
  get Phys(data[n=1]=f8313000)
  get Phys(data[n=2]=f8314000)
  get Phys(data[n=3]=f8315000)
  get Phys(data[n=3]=f8316000)
  get Phys(data[n=3]=f8317000)
  get Phys(data[n=3]=f8318000)
  get Phys(data[n=3]=f8319000)
  get Phys(data[n=4]=f831a000)
  get Phys(data[n=5]=f831b000)
  get Phys(data[n=5]=f831c000)
  get Phys(data[n=5]=f831d000)
  get Phys(data[n=5]=f831e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2738f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2738f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf85932d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2740f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2740f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f831f000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f831f000)
  get Phys(data[n=1]=f8320000)
  get Phys(data[n=1]=f8321000)
  get Phys(data[n=1]=f8322000)
  get Phys(data[n=1]=f8323000)
  get Phys(data[n=1]=f8324000)
  get Phys(data[n=2]=f8325000)
  get Phys(data[n=3]=f8326000)
  get Phys(data[n=3]=f8327000)
  get Phys(data[n=3]=f8328000)
  get Phys(data[n=3]=f8329000)
  get Phys(data[n=4]=f832a000)
  get Phys(data[n=4]=f832b000)
  get Phys(data[n=5]=f832c000)
  get Phys(data[n=5]=f832d000)
  get Phys(data[n=6]=f832e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2740f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2740f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf85932d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2748f, OrigWordsRequested 0x1e00, DevSize 0x1e
IdeReadWrite (REQ): Starting sector is 2748f, Number of WORDS 0x1e00, DevSize 0x1e
AtapiDmaSetup: mode 0x45, data f832f000, count 3c00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f832f000)
  get Phys(data[n=1]=f8330000)
  get Phys(data[n=1]=f8331000)
  get Phys(data[n=1]=f8332000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2748f, Count 0x1e(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2748f count 0x1e feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 3c00, full size 3c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf85936cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2730f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 2730f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f833d000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f833d000)
  get Phys(data[n=1]=f833e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2730f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2730f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87056d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2f0ff, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2f0ff, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 846d4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=846d4000)
  get Phys(data[n=1]=846d5000)
  get Phys(data[n=1]=846d6000)
  get Phys(data[n=1]=846d7000)
  get Phys(data[n=2]=846d8000)
  get Phys(data[n=2]=846d9000)
  get Phys(data[n=3]=846da000)
  get Phys(data[n=3]=846db000)
  get Phys(data[n=3]=846dc000)
  get Phys(data[n=3]=846dd000)
  get Phys(data[n=3]=846de000)
  get Phys(data[n=3]=846df000)
  get Phys(data[n=3]=846e0000)
  get Phys(data[n=3]=846e1000)
  get Phys(data[n=4]=846e2000)
  get Phys(data[n=4]=846e3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2f0ff, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2f0ff count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
err:(../../win32ss/user/user32/windows/window.c:321) CreateWindowExA RegisterSystemControls
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87056d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2f17f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2f17f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 846e4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=846e4000)
  get Phys(data[n=1]=846e5000)
  get Phys(data[n=1]=846e6000)
  get Phys(data[n=1]=846e7000)
  get Phys(data[n=2]=846e8000)
  get Phys(data[n=2]=846e9000)
  get Phys(data[n=2]=846ea000)
  get Phys(data[n=2]=846eb000)
  get Phys(data[n=3]=846ec000)
  get Phys(data[n=3]=846ed000)
  get Phys(data[n=4]=846ee000)
  get Phys(data[n=4]=846ef000)
  get Phys(data[n=4]=846f0000)
  get Phys(data[n=4]=846f1000)
  get Phys(data[n=4]=846f2000)
  get Phys(data[n=5]=846f3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2f17f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2f17f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87056d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2f1ff, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2f1ff, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 846f4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=846f4000)
  get Phys(data[n=1]=846f5000)
  get Phys(data[n=1]=846f6000)
  get Phys(data[n=1]=846f7000)
  get Phys(data[n=2]=846f8000)
  get Phys(data[n=2]=846f9000)
  get Phys(data[n=2]=846fa000)
  get Phys(data[n=2]=846fb000)
  get Phys(data[n=2]=846fc000)
  get Phys(data[n=2]=846fd000)
  get Phys(data[n=2]=846fe000)
  get Phys(data[n=3]=846ff000)
  get Phys(data[n=3]=84700000)
  get Phys(data[n=3]=84701000)
  get Phys(data[n=3]=84702000)
  get Phys(data[n=4]=84703000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2f1ff, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2f1ff count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87056d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2f27f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2f27f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84704000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84704000)
  get Phys(data[n=1]=84705000)
  get Phys(data[n=1]=84706000)
  get Phys(data[n=2]=84707000)
  get Phys(data[n=3]=84708000)
  get Phys(data[n=4]=84709000)
  get Phys(data[n=4]=8470a000)
  get Phys(data[n=4]=8470b000)
  get Phys(data[n=4]=8470c000)
  get Phys(data[n=5]=8470d000)
  get Phys(data[n=5]=8470e000)
  get Phys(data[n=5]=8470f000)
  get Phys(data[n=5]=84710000)
  get Phys(data[n=5]=84711000)
  get Phys(data[n=6]=84712000)
  get Phys(data[n=6]=84713000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2f27f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2f27f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f92d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3aecf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3aecf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f82ef000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ef000)
  get Phys(data[n=1]=f82f0000)
  get Phys(data[n=1]=f82f1000)
  get Phys(data[n=1]=f82f2000)
  get Phys(data[n=1]=f82f3000)
  get Phys(data[n=2]=f82f4000)
  get Phys(data[n=2]=f82f5000)
  get Phys(data[n=2]=f82f6000)
  get Phys(data[n=2]=f82f7000)
  get Phys(data[n=2]=f82f8000)
  get Phys(data[n=3]=f82f9000)
  get Phys(data[n=4]=f82fa000)
  get Phys(data[n=4]=f82fb000)
  get Phys(data[n=4]=f82fc000)
  get Phys(data[n=4]=f82fd000)
  get Phys(data[n=5]=f82fe000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3aecf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3aecf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f92d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3af4f, OrigWordsRequested 0x7000, DevSize 0x70
IdeReadWrite (REQ): Starting sector is 3af4f, Number of WORDS 0x7000, DevSize 0x70
AtapiDmaSetup: mode 0x45, data f82ff000, count e000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ff000)
  get Phys(data[n=1]=f8300000)
  get Phys(data[n=1]=f8301000)
  get Phys(data[n=2]=f8302000)
  get Phys(data[n=2]=f8303000)
  get Phys(data[n=2]=f8304000)
  get Phys(data[n=3]=f8305000)
  get Phys(data[n=3]=f8306000)
  get Phys(data[n=4]=f8307000)
  get Phys(data[n=5]=f8308000)
  get Phys(data[n=6]=f8309000)
  get Phys(data[n=7]=f830a000)
  get Phys(data[n=8]=f830b000)
  get Phys(data[n=8]=f830c000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3af4f, Count 0x70(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3af4f count 0x70 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e000, full size e000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3aecf, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3aecf, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f832d000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f832d000)
  get Phys(data[n=1]=f832e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3aecf, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3aecf count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87052d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 23667, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 23667, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f82ef000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ef000)
  get Phys(data[n=1]=f82f0000)
  get Phys(data[n=1]=f82f1000)
  get Phys(data[n=2]=f82f2000)
  get Phys(data[n=3]=f82f3000)
  get Phys(data[n=3]=f82f4000)
  get Phys(data[n=3]=f82f5000)
  get Phys(data[n=3]=f82f6000)
  get Phys(data[n=4]=f82f7000)
  get Phys(data[n=4]=f82f8000)
  get Phys(data[n=4]=f82f9000)
  get Phys(data[n=4]=f82fa000)
  get Phys(data[n=5]=f82fb000)
  get Phys(data[n=5]=f82fc000)
  get Phys(data[n=5]=f82fd000)
  get Phys(data[n=6]=f82fe000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x23667, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x23667 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87052d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 236e7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 236e7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f82ff000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ff000)
  get Phys(data[n=1]=f8300000)
  get Phys(data[n=1]=f8301000)
  get Phys(data[n=1]=f8302000)
  get Phys(data[n=1]=f8303000)
  get Phys(data[n=2]=f8304000)
  get Phys(data[n=2]=f8305000)
  get Phys(data[n=3]=f8306000)
  get Phys(data[n=4]=f8307000)
  get Phys(data[n=5]=f8308000)
  get Phys(data[n=5]=f8309000)
  get Phys(data[n=5]=f830a000)
  get Phys(data[n=5]=f830b000)
  get Phys(data[n=6]=f830c000)
  get Phys(data[n=6]=f830d000)
  get Phys(data[n=6]=f830e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x236e7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x236e7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87052d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 23767, OrigWordsRequested 0x2900, DevSize 0x29
IdeReadWrite (REQ): Starting sector is 23767, Number of WORDS 0x2900, DevSize 0x29
AtapiDmaSetup: mode 0x45, data f830f000, count 5200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f830f000)
  get Phys(data[n=1]=f8310000)
  get Phys(data[n=2]=f8311000)
  get Phys(data[n=2]=f8312000)
  get Phys(data[n=3]=f8313000)
  get Phys(data[n=3]=f8314000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x23767, Count 0x29(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x23767 count 0x29 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 5200, full size 5200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 23667, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 23667, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f832d000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f832d000)
  get Phys(data[n=1]=f832e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x23667, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x23667 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f92d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 24f97, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 24f97, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f82ef000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ef000)
  get Phys(data[n=1]=f82f0000)
  get Phys(data[n=2]=f82f1000)
  get Phys(data[n=2]=f82f2000)
  get Phys(data[n=2]=f82f3000)
  get Phys(data[n=2]=f82f4000)
  get Phys(data[n=3]=f82f5000)
  get Phys(data[n=3]=f82f6000)
  get Phys(data[n=3]=f82f7000)
  get Phys(data[n=4]=f82f8000)
  get Phys(data[n=4]=f82f9000)
  get Phys(data[n=5]=f82fa000)
  get Phys(data[n=5]=f82fb000)
  get Phys(data[n=5]=f82fc000)
  get Phys(data[n=5]=f82fd000)
  get Phys(data[n=6]=f82fe000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x24f97, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x24f97 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f92d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 25017, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 25017, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f82ff000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ff000)
  get Phys(data[n=1]=f8300000)
  get Phys(data[n=2]=f8301000)
  get Phys(data[n=3]=f8302000)
  get Phys(data[n=3]=f8303000)
  get Phys(data[n=3]=f8304000)
  get Phys(data[n=3]=f8305000)
  get Phys(data[n=4]=f8306000)
  get Phys(data[n=4]=f8307000)
  get Phys(data[n=4]=f8308000)
  get Phys(data[n=4]=f8309000)
  get Phys(data[n=4]=f830a000)
  get Phys(data[n=5]=f830b000)
  get Phys(data[n=5]=f830c000)
  get Phys(data[n=6]=f830d000)
  get Phys(data[n=6]=f830e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x25017, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x25017 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f92d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 25097, OrigWordsRequested 0x1300, DevSize 0x13
IdeReadWrite (REQ): Starting sector is 25097, Number of WORDS 0x1300, DevSize 0x13
AtapiDmaSetup: mode 0x45, data f830f000, count 2600, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f830f000)
  get Phys(data[n=1]=f8310000)
  get Phys(data[n=2]=f8311000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x25097, Count 0x13(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x25097 count 0x13 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2600, full size 2600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 24f97, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 24f97, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f832d000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f832d000)
  get Phys(data[n=1]=f832e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x24f97, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x24f97 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87056cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 24f97, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 24f97, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f832b000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f832b000)
  get Phys(data[n=1]=f832c000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x24f97, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x24f97 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87052d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 23567, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 23567, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f82ef000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ef000)
  get Phys(data[n=1]=f82f0000)
  get Phys(data[n=2]=f82f1000)
  get Phys(data[n=2]=f82f2000)
  get Phys(data[n=3]=f82f3000)
  get Phys(data[n=4]=f82f4000)
  get Phys(data[n=5]=f82f5000)
  get Phys(data[n=6]=f82f6000)
  get Phys(data[n=7]=f82f7000)
  get Phys(data[n=8]=f82f8000)
  get Phys(data[n=9]=f82f9000)
  get Phys(data[n=9]=f82fa000)
  get Phys(data[n=9]=f82fb000)
  get Phys(data[n=9]=f82fc000)
  get Phys(data[n=10]=f82fd000)
  get Phys(data[n=10]=f82fe000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x23567, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x23567 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87052d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 235e7, OrigWordsRequested 0x7a00, DevSize 0x7a
IdeReadWrite (REQ): Starting sector is 235e7, Number of WORDS 0x7a00, DevSize 0x7a
AtapiDmaSetup: mode 0x45, data f82ff000, count f400, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ff000)
  get Phys(data[n=1]=f8300000)
  get Phys(data[n=1]=f8301000)
  get Phys(data[n=2]=f8302000)
  get Phys(data[n=2]=f8303000)
  get Phys(data[n=3]=f8304000)
  get Phys(data[n=3]=f8305000)
  get Phys(data[n=3]=f8306000)
  get Phys(data[n=3]=f8307000)
  get Phys(data[n=4]=f8308000)
  get Phys(data[n=4]=f8309000)
  get Phys(data[n=5]=f830a000)
  get Phys(data[n=5]=f830b000)
  get Phys(data[n=5]=f830c000)
  get Phys(data[n=5]=f830d000)
  get Phys(data[n=5]=f830e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x235e7, Count 0x7a(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x235e7 count 0x7a feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered f400, full size f400
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf87056cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 23567, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 23567, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f832d000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f832d000)
  get Phys(data[n=1]=f832e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x23567, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x23567 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f92d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2f66f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2f66f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f82ef000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ef000)
  get Phys(data[n=1]=f82f0000)
  get Phys(data[n=1]=f82f1000)
  get Phys(data[n=1]=f82f2000)
  get Phys(data[n=2]=f82f3000)
  get Phys(data[n=3]=f82f4000)
  get Phys(data[n=3]=f82f5000)
  get Phys(data[n=3]=f82f6000)
  get Phys(data[n=3]=f82f7000)
  get Phys(data[n=4]=f82f8000)
  get Phys(data[n=4]=f82f9000)
  get Phys(data[n=4]=f82fa000)
  get Phys(data[n=4]=f82fb000)
  get Phys(data[n=5]=f82fc000)
  get Phys(data[n=5]=f82fd000)
  get Phys(data[n=5]=f82fe000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2f66f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2f66f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/se/semgr.c:705) HACK: Should deny access for caller: granted 0x90003, desired 0x190003 (generic mapping B1286ED8).
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f92d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2f6ef, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2f6ef, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f82ff000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ff000)
  get Phys(data[n=1]=f8300000)
  get Phys(data[n=2]=f8301000)
  get Phys(data[n=2]=f8302000)
  get Phys(data[n=3]=f8303000)
  get Phys(data[n=3]=f8304000)
  get Phys(data[n=4]=f8305000)
  get Phys(data[n=5]=f8306000)
  get Phys(data[n=6]=f8307000)
  get Phys(data[n=7]=f8308000)
  get Phys(data[n=8]=f8309000)
  get Phys(data[n=8]=f830a000)
  get Phys(data[n=8]=f830b000)
  get Phys(data[n=8]=f830c000)
  get Phys(data[n=9]=f830d000)
  get Phys(data[n=9]=f830e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2f6ef, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2f6ef count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f92d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2f76f, OrigWordsRequested 0x1d00, DevSize 0x1d
IdeReadWrite (REQ): Starting sector is 2f76f, Number of WORDS 0x1d00, DevSize 0x1d
AtapiDmaSetup: mode 0x45, data f830f000, count 3a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f830f000)
  get Phys(data[n=1]=f8310000)
  get Phys(data[n=1]=f8311000)
  get Phys(data[n=2]=f8312000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2f76f, Count 0x1d(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2f76f count 0x1d feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 3a00, full size 3a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f96cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2f66f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 2f66f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f832d000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f832d000)
  get Phys(data[n=1]=f832e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2f66f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2f66f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/se/semgr.c:705) HACK: Should deny access for caller: granted 0x90003, desired 0x190003 (generic mapping B1286ED8).
Boot took 111853322354 cycles!
Interrupts: 4693 System Calls: 15556 Context Switches: 1270
(../../ntoskrnl/se/semgr.c:705) HACK: Should deny access for caller: granted 0x90003, desired 0x190003 (generic mapping B1286ED8).
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ee2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 117df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 117df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f829f000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f829f000)
  get Phys(data[n=1]=f82a0000)
  get Phys(data[n=1]=f82a1000)
  get Phys(data[n=1]=f82a2000)
  get Phys(data[n=1]=f82a3000)
  get Phys(data[n=1]=f82a4000)
  get Phys(data[n=1]=f82a5000)
  get Phys(data[n=1]=f82a6000)
  get Phys(data[n=1]=f82a7000)
  get Phys(data[n=1]=f82a8000)
  get Phys(data[n=1]=f82a9000)
  get Phys(data[n=2]=f82aa000)
  get Phys(data[n=2]=f82ab000)
  get Phys(data[n=2]=f82ac000)
  get Phys(data[n=2]=f82ad000)
  get Phys(data[n=2]=f82ae000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x117df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x117df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ee2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1185f, OrigWordsRequested 0x2700, DevSize 0x27
IdeReadWrite (REQ): Starting sector is 1185f, Number of WORDS 0x2700, DevSize 0x27
AtapiDmaSetup: mode 0x45, data f82af000, count 4e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82af000)
  get Phys(data[n=1]=f82b0000)
  get Phys(data[n=1]=f82b1000)
  get Phys(data[n=1]=f82b2000)
  get Phys(data[n=1]=f82b3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1185f, Count 0x27(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1185f count 0x27 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 4e00, full size 4e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ee6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 117df, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 117df, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8339000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8339000)
  get Phys(data[n=1]=f833a000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x117df, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x117df count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f94dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d2887, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 1d2887, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f829f000, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f829f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d2887, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d2887 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f9650
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d2887, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d2887, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 84914000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84914000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d2887, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d2887 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f94dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d288f, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 1d288f, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f829f000, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f829f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d288f, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d288f count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../base/services/eventlog/eventlog.c:333) Failed to create C:\ReactOS\system32\config\SysEvent.Evt! (Status c000018e)
(../../base/services/eventlog/eventlog.c:393) Failed to load System
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f94dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d2897, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 1d2897, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f829f000, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f829f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d2897, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d2897 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f9650
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d2897, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d2897, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 84954000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84954000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d2897, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d2897 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ee338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11887, OrigWordsRequested 0x6d00, DevSize 0x6d
IdeReadWrite (REQ): Starting sector is 11887, Number of WORDS 0x6d00, DevSize 0x6d
AtapiDmaSetup: mode 0x45, data f829f000, count da00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f829f000)
  get Phys(data[n=1]=f82a0000)
  get Phys(data[n=1]=f82a1000)
  get Phys(data[n=1]=f82a2000)
  get Phys(data[n=1]=f82a3000)
  get Phys(data[n=1]=f82a4000)
  get Phys(data[n=1]=f82a5000)
  get Phys(data[n=1]=f82a6000)
  get Phys(data[n=1]=f82a7000)
  get Phys(data[n=1]=f82a8000)
  get Phys(data[n=1]=f82a9000)
  get Phys(data[n=1]=f82aa000)
  get Phys(data[n=2]=f82ab000)
  get Phys(data[n=2]=f82ac000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x11887, Count 0x6d(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x11887 count 0x6d feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered da00, full size da00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ee6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11887, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 11887, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f830b000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f830b000)
  get Phys(data[n=1]=f830c000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x11887, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x11887 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ee338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11b57, OrigWordsRequested 0x5100, DevSize 0x51
IdeReadWrite (REQ): Starting sector is 11b57, Number of WORDS 0x5100, DevSize 0x51
AtapiDmaSetup: mode 0x45, data f829f000, count a200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f829f000)
  get Phys(data[n=1]=f82a0000)
  get Phys(data[n=1]=f82a1000)
  get Phys(data[n=1]=f82a2000)
  get Phys(data[n=1]=f82a3000)
  get Phys(data[n=1]=f82a4000)
  get Phys(data[n=1]=f82a5000)
  get Phys(data[n=2]=f82a6000)
  get Phys(data[n=2]=f82a7000)
  get Phys(data[n=2]=f82a8000)
  get Phys(data[n=3]=f82a9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x11b57, Count 0x51(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x11b57 count 0x51 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a200, full size a200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ee6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11b57, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 11b57, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f82f9000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82f9000)
  get Phys(data[n=1]=f82fa000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x11b57, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x11b57 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../base/services/wlansvc/wlansvc.c:145) wlansvc: main() started
(../../base/services/wlansvc/wlansvc.c:96) ServiceMain() called
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ee338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11947, OrigWordsRequested 0x4200, DevSize 0x42
IdeReadWrite (REQ): Starting sector is 11947, Number of WORDS 0x4200, DevSize 0x42
AtapiDmaSetup: mode 0x45, data f8287000, count 8400, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8287000)
  get Phys(data[n=1]=f8288000)
  get Phys(data[n=2]=f8289000)
  get Phys(data[n=3]=f828a000)
  get Phys(data[n=4]=f828b000)
  get Phys(data[n=5]=f828c000)
  get Phys(data[n=5]=f828d000)
  get Phys(data[n=5]=f828e000)
  get Phys(data[n=6]=f828f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x11947, Count 0x42(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x11947 count 0x42 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 8400, full size 8400
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ee6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11947, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 11947, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f82c5000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82c5000)
  get Phys(data[n=1]=f82c6000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x11947, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x11947 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2dc9f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2dc9f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f823a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=2]=f823c000)
  get Phys(data[n=3]=f823d000)
  get Phys(data[n=4]=f823e000)
  get Phys(data[n=5]=f823f000)
  get Phys(data[n=6]=f8240000)
  get Phys(data[n=6]=f8241000)
  get Phys(data[n=6]=f8242000)
  get Phys(data[n=7]=f8243000)
  get Phys(data[n=8]=f8244000)
  get Phys(data[n=8]=f8245000)
  get Phys(data[n=8]=f8246000)
  get Phys(data[n=9]=f8247000)
  get Phys(data[n=10]=f8248000)
  get Phys(data[n=11]=f8249000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2dc9f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2dc9f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2dd1f, OrigWordsRequested 0x1f00, DevSize 0x1f
IdeReadWrite (REQ): Starting sector is 2dd1f, Number of WORDS 0x1f00, DevSize 0x1f
AtapiDmaSetup: mode 0x45, data f824a000, count 3e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f824a000)
  get Phys(data[n=1]=f824b000)
  get Phys(data[n=2]=f824c000)
  get Phys(data[n=3]=f824d000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2dd1f, Count 0x1f(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2dd1f count 0x1f feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 3e00, full size 3e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2dc9f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 2dc9f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f82bc000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82bc000)
  get Phys(data[n=1]=f82bd000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2dc9f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2dc9f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../base/services/wlansvc/wlansvc.c:130) ServiceMain() done
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2c1bf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2c1bf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84a94000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84a94000)
  get Phys(data[n=1]=84a95000)
  get Phys(data[n=2]=84a96000)
  get Phys(data[n=3]=84a97000)
  get Phys(data[n=4]=84a98000)
  get Phys(data[n=4]=84a99000)
  get Phys(data[n=4]=84a9a000)
  get Phys(data[n=5]=84a9b000)
  get Phys(data[n=6]=84a9c000)
  get Phys(data[n=7]=84a9d000)
  get Phys(data[n=8]=84a9e000)
  get Phys(data[n=9]=84a9f000)
  get Phys(data[n=10]=84aa0000)
  get Phys(data[n=10]=84aa1000)
  get Phys(data[n=11]=84aa2000)
  get Phys(data[n=11]=84aa3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2c1bf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2c1bf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2c23f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2c23f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84aa4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84aa4000)
  get Phys(data[n=1]=84aa5000)
  get Phys(data[n=1]=84aa6000)
  get Phys(data[n=1]=84aa7000)
  get Phys(data[n=1]=84aa8000)
  get Phys(data[n=2]=84aa9000)
  get Phys(data[n=3]=84aaa000)
  get Phys(data[n=4]=84aab000)
  get Phys(data[n=4]=84aac000)
  get Phys(data[n=4]=84aad000)
  get Phys(data[n=5]=84aae000)
  get Phys(data[n=5]=84aaf000)
  get Phys(data[n=6]=84ab0000)
  get Phys(data[n=7]=84ab1000)
  get Phys(data[n=7]=84ab2000)
  get Phys(data[n=7]=84ab3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2c23f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2c23f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2c2bf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2c2bf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84ab4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84ab4000)
  get Phys(data[n=1]=84ab5000)
  get Phys(data[n=2]=84ab6000)
  get Phys(data[n=3]=84ab7000)
  get Phys(data[n=3]=84ab8000)
  get Phys(data[n=3]=84ab9000)
  get Phys(data[n=3]=84aba000)
  get Phys(data[n=4]=84abb000)
  get Phys(data[n=5]=84abc000)
  get Phys(data[n=5]=84abd000)
  get Phys(data[n=6]=84abe000)
  get Phys(data[n=7]=84abf000)
  get Phys(data[n=7]=84ac0000)
  get Phys(data[n=8]=84ac1000)
  get Phys(data[n=8]=84ac2000)
  get Phys(data[n=9]=84ac3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2c2bf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2c2bf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2c33f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2c33f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84ac4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84ac4000)
  get Phys(data[n=1]=84ac5000)
  get Phys(data[n=2]=84ac6000)
  get Phys(data[n=2]=84ac7000)
  get Phys(data[n=2]=84ac8000)
  get Phys(data[n=3]=84ac9000)
  get Phys(data[n=4]=84aca000)
  get Phys(data[n=5]=84acb000)
  get Phys(data[n=6]=84acc000)
  get Phys(data[n=7]=84acd000)
  get Phys(data[n=8]=84ace000)
  get Phys(data[n=9]=84acf000)
  get Phys(data[n=9]=84ad0000)
  get Phys(data[n=10]=84ad1000)
  get Phys(data[n=11]=84ad2000)
  get Phys(data[n=12]=84ad3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2c33f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2c33f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3866f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3866f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84ad4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84ad4000)
  get Phys(data[n=1]=84ad5000)
  get Phys(data[n=2]=84ad6000)
  get Phys(data[n=3]=84ad7000)
  get Phys(data[n=3]=84ad8000)
  get Phys(data[n=3]=84ad9000)
  get Phys(data[n=3]=84ada000)
  get Phys(data[n=4]=84adb000)
  get Phys(data[n=5]=84adc000)
  get Phys(data[n=6]=84add000)
  get Phys(data[n=6]=84ade000)
  get Phys(data[n=6]=84adf000)
  get Phys(data[n=7]=84ae0000)
  get Phys(data[n=7]=84ae1000)
  get Phys(data[n=8]=84ae2000)
  get Phys(data[n=9]=84ae3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3866f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3866f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 386ef, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 386ef, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84ae4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84ae4000)
  get Phys(data[n=1]=84ae5000)
  get Phys(data[n=2]=84ae6000)
  get Phys(data[n=2]=84ae7000)
  get Phys(data[n=3]=84ae8000)
  get Phys(data[n=4]=84ae9000)
  get Phys(data[n=4]=84aea000)
  get Phys(data[n=4]=84aeb000)
  get Phys(data[n=4]=84aec000)
  get Phys(data[n=5]=84aed000)
  get Phys(data[n=6]=84aee000)
  get Phys(data[n=6]=84aef000)
  get Phys(data[n=7]=84af0000)
  get Phys(data[n=7]=84af1000)
  get Phys(data[n=7]=84af2000)
  get Phys(data[n=8]=84af3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x386ef, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x386ef count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3876f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3876f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84af4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84af4000)
  get Phys(data[n=1]=84af5000)
  get Phys(data[n=2]=84af6000)
  get Phys(data[n=3]=84af7000)
  get Phys(data[n=4]=84af8000)
  get Phys(data[n=4]=84af9000)
  get Phys(data[n=4]=84afa000)
  get Phys(data[n=5]=84afb000)
  get Phys(data[n=6]=84afc000)
  get Phys(data[n=7]=84afd000)
  get Phys(data[n=8]=84afe000)
  get Phys(data[n=9]=84aff000)
  get Phys(data[n=10]=84b00000)
  get Phys(data[n=11]=84b01000)
  get Phys(data[n=11]=84b02000)
  get Phys(data[n=12]=84b03000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3876f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3876f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 387ef, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 387ef, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84b04000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84b04000)
  get Phys(data[n=1]=84b05000)
  get Phys(data[n=1]=84b06000)
  get Phys(data[n=2]=84b07000)
  get Phys(data[n=3]=84b08000)
  get Phys(data[n=4]=84b09000)
  get Phys(data[n=5]=84b0a000)
  get Phys(data[n=5]=84b0b000)
  get Phys(data[n=5]=84b0c000)
  get Phys(data[n=6]=84b0d000)
  get Phys(data[n=7]=84b0e000)
  get Phys(data[n=8]=84b0f000)
  get Phys(data[n=9]=84b10000)
  get Phys(data[n=10]=84b11000)
  get Phys(data[n=11]=84b12000)
  get Phys(data[n=11]=84b13000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x387ef, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x387ef count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2cf8f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2cf8f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84b14000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84b14000)
  get Phys(data[n=1]=84b15000)
  get Phys(data[n=2]=84b16000)
  get Phys(data[n=3]=84b17000)
  get Phys(data[n=3]=84b18000)
  get Phys(data[n=3]=84b19000)
  get Phys(data[n=4]=84b1a000)
  get Phys(data[n=4]=84b1b000)
  get Phys(data[n=5]=84b1c000)
  get Phys(data[n=6]=84b1d000)
  get Phys(data[n=6]=84b1e000)
  get Phys(data[n=6]=84b1f000)
  get Phys(data[n=7]=84b20000)
  get Phys(data[n=7]=84b21000)
  get Phys(data[n=8]=84b22000)
  get Phys(data[n=9]=84b23000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2cf8f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2cf8f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2d00f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2d00f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84b24000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84b24000)
  get Phys(data[n=1]=84b25000)
  get Phys(data[n=1]=84b26000)
  get Phys(data[n=2]=84b27000)
  get Phys(data[n=3]=84b28000)
  get Phys(data[n=3]=84b29000)
  get Phys(data[n=4]=84b2a000)
  get Phys(data[n=4]=84b2b000)
  get Phys(data[n=4]=84b2c000)
  get Phys(data[n=5]=84b2d000)
  get Phys(data[n=5]=84b2e000)
  get Phys(data[n=5]=84b2f000)
  get Phys(data[n=6]=84b30000)
  get Phys(data[n=7]=84b31000)
  get Phys(data[n=8]=84b32000)
  get Phys(data[n=8]=84b33000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2d00f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2d00f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2d08f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2d08f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84b34000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84b34000)
  get Phys(data[n=1]=84b35000)
  get Phys(data[n=2]=84b36000)
  get Phys(data[n=3]=84b37000)
  get Phys(data[n=4]=84b38000)
  get Phys(data[n=5]=84b39000)
  get Phys(data[n=6]=84b3a000)
  get Phys(data[n=7]=84b3b000)
  get Phys(data[n=7]=84b3c000)
  get Phys(data[n=8]=84b3d000)
  get Phys(data[n=9]=84b3e000)
  get Phys(data[n=10]=84b3f000)
  get Phys(data[n=10]=84b40000)
  get Phys(data[n=11]=84b41000)
  get Phys(data[n=12]=84b42000)
  get Phys(data[n=13]=84b43000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2d08f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2d08f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2d10f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2d10f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84b44000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84b44000)
  get Phys(data[n=1]=84b45000)
  get Phys(data[n=1]=84b46000)
  get Phys(data[n=2]=84b47000)
  get Phys(data[n=3]=84b48000)
  get Phys(data[n=4]=84b49000)
  get Phys(data[n=5]=84b4a000)
  get Phys(data[n=6]=84b4b000)
  get Phys(data[n=7]=84b4c000)
  get Phys(data[n=7]=84b4d000)
  get Phys(data[n=8]=84b4e000)
  get Phys(data[n=9]=84b4f000)
  get Phys(data[n=10]=84b50000)
  get Phys(data[n=11]=84b51000)
  get Phys(data[n=11]=84b52000)
  get Phys(data[n=12]=84b53000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2d10f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2d10f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 30f47, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 30f47, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84b54000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84b54000)
  get Phys(data[n=1]=84b55000)
  get Phys(data[n=1]=84b56000)
  get Phys(data[n=2]=84b57000)
  get Phys(data[n=2]=84b58000)
  get Phys(data[n=3]=84b59000)
  get Phys(data[n=4]=84b5a000)
  get Phys(data[n=4]=84b5b000)
  get Phys(data[n=4]=84b5c000)
  get Phys(data[n=4]=84b5d000)
  get Phys(data[n=5]=84b5e000)
  get Phys(data[n=6]=84b5f000)
  get Phys(data[n=6]=84b60000)
  get Phys(data[n=7]=84b61000)
  get Phys(data[n=7]=84b62000)
  get Phys(data[n=7]=84b63000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x30f47, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x30f47 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 30fc7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 30fc7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84b64000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84b64000)
  get Phys(data[n=1]=84b65000)
  get Phys(data[n=2]=84b66000)
  get Phys(data[n=3]=84b67000)
  get Phys(data[n=4]=84b68000)
  get Phys(data[n=5]=84b69000)
  get Phys(data[n=5]=84b6a000)
  get Phys(data[n=5]=84b6b000)
  get Phys(data[n=6]=84b6c000)
  get Phys(data[n=7]=84b6d000)
  get Phys(data[n=8]=84b6e000)
  get Phys(data[n=9]=84b6f000)
  get Phys(data[n=10]=84b70000)
  get Phys(data[n=11]=84b71000)
  get Phys(data[n=12]=84b72000)
  get Phys(data[n=12]=84b73000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x30fc7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x30fc7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 31047, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 31047, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84b74000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84b74000)
  get Phys(data[n=1]=84b75000)
  get Phys(data[n=2]=84b76000)
  get Phys(data[n=2]=84b77000)
  get Phys(data[n=3]=84b78000)
  get Phys(data[n=4]=84b79000)
  get Phys(data[n=5]=84b7a000)
  get Phys(data[n=6]=84b7b000)
  get Phys(data[n=6]=84b7c000)
  get Phys(data[n=6]=84b7d000)
  get Phys(data[n=7]=84b7e000)
  get Phys(data[n=8]=84b7f000)
  get Phys(data[n=9]=84b80000)
  get Phys(data[n=10]=84b81000)
  get Phys(data[n=11]=84b82000)
  get Phys(data[n=12]=84b83000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x31047, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x31047 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 310c7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 310c7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84b84000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84b84000)
  get Phys(data[n=1]=84b85000)
  get Phys(data[n=2]=84b86000)
  get Phys(data[n=3]=84b87000)
  get Phys(data[n=4]=84b88000)
  get Phys(data[n=4]=84b89000)
  get Phys(data[n=5]=84b8a000)
  get Phys(data[n=5]=84b8b000)
  get Phys(data[n=5]=84b8c000)
  get Phys(data[n=6]=84b8d000)
  get Phys(data[n=7]=84b8e000)
  get Phys(data[n=7]=84b8f000)
  get Phys(data[n=7]=84b90000)
  get Phys(data[n=8]=84b91000)
  get Phys(data[n=8]=84b92000)
  get Phys(data[n=9]=84b93000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x310c7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x310c7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 20fe7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 20fe7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f823a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=1]=f823c000)
  get Phys(data[n=1]=f823d000)
  get Phys(data[n=1]=f823e000)
  get Phys(data[n=2]=f823f000)
  get Phys(data[n=3]=f8240000)
  get Phys(data[n=3]=f8241000)
  get Phys(data[n=4]=f8242000)
  get Phys(data[n=4]=f8243000)
  get Phys(data[n=4]=f8244000)
  get Phys(data[n=5]=f8245000)
  get Phys(data[n=5]=f8246000)
  get Phys(data[n=6]=f8247000)
  get Phys(data[n=7]=f8248000)
  get Phys(data[n=8]=f8249000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x20fe7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x20fe7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 21067, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 21067, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f824a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f824a000)
  get Phys(data[n=1]=f824b000)
  get Phys(data[n=1]=f824c000)
  get Phys(data[n=2]=f824d000)
  get Phys(data[n=3]=f824e000)
  get Phys(data[n=4]=f824f000)
  get Phys(data[n=5]=f8250000)
  get Phys(data[n=6]=f8251000)
  get Phys(data[n=7]=f8252000)
  get Phys(data[n=8]=f8253000)
  get Phys(data[n=8]=f8254000)
  get Phys(data[n=9]=f8255000)
  get Phys(data[n=10]=f8256000)
  get Phys(data[n=11]=f8257000)
  get Phys(data[n=11]=f8258000)
  get Phys(data[n=12]=f8259000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x21067, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x21067 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 210e7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 210e7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f825a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f825a000)
  get Phys(data[n=1]=f825b000)
  get Phys(data[n=2]=f825c000)
  get Phys(data[n=2]=f825d000)
  get Phys(data[n=2]=f825e000)
  get Phys(data[n=3]=f825f000)
  get Phys(data[n=4]=f8260000)
  get Phys(data[n=5]=f8261000)
  get Phys(data[n=6]=f8262000)
  get Phys(data[n=7]=f8263000)
  get Phys(data[n=8]=f8264000)
  get Phys(data[n=8]=f8265000)
  get Phys(data[n=9]=f8266000)
  get Phys(data[n=10]=f8267000)
  get Phys(data[n=11]=f8268000)
  get Phys(data[n=12]=f8269000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x210e7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x210e7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 21167, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 21167, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f826a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f826a000)
  get Phys(data[n=1]=f826b000)
  get Phys(data[n=1]=f826c000)
  get Phys(data[n=1]=f826d000)
  get Phys(data[n=2]=f826e000)
  get Phys(data[n=3]=f826f000)
  get Phys(data[n=3]=f8270000)
  get Phys(data[n=3]=f8271000)
  get Phys(data[n=4]=f8272000)
  get Phys(data[n=4]=f8273000)
  get Phys(data[n=5]=f8274000)
  get Phys(data[n=6]=f8275000)
  get Phys(data[n=7]=f8276000)
  get Phys(data[n=7]=f8277000)
  get Phys(data[n=8]=f8278000)
  get Phys(data[n=8]=f8279000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x21167, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x21167 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 20fe7, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 20fe7, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f82bc000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82bc000)
  get Phys(data[n=1]=f82bd000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x20fe7, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x20fe7 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 213e7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 213e7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84bd4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84bd4000)
  get Phys(data[n=1]=84bd5000)
  get Phys(data[n=2]=84bd6000)
  get Phys(data[n=2]=84bd7000)
  get Phys(data[n=3]=84bd8000)
  get Phys(data[n=3]=84bd9000)
  get Phys(data[n=3]=84bda000)
  get Phys(data[n=4]=84bdb000)
  get Phys(data[n=4]=84bdc000)
  get Phys(data[n=5]=84bdd000)
  get Phys(data[n=6]=84bde000)
  get Phys(data[n=7]=84bdf000)
  get Phys(data[n=8]=84be0000)
  get Phys(data[n=9]=84be1000)
  get Phys(data[n=9]=84be2000)
  get Phys(data[n=10]=84be3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x213e7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x213e7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 21467, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 21467, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84be4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84be4000)
  get Phys(data[n=1]=84be5000)
  get Phys(data[n=2]=84be6000)
  get Phys(data[n=3]=84be7000)
  get Phys(data[n=4]=84be8000)
  get Phys(data[n=5]=84be9000)
  get Phys(data[n=5]=84bea000)
  get Phys(data[n=6]=84beb000)
  get Phys(data[n=7]=84bec000)
  get Phys(data[n=8]=84bed000)
  get Phys(data[n=8]=84bee000)
  get Phys(data[n=9]=84bef000)
  get Phys(data[n=10]=84bf0000)
  get Phys(data[n=11]=84bf1000)
  get Phys(data[n=12]=84bf2000)
  get Phys(data[n=12]=84bf3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x21467, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x21467 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 214e7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 214e7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84bf4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84bf4000)
  get Phys(data[n=1]=84bf5000)
  get Phys(data[n=2]=84bf6000)
  get Phys(data[n=3]=84bf7000)
  get Phys(data[n=4]=84bf8000)
  get Phys(data[n=5]=84bf9000)
  get Phys(data[n=6]=84bfa000)
  get Phys(data[n=6]=84bfb000)
  get Phys(data[n=7]=84bfc000)
  get Phys(data[n=8]=84bfd000)
  get Phys(data[n=9]=84bfe000)
  get Phys(data[n=10]=84bff000)
  get Phys(data[n=10]=84c00000)
  get Phys(data[n=11]=84c01000)
  get Phys(data[n=12]=84c02000)
  get Phys(data[n=13]=84c03000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x214e7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x214e7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 21567, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 21567, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84c04000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84c04000)
  get Phys(data[n=1]=84c05000)
  get Phys(data[n=1]=84c06000)
  get Phys(data[n=2]=84c07000)
  get Phys(data[n=2]=84c08000)
  get Phys(data[n=3]=84c09000)
  get Phys(data[n=4]=84c0a000)
  get Phys(data[n=5]=84c0b000)
  get Phys(data[n=5]=84c0c000)
  get Phys(data[n=6]=84c0d000)
  get Phys(data[n=6]=84c0e000)
  get Phys(data[n=7]=84c0f000)
  get Phys(data[n=8]=84c10000)
  get Phys(data[n=8]=84c11000)
  get Phys(data[n=9]=84c12000)
  get Phys(data[n=9]=84c13000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x21567, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x21567 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2329f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2329f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f823a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=1]=f823c000)
  get Phys(data[n=2]=f823d000)
  get Phys(data[n=3]=f823e000)
  get Phys(data[n=4]=f823f000)
  get Phys(data[n=4]=f8240000)
  get Phys(data[n=5]=f8241000)
  get Phys(data[n=6]=f8242000)
  get Phys(data[n=7]=f8243000)
  get Phys(data[n=8]=f8244000)
  get Phys(data[n=8]=f8245000)
  get Phys(data[n=8]=f8246000)
  get Phys(data[n=9]=f8247000)
  get Phys(data[n=10]=f8248000)
  get Phys(data[n=11]=f8249000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2329f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2329f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2331f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2331f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f824a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f824a000)
  get Phys(data[n=1]=f824b000)
  get Phys(data[n=2]=f824c000)
  get Phys(data[n=2]=f824d000)
  get Phys(data[n=3]=f824e000)
  get Phys(data[n=4]=f824f000)
  get Phys(data[n=5]=f8250000)
  get Phys(data[n=6]=f8251000)
  get Phys(data[n=6]=f8252000)
  get Phys(data[n=6]=f8253000)
  get Phys(data[n=7]=f8254000)
  get Phys(data[n=7]=f8255000)
  get Phys(data[n=8]=f8256000)
  get Phys(data[n=9]=f8257000)
  get Phys(data[n=9]=f8258000)
  get Phys(data[n=9]=f8259000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2331f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2331f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2339f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2339f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f825a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f825a000)
  get Phys(data[n=1]=f825b000)
  get Phys(data[n=2]=f825c000)
  get Phys(data[n=3]=f825d000)
  get Phys(data[n=4]=f825e000)
  get Phys(data[n=4]=f825f000)
  get Phys(data[n=5]=f8260000)
  get Phys(data[n=5]=f8261000)
  get Phys(data[n=6]=f8262000)
  get Phys(data[n=7]=f8263000)
  get Phys(data[n=7]=f8264000)
  get Phys(data[n=8]=f8265000)
  get Phys(data[n=8]=f8266000)
  get Phys(data[n=9]=f8267000)
  get Phys(data[n=9]=f8268000)
  get Phys(data[n=9]=f8269000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2339f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2339f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2341f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2341f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f826a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f826a000)
  get Phys(data[n=1]=f826b000)
  get Phys(data[n=1]=f826c000)
  get Phys(data[n=2]=f826d000)
  get Phys(data[n=2]=f826e000)
  get Phys(data[n=3]=f826f000)
  get Phys(data[n=4]=f8270000)
  get Phys(data[n=5]=f8271000)
  get Phys(data[n=6]=f8272000)
  get Phys(data[n=6]=f8273000)
  get Phys(data[n=6]=f8274000)
  get Phys(data[n=6]=f8275000)
  get Phys(data[n=7]=f8276000)
  get Phys(data[n=8]=f8277000)
  get Phys(data[n=9]=f8278000)
  get Phys(data[n=10]=f8279000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2341f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2341f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2329f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 2329f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f82bc000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82bc000)
  get Phys(data[n=1]=f82bd000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2329f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2329f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2f95f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2f95f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f823a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=2]=f823c000)
  get Phys(data[n=2]=f823d000)
  get Phys(data[n=2]=f823e000)
  get Phys(data[n=3]=f823f000)
  get Phys(data[n=4]=f8240000)
  get Phys(data[n=5]=f8241000)
  get Phys(data[n=6]=f8242000)
  get Phys(data[n=7]=f8243000)
  get Phys(data[n=8]=f8244000)
  get Phys(data[n=8]=f8245000)
  get Phys(data[n=9]=f8246000)
  get Phys(data[n=10]=f8247000)
  get Phys(data[n=11]=f8248000)
  get Phys(data[n=12]=f8249000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2f95f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2f95f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2f9df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2f9df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f824a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f824a000)
  get Phys(data[n=1]=f824b000)
  get Phys(data[n=2]=f824c000)
  get Phys(data[n=2]=f824d000)
  get Phys(data[n=3]=f824e000)
  get Phys(data[n=4]=f824f000)
  get Phys(data[n=4]=f8250000)
  get Phys(data[n=4]=f8251000)
  get Phys(data[n=5]=f8252000)
  get Phys(data[n=5]=f8253000)
  get Phys(data[n=6]=f8254000)
  get Phys(data[n=7]=f8255000)
  get Phys(data[n=8]=f8256000)
  get Phys(data[n=8]=f8257000)
  get Phys(data[n=9]=f8258000)
  get Phys(data[n=9]=f8259000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2f9df, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2f9df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2fa5f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2fa5f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f825a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f825a000)
  get Phys(data[n=1]=f825b000)
  get Phys(data[n=1]=f825c000)
  get Phys(data[n=2]=f825d000)
  get Phys(data[n=2]=f825e000)
  get Phys(data[n=3]=f825f000)
  get Phys(data[n=3]=f8260000)
  get Phys(data[n=3]=f8261000)
  get Phys(data[n=3]=f8262000)
  get Phys(data[n=3]=f8263000)
  get Phys(data[n=3]=f8264000)
  get Phys(data[n=4]=f8265000)
  get Phys(data[n=4]=f8266000)
  get Phys(data[n=5]=f8267000)
  get Phys(data[n=6]=f8268000)
  get Phys(data[n=7]=f8269000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2fa5f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2fa5f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2fadf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2fadf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f826a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f826a000)
  get Phys(data[n=1]=f826b000)
  get Phys(data[n=1]=f826c000)
  get Phys(data[n=2]=f826d000)
  get Phys(data[n=3]=f826e000)
  get Phys(data[n=4]=f826f000)
  get Phys(data[n=5]=f8270000)
  get Phys(data[n=6]=f8271000)
  get Phys(data[n=7]=f8272000)
  get Phys(data[n=8]=f8273000)
  get Phys(data[n=8]=f8274000)
  get Phys(data[n=9]=f8275000)
  get Phys(data[n=10]=f8276000)
  get Phys(data[n=11]=f8277000)
  get Phys(data[n=11]=f8278000)
  get Phys(data[n=12]=f8279000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2fadf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2fadf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2f95f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 2f95f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f82bc000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82bc000)
  get Phys(data[n=1]=f82bd000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2f95f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2f95f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2fb5f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2fb5f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84c94000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84c94000)
  get Phys(data[n=1]=84c95000)
  get Phys(data[n=2]=84c96000)
  get Phys(data[n=3]=84c97000)
  get Phys(data[n=4]=84c98000)
  get Phys(data[n=5]=84c99000)
  get Phys(data[n=6]=84c9a000)
  get Phys(data[n=6]=84c9b000)
  get Phys(data[n=7]=84c9c000)
  get Phys(data[n=8]=84c9d000)
  get Phys(data[n=9]=84c9e000)
  get Phys(data[n=10]=84c9f000)
  get Phys(data[n=10]=84ca0000)
  get Phys(data[n=10]=84ca1000)
  get Phys(data[n=11]=84ca2000)
  get Phys(data[n=11]=84ca3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2fb5f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2fb5f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2fbdf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2fbdf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84ca4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84ca4000)
  get Phys(data[n=1]=84ca5000)
  get Phys(data[n=1]=84ca6000)
  get Phys(data[n=1]=84ca7000)
  get Phys(data[n=2]=84ca8000)
  get Phys(data[n=2]=84ca9000)
  get Phys(data[n=3]=84caa000)
  get Phys(data[n=4]=84cab000)
  get Phys(data[n=5]=84cac000)
  get Phys(data[n=5]=84cad000)
  get Phys(data[n=6]=84cae000)
  get Phys(data[n=6]=84caf000)
  get Phys(data[n=7]=84cb0000)
  get Phys(data[n=8]=84cb1000)
  get Phys(data[n=8]=84cb2000)
  get Phys(data[n=9]=84cb3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2fbdf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2fbdf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2fc5f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2fc5f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84cb4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84cb4000)
  get Phys(data[n=1]=84cb5000)
  get Phys(data[n=1]=84cb6000)
  get Phys(data[n=1]=84cb7000)
  get Phys(data[n=1]=84cb8000)
  get Phys(data[n=1]=84cb9000)
  get Phys(data[n=1]=84cba000)
  get Phys(data[n=2]=84cbb000)
  get Phys(data[n=2]=84cbc000)
  get Phys(data[n=3]=84cbd000)
  get Phys(data[n=4]=84cbe000)
  get Phys(data[n=5]=84cbf000)
  get Phys(data[n=6]=84cc0000)
  get Phys(data[n=6]=84cc1000)
  get Phys(data[n=6]=84cc2000)
  get Phys(data[n=7]=84cc3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2fc5f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2fc5f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2fcdf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2fcdf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84cc4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84cc4000)
  get Phys(data[n=1]=84cc5000)
  get Phys(data[n=2]=84cc6000)
  get Phys(data[n=3]=84cc7000)
  get Phys(data[n=4]=84cc8000)
  get Phys(data[n=5]=84cc9000)
  get Phys(data[n=5]=84cca000)
  get Phys(data[n=6]=84ccb000)
  get Phys(data[n=7]=84ccc000)
  get Phys(data[n=8]=84ccd000)
  get Phys(data[n=8]=84cce000)
  get Phys(data[n=9]=84ccf000)
  get Phys(data[n=10]=84cd0000)
  get Phys(data[n=11]=84cd1000)
  get Phys(data[n=12]=84cd2000)
  get Phys(data[n=13]=84cd3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2fcdf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2fcdf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 30807, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 30807, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f823a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=1]=f823c000)
  get Phys(data[n=2]=f823d000)
  get Phys(data[n=2]=f823e000)
  get Phys(data[n=3]=f823f000)
  get Phys(data[n=4]=f8240000)
  get Phys(data[n=4]=f8241000)
  get Phys(data[n=4]=f8242000)
  get Phys(data[n=5]=f8243000)
  get Phys(data[n=5]=f8244000)
  get Phys(data[n=6]=f8245000)
  get Phys(data[n=7]=f8246000)
  get Phys(data[n=8]=f8247000)
  get Phys(data[n=8]=f8248000)
  get Phys(data[n=9]=f8249000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x30807, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x30807 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 30887, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 30887, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f824a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f824a000)
  get Phys(data[n=1]=f824b000)
  get Phys(data[n=2]=f824c000)
  get Phys(data[n=2]=f824d000)
  get Phys(data[n=3]=f824e000)
  get Phys(data[n=3]=f824f000)
  get Phys(data[n=4]=f8250000)
  get Phys(data[n=4]=f8251000)
  get Phys(data[n=4]=f8252000)
  get Phys(data[n=4]=f8253000)
  get Phys(data[n=4]=f8254000)
  get Phys(data[n=4]=f8255000)
  get Phys(data[n=5]=f8256000)
  get Phys(data[n=5]=f8257000)
  get Phys(data[n=6]=f8258000)
  get Phys(data[n=7]=f8259000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x30887, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x30887 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 30907, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 30907, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f825a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f825a000)
  get Phys(data[n=1]=f825b000)
  get Phys(data[n=1]=f825c000)
  get Phys(data[n=1]=f825d000)
  get Phys(data[n=2]=f825e000)
  get Phys(data[n=3]=f825f000)
  get Phys(data[n=4]=f8260000)
  get Phys(data[n=5]=f8261000)
  get Phys(data[n=5]=f8262000)
  get Phys(data[n=6]=f8263000)
  get Phys(data[n=7]=f8264000)
  get Phys(data[n=7]=f8265000)
  get Phys(data[n=8]=f8266000)
  get Phys(data[n=9]=f8267000)
  get Phys(data[n=10]=f8268000)
  get Phys(data[n=10]=f8269000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x30907, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x30907 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 30987, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 30987, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f826a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f826a000)
  get Phys(data[n=1]=f826b000)
  get Phys(data[n=2]=f826c000)
  get Phys(data[n=3]=f826d000)
  get Phys(data[n=4]=f826e000)
  get Phys(data[n=4]=f826f000)
  get Phys(data[n=5]=f8270000)
  get Phys(data[n=6]=f8271000)
  get Phys(data[n=6]=f8272000)
  get Phys(data[n=7]=f8273000)
  get Phys(data[n=8]=f8274000)
  get Phys(data[n=9]=f8275000)
  get Phys(data[n=9]=f8276000)
  get Phys(data[n=10]=f8277000)
  get Phys(data[n=11]=f8278000)
  get Phys(data[n=12]=f8279000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x30987, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x30987 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 30807, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 30807, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f82bc000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82bc000)
  get Phys(data[n=1]=f82bd000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x30807, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x30807 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3a697, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3a697, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f823a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=2]=f823c000)
  get Phys(data[n=3]=f823d000)
  get Phys(data[n=4]=f823e000)
  get Phys(data[n=4]=f823f000)
  get Phys(data[n=5]=f8240000)
  get Phys(data[n=5]=f8241000)
  get Phys(data[n=6]=f8242000)
  get Phys(data[n=7]=f8243000)
  get Phys(data[n=7]=f8244000)
  get Phys(data[n=8]=f8245000)
  get Phys(data[n=8]=f8246000)
  get Phys(data[n=9]=f8247000)
  get Phys(data[n=9]=f8248000)
  get Phys(data[n=9]=f8249000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3a697, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3a697 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3a717, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3a717, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f824a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f824a000)
  get Phys(data[n=1]=f824b000)
  get Phys(data[n=1]=f824c000)
  get Phys(data[n=2]=f824d000)
  get Phys(data[n=2]=f824e000)
  get Phys(data[n=3]=f824f000)
  get Phys(data[n=4]=f8250000)
  get Phys(data[n=5]=f8251000)
  get Phys(data[n=6]=f8252000)
  get Phys(data[n=6]=f8253000)
  get Phys(data[n=6]=f8254000)
  get Phys(data[n=7]=f8255000)
  get Phys(data[n=8]=f8256000)
  get Phys(data[n=9]=f8257000)
  get Phys(data[n=10]=f8258000)
  get Phys(data[n=11]=f8259000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3a717, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3a717 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88657f8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4057, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 4057, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 81f80000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=81f80000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4057, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x4057 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3a797, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3a797, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f825a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f825a000)
  get Phys(data[n=1]=f825b000)
  get Phys(data[n=1]=f825c000)
  get Phys(data[n=2]=f825d000)
  get Phys(data[n=3]=f825e000)
  get Phys(data[n=4]=f825f000)
  get Phys(data[n=4]=f8260000)
  get Phys(data[n=5]=f8261000)
  get Phys(data[n=6]=f8262000)
  get Phys(data[n=7]=f8263000)
  get Phys(data[n=8]=f8264000)
  get Phys(data[n=9]=f8265000)
  get Phys(data[n=9]=f8266000)
  get Phys(data[n=10]=f8267000)
  get Phys(data[n=11]=f8268000)
  get Phys(data[n=11]=f8269000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3a797, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3a797 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3a817, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3a817, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f826a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f826a000)
  get Phys(data[n=1]=f826b000)
  get Phys(data[n=2]=f826c000)
  get Phys(data[n=2]=f826d000)
  get Phys(data[n=3]=f826e000)
  get Phys(data[n=4]=f826f000)
  get Phys(data[n=5]=f8270000)
  get Phys(data[n=6]=f8271000)
  get Phys(data[n=7]=f8272000)
  get Phys(data[n=7]=f8273000)
  get Phys(data[n=7]=f8274000)
  get Phys(data[n=7]=f8275000)
  get Phys(data[n=8]=f8276000)
  get Phys(data[n=9]=f8277000)
  get Phys(data[n=10]=f8278000)
  get Phys(data[n=11]=f8279000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3a817, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3a817 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3a697, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3a697, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f82bc000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82bc000)
  get Phys(data[n=1]=f82bd000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3a697, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3a697 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 26b07, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 26b07, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f823a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=1]=f823c000)
  get Phys(data[n=2]=f823d000)
  get Phys(data[n=2]=f823e000)
  get Phys(data[n=2]=f823f000)
  get Phys(data[n=2]=f8240000)
  get Phys(data[n=2]=f8241000)
  get Phys(data[n=2]=f8242000)
  get Phys(data[n=3]=f8243000)
  get Phys(data[n=3]=f8244000)
  get Phys(data[n=4]=f8245000)
  get Phys(data[n=5]=f8246000)
  get Phys(data[n=6]=f8247000)
  get Phys(data[n=7]=f8248000)
  get Phys(data[n=7]=f8249000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x26b07, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x26b07 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c62d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 26b87, OrigWordsRequested 0x6c00, DevSize 0x6c
IdeReadWrite (REQ): Starting sector is 26b87, Number of WORDS 0x6c00, DevSize 0x6c
AtapiDmaSetup: mode 0x45, data f824a000, count d800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f824a000)
  get Phys(data[n=1]=f824b000)
  get Phys(data[n=2]=f824c000)
  get Phys(data[n=3]=f824d000)
  get Phys(data[n=4]=f824e000)
  get Phys(data[n=5]=f824f000)
  get Phys(data[n=6]=f8250000)
  get Phys(data[n=7]=f8251000)
  get Phys(data[n=7]=f8252000)
  get Phys(data[n=8]=f8253000)
  get Phys(data[n=9]=f8254000)
  get Phys(data[n=10]=f8255000)
  get Phys(data[n=10]=f8256000)
  get Phys(data[n=11]=f8257000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x26b87, Count 0x6c(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x26b87 count 0x6c feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered d800, full size d800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82c66cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 26b07, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 26b07, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f82bc000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82bc000)
  get Phys(data[n=1]=f82bd000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x26b07, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x26b07 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2cd8f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2cd8f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84d94000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84d94000)
  get Phys(data[n=1]=84d95000)
  get Phys(data[n=2]=84d96000)
  get Phys(data[n=2]=84d97000)
  get Phys(data[n=2]=84d98000)
  get Phys(data[n=3]=84d99000)
  get Phys(data[n=4]=84d9a000)
  get Phys(data[n=5]=84d9b000)
  get Phys(data[n=6]=84d9c000)
  get Phys(data[n=7]=84d9d000)
  get Phys(data[n=8]=84d9e000)
  get Phys(data[n=9]=84d9f000)
  get Phys(data[n=10]=84da0000)
  get Phys(data[n=11]=84da1000)
  get Phys(data[n=12]=84da2000)
  get Phys(data[n=12]=84da3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2cd8f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2cd8f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2ce0f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2ce0f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84da4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84da4000)
  get Phys(data[n=1]=84da5000)
  get Phys(data[n=2]=84da6000)
  get Phys(data[n=3]=84da7000)
  get Phys(data[n=3]=84da8000)
  get Phys(data[n=3]=84da9000)
  get Phys(data[n=3]=84daa000)
  get Phys(data[n=4]=84dab000)
  get Phys(data[n=4]=84dac000)
  get Phys(data[n=4]=84dad000)
  get Phys(data[n=4]=84dae000)
  get Phys(data[n=4]=84daf000)
  get Phys(data[n=4]=84db0000)
  get Phys(data[n=5]=84db1000)
  get Phys(data[n=5]=84db2000)
  get Phys(data[n=6]=84db3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2ce0f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2ce0f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2ce8f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2ce8f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84db4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84db4000)
  get Phys(data[n=1]=84db5000)
  get Phys(data[n=2]=84db6000)
  get Phys(data[n=2]=84db7000)
  get Phys(data[n=3]=84db8000)
  get Phys(data[n=4]=84db9000)
  get Phys(data[n=5]=84dba000)
  get Phys(data[n=6]=84dbb000)
  get Phys(data[n=6]=84dbc000)
  get Phys(data[n=7]=84dbd000)
  get Phys(data[n=8]=84dbe000)
  get Phys(data[n=9]=84dbf000)
  get Phys(data[n=9]=84dc0000)
  get Phys(data[n=10]=84dc1000)
  get Phys(data[n=11]=84dc2000)
  get Phys(data[n=12]=84dc3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2ce8f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2ce8f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2cf0f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2cf0f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84dc4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84dc4000)
  get Phys(data[n=1]=84dc5000)
  get Phys(data[n=2]=84dc6000)
  get Phys(data[n=3]=84dc7000)
  get Phys(data[n=4]=84dc8000)
  get Phys(data[n=5]=84dc9000)
  get Phys(data[n=5]=84dca000)
  get Phys(data[n=6]=84dcb000)
  get Phys(data[n=7]=84dcc000)
  get Phys(data[n=7]=84dcd000)
  get Phys(data[n=8]=84dce000)
  get Phys(data[n=9]=84dcf000)
  get Phys(data[n=10]=84dd0000)
  get Phys(data[n=10]=84dd1000)
  get Phys(data[n=11]=84dd2000)
  get Phys(data[n=12]=84dd3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2cf0f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2cf0f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 211e7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 211e7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84dd4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84dd4000)
  get Phys(data[n=1]=84dd5000)
  get Phys(data[n=2]=84dd6000)
  get Phys(data[n=3]=84dd7000)
  get Phys(data[n=4]=84dd8000)
  get Phys(data[n=5]=84dd9000)
  get Phys(data[n=6]=84dda000)
  get Phys(data[n=7]=84ddb000)
  get Phys(data[n=8]=84ddc000)
  get Phys(data[n=9]=84ddd000)
  get Phys(data[n=10]=84dde000)
  get Phys(data[n=11]=84ddf000)
  get Phys(data[n=11]=84de0000)
  get Phys(data[n=12]=84de1000)
  get Phys(data[n=12]=84de2000)
  get Phys(data[n=13]=84de3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x211e7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x211e7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 21267, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 21267, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84de4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84de4000)
  get Phys(data[n=1]=84de5000)
  get Phys(data[n=1]=84de6000)
  get Phys(data[n=1]=84de7000)
  get Phys(data[n=2]=84de8000)
  get Phys(data[n=2]=84de9000)
  get Phys(data[n=2]=84dea000)
  get Phys(data[n=2]=84deb000)
  get Phys(data[n=2]=84dec000)
  get Phys(data[n=2]=84ded000)
  get Phys(data[n=3]=84dee000)
  get Phys(data[n=3]=84def000)
  get Phys(data[n=4]=84df0000)
  get Phys(data[n=4]=84df1000)
  get Phys(data[n=4]=84df2000)
  get Phys(data[n=5]=84df3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x21267, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x21267 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 212e7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 212e7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84df4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84df4000)
  get Phys(data[n=1]=84df5000)
  get Phys(data[n=2]=84df6000)
  get Phys(data[n=3]=84df7000)
  get Phys(data[n=4]=84df8000)
  get Phys(data[n=4]=84df9000)
  get Phys(data[n=5]=84dfa000)
  get Phys(data[n=6]=84dfb000)
  get Phys(data[n=7]=84dfc000)
  get Phys(data[n=7]=84dfd000)
  get Phys(data[n=7]=84dfe000)
  get Phys(data[n=8]=84dff000)
  get Phys(data[n=9]=84e00000)
  get Phys(data[n=9]=84e01000)
  get Phys(data[n=10]=84e02000)
  get Phys(data[n=11]=84e03000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x212e7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x212e7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 21367, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 21367, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84e04000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84e04000)
  get Phys(data[n=1]=84e05000)
  get Phys(data[n=2]=84e06000)
  get Phys(data[n=2]=84e07000)
  get Phys(data[n=3]=84e08000)
  get Phys(data[n=4]=84e09000)
  get Phys(data[n=4]=84e0a000)
  get Phys(data[n=5]=84e0b000)
  get Phys(data[n=6]=84e0c000)
  get Phys(data[n=7]=84e0d000)
  get Phys(data[n=7]=84e0e000)
  get Phys(data[n=8]=84e0f000)
  get Phys(data[n=9]=84e10000)
  get Phys(data[n=10]=84e11000)
  get Phys(data[n=10]=84e12000)
  get Phys(data[n=10]=84e13000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x21367, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x21367 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38cb7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 38cb7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f823a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=2]=f823c000)
  get Phys(data[n=2]=f823d000)
  get Phys(data[n=3]=f823e000)
  get Phys(data[n=4]=f823f000)
  get Phys(data[n=5]=f8240000)
  get Phys(data[n=6]=f8241000)
  get Phys(data[n=7]=f8242000)
  get Phys(data[n=7]=f8243000)
  get Phys(data[n=8]=f8244000)
  get Phys(data[n=9]=f8245000)
  get Phys(data[n=9]=f8246000)
  get Phys(data[n=10]=f8247000)
  get Phys(data[n=11]=f8248000)
  get Phys(data[n=12]=f8249000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38cb7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38cb7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38d37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 38d37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f824a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f824a000)
  get Phys(data[n=1]=f824b000)
  get Phys(data[n=2]=f824c000)
  get Phys(data[n=3]=f824d000)
  get Phys(data[n=3]=f824e000)
  get Phys(data[n=3]=f824f000)
  get Phys(data[n=3]=f8250000)
  get Phys(data[n=4]=f8251000)
  get Phys(data[n=5]=f8252000)
  get Phys(data[n=5]=f8253000)
  get Phys(data[n=6]=f8254000)
  get Phys(data[n=7]=f8255000)
  get Phys(data[n=8]=f8256000)
  get Phys(data[n=9]=f8257000)
  get Phys(data[n=10]=f8258000)
  get Phys(data[n=11]=f8259000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38d37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38d37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38db7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 38db7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f825a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f825a000)
  get Phys(data[n=1]=f825b000)
  get Phys(data[n=1]=f825c000)
  get Phys(data[n=2]=f825d000)
  get Phys(data[n=3]=f825e000)
  get Phys(data[n=4]=f825f000)
  get Phys(data[n=5]=f8260000)
  get Phys(data[n=5]=f8261000)
  get Phys(data[n=5]=f8262000)
  get Phys(data[n=5]=f8263000)
  get Phys(data[n=6]=f8264000)
  get Phys(data[n=6]=f8265000)
  get Phys(data[n=6]=f8266000)
  get Phys(data[n=6]=f8267000)
  get Phys(data[n=6]=f8268000)
  get Phys(data[n=6]=f8269000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38db7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38db7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38e37, OrigWordsRequested 0x6100, DevSize 0x61
IdeReadWrite (REQ): Starting sector is 38e37, Number of WORDS 0x6100, DevSize 0x61
AtapiDmaSetup: mode 0x45, data f826a000, count c200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f826a000)
  get Phys(data[n=1]=f826b000)
  get Phys(data[n=2]=f826c000)
  get Phys(data[n=2]=f826d000)
  get Phys(data[n=2]=f826e000)
  get Phys(data[n=3]=f826f000)
  get Phys(data[n=3]=f8270000)
  get Phys(data[n=4]=f8271000)
  get Phys(data[n=5]=f8272000)
  get Phys(data[n=6]=f8273000)
  get Phys(data[n=7]=f8274000)
  get Phys(data[n=8]=f8275000)
  get Phys(data[n=9]=f8276000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38e37, Count 0x61(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38e37 count 0x61 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered c200, full size c200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38cb7, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 38cb7, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f82ac000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ac000)
  get Phys(data[n=1]=f82ad000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38cb7, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38cb7 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3a667, OrigWordsRequested 0x2e00, DevSize 0x2e
IdeReadWrite (REQ): Starting sector is 3a667, Number of WORDS 0x2e00, DevSize 0x2e
AtapiDmaSetup: mode 0x45, data f823a000, count 5c00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=2]=f823c000)
  get Phys(data[n=2]=f823d000)
  get Phys(data[n=2]=f823e000)
  get Phys(data[n=2]=f823f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3a667, Count 0x2e(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3a667 count 0x2e feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 5c00, full size 5c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3a667, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3a667, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f82ac000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ac000)
  get Phys(data[n=1]=f82ad000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3a667, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3a667 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 26d87, OrigWordsRequested 0x5500, DevSize 0x55
IdeReadWrite (REQ): Starting sector is 26d87, Number of WORDS 0x5500, DevSize 0x55
AtapiDmaSetup: mode 0x45, data f823a000, count aa00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=2]=f823c000)
  get Phys(data[n=2]=f823d000)
  get Phys(data[n=3]=f823e000)
  get Phys(data[n=4]=f823f000)
  get Phys(data[n=5]=f8240000)
  get Phys(data[n=6]=f8241000)
  get Phys(data[n=6]=f8242000)
  get Phys(data[n=6]=f8243000)
  get Phys(data[n=6]=f8244000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x26d87, Count 0x55(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x26d87 count 0x55 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered aa00, full size aa00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 26d87, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 26d87, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f82ac000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ac000)
  get Phys(data[n=1]=f82ad000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x26d87, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x26d87 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 26c9f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 26c9f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f823a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=2]=f823c000)
  get Phys(data[n=2]=f823d000)
  get Phys(data[n=2]=f823e000)
  get Phys(data[n=2]=f823f000)
  get Phys(data[n=3]=f8240000)
  get Phys(data[n=3]=f8241000)
  get Phys(data[n=3]=f8242000)
  get Phys(data[n=3]=f8243000)
  get Phys(data[n=3]=f8244000)
  get Phys(data[n=3]=f8245000)
  get Phys(data[n=4]=f8246000)
  get Phys(data[n=4]=f8247000)
  get Phys(data[n=5]=f8248000)
  get Phys(data[n=5]=f8249000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x26c9f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x26c9f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 26d1f, OrigWordsRequested 0x6600, DevSize 0x66
IdeReadWrite (REQ): Starting sector is 26d1f, Number of WORDS 0x6600, DevSize 0x66
AtapiDmaSetup: mode 0x45, data f824a000, count cc00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f824a000)
  get Phys(data[n=1]=f824b000)
  get Phys(data[n=1]=f824c000)
  get Phys(data[n=2]=f824d000)
  get Phys(data[n=3]=f824e000)
  get Phys(data[n=4]=f824f000)
  get Phys(data[n=5]=f8250000)
  get Phys(data[n=6]=f8251000)
  get Phys(data[n=7]=f8252000)
  get Phys(data[n=7]=f8253000)
  get Phys(data[n=8]=f8254000)
  get Phys(data[n=8]=f8255000)
  get Phys(data[n=9]=f8256000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x26d1f, Count 0x66(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x26d1f count 0x66 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered cc00, full size cc00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 26c9f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 26c9f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f82ac000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ac000)
  get Phys(data[n=1]=f82ad000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x26c9f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x26c9f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2043f, OrigWordsRequested 0x1800, DevSize 0x18
IdeReadWrite (REQ): Starting sector is 2043f, Number of WORDS 0x1800, DevSize 0x18
AtapiDmaSetup: mode 0x45, data f823a000, count 3000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=2]=f823c000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2043f, Count 0x18(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2043f count 0x18 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 3000, full size 3000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2043f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 2043f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f82ac000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ac000)
  get Phys(data[n=1]=f82ad000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2043f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2043f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38f37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 38f37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f823a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=2]=f823c000)
  get Phys(data[n=3]=f823d000)
  get Phys(data[n=4]=f823e000)
  get Phys(data[n=4]=f823f000)
  get Phys(data[n=5]=f8240000)
  get Phys(data[n=6]=f8241000)
  get Phys(data[n=7]=f8242000)
  get Phys(data[n=8]=f8243000)
  get Phys(data[n=8]=f8244000)
  get Phys(data[n=8]=f8245000)
  get Phys(data[n=9]=f8246000)
  get Phys(data[n=10]=f8247000)
  get Phys(data[n=10]=f8248000)
  get Phys(data[n=11]=f8249000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38f37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38f37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38fb7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 38fb7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f824a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f824a000)
  get Phys(data[n=1]=f824b000)
  get Phys(data[n=2]=f824c000)
  get Phys(data[n=3]=f824d000)
  get Phys(data[n=4]=f824e000)
  get Phys(data[n=4]=f824f000)
  get Phys(data[n=5]=f8250000)
  get Phys(data[n=6]=f8251000)
  get Phys(data[n=7]=f8252000)
  get Phys(data[n=8]=f8253000)
  get Phys(data[n=8]=f8254000)
  get Phys(data[n=9]=f8255000)
  get Phys(data[n=9]=f8256000)
  get Phys(data[n=9]=f8257000)
  get Phys(data[n=10]=f8258000)
  get Phys(data[n=11]=f8259000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38fb7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38fb7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 39037, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 39037, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f825a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f825a000)
  get Phys(data[n=1]=f825b000)
  get Phys(data[n=1]=f825c000)
  get Phys(data[n=1]=f825d000)
  get Phys(data[n=1]=f825e000)
  get Phys(data[n=2]=f825f000)
  get Phys(data[n=2]=f8260000)
  get Phys(data[n=3]=f8261000)
  get Phys(data[n=3]=f8262000)
  get Phys(data[n=3]=f8263000)
  get Phys(data[n=4]=f8264000)
  get Phys(data[n=4]=f8265000)
  get Phys(data[n=5]=f8266000)
  get Phys(data[n=6]=f8267000)
  get Phys(data[n=7]=f8268000)
  get Phys(data[n=8]=f8269000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x39037, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x39037 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 390b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 390b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f826a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f826a000)
  get Phys(data[n=1]=f826b000)
  get Phys(data[n=1]=f826c000)
  get Phys(data[n=2]=f826d000)
  get Phys(data[n=2]=f826e000)
  get Phys(data[n=3]=f826f000)
  get Phys(data[n=3]=f8270000)
  get Phys(data[n=4]=f8271000)
  get Phys(data[n=5]=f8272000)
  get Phys(data[n=6]=f8273000)
  get Phys(data[n=7]=f8274000)
  get Phys(data[n=8]=f8275000)
  get Phys(data[n=9]=f8276000)
  get Phys(data[n=10]=f8277000)
  get Phys(data[n=10]=f8278000)
  get Phys(data[n=11]=f8279000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x390b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x390b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38f37, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 38f37, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f82ac000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ac000)
  get Phys(data[n=1]=f82ad000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38f37, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38f37 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 39937, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 39937, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84f94000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84f94000)
  get Phys(data[n=1]=84f95000)
  get Phys(data[n=2]=84f96000)
  get Phys(data[n=3]=84f97000)
  get Phys(data[n=4]=84f98000)
  get Phys(data[n=5]=84f99000)
  get Phys(data[n=5]=84f9a000)
  get Phys(data[n=5]=84f9b000)
  get Phys(data[n=6]=84f9c000)
  get Phys(data[n=7]=84f9d000)
  get Phys(data[n=7]=84f9e000)
  get Phys(data[n=8]=84f9f000)
  get Phys(data[n=9]=84fa0000)
  get Phys(data[n=10]=84fa1000)
  get Phys(data[n=11]=84fa2000)
  get Phys(data[n=12]=84fa3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x39937, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x39937 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 399b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 399b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84fa4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84fa4000)
  get Phys(data[n=1]=84fa5000)
  get Phys(data[n=2]=84fa6000)
  get Phys(data[n=3]=84fa7000)
  get Phys(data[n=4]=84fa8000)
  get Phys(data[n=5]=84fa9000)
  get Phys(data[n=5]=84faa000)
  get Phys(data[n=6]=84fab000)
  get Phys(data[n=6]=84fac000)
  get Phys(data[n=6]=84fad000)
  get Phys(data[n=7]=84fae000)
  get Phys(data[n=8]=84faf000)
  get Phys(data[n=8]=84fb0000)
  get Phys(data[n=8]=84fb1000)
  get Phys(data[n=8]=84fb2000)
  get Phys(data[n=8]=84fb3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x399b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x399b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 39a37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 39a37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84fb4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84fb4000)
  get Phys(data[n=1]=84fb5000)
  get Phys(data[n=1]=84fb6000)
  get Phys(data[n=2]=84fb7000)
  get Phys(data[n=2]=84fb8000)
  get Phys(data[n=2]=84fb9000)
  get Phys(data[n=3]=84fba000)
  get Phys(data[n=3]=84fbb000)
  get Phys(data[n=4]=84fbc000)
  get Phys(data[n=5]=84fbd000)
  get Phys(data[n=6]=84fbe000)
  get Phys(data[n=7]=84fbf000)
  get Phys(data[n=8]=84fc0000)
  get Phys(data[n=9]=84fc1000)
  get Phys(data[n=9]=84fc2000)
  get Phys(data[n=10]=84fc3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x39a37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x39a37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 39ab7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 39ab7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84fc4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84fc4000)
  get Phys(data[n=1]=84fc5000)
  get Phys(data[n=1]=84fc6000)
  get Phys(data[n=2]=84fc7000)
  get Phys(data[n=3]=84fc8000)
  get Phys(data[n=4]=84fc9000)
  get Phys(data[n=5]=84fca000)
  get Phys(data[n=6]=84fcb000)
  get Phys(data[n=7]=84fcc000)
  get Phys(data[n=8]=84fcd000)
  get Phys(data[n=8]=84fce000)
  get Phys(data[n=9]=84fcf000)
  get Phys(data[n=10]=84fd0000)
  get Phys(data[n=11]=84fd1000)
  get Phys(data[n=12]=84fd2000)
  get Phys(data[n=12]=84fd3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x39ab7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x39ab7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1b99f, OrigWordsRequested 0x3600, DevSize 0x36
IdeReadWrite (REQ): Starting sector is 1b99f, Number of WORDS 0x3600, DevSize 0x36
AtapiDmaSetup: mode 0x45, data f823a000, count 6c00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=1]=f823c000)
  get Phys(data[n=1]=f823d000)
  get Phys(data[n=2]=f823e000)
  get Phys(data[n=3]=f823f000)
  get Phys(data[n=3]=f8240000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1b99f, Count 0x36(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1b99f count 0x36 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 6c00, full size 6c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1b99f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 1b99f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f82ac000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ac000)
  get Phys(data[n=1]=f82ad000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1b99f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1b99f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 30d47, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 30d47, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84f54000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84f54000)
  get Phys(data[n=1]=84f55000)
  get Phys(data[n=2]=84f56000)
  get Phys(data[n=2]=84f57000)
  get Phys(data[n=2]=84f58000)
  get Phys(data[n=3]=84f59000)
  get Phys(data[n=3]=84f5a000)
  get Phys(data[n=4]=84f5b000)
  get Phys(data[n=5]=84f5c000)
  get Phys(data[n=6]=84f5d000)
  get Phys(data[n=7]=84f5e000)
  get Phys(data[n=8]=84f5f000)
  get Phys(data[n=9]=84f60000)
  get Phys(data[n=9]=84f61000)
  get Phys(data[n=10]=84f62000)
  get Phys(data[n=10]=84f63000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x30d47, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x30d47 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 30dc7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 30dc7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84f64000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84f64000)
  get Phys(data[n=1]=84f65000)
  get Phys(data[n=2]=84f66000)
  get Phys(data[n=3]=84f67000)
  get Phys(data[n=4]=84f68000)
  get Phys(data[n=5]=84f69000)
  get Phys(data[n=6]=84f6a000)
  get Phys(data[n=7]=84f6b000)
  get Phys(data[n=8]=84f6c000)
  get Phys(data[n=8]=84f6d000)
  get Phys(data[n=9]=84f6e000)
  get Phys(data[n=10]=84f6f000)
  get Phys(data[n=11]=84f70000)
  get Phys(data[n=12]=84f71000)
  get Phys(data[n=12]=84f72000)
  get Phys(data[n=13]=84f73000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x30dc7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x30dc7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 30e47, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 30e47, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84f74000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84f74000)
  get Phys(data[n=1]=84f75000)
  get Phys(data[n=2]=84f76000)
  get Phys(data[n=3]=84f77000)
  get Phys(data[n=4]=84f78000)
  get Phys(data[n=5]=84f79000)
  get Phys(data[n=5]=84f7a000)
  get Phys(data[n=5]=84f7b000)
  get Phys(data[n=6]=84f7c000)
  get Phys(data[n=6]=84f7d000)
  get Phys(data[n=7]=84f7e000)
  get Phys(data[n=8]=84f7f000)
  get Phys(data[n=9]=84f80000)
  get Phys(data[n=10]=84f81000)
  get Phys(data[n=11]=84f82000)
  get Phys(data[n=12]=84f83000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x30e47, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x30e47 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 30ec7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 30ec7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84f84000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84f84000)
  get Phys(data[n=1]=84f85000)
  get Phys(data[n=1]=84f86000)
  get Phys(data[n=2]=84f87000)
  get Phys(data[n=3]=84f88000)
  get Phys(data[n=3]=84f89000)
  get Phys(data[n=4]=84f8a000)
  get Phys(data[n=4]=84f8b000)
  get Phys(data[n=4]=84f8c000)
  get Phys(data[n=5]=84f8d000)
  get Phys(data[n=6]=84f8e000)
  get Phys(data[n=6]=84f8f000)
  get Phys(data[n=6]=84f90000)
  get Phys(data[n=6]=84f91000)
  get Phys(data[n=6]=84f92000)
  get Phys(data[n=6]=84f93000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x30ec7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x30ec7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 31147, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 31147, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84f94000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84f94000)
  get Phys(data[n=1]=84f95000)
  get Phys(data[n=1]=84f96000)
  get Phys(data[n=1]=84f97000)
  get Phys(data[n=2]=84f98000)
  get Phys(data[n=2]=84f99000)
  get Phys(data[n=3]=84f9a000)
  get Phys(data[n=4]=84f9b000)
  get Phys(data[n=5]=84f9c000)
  get Phys(data[n=6]=84f9d000)
  get Phys(data[n=7]=84f9e000)
  get Phys(data[n=8]=84f9f000)
  get Phys(data[n=9]=84fa0000)
  get Phys(data[n=10]=84fa1000)
  get Phys(data[n=11]=84fa2000)
  get Phys(data[n=12]=84fa3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x31147, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x31147 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 311c7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 311c7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84fa4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84fa4000)
  get Phys(data[n=1]=84fa5000)
  get Phys(data[n=2]=84fa6000)
  get Phys(data[n=2]=84fa7000)
  get Phys(data[n=2]=84fa8000)
  get Phys(data[n=3]=84fa9000)
  get Phys(data[n=4]=84faa000)
  get Phys(data[n=4]=84fab000)
  get Phys(data[n=4]=84fac000)
  get Phys(data[n=4]=84fad000)
  get Phys(data[n=4]=84fae000)
  get Phys(data[n=4]=84faf000)
  get Phys(data[n=5]=84fb0000)
  get Phys(data[n=6]=84fb1000)
  get Phys(data[n=7]=84fb2000)
  get Phys(data[n=8]=84fb3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x311c7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x311c7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 31247, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 31247, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84fb4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84fb4000)
  get Phys(data[n=1]=84fb5000)
  get Phys(data[n=1]=84fb6000)
  get Phys(data[n=2]=84fb7000)
  get Phys(data[n=3]=84fb8000)
  get Phys(data[n=4]=84fb9000)
  get Phys(data[n=5]=84fba000)
  get Phys(data[n=6]=84fbb000)
  get Phys(data[n=7]=84fbc000)
  get Phys(data[n=7]=84fbd000)
  get Phys(data[n=8]=84fbe000)
  get Phys(data[n=8]=84fbf000)
  get Phys(data[n=9]=84fc0000)
  get Phys(data[n=9]=84fc1000)
  get Phys(data[n=10]=84fc2000)
  get Phys(data[n=11]=84fc3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x31247, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x31247 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 312c7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 312c7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84fc4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84fc4000)
  get Phys(data[n=1]=84fc5000)
  get Phys(data[n=2]=84fc6000)
  get Phys(data[n=3]=84fc7000)
  get Phys(data[n=4]=84fc8000)
  get Phys(data[n=4]=84fc9000)
  get Phys(data[n=5]=84fca000)
  get Phys(data[n=6]=84fcb000)
  get Phys(data[n=7]=84fcc000)
  get Phys(data[n=7]=84fcd000)
  get Phys(data[n=8]=84fce000)
  get Phys(data[n=8]=84fcf000)
  get Phys(data[n=9]=84fd0000)
  get Phys(data[n=10]=84fd1000)
  get Phys(data[n=11]=84fd2000)
  get Phys(data[n=12]=84fd3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x312c7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x312c7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../base/system/services/rpcserver.c:1714) RNotifyBootConfigStatus(00000000 1) called
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8592e50
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d2747, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d2747, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85014000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85014000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d2747, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d2747 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8592e50
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e21cf, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1e21cf, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85054000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85054000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e21cf, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e21cf count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf85930a4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e233f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1e233f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f823a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=1]=f823c000)
  get Phys(data[n=1]=f823d000)
  get Phys(data[n=1]=f823e000)
  get Phys(data[n=1]=f823f000)
  get Phys(data[n=1]=f8240000)
  get Phys(data[n=2]=f8241000)
  get Phys(data[n=3]=f8242000)
  get Phys(data[n=4]=f8243000)
  get Phys(data[n=5]=f8244000)
  get Phys(data[n=5]=f8245000)
  get Phys(data[n=6]=f8246000)
  get Phys(data[n=6]=f8247000)
  get Phys(data[n=7]=f8248000)
  get Phys(data[n=8]=f8249000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e233f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e233f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf85930a4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e23bf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1e23bf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f824a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f824a000)
  get Phys(data[n=1]=f824b000)
  get Phys(data[n=2]=f824c000)
  get Phys(data[n=3]=f824d000)
  get Phys(data[n=3]=f824e000)
  get Phys(data[n=4]=f824f000)
  get Phys(data[n=4]=f8250000)
  get Phys(data[n=5]=f8251000)
  get Phys(data[n=5]=f8252000)
  get Phys(data[n=6]=f8253000)
  get Phys(data[n=7]=f8254000)
  get Phys(data[n=8]=f8255000)
  get Phys(data[n=9]=f8256000)
  get Phys(data[n=10]=f8257000)
  get Phys(data[n=11]=f8258000)
  get Phys(data[n=12]=f8259000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e23bf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e23bf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf85930a4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e243f, OrigWordsRequested 0x1800, DevSize 0x18
IdeReadWrite (REQ): Starting sector is 1e243f, Number of WORDS 0x1800, DevSize 0x18
AtapiDmaSetup: mode 0x45, data f825a000, count 3000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f825a000)
  get Phys(data[n=1]=f825b000)
  get Phys(data[n=2]=f825c000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e243f, Count 0x18(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e243f count 0x18 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 3000, full size 3000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8592e50
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e230f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1e230f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 850d4000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=850d4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e230f, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e230f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8593338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 14d4f, OrigWordsRequested 0x6d00, DevSize 0x6d
IdeReadWrite (REQ): Starting sector is 14d4f, Number of WORDS 0x6d00, DevSize 0x6d
AtapiDmaSetup: mode 0x45, data f823a000, count da00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=2]=f823c000)
  get Phys(data[n=3]=f823d000)
  get Phys(data[n=4]=f823e000)
  get Phys(data[n=4]=f823f000)
  get Phys(data[n=5]=f8240000)
  get Phys(data[n=5]=f8241000)
  get Phys(data[n=6]=f8242000)
  get Phys(data[n=6]=f8243000)
  get Phys(data[n=7]=f8244000)
  get Phys(data[n=8]=f8245000)
  get Phys(data[n=9]=f8246000)
  get Phys(data[n=10]=f8247000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x14d4f, Count 0x6d(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x14d4f count 0x6d feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered da00, full size da00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf85936cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 14d4f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 14d4f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f829c000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f829c000)
  get Phys(data[n=1]=f829d000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x14d4f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x14d4f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Boot took 128166943966 cycles!
Interrupts: 5390 System Calls: 25911 Context Switches: 3519
(../../ntoskrnl/se/semgr.c:705) HACK: Should deny access for caller: granted 0x0, desired 0x100000 (generic mapping B1286ED8).
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38f37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 38f37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f823a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=2]=f823c000)
  get Phys(data[n=3]=f823d000)
  get Phys(data[n=4]=f823e000)
  get Phys(data[n=5]=f823f000)
  get Phys(data[n=6]=f8240000)
  get Phys(data[n=7]=f8241000)
  get Phys(data[n=8]=f8242000)
  get Phys(data[n=9]=f8243000)
  get Phys(data[n=10]=f8244000)
  get Phys(data[n=11]=f8245000)
  get Phys(data[n=12]=f8246000)
  get Phys(data[n=13]=f8247000)
  get Phys(data[n=13]=f8248000)
  get Phys(data[n=13]=f8249000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38f37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38f37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38fb7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 38fb7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f824a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f824a000)
  get Phys(data[n=1]=f824b000)
  get Phys(data[n=1]=f824c000)
  get Phys(data[n=2]=f824d000)
  get Phys(data[n=2]=f824e000)
  get Phys(data[n=3]=f824f000)
  get Phys(data[n=3]=f8250000)
  get Phys(data[n=4]=f8251000)
  get Phys(data[n=5]=f8252000)
  get Phys(data[n=5]=f8253000)
  get Phys(data[n=6]=f8254000)
  get Phys(data[n=6]=f8255000)
  get Phys(data[n=7]=f8256000)
  get Phys(data[n=8]=f8257000)
  get Phys(data[n=9]=f8258000)
  get Phys(data[n=10]=f8259000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38fb7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38fb7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 39037, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 39037, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f825a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f825a000)
  get Phys(data[n=1]=f825b000)
  get Phys(data[n=1]=f825c000)
  get Phys(data[n=2]=f825d000)
  get Phys(data[n=2]=f825e000)
  get Phys(data[n=3]=f825f000)
  get Phys(data[n=4]=f8260000)
  get Phys(data[n=5]=f8261000)
  get Phys(data[n=6]=f8262000)
  get Phys(data[n=7]=f8263000)
  get Phys(data[n=8]=f8264000)
  get Phys(data[n=9]=f8265000)
  get Phys(data[n=9]=f8266000)
  get Phys(data[n=10]=f8267000)
  get Phys(data[n=11]=f8268000)
  get Phys(data[n=12]=f8269000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x39037, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x39037 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 390b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 390b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f826a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f826a000)
  get Phys(data[n=1]=f826b000)
  get Phys(data[n=1]=f826c000)
  get Phys(data[n=2]=f826d000)
  get Phys(data[n=3]=f826e000)
  get Phys(data[n=4]=f826f000)
  get Phys(data[n=5]=f8270000)
  get Phys(data[n=6]=f8271000)
  get Phys(data[n=7]=f8272000)
  get Phys(data[n=7]=f8273000)
  get Phys(data[n=7]=f8274000)
  get Phys(data[n=7]=f8275000)
  get Phys(data[n=7]=f8276000)
  get Phys(data[n=8]=f8277000)
  get Phys(data[n=9]=f8278000)
  get Phys(data[n=9]=f8279000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x390b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x390b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38f37, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 38f37, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8288000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8288000)
  get Phys(data[n=1]=f8289000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38f37, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38f37 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 39937, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 39937, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85194000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85194000)
  get Phys(data[n=1]=85195000)
  get Phys(data[n=2]=85196000)
  get Phys(data[n=3]=85197000)
  get Phys(data[n=4]=85198000)
  get Phys(data[n=5]=85199000)
  get Phys(data[n=6]=8519a000)
  get Phys(data[n=7]=8519b000)
  get Phys(data[n=8]=8519c000)
  get Phys(data[n=8]=8519d000)
  get Phys(data[n=8]=8519e000)
  get Phys(data[n=8]=8519f000)
  get Phys(data[n=8]=851a0000)
  get Phys(data[n=8]=851a1000)
  get Phys(data[n=9]=851a2000)
  get Phys(data[n=9]=851a3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x39937, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x39937 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 399b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 399b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 851a4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=851a4000)
  get Phys(data[n=1]=851a5000)
  get Phys(data[n=2]=851a6000)
  get Phys(data[n=3]=851a7000)
  get Phys(data[n=4]=851a8000)
  get Phys(data[n=5]=851a9000)
  get Phys(data[n=5]=851aa000)
  get Phys(data[n=6]=851ab000)
  get Phys(data[n=7]=851ac000)
  get Phys(data[n=8]=851ad000)
  get Phys(data[n=9]=851ae000)
  get Phys(data[n=10]=851af000)
  get Phys(data[n=10]=851b0000)
  get Phys(data[n=10]=851b1000)
  get Phys(data[n=11]=851b2000)
  get Phys(data[n=11]=851b3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x399b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x399b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 39a37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 39a37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 851b4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=851b4000)
  get Phys(data[n=1]=851b5000)
  get Phys(data[n=2]=851b6000)
  get Phys(data[n=3]=851b7000)
  get Phys(data[n=4]=851b8000)
  get Phys(data[n=5]=851b9000)
  get Phys(data[n=6]=851ba000)
  get Phys(data[n=6]=851bb000)
  get Phys(data[n=7]=851bc000)
  get Phys(data[n=8]=851bd000)
  get Phys(data[n=9]=851be000)
  get Phys(data[n=9]=851bf000)
  get Phys(data[n=10]=851c0000)
  get Phys(data[n=10]=851c1000)
  get Phys(data[n=11]=851c2000)
  get Phys(data[n=12]=851c3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x39a37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x39a37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 39ab7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 39ab7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 851c4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=851c4000)
  get Phys(data[n=1]=851c5000)
  get Phys(data[n=2]=851c6000)
  get Phys(data[n=3]=851c7000)
  get Phys(data[n=3]=851c8000)
  get Phys(data[n=3]=851c9000)
  get Phys(data[n=3]=851ca000)
  get Phys(data[n=3]=851cb000)
  get Phys(data[n=4]=851cc000)
  get Phys(data[n=5]=851cd000)
  get Phys(data[n=5]=851ce000)
  get Phys(data[n=6]=851cf000)
  get Phys(data[n=6]=851d0000)
  get Phys(data[n=7]=851d1000)
  get Phys(data[n=8]=851d2000)
  get Phys(data[n=8]=851d3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x39ab7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x39ab7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1b99f, OrigWordsRequested 0x3600, DevSize 0x36
IdeReadWrite (REQ): Starting sector is 1b99f, Number of WORDS 0x3600, DevSize 0x36
AtapiDmaSetup: mode 0x45, data f823a000, count 6c00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=2]=f823c000)
  get Phys(data[n=3]=f823d000)
  get Phys(data[n=4]=f823e000)
  get Phys(data[n=5]=f823f000)
  get Phys(data[n=6]=f8240000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1b99f, Count 0x36(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1b99f count 0x36 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 6c00, full size 6c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1b99f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 1b99f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8288000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8288000)
  get Phys(data[n=1]=f8289000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1b99f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1b99f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 36947, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 36947, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84fd4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84fd4000)
  get Phys(data[n=1]=84fd5000)
  get Phys(data[n=1]=84fd6000)
  get Phys(data[n=2]=84fd7000)
  get Phys(data[n=3]=84fd8000)
  get Phys(data[n=4]=84fd9000)
  get Phys(data[n=5]=84fda000)
  get Phys(data[n=6]=84fdb000)
  get Phys(data[n=7]=84fdc000)
  get Phys(data[n=8]=84fdd000)
  get Phys(data[n=9]=84fde000)
  get Phys(data[n=10]=84fdf000)
  get Phys(data[n=11]=84fe0000)
  get Phys(data[n=12]=84fe1000)
  get Phys(data[n=12]=84fe2000)
  get Phys(data[n=13]=84fe3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x36947, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x36947 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 369c7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 369c7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84fe4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84fe4000)
  get Phys(data[n=1]=84fe5000)
  get Phys(data[n=2]=84fe6000)
  get Phys(data[n=3]=84fe7000)
  get Phys(data[n=3]=84fe8000)
  get Phys(data[n=3]=84fe9000)
  get Phys(data[n=3]=84fea000)
  get Phys(data[n=3]=84feb000)
  get Phys(data[n=3]=84fec000)
  get Phys(data[n=4]=84fed000)
  get Phys(data[n=5]=84fee000)
  get Phys(data[n=6]=84fef000)
  get Phys(data[n=7]=84ff0000)
  get Phys(data[n=7]=84ff1000)
  get Phys(data[n=8]=84ff2000)
  get Phys(data[n=8]=84ff3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x369c7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x369c7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 36a47, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 36a47, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 84ff4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=84ff4000)
  get Phys(data[n=1]=84ff5000)
  get Phys(data[n=2]=84ff6000)
  get Phys(data[n=3]=84ff7000)
  get Phys(data[n=4]=84ff8000)
  get Phys(data[n=5]=84ff9000)
  get Phys(data[n=5]=84ffa000)
  get Phys(data[n=6]=84ffb000)
  get Phys(data[n=6]=84ffc000)
  get Phys(data[n=7]=84ffd000)
  get Phys(data[n=7]=84ffe000)
  get Phys(data[n=8]=84fff000)
  get Phys(data[n=9]=85000000)
  get Phys(data[n=10]=85001000)
  get Phys(data[n=11]=85002000)
  get Phys(data[n=12]=85003000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x36a47, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x36a47 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 36ac7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 36ac7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85004000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85004000)
  get Phys(data[n=1]=85005000)
  get Phys(data[n=1]=85006000)
  get Phys(data[n=2]=85007000)
  get Phys(data[n=3]=85008000)
  get Phys(data[n=4]=85009000)
  get Phys(data[n=4]=8500a000)
  get Phys(data[n=4]=8500b000)
  get Phys(data[n=4]=8500c000)
  get Phys(data[n=5]=8500d000)
  get Phys(data[n=6]=8500e000)
  get Phys(data[n=7]=8500f000)
  get Phys(data[n=8]=85010000)
  get Phys(data[n=9]=85011000)
  get Phys(data[n=10]=85012000)
  get Phys(data[n=10]=85013000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x36ac7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x36ac7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 33f47, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 33f47, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85154000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85154000)
  get Phys(data[n=1]=85155000)
  get Phys(data[n=1]=85156000)
  get Phys(data[n=2]=85157000)
  get Phys(data[n=2]=85158000)
  get Phys(data[n=3]=85159000)
  get Phys(data[n=4]=8515a000)
  get Phys(data[n=5]=8515b000)
  get Phys(data[n=6]=8515c000)
  get Phys(data[n=7]=8515d000)
  get Phys(data[n=8]=8515e000)
  get Phys(data[n=8]=8515f000)
  get Phys(data[n=8]=85160000)
  get Phys(data[n=8]=85161000)
  get Phys(data[n=8]=85162000)
  get Phys(data[n=9]=85163000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x33f47, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x33f47 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 33fc7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 33fc7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85164000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85164000)
  get Phys(data[n=1]=85165000)
  get Phys(data[n=2]=85166000)
  get Phys(data[n=2]=85167000)
  get Phys(data[n=3]=85168000)
  get Phys(data[n=4]=85169000)
  get Phys(data[n=4]=8516a000)
  get Phys(data[n=5]=8516b000)
  get Phys(data[n=5]=8516c000)
  get Phys(data[n=6]=8516d000)
  get Phys(data[n=6]=8516e000)
  get Phys(data[n=7]=8516f000)
  get Phys(data[n=8]=85170000)
  get Phys(data[n=9]=85171000)
  get Phys(data[n=10]=85172000)
  get Phys(data[n=11]=85173000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x33fc7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x33fc7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 34047, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 34047, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85174000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85174000)
  get Phys(data[n=1]=85175000)
  get Phys(data[n=1]=85176000)
  get Phys(data[n=1]=85177000)
  get Phys(data[n=1]=85178000)
  get Phys(data[n=2]=85179000)
  get Phys(data[n=2]=8517a000)
  get Phys(data[n=3]=8517b000)
  get Phys(data[n=3]=8517c000)
  get Phys(data[n=4]=8517d000)
  get Phys(data[n=5]=8517e000)
  get Phys(data[n=5]=8517f000)
  get Phys(data[n=6]=85180000)
  get Phys(data[n=6]=85181000)
  get Phys(data[n=7]=85182000)
  get Phys(data[n=8]=85183000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x34047, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x34047 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82bd6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 340c7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 340c7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85184000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85184000)
  get Phys(data[n=1]=85185000)
  get Phys(data[n=2]=85186000)
  get Phys(data[n=2]=85187000)
  get Phys(data[n=2]=85188000)
  get Phys(data[n=3]=85189000)
  get Phys(data[n=3]=8518a000)
  get Phys(data[n=4]=8518b000)
  get Phys(data[n=5]=8518c000)
  get Phys(data[n=6]=8518d000)
  get Phys(data[n=7]=8518e000)
  get Phys(data[n=8]=8518f000)
  get Phys(data[n=9]=85190000)
  get Phys(data[n=10]=85191000)
  get Phys(data[n=10]=85192000)
  get Phys(data[n=11]=85193000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x340c7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x340c7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ee2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11ab7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 11ab7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f81fa000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f81fa000)
  get Phys(data[n=1]=f81fb000)
  get Phys(data[n=2]=f81fc000)
  get Phys(data[n=2]=f81fd000)
  get Phys(data[n=3]=f81fe000)
  get Phys(data[n=4]=f81ff000)
  get Phys(data[n=4]=f8200000)
  get Phys(data[n=5]=f8201000)
  get Phys(data[n=5]=f8202000)
  get Phys(data[n=6]=f8203000)
  get Phys(data[n=7]=f8204000)
  get Phys(data[n=7]=f8205000)
  get Phys(data[n=8]=f8206000)
  get Phys(data[n=8]=f8207000)
  get Phys(data[n=9]=f8208000)
  get Phys(data[n=9]=f8209000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x11ab7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x11ab7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ee2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11b37, OrigWordsRequested 0x1900, DevSize 0x19
IdeReadWrite (REQ): Starting sector is 11b37, Number of WORDS 0x1900, DevSize 0x19
AtapiDmaSetup: mode 0x45, data f820a000, count 3200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f820a000)
  get Phys(data[n=1]=f820b000)
  get Phys(data[n=2]=f820c000)
  get Phys(data[n=3]=f820d000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x11b37, Count 0x19(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x11b37 count 0x19 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 3200, full size 3200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ee6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11ab7, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 11ab7, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8238000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8238000)
  get Phys(data[n=1]=f8239000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x11ab7, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x11ab7 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 128af, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 128af, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f823a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=2]=f823c000)
  get Phys(data[n=3]=f823d000)
  get Phys(data[n=4]=f823e000)
  get Phys(data[n=5]=f823f000)
  get Phys(data[n=6]=f8240000)
  get Phys(data[n=6]=f8241000)
  get Phys(data[n=7]=f8242000)
  get Phys(data[n=8]=f8243000)
  get Phys(data[n=8]=f8244000)
  get Phys(data[n=9]=f8245000)
  get Phys(data[n=9]=f8246000)
  get Phys(data[n=10]=f8247000)
  get Phys(data[n=11]=f8248000)
  get Phys(data[n=11]=f8249000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x128af, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x128af count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1292f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1292f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f824a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f824a000)
  get Phys(data[n=1]=f824b000)
  get Phys(data[n=2]=f824c000)
  get Phys(data[n=2]=f824d000)
  get Phys(data[n=3]=f824e000)
  get Phys(data[n=4]=f824f000)
  get Phys(data[n=5]=f8250000)
  get Phys(data[n=6]=f8251000)
  get Phys(data[n=7]=f8252000)
  get Phys(data[n=7]=f8253000)
  get Phys(data[n=7]=f8254000)
  get Phys(data[n=7]=f8255000)
  get Phys(data[n=7]=f8256000)
  get Phys(data[n=7]=f8257000)
  get Phys(data[n=8]=f8258000)
  get Phys(data[n=8]=f8259000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1292f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1292f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 129af, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 129af, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f825a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f825a000)
  get Phys(data[n=1]=f825b000)
  get Phys(data[n=2]=f825c000)
  get Phys(data[n=3]=f825d000)
  get Phys(data[n=3]=f825e000)
  get Phys(data[n=4]=f825f000)
  get Phys(data[n=4]=f8260000)
  get Phys(data[n=5]=f8261000)
  get Phys(data[n=6]=f8262000)
  get Phys(data[n=7]=f8263000)
  get Phys(data[n=7]=f8264000)
  get Phys(data[n=8]=f8265000)
  get Phys(data[n=8]=f8266000)
  get Phys(data[n=9]=f8267000)
  get Phys(data[n=10]=f8268000)
  get Phys(data[n=10]=f8269000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x129af, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x129af count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 12a2f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 12a2f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f826a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f826a000)
  get Phys(data[n=1]=f826b000)
  get Phys(data[n=2]=f826c000)
  get Phys(data[n=3]=f826d000)
  get Phys(data[n=4]=f826e000)
  get Phys(data[n=5]=f826f000)
  get Phys(data[n=6]=f8270000)
  get Phys(data[n=6]=f8271000)
  get Phys(data[n=7]=f8272000)
  get Phys(data[n=8]=f8273000)
  get Phys(data[n=9]=f8274000)
  get Phys(data[n=10]=f8275000)
  get Phys(data[n=10]=f8276000)
  get Phys(data[n=10]=f8277000)
  get Phys(data[n=11]=f8278000)
  get Phys(data[n=12]=f8279000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x12a2f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x12a2f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 128af, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 128af, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8234000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8234000)
  get Phys(data[n=1]=f8235000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x128af, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x128af count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ace50
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e223f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1e223f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85254000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85254000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e223f, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e223f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ace50
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e2247, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1e2247, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85294000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85294000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e2247, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e2247 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad324
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e224f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1e224f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 852d4000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=852d4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e224f, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e224f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ace50
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d27ff, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d27ff, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85314000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85314000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d27ff, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d27ff count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ace50
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d281f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d281f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85354000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85354000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d281f, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d281f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
DHCPCSVC: DHCP service is starting up
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ace50
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d2827, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d2827, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85394000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85394000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d2827, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d2827 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad324
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d2837, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d2837, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 853d4000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=853d4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d2837, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d2837 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ee338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 118f7, OrigWordsRequested 0x4c00, DevSize 0x4c
IdeReadWrite (REQ): Starting sector is 118f7, Number of WORDS 0x4c00, DevSize 0x4c
AtapiDmaSetup: mode 0x45, data f81b6000, count 9800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f81b6000)
  get Phys(data[n=1]=f81b7000)
  get Phys(data[n=2]=f81b8000)
  get Phys(data[n=3]=f81b9000)
  get Phys(data[n=4]=f81ba000)
  get Phys(data[n=5]=f81bb000)
  get Phys(data[n=6]=f81bc000)
  get Phys(data[n=7]=f81bd000)
  get Phys(data[n=7]=f81be000)
  get Phys(data[n=8]=f81bf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x118f7, Count 0x4c(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x118f7 count 0x4c feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 9800, full size 9800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ee6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 118f7, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 118f7, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8211000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8211000)
  get Phys(data[n=1]=f8212000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x118f7, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x118f7 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf821f2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 26e0f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 26e0f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f823a000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=2]=f823c000)
  get Phys(data[n=3]=f823d000)
  get Phys(data[n=4]=f823e000)
  get Phys(data[n=5]=f823f000)
  get Phys(data[n=6]=f8240000)
  get Phys(data[n=7]=f8241000)
  get Phys(data[n=8]=f8242000)
  get Phys(data[n=8]=f8243000)
  get Phys(data[n=9]=f8244000)
  get Phys(data[n=10]=f8245000)
  get Phys(data[n=11]=f8246000)
  get Phys(data[n=12]=f8247000)
  get Phys(data[n=12]=f8248000)
  get Phys(data[n=13]=f8249000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x26e0f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x26e0f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf821f2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 26e8f, OrigWordsRequested 0x3900, DevSize 0x39
IdeReadWrite (REQ): Starting sector is 26e8f, Number of WORDS 0x3900, DevSize 0x39
AtapiDmaSetup: mode 0x45, data f824a000, count 7200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f824a000)
  get Phys(data[n=1]=f824b000)
  get Phys(data[n=1]=f824c000)
  get Phys(data[n=2]=f824d000)
  get Phys(data[n=2]=f824e000)
  get Phys(data[n=2]=f824f000)
  get Phys(data[n=3]=f8250000)
  get Phys(data[n=4]=f8251000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x26e8f, Count 0x39(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x26e8f count 0x39 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 7200, full size 7200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf821f6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 26e0f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 26e0f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f820d000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f820d000)
  get Phys(data[n=1]=f820e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x26e0f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x26e0f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf821f338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b1b7, OrigWordsRequested 0x2000, DevSize 0x20
IdeReadWrite (REQ): Starting sector is 3b1b7, Number of WORDS 0x2000, DevSize 0x20
AtapiDmaSetup: mode 0x45, data f823a000, count 4000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=2]=f823c000)
  get Phys(data[n=3]=f823d000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b1b7, Count 0x20(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b1b7 count 0x20 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 4000, full size 4000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf821f6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3b1b7, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3b1b7, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f820d000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f820d000)
  get Phys(data[n=1]=f820e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3b1b7, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3b1b7 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ee338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1178f, OrigWordsRequested 0x4f00, DevSize 0x4f
IdeReadWrite (REQ): Starting sector is 1178f, Number of WORDS 0x4f00, DevSize 0x4f
AtapiDmaSetup: mode 0x45, data f823a000, count 9e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f823a000)
  get Phys(data[n=1]=f823b000)
  get Phys(data[n=2]=f823c000)
  get Phys(data[n=3]=f823d000)
  get Phys(data[n=4]=f823e000)
  get Phys(data[n=5]=f823f000)
  get Phys(data[n=6]=f8240000)
  get Phys(data[n=7]=f8241000)
  get Phys(data[n=7]=f8242000)
  get Phys(data[n=8]=f8243000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1178f, Count 0x4f(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1178f count 0x4f feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 9e00, full size 9e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/pool.c:482) Paged pool expansion: 1 10
DHCPCSVC: Adapter Name: [{3cd326a3-11bb-4ada-8137-3927ee070294}] (dynamic)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ee6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1178f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 1178f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f820d000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f820d000)
  get Phys(data[n=1]=f820e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1178f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1178f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8271604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x400, DevSize 0x4
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x400, DevSize 0x4
AtapiDmaSetup: mode 0x45, data 85514000, count 800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x4(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d289f count 0x4 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 800, full size 800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf827158c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85514000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d289f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82356d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 130af, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 130af, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85214000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85214000)
  get Phys(data[n=1]=85215000)
  get Phys(data[n=2]=85216000)
  get Phys(data[n=3]=85217000)
  get Phys(data[n=4]=85218000)
  get Phys(data[n=5]=85219000)
  get Phys(data[n=6]=8521a000)
  get Phys(data[n=6]=8521b000)
  get Phys(data[n=7]=8521c000)
  get Phys(data[n=8]=8521d000)
  get Phys(data[n=9]=8521e000)
  get Phys(data[n=10]=8521f000)
  get Phys(data[n=10]=85220000)
  get Phys(data[n=10]=85221000)
  get Phys(data[n=11]=85222000)
  get Phys(data[n=12]=85223000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x130af, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x130af count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82356d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1312f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1312f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85224000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85224000)
  get Phys(data[n=1]=85225000)
  get Phys(data[n=2]=85226000)
  get Phys(data[n=3]=85227000)
  get Phys(data[n=4]=85228000)
  get Phys(data[n=5]=85229000)
  get Phys(data[n=6]=8522a000)
  get Phys(data[n=6]=8522b000)
  get Phys(data[n=7]=8522c000)
  get Phys(data[n=8]=8522d000)
  get Phys(data[n=9]=8522e000)
  get Phys(data[n=10]=8522f000)
  get Phys(data[n=11]=85230000)
  get Phys(data[n=12]=85231000)
  get Phys(data[n=13]=85232000)
  get Phys(data[n=14]=85233000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1312f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1312f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82356d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 131af, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 131af, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85234000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85234000)
  get Phys(data[n=1]=85235000)
  get Phys(data[n=2]=85236000)
  get Phys(data[n=3]=85237000)
  get Phys(data[n=4]=85238000)
  get Phys(data[n=5]=85239000)
  get Phys(data[n=5]=8523a000)
  get Phys(data[n=6]=8523b000)
  get Phys(data[n=7]=8523c000)
  get Phys(data[n=7]=8523d000)
  get Phys(data[n=7]=8523e000)
  get Phys(data[n=8]=8523f000)
  get Phys(data[n=8]=85240000)
  get Phys(data[n=8]=85241000)
  get Phys(data[n=9]=85242000)
  get Phys(data[n=10]=85243000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x131af, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x131af count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x400, DevSize 0x4
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x400, DevSize 0x4
AtapiDmaSetup: mode 0x45, data 85514000, count 800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x4(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d289f count 0x4 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 800, full size 800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c58c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85514000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d289f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82356d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1322f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1322f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85244000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85244000)
  get Phys(data[n=1]=85245000)
  get Phys(data[n=2]=85246000)
  get Phys(data[n=3]=85247000)
  get Phys(data[n=3]=85248000)
  get Phys(data[n=4]=85249000)
  get Phys(data[n=4]=8524a000)
  get Phys(data[n=5]=8524b000)
  get Phys(data[n=6]=8524c000)
  get Phys(data[n=7]=8524d000)
  get Phys(data[n=7]=8524e000)
  get Phys(data[n=8]=8524f000)
  get Phys(data[n=9]=85250000)
  get Phys(data[n=9]=85251000)
  get Phys(data[n=10]=85252000)
  get Phys(data[n=10]=85253000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1322f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1322f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x400, DevSize 0x4
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x400, DevSize 0x4
AtapiDmaSetup: mode 0x45, data 85514000, count 800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x4(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d289f count 0x4 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 800, full size 800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c58c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85514000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d289f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x400, DevSize 0x4
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x400, DevSize 0x4
AtapiDmaSetup: mode 0x45, data 85514000, count 800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x4(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d289f count 0x4 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 800, full size 800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c58c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85514000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d289f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x400, DevSize 0x4
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x400, DevSize 0x4
AtapiDmaSetup: mode 0x45, data 85514000, count 800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x4(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d289f count 0x4 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 800, full size 800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c58c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85514000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d289f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x400, DevSize 0x4
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x400, DevSize 0x4
AtapiDmaSetup: mode 0x45, data 85514000, count 800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x4(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d289f count 0x4 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 800, full size 800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c58c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85514000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d289f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x500, DevSize 0x5
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x500, DevSize 0x5
AtapiDmaSetup: mode 0x45, data 85514000, count a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x5(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d289f count 0x5 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a00, full size a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c58c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85514000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d289f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x500, DevSize 0x5
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x500, DevSize 0x5
AtapiDmaSetup: mode 0x45, data 85514000, count a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x5(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d289f count 0x5 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a00, full size a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c58c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85514000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d289f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x500, DevSize 0x5
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x500, DevSize 0x5
AtapiDmaSetup: mode 0x45, data 85514000, count a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x5(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d289f count 0x5 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a00, full size a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c58c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85514000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d289f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
fixme:(../../dll/win32/setupapi/cfgmgr.c:127) Stub 00235220 00C0FF3C 1 00C0FF20
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x500, DevSize 0x5
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x500, DevSize 0x5
AtapiDmaSetup: mode 0x45, data 85514000, count a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x5(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d289f count 0x5 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a00, full size a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c58c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85514000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d289f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x500, DevSize 0x5
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x500, DevSize 0x5
AtapiDmaSetup: mode 0x45, data 85514000, count a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x5(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d289f count 0x5 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a00, full size a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c58c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85514000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d289f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82356d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 13aaf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 13aaf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85554000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85554000)
  get Phys(data[n=1]=85555000)
  get Phys(data[n=2]=85556000)
  get Phys(data[n=2]=85557000)
  get Phys(data[n=3]=85558000)
  get Phys(data[n=4]=85559000)
  get Phys(data[n=4]=8555a000)
  get Phys(data[n=5]=8555b000)
  get Phys(data[n=5]=8555c000)
  get Phys(data[n=6]=8555d000)
  get Phys(data[n=7]=8555e000)
  get Phys(data[n=8]=8555f000)
  get Phys(data[n=9]=85560000)
  get Phys(data[n=10]=85561000)
  get Phys(data[n=11]=85562000)
  get Phys(data[n=12]=85563000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x13aaf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x13aaf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x500, DevSize 0x5
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x500, DevSize 0x5
AtapiDmaSetup: mode 0x45, data 85514000, count a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x5(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d289f count 0x5 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a00, full size a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c58c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85514000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d289f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82356d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 13b2f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 13b2f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85564000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85564000)
  get Phys(data[n=1]=85565000)
  get Phys(data[n=1]=85566000)
  get Phys(data[n=2]=85567000)
  get Phys(data[n=2]=85568000)
  get Phys(data[n=3]=85569000)
  get Phys(data[n=4]=8556a000)
  get Phys(data[n=5]=8556b000)
  get Phys(data[n=6]=8556c000)
  get Phys(data[n=7]=8556d000)
  get Phys(data[n=8]=8556e000)
  get Phys(data[n=9]=8556f000)
  get Phys(data[n=10]=85570000)
  get Phys(data[n=11]=85571000)
  get Phys(data[n=12]=85572000)
  get Phys(data[n=13]=85573000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x13b2f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x13b2f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82356d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 13baf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 13baf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85574000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85574000)
  get Phys(data[n=1]=85575000)
  get Phys(data[n=2]=85576000)
  get Phys(data[n=3]=85577000)
  get Phys(data[n=4]=85578000)
  get Phys(data[n=5]=85579000)
  get Phys(data[n=6]=8557a000)
  get Phys(data[n=7]=8557b000)
  get Phys(data[n=8]=8557c000)
  get Phys(data[n=9]=8557d000)
  get Phys(data[n=10]=8557e000)
  get Phys(data[n=11]=8557f000)
  get Phys(data[n=12]=85580000)
  get Phys(data[n=13]=85581000)
  get Phys(data[n=14]=85582000)
  get Phys(data[n=15]=85583000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x13baf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x13baf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/se/semgr.c:705) HACK: Should deny access for caller: granted 0x0, desired 0x100000 (generic mapping B1286ED8).
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82356d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 13c2f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 13c2f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85584000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85584000)
  get Phys(data[n=1]=85585000)
  get Phys(data[n=1]=85586000)
  get Phys(data[n=2]=85587000)
  get Phys(data[n=2]=85588000)
  get Phys(data[n=3]=85589000)
  get Phys(data[n=4]=8558a000)
  get Phys(data[n=5]=8558b000)
  get Phys(data[n=5]=8558c000)
  get Phys(data[n=6]=8558d000)
  get Phys(data[n=7]=8558e000)
  get Phys(data[n=7]=8558f000)
  get Phys(data[n=8]=85590000)
  get Phys(data[n=9]=85591000)
  get Phys(data[n=9]=85592000)
  get Phys(data[n=9]=85593000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x13c2f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x13c2f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../lib/rtl/actctx.c:874) Unsupported yet language attribute (*)
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8234ee8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d29b7, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d29b7, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85514000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85514000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d29b7, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d29b7 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8235324
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d29bf, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d29bf, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85594000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85594000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d29bf, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d29bf count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8235338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d29c7, OrigWordsRequested 0x400, DevSize 0x4
IdeReadWrite (REQ): Starting sector is 1d29c7, Number of WORDS 0x400, DevSize 0x4
AtapiDmaSetup: mode 0x45, data f81b2000, count 800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f81b2000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d29c7, Count 0x4(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d29c7 count 0x4 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 800, full size 800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8235338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 12877, OrigWordsRequested 0x3600, DevSize 0x36
IdeReadWrite (REQ): Starting sector is 12877, Number of WORDS 0x3600, DevSize 0x36
AtapiDmaSetup: mode 0x45, data f81b2000, count 6c00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f81b2000)
  get Phys(data[n=1]=f81b3000)
  get Phys(data[n=2]=f81b4000)
  get Phys(data[n=3]=f81b5000)
  get Phys(data[n=3]=f81b6000)
  get Phys(data[n=4]=f81b7000)
  get Phys(data[n=5]=f81b8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x12877, Count 0x36(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x12877 count 0x36 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 6c00, full size 6c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x500, DevSize 0x5
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x500, DevSize 0x5
AtapiDmaSetup: mode 0x45, data 85614000, count a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85614000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x5(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d289f count 0x5 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a00, full size a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82356cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 12877, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 12877, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f820d000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f820d000)
  get Phys(data[n=1]=f820e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x12877, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x12877 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c58c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85614000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85614000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d289f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8235338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 28c37, OrigWordsRequested 0x4100, DevSize 0x41
IdeReadWrite (REQ): Starting sector is 28c37, Number of WORDS 0x4100, DevSize 0x41
AtapiDmaSetup: mode 0x45, data f81b2000, count 8200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f81b2000)
  get Phys(data[n=1]=f81b3000)
  get Phys(data[n=1]=f81b4000)
  get Phys(data[n=2]=f81b5000)
  get Phys(data[n=3]=f81b6000)
  get Phys(data[n=4]=f81b7000)
  get Phys(data[n=4]=f81b8000)
  get Phys(data[n=5]=f81b9000)
  get Phys(data[n=5]=f81ba000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x28c37, Count 0x41(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x28c37 count 0x41 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 8200, full size 8200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82356cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 28c37, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 28c37, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f820d000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f820d000)
  get Phys(data[n=1]=f820e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x28c37, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x28c37 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8875088
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d55f, OrigWordsRequested 0x7000, DevSize 0x70
IdeReadWrite (REQ): Starting sector is 3d55f, Number of WORDS 0x7000, DevSize 0x70
AtapiDmaSetup: mode 0x45, data f81b2000, count e000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f81b2000)
  get Phys(data[n=1]=f81b3000)
  get Phys(data[n=1]=f81b4000)
  get Phys(data[n=2]=f81b5000)
  get Phys(data[n=3]=f81b6000)
  get Phys(data[n=4]=f81b7000)
  get Phys(data[n=4]=f81b8000)
  get Phys(data[n=5]=f81b9000)
  get Phys(data[n=6]=f81ba000)
  get Phys(data[n=6]=f81bb000)
  get Phys(data[n=7]=f81bc000)
  get Phys(data[n=7]=f81bd000)
  get Phys(data[n=8]=f81be000)
  get Phys(data[n=9]=f81bf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d55f, Count 0x70(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d55f count 0x70 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e000, full size e000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf887541c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d55f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3d55f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f820d000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f820d000)
  get Phys(data[n=1]=f820e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d55f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d55f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\sysaudio.sys at F8259000 with 9 pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874ed0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3baaf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3baaf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f81b2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f81b2000)
  get Phys(data[n=1]=f81b3000)
  get Phys(data[n=2]=f81b4000)
  get Phys(data[n=3]=f81b5000)
  get Phys(data[n=4]=f81b6000)
  get Phys(data[n=5]=f81b7000)
  get Phys(data[n=6]=f81b8000)
  get Phys(data[n=7]=f81b9000)
  get Phys(data[n=8]=f81ba000)
  get Phys(data[n=9]=f81bb000)
  get Phys(data[n=9]=f81bc000)
  get Phys(data[n=10]=f81bd000)
  get Phys(data[n=10]=f81be000)
  get Phys(data[n=11]=f81bf000)
  get Phys(data[n=12]=f81c0000)
  get Phys(data[n=13]=f81c1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3baaf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3baaf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874ed0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3bb2f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3bb2f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f81c2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f81c2000)
  get Phys(data[n=1]=f81c3000)
  get Phys(data[n=2]=f81c4000)
  get Phys(data[n=3]=f81c5000)
  get Phys(data[n=3]=f81c6000)
  get Phys(data[n=4]=f81c7000)
  get Phys(data[n=5]=f81c8000)
  get Phys(data[n=6]=f81c9000)
  get Phys(data[n=7]=f81ca000)
  get Phys(data[n=8]=f81cb000)
  get Phys(data[n=9]=f81cc000)
  get Phys(data[n=10]=f81cd000)
  get Phys(data[n=10]=f81ce000)
  get Phys(data[n=11]=f81cf000)
  get Phys(data[n=12]=f81d0000)
  get Phys(data[n=13]=f81d1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3bb2f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3bb2f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874ed0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3bbaf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3bbaf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f81d2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f81d2000)
  get Phys(data[n=1]=f81d3000)
  get Phys(data[n=2]=f81d4000)
  get Phys(data[n=3]=f81d5000)
  get Phys(data[n=4]=f81d6000)
  get Phys(data[n=5]=f81d7000)
  get Phys(data[n=5]=f81d8000)
  get Phys(data[n=5]=f81d9000)
  get Phys(data[n=6]=f81da000)
  get Phys(data[n=7]=f81db000)
  get Phys(data[n=7]=f81dc000)
  get Phys(data[n=8]=f81dd000)
  get Phys(data[n=8]=f81de000)
  get Phys(data[n=9]=f81df000)
  get Phys(data[n=10]=f81e0000)
  get Phys(data[n=11]=f81e1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3bbaf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3bbaf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874ed0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3bc2f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3bc2f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f81e2000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f81e2000)
  get Phys(data[n=1]=f81e3000)
  get Phys(data[n=2]=f81e4000)
  get Phys(data[n=3]=f81e5000)
  get Phys(data[n=4]=f81e6000)
  get Phys(data[n=5]=f81e7000)
  get Phys(data[n=6]=f81e8000)
  get Phys(data[n=6]=f81e9000)
  get Phys(data[n=7]=f81ea000)
  get Phys(data[n=8]=f81eb000)
  get Phys(data[n=9]=f81ec000)
  get Phys(data[n=9]=f81ed000)
  get Phys(data[n=10]=f81ee000)
  get Phys(data[n=11]=f81ef000)
  get Phys(data[n=11]=f81f0000)
  get Phys(data[n=12]=f81f1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3bc2f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3bc2f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88752cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3baaf, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3baaf, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f820d000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f820d000)
  get Phys(data[n=1]=f820e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3baaf, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3baaf count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\ks.sys at F81CF000 with 23 pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88749c0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3bcaf, OrigWordsRequested 0x600, DevSize 0x6
IdeReadWrite (REQ): Starting sector is 3bcaf, Number of WORDS 0x600, DevSize 0x6
AtapiDmaSetup: mode 0x45, data f816a000, count c00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f816a000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3bcaf, Count 0x6(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3bcaf count 0x6 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered c00, full size c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf887498c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3c837, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3c837, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f818f000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f818f000)
  get Phys(data[n=1]=f8190000)
  get Phys(data[n=2]=f8191000)
  get Phys(data[n=2]=f8192000)
  get Phys(data[n=3]=f8193000)
  get Phys(data[n=4]=f8194000)
  get Phys(data[n=5]=f8195000)
  get Phys(data[n=6]=f8196000)
  get Phys(data[n=7]=f8197000)
  get Phys(data[n=8]=f8198000)
  get Phys(data[n=9]=f8199000)
  get Phys(data[n=9]=f819a000)
  get Phys(data[n=10]=f819b000)
  get Phys(data[n=11]=f819c000)
  get Phys(data[n=12]=f819d000)
  get Phys(data[n=13]=f819e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3c837, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3c837 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf887498c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3c8b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3c8b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f819f000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f819f000)
  get Phys(data[n=1]=f81a0000)
  get Phys(data[n=2]=f81a1000)
  get Phys(data[n=2]=f81a2000)
  get Phys(data[n=3]=f81a3000)
  get Phys(data[n=4]=f81a4000)
  get Phys(data[n=5]=f81a5000)
  get Phys(data[n=5]=f81a6000)
  get Phys(data[n=6]=f81a7000)
  get Phys(data[n=7]=f81a8000)
  get Phys(data[n=8]=f81a9000)
  get Phys(data[n=9]=f81aa000)
  get Phys(data[n=10]=f81ab000)
  get Phys(data[n=10]=f81ac000)
  get Phys(data[n=11]=f81ad000)
  get Phys(data[n=12]=f81ae000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3c8b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3c8b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf887498c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3c937, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3c937, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f81af000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f81af000)
  get Phys(data[n=1]=f81b0000)
  get Phys(data[n=2]=f81b1000)
  get Phys(data[n=2]=f81b2000)
  get Phys(data[n=3]=f81b3000)
  get Phys(data[n=4]=f81b4000)
  get Phys(data[n=5]=f81b5000)
  get Phys(data[n=5]=f81b6000)
  get Phys(data[n=6]=f81b7000)
  get Phys(data[n=7]=f81b8000)
  get Phys(data[n=8]=f81b9000)
  get Phys(data[n=9]=f81ba000)
  get Phys(data[n=10]=f81bb000)
  get Phys(data[n=11]=f81bc000)
  get Phys(data[n=11]=f81bd000)
  get Phys(data[n=12]=f81be000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3c937, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3c937 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf887498c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3c9b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3c9b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f81bf000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f81bf000)
  get Phys(data[n=1]=f81c0000)
  get Phys(data[n=1]=f81c1000)
  get Phys(data[n=2]=f81c2000)
  get Phys(data[n=3]=f81c3000)
  get Phys(data[n=3]=f81c4000)
  get Phys(data[n=4]=f81c5000)
  get Phys(data[n=4]=f81c6000)
  get Phys(data[n=5]=f81c7000)
  get Phys(data[n=6]=f81c8000)
  get Phys(data[n=6]=f81c9000)
  get Phys(data[n=7]=f81ca000)
  get Phys(data[n=8]=f81cb000)
  get Phys(data[n=9]=f81cc000)
  get Phys(data[n=10]=f81cd000)
  get Phys(data[n=11]=f81ce000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3c9b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3c9b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874d88
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3c837, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3c837, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f820d000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f820d000)
  get Phys(data[n=1]=f820e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3c837, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3c837 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\kmixer.sys at F805F000 with 170 pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ca37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3ca37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85694000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85694000)
  get Phys(data[n=1]=85695000)
  get Phys(data[n=2]=85696000)
  get Phys(data[n=2]=85697000)
  get Phys(data[n=3]=85698000)
  get Phys(data[n=3]=85699000)
  get Phys(data[n=4]=8569a000)
  get Phys(data[n=5]=8569b000)
  get Phys(data[n=5]=8569c000)
  get Phys(data[n=6]=8569d000)
  get Phys(data[n=7]=8569e000)
  get Phys(data[n=8]=8569f000)
  get Phys(data[n=9]=856a0000)
  get Phys(data[n=10]=856a1000)
  get Phys(data[n=11]=856a2000)
  get Phys(data[n=11]=856a3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ca37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3ca37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3cab7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3cab7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 856a4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856a4000)
  get Phys(data[n=1]=856a5000)
  get Phys(data[n=2]=856a6000)
  get Phys(data[n=3]=856a7000)
  get Phys(data[n=4]=856a8000)
  get Phys(data[n=5]=856a9000)
  get Phys(data[n=6]=856aa000)
  get Phys(data[n=7]=856ab000)
  get Phys(data[n=8]=856ac000)
  get Phys(data[n=8]=856ad000)
  get Phys(data[n=9]=856ae000)
  get Phys(data[n=10]=856af000)
  get Phys(data[n=11]=856b0000)
  get Phys(data[n=12]=856b1000)
  get Phys(data[n=13]=856b2000)
  get Phys(data[n=14]=856b3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3cab7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3cab7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3cb37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3cb37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 856b4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856b4000)
  get Phys(data[n=1]=856b5000)
  get Phys(data[n=2]=856b6000)
  get Phys(data[n=3]=856b7000)
  get Phys(data[n=4]=856b8000)
  get Phys(data[n=4]=856b9000)
  get Phys(data[n=5]=856ba000)
  get Phys(data[n=6]=856bb000)
  get Phys(data[n=7]=856bc000)
  get Phys(data[n=8]=856bd000)
  get Phys(data[n=9]=856be000)
  get Phys(data[n=9]=856bf000)
  get Phys(data[n=10]=856c0000)
  get Phys(data[n=11]=856c1000)
  get Phys(data[n=12]=856c2000)
  get Phys(data[n=12]=856c3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3cb37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3cb37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3cbb7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3cbb7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 856c4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856c4000)
  get Phys(data[n=1]=856c5000)
  get Phys(data[n=2]=856c6000)
  get Phys(data[n=3]=856c7000)
  get Phys(data[n=4]=856c8000)
  get Phys(data[n=4]=856c9000)
  get Phys(data[n=5]=856ca000)
  get Phys(data[n=6]=856cb000)
  get Phys(data[n=7]=856cc000)
  get Phys(data[n=8]=856cd000)
  get Phys(data[n=9]=856ce000)
  get Phys(data[n=10]=856cf000)
  get Phys(data[n=10]=856d0000)
  get Phys(data[n=11]=856d1000)
  get Phys(data[n=12]=856d2000)
  get Phys(data[n=13]=856d3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3cbb7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3cbb7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3cc37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3cc37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 856d4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856d4000)
  get Phys(data[n=1]=856d5000)
  get Phys(data[n=2]=856d6000)
  get Phys(data[n=2]=856d7000)
  get Phys(data[n=3]=856d8000)
  get Phys(data[n=3]=856d9000)
  get Phys(data[n=4]=856da000)
  get Phys(data[n=5]=856db000)
  get Phys(data[n=5]=856dc000)
  get Phys(data[n=6]=856dd000)
  get Phys(data[n=7]=856de000)
  get Phys(data[n=8]=856df000)
  get Phys(data[n=9]=856e0000)
  get Phys(data[n=10]=856e1000)
  get Phys(data[n=11]=856e2000)
  get Phys(data[n=11]=856e3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3cc37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3cc37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ccb7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3ccb7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 856e4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856e4000)
  get Phys(data[n=1]=856e5000)
  get Phys(data[n=2]=856e6000)
  get Phys(data[n=3]=856e7000)
  get Phys(data[n=4]=856e8000)
  get Phys(data[n=5]=856e9000)
  get Phys(data[n=6]=856ea000)
  get Phys(data[n=7]=856eb000)
  get Phys(data[n=8]=856ec000)
  get Phys(data[n=8]=856ed000)
  get Phys(data[n=9]=856ee000)
  get Phys(data[n=10]=856ef000)
  get Phys(data[n=11]=856f0000)
  get Phys(data[n=12]=856f1000)
  get Phys(data[n=13]=856f2000)
  get Phys(data[n=14]=856f3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ccb7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3ccb7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3cd37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3cd37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 856f4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856f4000)
  get Phys(data[n=1]=856f5000)
  get Phys(data[n=2]=856f6000)
  get Phys(data[n=3]=856f7000)
  get Phys(data[n=4]=856f8000)
  get Phys(data[n=4]=856f9000)
  get Phys(data[n=5]=856fa000)
  get Phys(data[n=6]=856fb000)
  get Phys(data[n=7]=856fc000)
  get Phys(data[n=8]=856fd000)
  get Phys(data[n=9]=856fe000)
  get Phys(data[n=9]=856ff000)
  get Phys(data[n=10]=85700000)
  get Phys(data[n=11]=85701000)
  get Phys(data[n=12]=85702000)
  get Phys(data[n=12]=85703000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3cd37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3cd37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3cdb7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3cdb7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85704000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85704000)
  get Phys(data[n=1]=85705000)
  get Phys(data[n=2]=85706000)
  get Phys(data[n=3]=85707000)
  get Phys(data[n=4]=85708000)
  get Phys(data[n=4]=85709000)
  get Phys(data[n=5]=8570a000)
  get Phys(data[n=6]=8570b000)
  get Phys(data[n=7]=8570c000)
  get Phys(data[n=8]=8570d000)
  get Phys(data[n=9]=8570e000)
  get Phys(data[n=10]=8570f000)
  get Phys(data[n=10]=85710000)
  get Phys(data[n=11]=85711000)
  get Phys(data[n=12]=85712000)
  get Phys(data[n=13]=85713000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3cdb7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3cdb7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ce37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3ce37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85714000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85714000)
  get Phys(data[n=1]=85715000)
  get Phys(data[n=2]=85716000)
  get Phys(data[n=2]=85717000)
  get Phys(data[n=3]=85718000)
  get Phys(data[n=3]=85719000)
  get Phys(data[n=4]=8571a000)
  get Phys(data[n=5]=8571b000)
  get Phys(data[n=5]=8571c000)
  get Phys(data[n=6]=8571d000)
  get Phys(data[n=7]=8571e000)
  get Phys(data[n=8]=8571f000)
  get Phys(data[n=9]=85720000)
  get Phys(data[n=10]=85721000)
  get Phys(data[n=11]=85722000)
  get Phys(data[n=11]=85723000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ce37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3ce37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3ceb7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3ceb7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85724000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85724000)
  get Phys(data[n=1]=85725000)
  get Phys(data[n=2]=85726000)
  get Phys(data[n=3]=85727000)
  get Phys(data[n=4]=85728000)
  get Phys(data[n=5]=85729000)
  get Phys(data[n=6]=8572a000)
  get Phys(data[n=7]=8572b000)
  get Phys(data[n=8]=8572c000)
  get Phys(data[n=8]=8572d000)
  get Phys(data[n=9]=8572e000)
  get Phys(data[n=10]=8572f000)
  get Phys(data[n=11]=85730000)
  get Phys(data[n=12]=85731000)
  get Phys(data[n=13]=85732000)
  get Phys(data[n=14]=85733000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3ceb7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3ceb7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3cf37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3cf37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85734000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85734000)
  get Phys(data[n=1]=85735000)
  get Phys(data[n=2]=85736000)
  get Phys(data[n=3]=85737000)
  get Phys(data[n=4]=85738000)
  get Phys(data[n=4]=85739000)
  get Phys(data[n=5]=8573a000)
  get Phys(data[n=6]=8573b000)
  get Phys(data[n=7]=8573c000)
  get Phys(data[n=8]=8573d000)
  get Phys(data[n=9]=8573e000)
  get Phys(data[n=9]=8573f000)
  get Phys(data[n=10]=85740000)
  get Phys(data[n=11]=85741000)
  get Phys(data[n=12]=85742000)
  get Phys(data[n=12]=85743000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3cf37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3cf37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3cfb7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3cfb7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85744000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85744000)
  get Phys(data[n=1]=85745000)
  get Phys(data[n=2]=85746000)
  get Phys(data[n=3]=85747000)
  get Phys(data[n=4]=85748000)
  get Phys(data[n=4]=85749000)
  get Phys(data[n=5]=8574a000)
  get Phys(data[n=6]=8574b000)
  get Phys(data[n=7]=8574c000)
  get Phys(data[n=8]=8574d000)
  get Phys(data[n=9]=8574e000)
  get Phys(data[n=10]=8574f000)
  get Phys(data[n=10]=85750000)
  get Phys(data[n=11]=85751000)
  get Phys(data[n=12]=85752000)
  get Phys(data[n=13]=85753000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3cfb7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3cfb7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d037, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3d037, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85754000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85754000)
  get Phys(data[n=1]=85755000)
  get Phys(data[n=2]=85756000)
  get Phys(data[n=2]=85757000)
  get Phys(data[n=3]=85758000)
  get Phys(data[n=3]=85759000)
  get Phys(data[n=4]=8575a000)
  get Phys(data[n=5]=8575b000)
  get Phys(data[n=5]=8575c000)
  get Phys(data[n=6]=8575d000)
  get Phys(data[n=7]=8575e000)
  get Phys(data[n=8]=8575f000)
  get Phys(data[n=9]=85760000)
  get Phys(data[n=10]=85761000)
  get Phys(data[n=11]=85762000)
  get Phys(data[n=11]=85763000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d037, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d037 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d0b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3d0b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85764000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85764000)
  get Phys(data[n=1]=85765000)
  get Phys(data[n=2]=85766000)
  get Phys(data[n=3]=85767000)
  get Phys(data[n=4]=85768000)
  get Phys(data[n=5]=85769000)
  get Phys(data[n=6]=8576a000)
  get Phys(data[n=7]=8576b000)
  get Phys(data[n=8]=8576c000)
  get Phys(data[n=8]=8576d000)
  get Phys(data[n=9]=8576e000)
  get Phys(data[n=10]=8576f000)
  get Phys(data[n=11]=85770000)
  get Phys(data[n=12]=85771000)
  get Phys(data[n=13]=85772000)
  get Phys(data[n=14]=85773000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d0b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d0b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d137, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3d137, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85774000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85774000)
  get Phys(data[n=1]=85775000)
  get Phys(data[n=2]=85776000)
  get Phys(data[n=3]=85777000)
  get Phys(data[n=4]=85778000)
  get Phys(data[n=4]=85779000)
  get Phys(data[n=5]=8577a000)
  get Phys(data[n=6]=8577b000)
  get Phys(data[n=7]=8577c000)
  get Phys(data[n=8]=8577d000)
  get Phys(data[n=9]=8577e000)
  get Phys(data[n=9]=8577f000)
  get Phys(data[n=10]=85780000)
  get Phys(data[n=11]=85781000)
  get Phys(data[n=12]=85782000)
  get Phys(data[n=12]=85783000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d137, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d137 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d1b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3d1b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85784000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85784000)
  get Phys(data[n=1]=85785000)
  get Phys(data[n=2]=85786000)
  get Phys(data[n=3]=85787000)
  get Phys(data[n=4]=85788000)
  get Phys(data[n=4]=85789000)
  get Phys(data[n=5]=8578a000)
  get Phys(data[n=6]=8578b000)
  get Phys(data[n=7]=8578c000)
  get Phys(data[n=8]=8578d000)
  get Phys(data[n=9]=8578e000)
  get Phys(data[n=10]=8578f000)
  get Phys(data[n=10]=85790000)
  get Phys(data[n=11]=85791000)
  get Phys(data[n=12]=85792000)
  get Phys(data[n=13]=85793000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d1b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d1b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d237, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3d237, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85794000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85794000)
  get Phys(data[n=1]=85795000)
  get Phys(data[n=2]=85796000)
  get Phys(data[n=2]=85797000)
  get Phys(data[n=3]=85798000)
  get Phys(data[n=3]=85799000)
  get Phys(data[n=4]=8579a000)
  get Phys(data[n=5]=8579b000)
  get Phys(data[n=5]=8579c000)
  get Phys(data[n=6]=8579d000)
  get Phys(data[n=7]=8579e000)
  get Phys(data[n=8]=8579f000)
  get Phys(data[n=9]=857a0000)
  get Phys(data[n=10]=857a1000)
  get Phys(data[n=11]=857a2000)
  get Phys(data[n=11]=857a3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d237, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d237 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d2b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3d2b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 857a4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=857a4000)
  get Phys(data[n=1]=857a5000)
  get Phys(data[n=2]=857a6000)
  get Phys(data[n=3]=857a7000)
  get Phys(data[n=4]=857a8000)
  get Phys(data[n=5]=857a9000)
  get Phys(data[n=6]=857aa000)
  get Phys(data[n=7]=857ab000)
  get Phys(data[n=8]=857ac000)
  get Phys(data[n=8]=857ad000)
  get Phys(data[n=9]=857ae000)
  get Phys(data[n=10]=857af000)
  get Phys(data[n=11]=857b0000)
  get Phys(data[n=12]=857b1000)
  get Phys(data[n=13]=857b2000)
  get Phys(data[n=14]=857b3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d2b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d2b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/ex/work.c:351) EX: Work Queue Deadlock detected: 1
(../../ntoskrnl/ex/work.c:353) Dynamic threads queued 1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d337, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3d337, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 857b4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=857b4000)
  get Phys(data[n=1]=857b5000)
  get Phys(data[n=2]=857b6000)
  get Phys(data[n=3]=857b7000)
  get Phys(data[n=4]=857b8000)
  get Phys(data[n=4]=857b9000)
  get Phys(data[n=5]=857ba000)
  get Phys(data[n=6]=857bb000)
  get Phys(data[n=7]=857bc000)
  get Phys(data[n=8]=857bd000)
  get Phys(data[n=9]=857be000)
  get Phys(data[n=9]=857bf000)
  get Phys(data[n=10]=857c0000)
  get Phys(data[n=11]=857c1000)
  get Phys(data[n=12]=857c2000)
  get Phys(data[n=12]=857c3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d337, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d337 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8874da8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d3b7, OrigWordsRequested 0x4800, DevSize 0x48
IdeReadWrite (REQ): Starting sector is 3d3b7, Number of WORDS 0x4800, DevSize 0x48
AtapiDmaSetup: mode 0x45, data 857c4000, count 9000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=857c4000)
  get Phys(data[n=1]=857c5000)
  get Phys(data[n=2]=857c6000)
  get Phys(data[n=3]=857c7000)
  get Phys(data[n=4]=857c8000)
  get Phys(data[n=4]=857c9000)
  get Phys(data[n=5]=857ca000)
  get Phys(data[n=6]=857cb000)
  get Phys(data[n=7]=857cc000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d3b7, Count 0x48(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d3b7 count 0x48 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 9000, full size 9000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../drivers/wdm/audio/filters/kmixer/kmixer.c:99) KMixer.sys loaded
(../../drivers/wdm/audio/filters/kmixer/kmixer.c:48) KMix_InstallDevice called
(../../drivers/wdm/audio/filters/kmixer/kmixer.c:83) KMix_InstallDevice result 0
(../../drivers/wdm/audio/filters/kmixer/filter.c:104) DispatchCreateKMix entered
(../../drivers/wdm/audio/filters/kmixer/filter.c:163) KsAllocateObjectHeader result 0
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38f37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 38f37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f800f000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f800f000)
  get Phys(data[n=1]=f8010000)
  get Phys(data[n=2]=f8011000)
  get Phys(data[n=3]=f8012000)
  get Phys(data[n=4]=f8013000)
  get Phys(data[n=4]=f8014000)
  get Phys(data[n=5]=f8015000)
  get Phys(data[n=6]=f8016000)
  get Phys(data[n=7]=f8017000)
  get Phys(data[n=7]=f8018000)
  get Phys(data[n=8]=f8019000)
  get Phys(data[n=8]=f801a000)
  get Phys(data[n=9]=f801b000)
  get Phys(data[n=10]=f801c000)
  get Phys(data[n=11]=f801d000)
  get Phys(data[n=11]=f801e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38f37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38f37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38fb7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 38fb7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f801f000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f801f000)
  get Phys(data[n=1]=f8020000)
  get Phys(data[n=2]=f8021000)
  get Phys(data[n=3]=f8022000)
  get Phys(data[n=4]=f8023000)
  get Phys(data[n=5]=f8024000)
  get Phys(data[n=5]=f8025000)
  get Phys(data[n=6]=f8026000)
  get Phys(data[n=7]=f8027000)
  get Phys(data[n=8]=f8028000)
  get Phys(data[n=8]=f8029000)
  get Phys(data[n=8]=f802a000)
  get Phys(data[n=8]=f802b000)
  get Phys(data[n=8]=f802c000)
  get Phys(data[n=9]=f802d000)
  get Phys(data[n=9]=f802e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38fb7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38fb7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 39037, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 39037, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f802f000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f802f000)
  get Phys(data[n=1]=f8030000)
  get Phys(data[n=1]=f8031000)
  get Phys(data[n=2]=f8032000)
  get Phys(data[n=3]=f8033000)
  get Phys(data[n=4]=f8034000)
  get Phys(data[n=5]=f8035000)
  get Phys(data[n=6]=f8036000)
  get Phys(data[n=7]=f8037000)
  get Phys(data[n=8]=f8038000)
  get Phys(data[n=9]=f8039000)
  get Phys(data[n=9]=f803a000)
  get Phys(data[n=9]=f803b000)
  get Phys(data[n=10]=f803c000)
  get Phys(data[n=11]=f803d000)
  get Phys(data[n=12]=f803e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x39037, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x39037 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 390b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 390b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f803f000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f803f000)
  get Phys(data[n=1]=f8040000)
  get Phys(data[n=2]=f8041000)
  get Phys(data[n=2]=f8042000)
  get Phys(data[n=3]=f8043000)
  get Phys(data[n=4]=f8044000)
  get Phys(data[n=5]=f8045000)
  get Phys(data[n=6]=f8046000)
  get Phys(data[n=7]=f8047000)
  get Phys(data[n=8]=f8048000)
  get Phys(data[n=9]=f8049000)
  get Phys(data[n=10]=f804a000)
  get Phys(data[n=11]=f804b000)
  get Phys(data[n=12]=f804c000)
  get Phys(data[n=13]=f804d000)
  get Phys(data[n=13]=f804e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x390b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x390b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38f37, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 38f37, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8252000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8252000)
  get Phys(data[n=1]=f8253000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38f37, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38f37 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x500, DevSize 0x5
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x500, DevSize 0x5
AtapiDmaSetup: mode 0x45, data 856d4000, count a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856d4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x5(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d289f count 0x5 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a00, full size a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c58c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 856d4000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856d4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d289f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8875020
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d3ff, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3d3ff, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f800f000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f800f000)
  get Phys(data[n=1]=f8010000)
  get Phys(data[n=2]=f8011000)
  get Phys(data[n=2]=f8012000)
  get Phys(data[n=3]=f8013000)
  get Phys(data[n=4]=f8014000)
  get Phys(data[n=5]=f8015000)
  get Phys(data[n=6]=f8016000)
  get Phys(data[n=7]=f8017000)
  get Phys(data[n=7]=f8018000)
  get Phys(data[n=8]=f8019000)
  get Phys(data[n=9]=f801a000)
  get Phys(data[n=10]=f801b000)
  get Phys(data[n=11]=f801c000)
  get Phys(data[n=12]=f801d000)
  get Phys(data[n=13]=f801e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d3ff, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d3ff count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8875020
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d47f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 3d47f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f801f000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f801f000)
  get Phys(data[n=1]=f8020000)
  get Phys(data[n=2]=f8021000)
  get Phys(data[n=3]=f8022000)
  get Phys(data[n=3]=f8023000)
  get Phys(data[n=3]=f8024000)
  get Phys(data[n=3]=f8025000)
  get Phys(data[n=3]=f8026000)
  get Phys(data[n=4]=f8027000)
  get Phys(data[n=4]=f8028000)
  get Phys(data[n=5]=f8029000)
  get Phys(data[n=6]=f802a000)
  get Phys(data[n=6]=f802b000)
  get Phys(data[n=7]=f802c000)
  get Phys(data[n=8]=f802d000)
  get Phys(data[n=9]=f802e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d47f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d47f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8875020
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d4ff, OrigWordsRequested 0x6000, DevSize 0x60
IdeReadWrite (REQ): Starting sector is 3d4ff, Number of WORDS 0x6000, DevSize 0x60
AtapiDmaSetup: mode 0x45, data f802f000, count c000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f802f000)
  get Phys(data[n=1]=f8030000)
  get Phys(data[n=2]=f8031000)
  get Phys(data[n=3]=f8032000)
  get Phys(data[n=4]=f8033000)
  get Phys(data[n=4]=f8034000)
  get Phys(data[n=4]=f8035000)
  get Phys(data[n=5]=f8036000)
  get Phys(data[n=6]=f8037000)
  get Phys(data[n=7]=f8038000)
  get Phys(data[n=8]=f8039000)
  get Phys(data[n=9]=f803a000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d4ff, Count 0x60(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d4ff count 0x60 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered c000, full size c000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf887541c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 3d3ff, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 3d3ff, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8253000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8253000)
  get Phys(data[n=1]=f8254000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x3d3ff, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x3d3ff count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../ntoskrnl/mm/ARM3/sysldr.c:174) Loading: \SystemRoot\system32\drivers\wdmaud.sys at F8038000 with 17 pages
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x500, DevSize 0x5
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x500, DevSize 0x5
AtapiDmaSetup: mode 0x45, data 856d4000, count a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856d4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x5(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d289f count 0x5 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a00, full size a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 39937, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 39937, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85694000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85694000)
  get Phys(data[n=1]=85695000)
  get Phys(data[n=2]=85696000)
  get Phys(data[n=3]=85697000)
  get Phys(data[n=3]=85698000)
  get Phys(data[n=4]=85699000)
  get Phys(data[n=5]=8569a000)
  get Phys(data[n=6]=8569b000)
  get Phys(data[n=7]=8569c000)
  get Phys(data[n=8]=8569d000)
  get Phys(data[n=8]=8569e000)
  get Phys(data[n=9]=8569f000)
  get Phys(data[n=10]=856a0000)
  get Phys(data[n=11]=856a1000)
  get Phys(data[n=12]=856a2000)
  get Phys(data[n=13]=856a3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x39937, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x39937 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 399b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 399b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 856a4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856a4000)
  get Phys(data[n=1]=856a5000)
  get Phys(data[n=2]=856a6000)
  get Phys(data[n=3]=856a7000)
  get Phys(data[n=4]=856a8000)
  get Phys(data[n=4]=856a9000)
  get Phys(data[n=4]=856aa000)
  get Phys(data[n=4]=856ab000)
  get Phys(data[n=4]=856ac000)
  get Phys(data[n=5]=856ad000)
  get Phys(data[n=5]=856ae000)
  get Phys(data[n=6]=856af000)
  get Phys(data[n=7]=856b0000)
  get Phys(data[n=7]=856b1000)
  get Phys(data[n=8]=856b2000)
  get Phys(data[n=9]=856b3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x399b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x399b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c58c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 856d4000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856d4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d289f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x500, DevSize 0x5
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x500, DevSize 0x5
AtapiDmaSetup: mode 0x45, data 856d4000, count a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856d4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x5(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d289f count 0x5 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a00, full size a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 39a37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 39a37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 856b4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856b4000)
  get Phys(data[n=1]=856b5000)
  get Phys(data[n=2]=856b6000)
  get Phys(data[n=3]=856b7000)
  get Phys(data[n=4]=856b8000)
  get Phys(data[n=5]=856b9000)
  get Phys(data[n=5]=856ba000)
  get Phys(data[n=5]=856bb000)
  get Phys(data[n=6]=856bc000)
  get Phys(data[n=7]=856bd000)
  get Phys(data[n=8]=856be000)
  get Phys(data[n=9]=856bf000)
  get Phys(data[n=10]=856c0000)
  get Phys(data[n=11]=856c1000)
  get Phys(data[n=11]=856c2000)
  get Phys(data[n=12]=856c3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x39a37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x39a37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 39ab7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 39ab7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 856c4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856c4000)
  get Phys(data[n=1]=856c5000)
  get Phys(data[n=2]=856c6000)
  get Phys(data[n=3]=856c7000)
  get Phys(data[n=4]=856c8000)
  get Phys(data[n=5]=856c9000)
  get Phys(data[n=6]=856ca000)
  get Phys(data[n=7]=856cb000)
  get Phys(data[n=8]=856cc000)
  get Phys(data[n=9]=856cd000)
  get Phys(data[n=9]=856ce000)
  get Phys(data[n=10]=856cf000)
  get Phys(data[n=10]=856d0000)
  get Phys(data[n=11]=856d1000)
  get Phys(data[n=12]=856d2000)
  get Phys(data[n=13]=856d3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x39ab7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x39ab7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c58c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 856d4000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856d4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d289f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1b99f, OrigWordsRequested 0x3600, DevSize 0x36
IdeReadWrite (REQ): Starting sector is 1b99f, Number of WORDS 0x3600, DevSize 0x36
AtapiDmaSetup: mode 0x45, data f7ff8000, count 6c00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=2]=f7ffa000)
  get Phys(data[n=3]=f7ffb000)
  get Phys(data[n=3]=f7ffc000)
  get Phys(data[n=3]=f7ffd000)
  get Phys(data[n=4]=f7ffe000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1b99f, Count 0x36(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1b99f count 0x36 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 6c00, full size 6c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1b99f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 1b99f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f8253000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8253000)
  get Phys(data[n=1]=f8254000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1b99f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1b99f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 12aaf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 12aaf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85654000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85654000)
  get Phys(data[n=1]=85655000)
  get Phys(data[n=2]=85656000)
  get Phys(data[n=2]=85657000)
  get Phys(data[n=3]=85658000)
  get Phys(data[n=4]=85659000)
  get Phys(data[n=4]=8565a000)
  get Phys(data[n=5]=8565b000)
  get Phys(data[n=6]=8565c000)
  get Phys(data[n=7]=8565d000)
  get Phys(data[n=8]=8565e000)
  get Phys(data[n=8]=8565f000)
  get Phys(data[n=9]=85660000)
  get Phys(data[n=10]=85661000)
  get Phys(data[n=11]=85662000)
  get Phys(data[n=12]=85663000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x12aaf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x12aaf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 12b2f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 12b2f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85664000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85664000)
  get Phys(data[n=1]=85665000)
  get Phys(data[n=2]=85666000)
  get Phys(data[n=3]=85667000)
  get Phys(data[n=4]=85668000)
  get Phys(data[n=5]=85669000)
  get Phys(data[n=6]=8566a000)
  get Phys(data[n=6]=8566b000)
  get Phys(data[n=7]=8566c000)
  get Phys(data[n=7]=8566d000)
  get Phys(data[n=8]=8566e000)
  get Phys(data[n=9]=8566f000)
  get Phys(data[n=10]=85670000)
  get Phys(data[n=10]=85671000)
  get Phys(data[n=11]=85672000)
  get Phys(data[n=12]=85673000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x12b2f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x12b2f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 12baf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 12baf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85674000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85674000)
  get Phys(data[n=1]=85675000)
  get Phys(data[n=2]=85676000)
  get Phys(data[n=3]=85677000)
  get Phys(data[n=4]=85678000)
  get Phys(data[n=5]=85679000)
  get Phys(data[n=6]=8567a000)
  get Phys(data[n=7]=8567b000)
  get Phys(data[n=8]=8567c000)
  get Phys(data[n=9]=8567d000)
  get Phys(data[n=10]=8567e000)
  get Phys(data[n=11]=8567f000)
  get Phys(data[n=12]=85680000)
  get Phys(data[n=13]=85681000)
  get Phys(data[n=14]=85682000)
  get Phys(data[n=15]=85683000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x12baf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x12baf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 12c2f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 12c2f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85684000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85684000)
  get Phys(data[n=1]=85685000)
  get Phys(data[n=2]=85686000)
  get Phys(data[n=2]=85687000)
  get Phys(data[n=3]=85688000)
  get Phys(data[n=3]=85689000)
  get Phys(data[n=4]=8568a000)
  get Phys(data[n=4]=8568b000)
  get Phys(data[n=5]=8568c000)
  get Phys(data[n=6]=8568d000)
  get Phys(data[n=7]=8568e000)
  get Phys(data[n=8]=8568f000)
  get Phys(data[n=9]=85690000)
  get Phys(data[n=10]=85691000)
  get Phys(data[n=11]=85692000)
  get Phys(data[n=12]=85693000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x12c2f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x12c2f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../base/services/umpnpmgr/umpnpmgr.c:2828) Installing: PCI\VEN_80EE&DEV_CAFE&SUBSYS_00000000&REV_00\3&609b8881&04
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88657f8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 403f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 403f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 80c40000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80c40000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x403f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x403f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf81fe338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 149e7, OrigWordsRequested 0x4d00, DevSize 0x4d
IdeReadWrite (REQ): Starting sector is 149e7, Number of WORDS 0x4d00, DevSize 0x4d
AtapiDmaSetup: mode 0x45, data f7fb0000, count 9a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7fb0000)
  get Phys(data[n=1]=f7fb1000)
  get Phys(data[n=1]=f7fb2000)
  get Phys(data[n=2]=f7fb3000)
  get Phys(data[n=2]=f7fb4000)
  get Phys(data[n=3]=f7fb5000)
  get Phys(data[n=4]=f7fb6000)
  get Phys(data[n=5]=f7fb7000)
  get Phys(data[n=6]=f7fb8000)
  get Phys(data[n=7]=f7fb9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x149e7, Count 0x4d(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x149e7 count 0x4d feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 9a00, full size 9a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf81fe6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 149e7, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 149e7, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f82ac000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ac000)
  get Phys(data[n=1]=f82ad000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x149e7, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x149e7 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf829d2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38f37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 38f37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f7ff8000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=2]=f7ffa000)
  get Phys(data[n=3]=f7ffb000)
  get Phys(data[n=4]=f7ffc000)
  get Phys(data[n=4]=f7ffd000)
  get Phys(data[n=5]=f7ffe000)
  get Phys(data[n=6]=f7fff000)
  get Phys(data[n=7]=f8000000)
  get Phys(data[n=8]=f8001000)
  get Phys(data[n=9]=f8002000)
  get Phys(data[n=10]=f8003000)
  get Phys(data[n=11]=f8004000)
  get Phys(data[n=12]=f8005000)
  get Phys(data[n=13]=f8006000)
  get Phys(data[n=14]=f8007000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38f37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38f37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf829d2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38fb7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 38fb7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8008000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8008000)
  get Phys(data[n=1]=f8009000)
  get Phys(data[n=2]=f800a000)
  get Phys(data[n=3]=f800b000)
  get Phys(data[n=4]=f800c000)
  get Phys(data[n=5]=f800d000)
  get Phys(data[n=6]=f800e000)
  get Phys(data[n=6]=f800f000)
  get Phys(data[n=7]=f8010000)
  get Phys(data[n=7]=f8011000)
  get Phys(data[n=8]=f8012000)
  get Phys(data[n=8]=f8013000)
  get Phys(data[n=9]=f8014000)
  get Phys(data[n=10]=f8015000)
  get Phys(data[n=11]=f8016000)
  get Phys(data[n=12]=f8017000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38fb7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38fb7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x500, DevSize 0x5
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x500, DevSize 0x5
AtapiDmaSetup: mode 0x45, data 85714000, count a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85714000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x5(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d289f count 0x5 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a00, full size a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c58c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85714000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85714000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d289f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf829d2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 39037, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 39037, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8018000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8018000)
  get Phys(data[n=1]=f8019000)
  get Phys(data[n=2]=f801a000)
  get Phys(data[n=3]=f801b000)
  get Phys(data[n=4]=f801c000)
  get Phys(data[n=5]=f801d000)
  get Phys(data[n=6]=f801e000)
  get Phys(data[n=6]=f801f000)
  get Phys(data[n=7]=f8020000)
  get Phys(data[n=8]=f8021000)
  get Phys(data[n=9]=f8022000)
  get Phys(data[n=10]=f8023000)
  get Phys(data[n=11]=f8024000)
  get Phys(data[n=12]=f8025000)
  get Phys(data[n=13]=f8026000)
  get Phys(data[n=13]=f8027000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x39037, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x39037 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf829d2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 390b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 390b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8028000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8028000)
  get Phys(data[n=1]=f8029000)
  get Phys(data[n=2]=f802a000)
  get Phys(data[n=3]=f802b000)
  get Phys(data[n=4]=f802c000)
  get Phys(data[n=5]=f802d000)
  get Phys(data[n=6]=f802e000)
  get Phys(data[n=7]=f802f000)
  get Phys(data[n=8]=f8030000)
  get Phys(data[n=9]=f8031000)
  get Phys(data[n=10]=f8032000)
  get Phys(data[n=10]=f8033000)
  get Phys(data[n=11]=f8034000)
  get Phys(data[n=11]=f8035000)
  get Phys(data[n=12]=f8036000)
  get Phys(data[n=13]=f8037000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x390b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x390b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x500, DevSize 0x5
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x500, DevSize 0x5
AtapiDmaSetup: mode 0x45, data 85714000, count a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85714000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x5(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d289f count 0x5 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a00, full size a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c58c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85714000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85714000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d289f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf829d6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 38f37, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 38f37, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f82ac000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f82ac000)
  get Phys(data[n=1]=f82ad000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x38f37, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x38f37 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c604
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x500, DevSize 0x5
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x500, DevSize 0x5
AtapiDmaSetup: mode 0x45, data 85754000, count a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85754000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x5(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d289f count 0x5 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a00, full size a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 12eaf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 12eaf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 856d4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856d4000)
  get Phys(data[n=1]=856d5000)
  get Phys(data[n=2]=856d6000)
  get Phys(data[n=3]=856d7000)
  get Phys(data[n=4]=856d8000)
  get Phys(data[n=5]=856d9000)
  get Phys(data[n=6]=856da000)
  get Phys(data[n=7]=856db000)
  get Phys(data[n=8]=856dc000)
  get Phys(data[n=9]=856dd000)
  get Phys(data[n=10]=856de000)
  get Phys(data[n=11]=856df000)
  get Phys(data[n=12]=856e0000)
  get Phys(data[n=13]=856e1000)
  get Phys(data[n=14]=856e2000)
  get Phys(data[n=15]=856e3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x12eaf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x12eaf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 12f2f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 12f2f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 856e4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856e4000)
  get Phys(data[n=1]=856e5000)
  get Phys(data[n=2]=856e6000)
  get Phys(data[n=2]=856e7000)
  get Phys(data[n=3]=856e8000)
  get Phys(data[n=3]=856e9000)
  get Phys(data[n=4]=856ea000)
  get Phys(data[n=4]=856eb000)
  get Phys(data[n=5]=856ec000)
  get Phys(data[n=6]=856ed000)
  get Phys(data[n=7]=856ee000)
  get Phys(data[n=8]=856ef000)
  get Phys(data[n=9]=856f0000)
  get Phys(data[n=10]=856f1000)
  get Phys(data[n=11]=856f2000)
  get Phys(data[n=12]=856f3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x12f2f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x12f2f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf820c58c
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d289f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d289f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85754000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85754000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d289f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d289f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 12faf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 12faf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 856f4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856f4000)
  get Phys(data[n=1]=856f5000)
  get Phys(data[n=2]=856f6000)
  get Phys(data[n=2]=856f7000)
  get Phys(data[n=3]=856f8000)
  get Phys(data[n=4]=856f9000)
  get Phys(data[n=5]=856fa000)
  get Phys(data[n=6]=856fb000)
  get Phys(data[n=7]=856fc000)
  get Phys(data[n=8]=856fd000)
  get Phys(data[n=9]=856fe000)
  get Phys(data[n=9]=856ff000)
  get Phys(data[n=10]=85700000)
  get Phys(data[n=11]=85701000)
  get Phys(data[n=12]=85702000)
  get Phys(data[n=13]=85703000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x12faf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x12faf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1302f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1302f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85704000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85704000)
  get Phys(data[n=1]=85705000)
  get Phys(data[n=2]=85706000)
  get Phys(data[n=3]=85707000)
  get Phys(data[n=4]=85708000)
  get Phys(data[n=5]=85709000)
  get Phys(data[n=6]=8570a000)
  get Phys(data[n=6]=8570b000)
  get Phys(data[n=7]=8570c000)
  get Phys(data[n=7]=8570d000)
  get Phys(data[n=8]=8570e000)
  get Phys(data[n=9]=8570f000)
  get Phys(data[n=10]=85710000)
  get Phys(data[n=10]=85711000)
  get Phys(data[n=11]=85712000)
  get Phys(data[n=12]=85713000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1302f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1302f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2b8a7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2b8a7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f7ff8000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=2]=f7ffa000)
  get Phys(data[n=3]=f7ffb000)
  get Phys(data[n=4]=f7ffc000)
  get Phys(data[n=5]=f7ffd000)
  get Phys(data[n=6]=f7ffe000)
  get Phys(data[n=7]=f7fff000)
  get Phys(data[n=7]=f8000000)
  get Phys(data[n=8]=f8001000)
  get Phys(data[n=9]=f8002000)
  get Phys(data[n=9]=f8003000)
  get Phys(data[n=10]=f8004000)
  get Phys(data[n=11]=f8005000)
  get Phys(data[n=12]=f8006000)
  get Phys(data[n=13]=f8007000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2b8a7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2b8a7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2b927, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2b927, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8008000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8008000)
  get Phys(data[n=1]=f8009000)
  get Phys(data[n=2]=f800a000)
  get Phys(data[n=3]=f800b000)
  get Phys(data[n=4]=f800c000)
  get Phys(data[n=5]=f800d000)
  get Phys(data[n=5]=f800e000)
  get Phys(data[n=5]=f800f000)
  get Phys(data[n=6]=f8010000)
  get Phys(data[n=7]=f8011000)
  get Phys(data[n=8]=f8012000)
  get Phys(data[n=9]=f8013000)
  get Phys(data[n=10]=f8014000)
  get Phys(data[n=11]=f8015000)
  get Phys(data[n=12]=f8016000)
  get Phys(data[n=12]=f8017000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2b927, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2b927 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2b9a7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2b9a7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8018000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8018000)
  get Phys(data[n=1]=f8019000)
  get Phys(data[n=2]=f801a000)
  get Phys(data[n=3]=f801b000)
  get Phys(data[n=4]=f801c000)
  get Phys(data[n=5]=f801d000)
  get Phys(data[n=6]=f801e000)
  get Phys(data[n=7]=f801f000)
  get Phys(data[n=8]=f8020000)
  get Phys(data[n=9]=f8021000)
  get Phys(data[n=10]=f8022000)
  get Phys(data[n=10]=f8023000)
  get Phys(data[n=11]=f8024000)
  get Phys(data[n=11]=f8025000)
  get Phys(data[n=12]=f8026000)
  get Phys(data[n=13]=f8027000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2b9a7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2b9a7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2ba27, OrigWordsRequested 0x2c00, DevSize 0x2c
IdeReadWrite (REQ): Starting sector is 2ba27, Number of WORDS 0x2c00, DevSize 0x2c
AtapiDmaSetup: mode 0x45, data f8028000, count 5800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8028000)
  get Phys(data[n=1]=f8029000)
  get Phys(data[n=2]=f802a000)
  get Phys(data[n=3]=f802b000)
  get Phys(data[n=4]=f802c000)
  get Phys(data[n=5]=f802d000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2ba27, Count 0x2c(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2ba27 count 0x2c feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 5800, full size 5800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2b8a7, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 2b8a7, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f820d000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f820d000)
  get Phys(data[n=1]=f820e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2b8a7, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2b8a7 count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 12caf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 12caf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85754000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85754000)
  get Phys(data[n=1]=85755000)
  get Phys(data[n=1]=85756000)
  get Phys(data[n=2]=85757000)
  get Phys(data[n=3]=85758000)
  get Phys(data[n=4]=85759000)
  get Phys(data[n=5]=8575a000)
  get Phys(data[n=6]=8575b000)
  get Phys(data[n=7]=8575c000)
  get Phys(data[n=8]=8575d000)
  get Phys(data[n=9]=8575e000)
  get Phys(data[n=10]=8575f000)
  get Phys(data[n=11]=85760000)
  get Phys(data[n=12]=85761000)
  get Phys(data[n=12]=85762000)
  get Phys(data[n=13]=85763000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x12caf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x12caf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 12d2f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 12d2f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85764000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85764000)
  get Phys(data[n=1]=85765000)
  get Phys(data[n=2]=85766000)
  get Phys(data[n=3]=85767000)
  get Phys(data[n=3]=85768000)
  get Phys(data[n=4]=85769000)
  get Phys(data[n=5]=8576a000)
  get Phys(data[n=6]=8576b000)
  get Phys(data[n=7]=8576c000)
  get Phys(data[n=8]=8576d000)
  get Phys(data[n=9]=8576e000)
  get Phys(data[n=9]=8576f000)
  get Phys(data[n=10]=85770000)
  get Phys(data[n=11]=85771000)
  get Phys(data[n=12]=85772000)
  get Phys(data[n=13]=85773000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x12d2f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x12d2f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 12daf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 12daf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85774000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85774000)
  get Phys(data[n=1]=85775000)
  get Phys(data[n=2]=85776000)
  get Phys(data[n=3]=85777000)
  get Phys(data[n=4]=85778000)
  get Phys(data[n=5]=85779000)
  get Phys(data[n=6]=8577a000)
  get Phys(data[n=7]=8577b000)
  get Phys(data[n=8]=8577c000)
  get Phys(data[n=9]=8577d000)
  get Phys(data[n=10]=8577e000)
  get Phys(data[n=10]=8577f000)
  get Phys(data[n=11]=85780000)
  get Phys(data[n=12]=85781000)
  get Phys(data[n=12]=85782000)
  get Phys(data[n=13]=85783000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x12daf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x12daf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 12e2f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 12e2f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85784000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85784000)
  get Phys(data[n=1]=85785000)
  get Phys(data[n=2]=85786000)
  get Phys(data[n=3]=85787000)
  get Phys(data[n=4]=85788000)
  get Phys(data[n=5]=85789000)
  get Phys(data[n=6]=8578a000)
  get Phys(data[n=7]=8578b000)
  get Phys(data[n=8]=8578c000)
  get Phys(data[n=8]=8578d000)
  get Phys(data[n=8]=8578e000)
  get Phys(data[n=9]=8578f000)
  get Phys(data[n=10]=85790000)
  get Phys(data[n=11]=85791000)
  get Phys(data[n=12]=85792000)
  get Phys(data[n=13]=85793000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x12e2f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x12e2f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf829d6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 39937, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 39937, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85714000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85714000)
  get Phys(data[n=1]=85715000)
  get Phys(data[n=2]=85716000)
  get Phys(data[n=3]=85717000)
  get Phys(data[n=4]=85718000)
  get Phys(data[n=5]=85719000)
  get Phys(data[n=6]=8571a000)
  get Phys(data[n=7]=8571b000)
  get Phys(data[n=8]=8571c000)
  get Phys(data[n=8]=8571d000)
  get Phys(data[n=9]=8571e000)
  get Phys(data[n=10]=8571f000)
  get Phys(data[n=10]=85720000)
  get Phys(data[n=11]=85721000)
  get Phys(data[n=12]=85722000)
  get Phys(data[n=13]=85723000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x39937, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x39937 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf829d6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 399b7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 399b7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85724000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85724000)
  get Phys(data[n=1]=85725000)
  get Phys(data[n=2]=85726000)
  get Phys(data[n=3]=85727000)
  get Phys(data[n=4]=85728000)
  get Phys(data[n=5]=85729000)
  get Phys(data[n=6]=8572a000)
  get Phys(data[n=6]=8572b000)
  get Phys(data[n=6]=8572c000)
  get Phys(data[n=7]=8572d000)
  get Phys(data[n=8]=8572e000)
  get Phys(data[n=9]=8572f000)
  get Phys(data[n=10]=85730000)
  get Phys(data[n=11]=85731000)
  get Phys(data[n=12]=85732000)
  get Phys(data[n=13]=85733000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x399b7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x399b7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf829d6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 39a37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 39a37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85734000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85734000)
  get Phys(data[n=1]=85735000)
  get Phys(data[n=2]=85736000)
  get Phys(data[n=3]=85737000)
  get Phys(data[n=4]=85738000)
  get Phys(data[n=5]=85739000)
  get Phys(data[n=6]=8573a000)
  get Phys(data[n=7]=8573b000)
  get Phys(data[n=8]=8573c000)
  get Phys(data[n=9]=8573d000)
  get Phys(data[n=10]=8573e000)
  get Phys(data[n=11]=8573f000)
  get Phys(data[n=11]=85740000)
  get Phys(data[n=12]=85741000)
  get Phys(data[n=12]=85742000)
  get Phys(data[n=13]=85743000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x39a37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x39a37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf829d6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 39ab7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 39ab7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85744000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85744000)
  get Phys(data[n=1]=85745000)
  get Phys(data[n=1]=85746000)
  get Phys(data[n=2]=85747000)
  get Phys(data[n=3]=85748000)
  get Phys(data[n=4]=85749000)
  get Phys(data[n=5]=8574a000)
  get Phys(data[n=6]=8574b000)
  get Phys(data[n=7]=8574c000)
  get Phys(data[n=7]=8574d000)
  get Phys(data[n=8]=8574e000)
  get Phys(data[n=9]=8574f000)
  get Phys(data[n=10]=85750000)
  get Phys(data[n=11]=85751000)
  get Phys(data[n=12]=85752000)
  get Phys(data[n=13]=85753000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x39ab7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x39ab7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf829d338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1b99f, OrigWordsRequested 0x3600, DevSize 0x36
IdeReadWrite (REQ): Starting sector is 1b99f, Number of WORDS 0x3600, DevSize 0x36
AtapiDmaSetup: mode 0x45, data f7ff8000, count 6c00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=2]=f7ffa000)
  get Phys(data[n=3]=f7ffb000)
  get Phys(data[n=4]=f7ffc000)
  get Phys(data[n=5]=f7ffd000)
  get Phys(data[n=6]=f7ffe000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1b99f, Count 0x36(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1b99f count 0x36 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 6c00, full size 6c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf829d6cc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1b99f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 1b99f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f820d000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f820d000)
  get Phys(data[n=1]=f820e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1b99f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1b99f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 136af, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 136af, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 857d4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=857d4000)
  get Phys(data[n=1]=857d5000)
  get Phys(data[n=2]=857d6000)
  get Phys(data[n=3]=857d7000)
  get Phys(data[n=4]=857d8000)
  get Phys(data[n=5]=857d9000)
  get Phys(data[n=6]=857da000)
  get Phys(data[n=7]=857db000)
  get Phys(data[n=8]=857dc000)
  get Phys(data[n=9]=857dd000)
  get Phys(data[n=10]=857de000)
  get Phys(data[n=11]=857df000)
  get Phys(data[n=12]=857e0000)
  get Phys(data[n=13]=857e1000)
  get Phys(data[n=14]=857e2000)
  get Phys(data[n=15]=857e3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x136af, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x136af count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1372f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1372f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 857e4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=857e4000)
  get Phys(data[n=1]=857e5000)
  get Phys(data[n=2]=857e6000)
  get Phys(data[n=3]=857e7000)
  get Phys(data[n=4]=857e8000)
  get Phys(data[n=4]=857e9000)
  get Phys(data[n=5]=857ea000)
  get Phys(data[n=6]=857eb000)
  get Phys(data[n=6]=857ec000)
  get Phys(data[n=7]=857ed000)
  get Phys(data[n=8]=857ee000)
  get Phys(data[n=9]=857ef000)
  get Phys(data[n=10]=857f0000)
  get Phys(data[n=11]=857f1000)
  get Phys(data[n=12]=857f2000)
  get Phys(data[n=13]=857f3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1372f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1372f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 137af, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 137af, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 857f4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=857f4000)
  get Phys(data[n=1]=857f5000)
  get Phys(data[n=2]=857f6000)
  get Phys(data[n=2]=857f7000)
  get Phys(data[n=2]=857f8000)
  get Phys(data[n=3]=857f9000)
  get Phys(data[n=4]=857fa000)
  get Phys(data[n=5]=857fb000)
  get Phys(data[n=6]=857fc000)
  get Phys(data[n=7]=857fd000)
  get Phys(data[n=8]=857fe000)
  get Phys(data[n=9]=857ff000)
  get Phys(data[n=9]=85800000)
  get Phys(data[n=10]=85801000)
  get Phys(data[n=11]=85802000)
  get Phys(data[n=12]=85803000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x137af, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x137af count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1382f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1382f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85804000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85804000)
  get Phys(data[n=1]=85805000)
  get Phys(data[n=2]=85806000)
  get Phys(data[n=2]=85807000)
  get Phys(data[n=3]=85808000)
  get Phys(data[n=4]=85809000)
  get Phys(data[n=5]=8580a000)
  get Phys(data[n=5]=8580b000)
  get Phys(data[n=6]=8580c000)
  get Phys(data[n=6]=8580d000)
  get Phys(data[n=7]=8580e000)
  get Phys(data[n=8]=8580f000)
  get Phys(data[n=9]=85810000)
  get Phys(data[n=9]=85811000)
  get Phys(data[n=10]=85812000)
  get Phys(data[n=11]=85813000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1382f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1382f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad324
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4087, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 4087, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85714000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85714000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4087, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4087 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 86c7, OrigWordsRequested 0x7100, DevSize 0x71
IdeReadWrite (REQ): Starting sector is 86c7, Number of WORDS 0x7100, DevSize 0x71
AtapiDmaSetup: mode 0x45, data f7ff8000, count e200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=2]=f7ffa000)
  get Phys(data[n=3]=f7ffb000)
  get Phys(data[n=4]=f7ffc000)
  get Phys(data[n=5]=f7ffd000)
  get Phys(data[n=6]=f7ffe000)
  get Phys(data[n=7]=f7fff000)
  get Phys(data[n=8]=f8000000)
  get Phys(data[n=9]=f8001000)
  get Phys(data[n=10]=f8002000)
  get Phys(data[n=11]=f8003000)
  get Phys(data[n=12]=f8004000)
  get Phys(data[n=13]=f8005000)
  get Phys(data[n=14]=f8006000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x86c7, Count 0x71(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x86c7 count 0x71 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e200, full size e200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41297, OrigWordsRequested 0x900, DevSize 0x9
IdeReadWrite (REQ): Starting sector is 41297, Number of WORDS 0x900, DevSize 0x9
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41297, Count 0x9(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41297 count 0x9 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1200, full size 1200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 412a7, OrigWordsRequested 0x900, DevSize 0x9
IdeReadWrite (REQ): Starting sector is 412a7, Number of WORDS 0x900, DevSize 0x9
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x412a7, Count 0x9(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x412a7 count 0x9 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1200, full size 1200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 412b7, OrigWordsRequested 0x900, DevSize 0x9
IdeReadWrite (REQ): Starting sector is 412b7, Number of WORDS 0x900, DevSize 0x9
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x412b7, Count 0x9(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x412b7 count 0x9 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1200, full size 1200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 412c7, OrigWordsRequested 0x2700, DevSize 0x27
IdeReadWrite (REQ): Starting sector is 412c7, Number of WORDS 0x2700, DevSize 0x27
AtapiDmaSetup: mode 0x45, data f7ff8000, count 4e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=2]=f7ffa000)
  get Phys(data[n=3]=f7ffb000)
  get Phys(data[n=4]=f7ffc000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x412c7, Count 0x27(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x412c7 count 0x27 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 4e00, full size 4e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 412ef, OrigWordsRequested 0x600, DevSize 0x6
IdeReadWrite (REQ): Starting sector is 412ef, Number of WORDS 0x600, DevSize 0x6
AtapiDmaSetup: mode 0x45, data f7ff8000, count c00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x412ef, Count 0x6(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x412ef count 0x6 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered c00, full size c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 412f7, OrigWordsRequested 0x900, DevSize 0x9
IdeReadWrite (REQ): Starting sector is 412f7, Number of WORDS 0x900, DevSize 0x9
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x412f7, Count 0x9(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x412f7 count 0x9 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1200, full size 1200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41307, OrigWordsRequested 0x3f00, DevSize 0x3f
IdeReadWrite (REQ): Starting sector is 41307, Number of WORDS 0x3f00, DevSize 0x3f
AtapiDmaSetup: mode 0x45, data f7ff8000, count 7e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=2]=f7ffa000)
  get Phys(data[n=3]=f7ffb000)
  get Phys(data[n=4]=f7ffc000)
  get Phys(data[n=5]=f7ffd000)
  get Phys(data[n=6]=f7ffe000)
  get Phys(data[n=7]=f7fff000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41307, Count 0x3f(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41307 count 0x3f feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 7e00, full size 7e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41347, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 41347, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f7ff8000, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41347, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41347 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4134f, OrigWordsRequested 0x900, DevSize 0x9
IdeReadWrite (REQ): Starting sector is 4134f, Number of WORDS 0x900, DevSize 0x9
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4134f, Count 0x9(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4134f count 0x9 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1200, full size 1200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4135f, OrigWordsRequested 0xf00, DevSize 0xf
IdeReadWrite (REQ): Starting sector is 4135f, Number of WORDS 0xf00, DevSize 0xf
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4135f, Count 0xf(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4135f count 0xf feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1e00, full size 1e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4136f, OrigWordsRequested 0xf00, DevSize 0xf
IdeReadWrite (REQ): Starting sector is 4136f, Number of WORDS 0xf00, DevSize 0xf
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4136f, Count 0xf(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4136f count 0xf feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1e00, full size 1e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4137f, OrigWordsRequested 0x1500, DevSize 0x15
IdeReadWrite (REQ): Starting sector is 4137f, Number of WORDS 0x1500, DevSize 0x15
AtapiDmaSetup: mode 0x45, data f7ff8000, count 2a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=2]=f7ffa000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4137f, Count 0x15(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4137f count 0x15 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2a00, full size 2a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41397, OrigWordsRequested 0x700, DevSize 0x7
IdeReadWrite (REQ): Starting sector is 41397, Number of WORDS 0x700, DevSize 0x7
AtapiDmaSetup: mode 0x45, data f7ff8000, count e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41397, Count 0x7(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41397 count 0x7 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e00, full size e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4139f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4139f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f7ff8000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=2]=f7ffa000)
  get Phys(data[n=3]=f7ffb000)
  get Phys(data[n=4]=f7ffc000)
  get Phys(data[n=5]=f7ffd000)
  get Phys(data[n=6]=f7ffe000)
  get Phys(data[n=7]=f7fff000)
  get Phys(data[n=8]=f8000000)
  get Phys(data[n=9]=f8001000)
  get Phys(data[n=10]=f8002000)
  get Phys(data[n=11]=f8003000)
  get Phys(data[n=11]=f8004000)
  get Phys(data[n=12]=f8005000)
  get Phys(data[n=12]=f8006000)
  get Phys(data[n=13]=f8007000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4139f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4139f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4141f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4141f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8008000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8008000)
  get Phys(data[n=1]=f8009000)
  get Phys(data[n=2]=f800a000)
  get Phys(data[n=3]=f800b000)
  get Phys(data[n=4]=f800c000)
  get Phys(data[n=5]=f800d000)
  get Phys(data[n=6]=f800e000)
  get Phys(data[n=7]=f800f000)
  get Phys(data[n=8]=f8010000)
  get Phys(data[n=9]=f8011000)
  get Phys(data[n=10]=f8012000)
  get Phys(data[n=11]=f8013000)
  get Phys(data[n=11]=f8014000)
  get Phys(data[n=11]=f8015000)
  get Phys(data[n=12]=f8016000)
  get Phys(data[n=13]=f8017000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4141f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4141f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4149f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4149f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8018000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8018000)
  get Phys(data[n=1]=f8019000)
  get Phys(data[n=2]=f801a000)
  get Phys(data[n=3]=f801b000)
  get Phys(data[n=4]=f801c000)
  get Phys(data[n=4]=f801d000)
  get Phys(data[n=5]=f801e000)
  get Phys(data[n=6]=f801f000)
  get Phys(data[n=7]=f8020000)
  get Phys(data[n=8]=f8021000)
  get Phys(data[n=9]=f8022000)
  get Phys(data[n=10]=f8023000)
  get Phys(data[n=11]=f8024000)
  get Phys(data[n=11]=f8025000)
  get Phys(data[n=12]=f8026000)
  get Phys(data[n=13]=f8027000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4149f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4149f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4151f, OrigWordsRequested 0x5900, DevSize 0x59
IdeReadWrite (REQ): Starting sector is 4151f, Number of WORDS 0x5900, DevSize 0x59
AtapiDmaSetup: mode 0x45, data f8028000, count b200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8028000)
  get Phys(data[n=1]=f8029000)
  get Phys(data[n=2]=f802a000)
  get Phys(data[n=2]=f802b000)
  get Phys(data[n=3]=f802c000)
  get Phys(data[n=3]=f802d000)
  get Phys(data[n=4]=f802e000)
  get Phys(data[n=4]=f802f000)
  get Phys(data[n=5]=f8030000)
  get Phys(data[n=6]=f8031000)
  get Phys(data[n=7]=f8032000)
  get Phys(data[n=8]=f8033000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4151f, Count 0x59(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4151f count 0x59 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered b200, full size b200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 134af, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 134af, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85694000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85694000)
  get Phys(data[n=1]=85695000)
  get Phys(data[n=2]=85696000)
  get Phys(data[n=3]=85697000)
  get Phys(data[n=4]=85698000)
  get Phys(data[n=4]=85699000)
  get Phys(data[n=4]=8569a000)
  get Phys(data[n=5]=8569b000)
  get Phys(data[n=6]=8569c000)
  get Phys(data[n=7]=8569d000)
  get Phys(data[n=8]=8569e000)
  get Phys(data[n=9]=8569f000)
  get Phys(data[n=10]=856a0000)
  get Phys(data[n=11]=856a1000)
  get Phys(data[n=12]=856a2000)
  get Phys(data[n=13]=856a3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x134af, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x134af count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1352f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1352f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 856a4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856a4000)
  get Phys(data[n=1]=856a5000)
  get Phys(data[n=2]=856a6000)
  get Phys(data[n=3]=856a7000)
  get Phys(data[n=3]=856a8000)
  get Phys(data[n=4]=856a9000)
  get Phys(data[n=4]=856aa000)
  get Phys(data[n=5]=856ab000)
  get Phys(data[n=6]=856ac000)
  get Phys(data[n=6]=856ad000)
  get Phys(data[n=7]=856ae000)
  get Phys(data[n=8]=856af000)
  get Phys(data[n=9]=856b0000)
  get Phys(data[n=10]=856b1000)
  get Phys(data[n=11]=856b2000)
  get Phys(data[n=12]=856b3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1352f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1352f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 135af, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 135af, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 856b4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856b4000)
  get Phys(data[n=1]=856b5000)
  get Phys(data[n=2]=856b6000)
  get Phys(data[n=3]=856b7000)
  get Phys(data[n=3]=856b8000)
  get Phys(data[n=3]=856b9000)
  get Phys(data[n=3]=856ba000)
  get Phys(data[n=4]=856bb000)
  get Phys(data[n=5]=856bc000)
  get Phys(data[n=6]=856bd000)
  get Phys(data[n=7]=856be000)
  get Phys(data[n=8]=856bf000)
  get Phys(data[n=9]=856c0000)
  get Phys(data[n=9]=856c1000)
  get Phys(data[n=10]=856c2000)
  get Phys(data[n=11]=856c3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x135af, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x135af count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1362f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1362f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 856c4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=856c4000)
  get Phys(data[n=1]=856c5000)
  get Phys(data[n=2]=856c6000)
  get Phys(data[n=3]=856c7000)
  get Phys(data[n=4]=856c8000)
  get Phys(data[n=4]=856c9000)
  get Phys(data[n=5]=856ca000)
  get Phys(data[n=6]=856cb000)
  get Phys(data[n=7]=856cc000)
  get Phys(data[n=7]=856cd000)
  get Phys(data[n=8]=856ce000)
  get Phys(data[n=8]=856cf000)
  get Phys(data[n=9]=856d0000)
  get Phys(data[n=10]=856d1000)
  get Phys(data[n=11]=856d2000)
  get Phys(data[n=11]=856d3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1362f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1362f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4157f, OrigWordsRequested 0xd00, DevSize 0xd
IdeReadWrite (REQ): Starting sector is 4157f, Number of WORDS 0xd00, DevSize 0xd
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4157f, Count 0xd(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4157f count 0xd feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1a00, full size 1a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4158f, OrigWordsRequested 0x2800, DevSize 0x28
IdeReadWrite (REQ): Starting sector is 4158f, Number of WORDS 0x2800, DevSize 0x28
AtapiDmaSetup: mode 0x45, data f7ff8000, count 5000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=1]=f7ffa000)
  get Phys(data[n=2]=f7ffb000)
  get Phys(data[n=3]=f7ffc000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4158f, Count 0x28(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4158f count 0x28 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 5000, full size 5000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 415b7, OrigWordsRequested 0x1300, DevSize 0x13
IdeReadWrite (REQ): Starting sector is 415b7, Number of WORDS 0x1300, DevSize 0x13
AtapiDmaSetup: mode 0x45, data f7ff8000, count 2600, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=1]=f7ffa000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x415b7, Count 0x13(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x415b7 count 0x13 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2600, full size 2600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 415cf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 415cf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f7ff8000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=1]=f7ffa000)
  get Phys(data[n=2]=f7ffb000)
  get Phys(data[n=3]=f7ffc000)
  get Phys(data[n=4]=f7ffd000)
  get Phys(data[n=5]=f7ffe000)
  get Phys(data[n=6]=f7fff000)
  get Phys(data[n=7]=f8000000)
  get Phys(data[n=8]=f8001000)
  get Phys(data[n=8]=f8002000)
  get Phys(data[n=9]=f8003000)
  get Phys(data[n=10]=f8004000)
  get Phys(data[n=11]=f8005000)
  get Phys(data[n=12]=f8006000)
  get Phys(data[n=13]=f8007000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x415cf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x415cf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4164f, OrigWordsRequested 0x7300, DevSize 0x73
IdeReadWrite (REQ): Starting sector is 4164f, Number of WORDS 0x7300, DevSize 0x73
AtapiDmaSetup: mode 0x45, data f8008000, count e600, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8008000)
  get Phys(data[n=1]=f8009000)
  get Phys(data[n=1]=f800a000)
  get Phys(data[n=2]=f800b000)
  get Phys(data[n=3]=f800c000)
  get Phys(data[n=4]=f800d000)
  get Phys(data[n=4]=f800e000)
  get Phys(data[n=5]=f800f000)
  get Phys(data[n=5]=f8010000)
  get Phys(data[n=6]=f8011000)
  get Phys(data[n=7]=f8012000)
  get Phys(data[n=8]=f8013000)
  get Phys(data[n=8]=f8014000)
  get Phys(data[n=9]=f8015000)
  get Phys(data[n=10]=f8016000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4164f, Count 0x73(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4164f count 0x73 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e600, full size e600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 416c7, OrigWordsRequested 0x7a00, DevSize 0x7a
IdeReadWrite (REQ): Starting sector is 416c7, Number of WORDS 0x7a00, DevSize 0x7a
AtapiDmaSetup: mode 0x45, data f7ff8000, count f400, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=1]=f7ffa000)
  get Phys(data[n=2]=f7ffb000)
  get Phys(data[n=3]=f7ffc000)
  get Phys(data[n=4]=f7ffd000)
  get Phys(data[n=5]=f7ffe000)
  get Phys(data[n=6]=f7fff000)
  get Phys(data[n=7]=f8000000)
  get Phys(data[n=8]=f8001000)
  get Phys(data[n=8]=f8002000)
  get Phys(data[n=9]=f8003000)
  get Phys(data[n=10]=f8004000)
  get Phys(data[n=11]=f8005000)
  get Phys(data[n=12]=f8006000)
  get Phys(data[n=13]=f8007000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x416c7, Count 0x7a(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x416c7 count 0x7a feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered f400, full size f400
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41747, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 41747, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f7ff8000, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41747, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41747 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4174f, OrigWordsRequested 0x300, DevSize 0x3
IdeReadWrite (REQ): Starting sector is 4174f, Number of WORDS 0x300, DevSize 0x3
AtapiDmaSetup: mode 0x45, data f7ff8000, count 600, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4174f, Count 0x3(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4174f count 0x3 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 600, full size 600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41757, OrigWordsRequested 0x7200, DevSize 0x72
IdeReadWrite (REQ): Starting sector is 41757, Number of WORDS 0x7200, DevSize 0x72
AtapiDmaSetup: mode 0x45, data f7ff8000, count e400, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=1]=f7ffa000)
  get Phys(data[n=2]=f7ffb000)
  get Phys(data[n=3]=f7ffc000)
  get Phys(data[n=4]=f7ffd000)
  get Phys(data[n=5]=f7ffe000)
  get Phys(data[n=6]=f7fff000)
  get Phys(data[n=7]=f8000000)
  get Phys(data[n=8]=f8001000)
  get Phys(data[n=8]=f8002000)
  get Phys(data[n=9]=f8003000)
  get Phys(data[n=10]=f8004000)
  get Phys(data[n=11]=f8005000)
  get Phys(data[n=12]=f8006000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41757, Count 0x72(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41757 count 0x72 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e400, full size e400
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 417cf, OrigWordsRequested 0x700, DevSize 0x7
IdeReadWrite (REQ): Starting sector is 417cf, Number of WORDS 0x700, DevSize 0x7
AtapiDmaSetup: mode 0x45, data f7ff8000, count e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x417cf, Count 0x7(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x417cf count 0x7 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e00, full size e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 417d7, OrigWordsRequested 0x2e00, DevSize 0x2e
IdeReadWrite (REQ): Starting sector is 417d7, Number of WORDS 0x2e00, DevSize 0x2e
AtapiDmaSetup: mode 0x45, data f7ff8000, count 5c00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=1]=f7ffa000)
  get Phys(data[n=2]=f7ffb000)
  get Phys(data[n=3]=f7ffc000)
  get Phys(data[n=4]=f7ffd000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x417d7, Count 0x2e(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x417d7 count 0x2e feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 5c00, full size 5c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41807, OrigWordsRequested 0x700, DevSize 0x7
IdeReadWrite (REQ): Starting sector is 41807, Number of WORDS 0x700, DevSize 0x7
AtapiDmaSetup: mode 0x45, data f7ff8000, count e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41807, Count 0x7(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41807 count 0x7 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e00, full size e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4180f, OrigWordsRequested 0x600, DevSize 0x6
IdeReadWrite (REQ): Starting sector is 4180f, Number of WORDS 0x600, DevSize 0x6
AtapiDmaSetup: mode 0x45, data f7ff8000, count c00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4180f, Count 0x6(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4180f count 0x6 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered c00, full size c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41817, OrigWordsRequested 0xb00, DevSize 0xb
IdeReadWrite (REQ): Starting sector is 41817, Number of WORDS 0xb00, DevSize 0xb
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1600, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41817, Count 0xb(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41817 count 0xb feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1600, full size 1600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41827, OrigWordsRequested 0x600, DevSize 0x6
IdeReadWrite (REQ): Starting sector is 41827, Number of WORDS 0x600, DevSize 0x6
AtapiDmaSetup: mode 0x45, data f7ff8000, count c00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41827, Count 0x6(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41827 count 0x6 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered c00, full size c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4182f, OrigWordsRequested 0x1100, DevSize 0x11
IdeReadWrite (REQ): Starting sector is 4182f, Number of WORDS 0x1100, DevSize 0x11
AtapiDmaSetup: mode 0x45, data f7ff8000, count 2200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=1]=f7ffa000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4182f, Count 0x11(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4182f count 0x11 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2200, full size 2200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41847, OrigWordsRequested 0x1800, DevSize 0x18
IdeReadWrite (REQ): Starting sector is 41847, Number of WORDS 0x1800, DevSize 0x18
AtapiDmaSetup: mode 0x45, data f7ff8000, count 3000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=1]=f7ffa000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41847, Count 0x18(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41847 count 0x18 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 3000, full size 3000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 132af, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 132af, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85854000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85854000)
  get Phys(data[n=1]=85855000)
  get Phys(data[n=1]=85856000)
  get Phys(data[n=2]=85857000)
  get Phys(data[n=3]=85858000)
  get Phys(data[n=4]=85859000)
  get Phys(data[n=5]=8585a000)
  get Phys(data[n=6]=8585b000)
  get Phys(data[n=7]=8585c000)
  get Phys(data[n=8]=8585d000)
  get Phys(data[n=8]=8585e000)
  get Phys(data[n=9]=8585f000)
  get Phys(data[n=10]=85860000)
  get Phys(data[n=11]=85861000)
  get Phys(data[n=12]=85862000)
  get Phys(data[n=13]=85863000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x132af, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x132af count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0f31f68, CDB 0xb0f31f98, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=1
Non-empty queue
Try IDE prepare
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1299018
** --- **
** Ide: Command continue prep
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1332f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1332f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85864000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85864000)
  get Phys(data[n=1]=85865000)
  get Phys(data[n=1]=85866000)
  get Phys(data[n=2]=85867000)
  get Phys(data[n=3]=85868000)
  get Phys(data[n=4]=85869000)
  get Phys(data[n=4]=8586a000)
  get Phys(data[n=5]=8586b000)
  get Phys(data[n=5]=8586c000)
  get Phys(data[n=6]=8586d000)
  get Phys(data[n=7]=8586e000)
  get Phys(data[n=8]=8586f000)
  get Phys(data[n=8]=85870000)
  get Phys(data[n=9]=85871000)
  get Phys(data[n=10]=85872000)
  get Phys(data[n=11]=85873000)
  set TERM
AtapiDmaSetup: OK
IdeSendCommand: SRB_STATUS_PENDING
AtapiStartIo: Already have 2 request(s)!
AtapiStartIo: next Srb b0f31f68
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a632e0, CDB 0xb0a63310, AtaReq 0xb129a030, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=2
Non-empty queue
Try IDE prepare
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb129a030
** --- **
** Ide: Command continue prep
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 133af, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 133af, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85874000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129a088)
  get Phys(data[0]=85874000)
  get Phys(data[n=1]=85875000)
  get Phys(data[n=1]=85876000)
  get Phys(data[n=1]=85877000)
  get Phys(data[n=2]=85878000)
  get Phys(data[n=3]=85879000)
  get Phys(data[n=4]=8587a000)
  get Phys(data[n=5]=8587b000)
  get Phys(data[n=6]=8587c000)
  get Phys(data[n=6]=8587d000)
  get Phys(data[n=7]=8587e000)
  get Phys(data[n=8]=8587f000)
  get Phys(data[n=9]=85880000)
  get Phys(data[n=9]=85881000)
  get Phys(data[n=10]=85882000)
  get Phys(data[n=11]=85883000)
  set TERM
AtapiDmaSetup: OK
IdeSendCommand: SRB_STATUS_PENDING
AtapiStartIo: Already have 3 request(s)!
AtapiStartIo: next Srb b0a632e0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0xb0f31f68
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0f31f68, CDB 0xb0f31f98, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: qd=2
Send to device 28
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e5a4
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (ExecOnly):
IdeReadWrite: Lba 0x1332f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1332f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0f31f68
AtapiStartIo: query PORT for next request
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0f31f68, status 1
AtapiInterrupt: RequestComplete, srb 0xb0f31f68
AtapiInterrupt: NextRequest, srb=0xb0a632e0
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a632e0, CDB 0xb0a63310, AtaReq 0xb129a030, SCmd 0x28
UniataNeedQueueing: qd=1
Send to device 28
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e4d8
** Ide: Command AtaReq 0xb129a030
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (ExecOnly):
IdeReadWrite: Lba 0x133af, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x133af count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a632e0
AtapiStartIo: query PORT for next request
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a632e0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a632e0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4185f, OrigWordsRequested 0xf00, DevSize 0xf
IdeReadWrite (REQ): Starting sector is 4185f, Number of WORDS 0xf00, DevSize 0xf
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4185f, Count 0xf(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4185f count 0xf feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1e00, full size 1e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1342f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1342f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85884000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85884000)
  get Phys(data[n=1]=85885000)
  get Phys(data[n=2]=85886000)
  get Phys(data[n=3]=85887000)
  get Phys(data[n=4]=85888000)
  get Phys(data[n=5]=85889000)
  get Phys(data[n=6]=8588a000)
  get Phys(data[n=6]=8588b000)
  get Phys(data[n=7]=8588c000)
  get Phys(data[n=8]=8588d000)
  get Phys(data[n=9]=8588e000)
  get Phys(data[n=10]=8588f000)
  get Phys(data[n=11]=85890000)
  get Phys(data[n=12]=85891000)
  get Phys(data[n=13]=85892000)
  get Phys(data[n=14]=85893000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1342f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1342f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4186f, OrigWordsRequested 0x400, DevSize 0x4
IdeReadWrite (REQ): Starting sector is 4186f, Number of WORDS 0x400, DevSize 0x4
AtapiDmaSetup: mode 0x45, data f7ff8000, count 800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4186f, Count 0x4(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4186f count 0x4 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 800, full size 800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41877, OrigWordsRequested 0xc00, DevSize 0xc
IdeReadWrite (REQ): Starting sector is 41877, Number of WORDS 0xc00, DevSize 0xc
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1800, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41877, Count 0xc(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41877 count 0xc feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1800, full size 1800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41887, OrigWordsRequested 0x2300, DevSize 0x23
IdeReadWrite (REQ): Starting sector is 41887, Number of WORDS 0x2300, DevSize 0x23
AtapiDmaSetup: mode 0x45, data f7ff8000, count 4600, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=2]=f7ffa000)
  get Phys(data[n=3]=f7ffb000)
  get Phys(data[n=4]=f7ffc000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41887, Count 0x23(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41887 count 0x23 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 4600, full size 4600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 418af, OrigWordsRequested 0xb00, DevSize 0xb
IdeReadWrite (REQ): Starting sector is 418af, Number of WORDS 0xb00, DevSize 0xb
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1600, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x418af, Count 0xb(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x418af count 0xb feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1600, full size 1600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 418bf, OrigWordsRequested 0x700, DevSize 0x7
IdeReadWrite (REQ): Starting sector is 418bf, Number of WORDS 0x700, DevSize 0x7
AtapiDmaSetup: mode 0x45, data f7ff8000, count e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x418bf, Count 0x7(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x418bf count 0x7 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e00, full size e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 418c7, OrigWordsRequested 0x500, DevSize 0x5
IdeReadWrite (REQ): Starting sector is 418c7, Number of WORDS 0x500, DevSize 0x5
AtapiDmaSetup: mode 0x45, data f7ff8000, count a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x418c7, Count 0x5(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x418c7 count 0x5 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a00, full size a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 86c7, OrigWordsRequested 0x7100, DevSize 0x71
IdeReadWrite (REQ): Starting sector is 86c7, Number of WORDS 0x7100, DevSize 0x71
AtapiDmaSetup: mode 0x45, data f7ff8000, count e200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=2]=f7ffa000)
  get Phys(data[n=3]=f7ffb000)
  get Phys(data[n=4]=f7ffc000)
  get Phys(data[n=5]=f7ffd000)
  get Phys(data[n=5]=f7ffe000)
  get Phys(data[n=6]=f7fff000)
  get Phys(data[n=7]=f8000000)
  get Phys(data[n=8]=f8001000)
  get Phys(data[n=9]=f8002000)
  get Phys(data[n=10]=f8003000)
  get Phys(data[n=10]=f8004000)
  get Phys(data[n=11]=f8005000)
  get Phys(data[n=12]=f8006000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x86c7, Count 0x71(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x86c7 count 0x71 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e200, full size e200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41297, OrigWordsRequested 0x900, DevSize 0x9
IdeReadWrite (REQ): Starting sector is 41297, Number of WORDS 0x900, DevSize 0x9
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41297, Count 0x9(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41297 count 0x9 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1200, full size 1200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 412a7, OrigWordsRequested 0x900, DevSize 0x9
IdeReadWrite (REQ): Starting sector is 412a7, Number of WORDS 0x900, DevSize 0x9
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x412a7, Count 0x9(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x412a7 count 0x9 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1200, full size 1200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 412b7, OrigWordsRequested 0x900, DevSize 0x9
IdeReadWrite (REQ): Starting sector is 412b7, Number of WORDS 0x900, DevSize 0x9
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x412b7, Count 0x9(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x412b7 count 0x9 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1200, full size 1200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 138af, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 138af, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85814000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85814000)
  get Phys(data[n=1]=85815000)
  get Phys(data[n=2]=85816000)
  get Phys(data[n=3]=85817000)
  get Phys(data[n=4]=85818000)
  get Phys(data[n=5]=85819000)
  get Phys(data[n=6]=8581a000)
  get Phys(data[n=7]=8581b000)
  get Phys(data[n=7]=8581c000)
  get Phys(data[n=8]=8581d000)
  get Phys(data[n=9]=8581e000)
  get Phys(data[n=10]=8581f000)
  get Phys(data[n=11]=85820000)
  get Phys(data[n=12]=85821000)
  get Phys(data[n=12]=85822000)
  get Phys(data[n=13]=85823000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x138af, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x138af count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 412c7, OrigWordsRequested 0x2700, DevSize 0x27
IdeReadWrite (REQ): Starting sector is 412c7, Number of WORDS 0x2700, DevSize 0x27
AtapiDmaSetup: mode 0x45, data f7ff8000, count 4e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=2]=f7ffa000)
  get Phys(data[n=3]=f7ffb000)
  get Phys(data[n=4]=f7ffc000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x412c7, Count 0x27(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x412c7 count 0x27 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 4e00, full size 4e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1392f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1392f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85824000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85824000)
  get Phys(data[n=1]=85825000)
  get Phys(data[n=2]=85826000)
  get Phys(data[n=3]=85827000)
  get Phys(data[n=4]=85828000)
  get Phys(data[n=5]=85829000)
  get Phys(data[n=6]=8582a000)
  get Phys(data[n=7]=8582b000)
  get Phys(data[n=7]=8582c000)
  get Phys(data[n=7]=8582d000)
  get Phys(data[n=8]=8582e000)
  get Phys(data[n=9]=8582f000)
  get Phys(data[n=10]=85830000)
  get Phys(data[n=11]=85831000)
  get Phys(data[n=12]=85832000)
  get Phys(data[n=12]=85833000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1392f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1392f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 139af, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 139af, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85834000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85834000)
  get Phys(data[n=1]=85835000)
  get Phys(data[n=2]=85836000)
  get Phys(data[n=2]=85837000)
  get Phys(data[n=3]=85838000)
  get Phys(data[n=4]=85839000)
  get Phys(data[n=4]=8583a000)
  get Phys(data[n=5]=8583b000)
  get Phys(data[n=6]=8583c000)
  get Phys(data[n=7]=8583d000)
  get Phys(data[n=8]=8583e000)
  get Phys(data[n=9]=8583f000)
  get Phys(data[n=10]=85840000)
  get Phys(data[n=10]=85841000)
  get Phys(data[n=11]=85842000)
  get Phys(data[n=12]=85843000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x139af, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x139af count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 412ef, OrigWordsRequested 0x600, DevSize 0x6
IdeReadWrite (REQ): Starting sector is 412ef, Number of WORDS 0x600, DevSize 0x6
AtapiDmaSetup: mode 0x45, data f7ff8000, count c00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x412ef, Count 0x6(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x412ef count 0x6 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered c00, full size c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 13a2f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 13a2f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85844000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85844000)
  get Phys(data[n=1]=85845000)
  get Phys(data[n=2]=85846000)
  get Phys(data[n=3]=85847000)
  get Phys(data[n=4]=85848000)
  get Phys(data[n=5]=85849000)
  get Phys(data[n=6]=8584a000)
  get Phys(data[n=7]=8584b000)
  get Phys(data[n=8]=8584c000)
  get Phys(data[n=9]=8584d000)
  get Phys(data[n=10]=8584e000)
  get Phys(data[n=11]=8584f000)
  get Phys(data[n=12]=85850000)
  get Phys(data[n=13]=85851000)
  get Phys(data[n=13]=85852000)
  get Phys(data[n=14]=85853000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x13a2f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x13a2f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 412f7, OrigWordsRequested 0x900, DevSize 0x9
IdeReadWrite (REQ): Starting sector is 412f7, Number of WORDS 0x900, DevSize 0x9
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x412f7, Count 0x9(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x412f7 count 0x9 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1200, full size 1200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805ded4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e21d7, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1e21d7, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85894000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85894000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e21d7, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e21d7 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41307, OrigWordsRequested 0x3f00, DevSize 0x3f
IdeReadWrite (REQ): Starting sector is 41307, Number of WORDS 0x3f00, DevSize 0x3f
AtapiDmaSetup: mode 0x45, data f7ff8000, count 7e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=1]=f7ffa000)
  get Phys(data[n=1]=f7ffb000)
  get Phys(data[n=1]=f7ffc000)
  get Phys(data[n=1]=f7ffd000)
  get Phys(data[n=1]=f7ffe000)
  get Phys(data[n=1]=f7fff000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41307, Count 0x3f(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41307 count 0x3f feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 7e00, full size 7e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e4dc
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 14277, OrigWordsRequested 0x300, DevSize 0x3
IdeReadWrite (REQ): Starting sector is 14277, Number of WORDS 0x300, DevSize 0x3
AtapiDmaSetup: mode 0x45, data f7ff8000, count 600, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x14277, Count 0x3(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x14277 count 0x3 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 600, full size 600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41347, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 41347, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f7fb0000, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7fb0000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41347, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41347 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88657f8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 403f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 403f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 80c40000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=80c40000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x403f, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x403f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805de50
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d274f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d274f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85914000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85914000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d274f, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d274f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4134f, OrigWordsRequested 0x900, DevSize 0x9
IdeReadWrite (REQ): Starting sector is 4134f, Number of WORDS 0x900, DevSize 0x9
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4134f, Count 0x9(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4134f count 0x9 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1200, full size 1200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4135f, OrigWordsRequested 0xf00, DevSize 0xf
IdeReadWrite (REQ): Starting sector is 4135f, Number of WORDS 0xf00, DevSize 0xf
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4135f, Count 0xf(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4135f count 0xf feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1e00, full size 1e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805ded4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d2767, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d2767, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 858d4000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=858d4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d2767, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d2767 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4136f, OrigWordsRequested 0xf00, DevSize 0xf
IdeReadWrite (REQ): Starting sector is 4136f, Number of WORDS 0xf00, DevSize 0xf
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4136f, Count 0xf(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4136f count 0xf feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1e00, full size 1e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805ded4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e21ef, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1e21ef, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85994000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85994000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e21ef, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e21ef count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4137f, OrigWordsRequested 0x1500, DevSize 0x15
IdeReadWrite (REQ): Starting sector is 4137f, Number of WORDS 0x1500, DevSize 0x15
AtapiDmaSetup: mode 0x45, data f7fb0000, count 2a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7fb0000)
  get Phys(data[n=1]=f7fb1000)
  get Phys(data[n=1]=f7fb2000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4137f, Count 0x15(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4137f count 0x15 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2a00, full size 2a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41397, OrigWordsRequested 0x700, DevSize 0x7
IdeReadWrite (REQ): Starting sector is 41397, Number of WORDS 0x700, DevSize 0x7
AtapiDmaSetup: mode 0x45, data f7ff8000, count e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41397, Count 0x7(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41397 count 0x7 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e00, full size e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805d6c4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e21df, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1e21df, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 859d4000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=859d4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e21df, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e21df count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0f31f68, CDB 0xb0f31f98, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=1
Non-empty queue
Try IDE prepare
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1299018
** --- **
** Ide: Command continue prep
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4139f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4139f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f7ff8000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=1]=f7ffa000)
  get Phys(data[n=1]=f7ffb000)
  get Phys(data[n=1]=f7ffc000)
  get Phys(data[n=1]=f7ffd000)
  get Phys(data[n=1]=f7ffe000)
  get Phys(data[n=1]=f7fff000)
  get Phys(data[n=2]=f8000000)
  get Phys(data[n=2]=f8001000)
  get Phys(data[n=2]=f8002000)
  get Phys(data[n=2]=f8003000)
  get Phys(data[n=2]=f8004000)
  get Phys(data[n=2]=f8005000)
  get Phys(data[n=2]=f8006000)
  get Phys(data[n=2]=f8007000)
  set TERM
AtapiDmaSetup: OK
IdeSendCommand: SRB_STATUS_PENDING
AtapiStartIo: Already have 2 request(s)!
AtapiStartIo: next Srb b0f31f68
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0xb0f31f68
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0f31f68, CDB 0xb0f31f98, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: qd=1
Send to device 28
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad1a4
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (ExecOnly):
IdeReadWrite: Lba 0x4139f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4139f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0f31f68
AtapiStartIo: query PORT for next request
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0f31f68, status 1
AtapiInterrupt: RequestComplete, srb 0xb0f31f68
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4141f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4141f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8008000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8008000)
  get Phys(data[n=1]=f8009000)
  get Phys(data[n=1]=f800a000)
  get Phys(data[n=1]=f800b000)
  get Phys(data[n=1]=f800c000)
  get Phys(data[n=1]=f800d000)
  get Phys(data[n=1]=f800e000)
  get Phys(data[n=1]=f800f000)
  get Phys(data[n=2]=f8010000)
  get Phys(data[n=2]=f8011000)
  get Phys(data[n=3]=f8012000)
  get Phys(data[n=3]=f8013000)
  get Phys(data[n=3]=f8014000)
  get Phys(data[n=3]=f8015000)
  get Phys(data[n=3]=f8016000)
  get Phys(data[n=3]=f8017000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4141f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4141f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4149f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 4149f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f8018000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8018000)
  get Phys(data[n=1]=f8019000)
  get Phys(data[n=1]=f801a000)
  get Phys(data[n=1]=f801b000)
  get Phys(data[n=2]=f801c000)
  get Phys(data[n=3]=f801d000)
  get Phys(data[n=3]=f801e000)
  get Phys(data[n=3]=f801f000)
  get Phys(data[n=4]=f8020000)
  get Phys(data[n=4]=f8021000)
  get Phys(data[n=4]=f8022000)
  get Phys(data[n=4]=f8023000)
  get Phys(data[n=4]=f8024000)
  get Phys(data[n=5]=f8025000)
  get Phys(data[n=5]=f8026000)
  get Phys(data[n=6]=f8027000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4149f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4149f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805d6c4
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d280f, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d280f, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85a14000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85a14000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d280f, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d280f count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4151f, OrigWordsRequested 0x5900, DevSize 0x59
IdeReadWrite (REQ): Starting sector is 4151f, Number of WORDS 0x5900, DevSize 0x59
AtapiDmaSetup: mode 0x45, data f8028000, count b200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8028000)
  get Phys(data[n=1]=f8029000)
  get Phys(data[n=1]=f802a000)
  get Phys(data[n=1]=f802b000)
  get Phys(data[n=1]=f802c000)
  get Phys(data[n=1]=f802d000)
  get Phys(data[n=1]=f802e000)
  get Phys(data[n=1]=f802f000)
  get Phys(data[n=2]=f8030000)
  get Phys(data[n=2]=f8031000)
  get Phys(data[n=3]=f8032000)
  get Phys(data[n=4]=f8033000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4151f, Count 0x59(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4151f count 0x59 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered b200, full size b200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805d6d8
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 42ae7, OrigWordsRequested 0x8200, DevSize 0x82
IdeReadWrite (REQ): Starting sector is 42ae7, Number of WORDS 0x8200, DevSize 0x82
AtapiDmaSetup: mode 0x45, data f7ff8000, count 10400, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=2]=f7ffa000)
  get Phys(data[n=2]=f7ffb000)
  get Phys(data[n=2]=f7ffc000)
  get Phys(data[n=2]=f7ffd000)
  get Phys(data[n=3]=f7ffe000)
  get Phys(data[n=3]=f7fff000)
  get Phys(data[n=3]=f8000000)
  get Phys(data[n=3]=f8001000)
  get Phys(data[n=4]=f8002000)
  get Phys(data[n=4]=f8003000)
  get Phys(data[n=4]=f8004000)
  get Phys(data[n=5]=f8005000)
  get Phys(data[n=5]=f8006000)
  get Phys(data[n=6]=f8007000)
  get Phys(data[n=6]=f8008000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x42ae7, Count 0x82(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x42ae7 count 0x82 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10400, full size 10400
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4157f, OrigWordsRequested 0xd00, DevSize 0xd
IdeReadWrite (REQ): Starting sector is 4157f, Number of WORDS 0xd00, DevSize 0xd
AtapiDmaSetup: mode 0x45, data f7ff8000, count 1a00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4157f, Count 0xd(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4157f count 0xd feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1a00, full size 1a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4158f, OrigWordsRequested 0x2800, DevSize 0x28
IdeReadWrite (REQ): Starting sector is 4158f, Number of WORDS 0x2800, DevSize 0x28
AtapiDmaSetup: mode 0x45, data f7ff8000, count 5000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=2]=f7ffa000)
  get Phys(data[n=2]=f7ffb000)
  get Phys(data[n=3]=f7ffc000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4158f, Count 0x28(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4158f count 0x28 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 5000, full size 5000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 415b7, OrigWordsRequested 0x1300, DevSize 0x13
IdeReadWrite (REQ): Starting sector is 415b7, Number of WORDS 0x1300, DevSize 0x13
AtapiDmaSetup: mode 0x45, data f7ff8000, count 2600, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=2]=f7ffa000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x415b7, Count 0x13(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x415b7 count 0x13 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2600, full size 2600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805da70
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2bfbf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2bfbf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85a94000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85a94000)
  get Phys(data[n=1]=85a95000)
  get Phys(data[n=2]=85a96000)
  get Phys(data[n=2]=85a97000)
  get Phys(data[n=3]=85a98000)
  get Phys(data[n=3]=85a99000)
  get Phys(data[n=3]=85a9a000)
  get Phys(data[n=3]=85a9b000)
  get Phys(data[n=3]=85a9c000)
  get Phys(data[n=3]=85a9d000)
  get Phys(data[n=3]=85a9e000)
  get Phys(data[n=3]=85a9f000)
  get Phys(data[n=3]=85aa0000)
  get Phys(data[n=4]=85aa1000)
  get Phys(data[n=4]=85aa2000)
  get Phys(data[n=5]=85aa3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2bfbf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2bfbf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0f31f68, CDB 0xb0f31f98, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=1
Non-empty queue
Try IDE prepare
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805da70
** Ide: Command AtaReq 0xb1299018
** --- **
** Ide: Command continue prep
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2c03f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2c03f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85aa4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85aa4000)
  get Phys(data[n=1]=85aa5000)
  get Phys(data[n=1]=85aa6000)
  get Phys(data[n=1]=85aa7000)
  get Phys(data[n=1]=85aa8000)
  get Phys(data[n=1]=85aa9000)
  get Phys(data[n=1]=85aaa000)
  get Phys(data[n=1]=85aab000)
  get Phys(data[n=1]=85aac000)
  get Phys(data[n=1]=85aad000)
  get Phys(data[n=1]=85aae000)
  get Phys(data[n=2]=85aaf000)
  get Phys(data[n=2]=85ab0000)
  get Phys(data[n=3]=85ab1000)
  get Phys(data[n=3]=85ab2000)
  get Phys(data[n=3]=85ab3000)
  set TERM
AtapiDmaSetup: OK
IdeSendCommand: SRB_STATUS_PENDING
AtapiStartIo: Already have 2 request(s)!
AtapiStartIo: next Srb b0f31f68
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a632e0, CDB 0xb0a63310, AtaReq 0xb129a030, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=2
Non-empty queue
Try IDE prepare
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805da70
** Ide: Command AtaReq 0xb129a030
** --- **
** Ide: Command continue prep
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2c0bf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2c0bf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85ab4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129a088)
  get Phys(data[0]=85ab4000)
  get Phys(data[n=1]=85ab5000)
  get Phys(data[n=1]=85ab6000)
  get Phys(data[n=1]=85ab7000)
  get Phys(data[n=1]=85ab8000)
  get Phys(data[n=1]=85ab9000)
  get Phys(data[n=1]=85aba000)
  get Phys(data[n=1]=85abb000)
  get Phys(data[n=1]=85abc000)
  get Phys(data[n=1]=85abd000)
  get Phys(data[n=1]=85abe000)
  get Phys(data[n=1]=85abf000)
  get Phys(data[n=1]=85ac0000)
  get Phys(data[n=2]=85ac1000)
  get Phys(data[n=2]=85ac2000)
  get Phys(data[n=3]=85ac3000)
  set TERM
AtapiDmaSetup: OK
IdeSendCommand: SRB_STATUS_PENDING
AtapiStartIo: Already have 3 request(s)!
AtapiStartIo: next Srb b0a632e0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0xb0f31f68
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0f31f68, CDB 0xb0f31f98, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: qd=2
Send to device 28
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805d944
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (ExecOnly):
IdeReadWrite: Lba 0x2c03f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2c03f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0f31f68
AtapiStartIo: query PORT for next request
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0f31f68, status 1
AtapiInterrupt: RequestComplete, srb 0xb0f31f68
AtapiInterrupt: NextRequest, srb=0xb0a632e0
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a632e0, CDB 0xb0a63310, AtaReq 0xb129a030, SCmd 0x28
UniataNeedQueueing: qd=1
Send to device 28
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805d878
** Ide: Command AtaReq 0xb129a030
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (ExecOnly):
IdeReadWrite: Lba 0x2c0bf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2c0bf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a632e0
AtapiStartIo: query PORT for next request
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a632e0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a632e0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805da70
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 2c13f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 2c13f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85ac4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=85ac4000)
  get Phys(data[n=1]=85ac5000)
  get Phys(data[n=1]=85ac6000)
  get Phys(data[n=1]=85ac7000)
  get Phys(data[n=1]=85ac8000)
  get Phys(data[n=2]=85ac9000)
  get Phys(data[n=2]=85aca000)
  get Phys(data[n=2]=85acb000)
  get Phys(data[n=2]=85acc000)
  get Phys(data[n=3]=85acd000)
  get Phys(data[n=3]=85ace000)
  get Phys(data[n=3]=85acf000)
  get Phys(data[n=3]=85ad0000)
  get Phys(data[n=4]=85ad1000)
  get Phys(data[n=4]=85ad2000)
  get Phys(data[n=4]=85ad3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x2c13f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x2c13f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 415cf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 415cf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f7ff8000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=2]=f7ffa000)
  get Phys(data[n=3]=f7ffb000)
  get Phys(data[n=4]=f7ffc000)
  get Phys(data[n=4]=f7ffd000)
  get Phys(data[n=4]=f7ffe000)
  get Phys(data[n=4]=f7fff000)
  get Phys(data[n=4]=f8000000)
  get Phys(data[n=4]=f8001000)
  get Phys(data[n=4]=f8002000)
  get Phys(data[n=4]=f8003000)
  get Phys(data[n=4]=f8004000)
  get Phys(data[n=5]=f8005000)
  get Phys(data[n=5]=f8006000)
  get Phys(data[n=6]=f8007000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x415cf, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x415cf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4164f, OrigWordsRequested 0x7300, DevSize 0x73
IdeReadWrite (REQ): Starting sector is 4164f, Number of WORDS 0x7300, DevSize 0x73
AtapiDmaSetup: mode 0x45, data f8008000, count e600, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f8008000)
  get Phys(data[n=1]=f8009000)
  get Phys(data[n=1]=f800a000)
  get Phys(data[n=1]=f800b000)
  get Phys(data[n=1]=f800c000)
  get Phys(data[n=1]=f800d000)
  get Phys(data[n=1]=f800e000)
  get Phys(data[n=1]=f800f000)
  get Phys(data[n=1]=f8010000)
  get Phys(data[n=1]=f8011000)
  get Phys(data[n=1]=f8012000)
  get Phys(data[n=1]=f8013000)
  get Phys(data[n=1]=f8014000)
  get Phys(data[n=2]=f8015000)
  get Phys(data[n=2]=f8016000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4164f, Count 0x73(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4164f count 0x73 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e600, full size e600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Using shell hooks for notification of shell events.
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 416c7, OrigWordsRequested 0x7a00, DevSize 0x7a
IdeReadWrite (REQ): Starting sector is 416c7, Number of WORDS 0x7a00, DevSize 0x7a
AtapiDmaSetup: mode 0x45, data f7ff8000, count f400, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=2]=f7ffa000)
  get Phys(data[n=3]=f7ffb000)
  get Phys(data[n=3]=f7ffc000)
  get Phys(data[n=3]=f7ffd000)
  get Phys(data[n=3]=f7ffe000)
  get Phys(data[n=3]=f7fff000)
  get Phys(data[n=3]=f8000000)
  get Phys(data[n=3]=f8001000)
  get Phys(data[n=3]=f8002000)
  get Phys(data[n=3]=f8003000)
  get Phys(data[n=3]=f8004000)
  get Phys(data[n=3]=f8005000)
  get Phys(data[n=4]=f8006000)
  get Phys(data[n=5]=f8007000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x416c7, Count 0x7a(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x416c7 count 0x7a feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered f400, full size f400
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
WARNING:  BackupRead at ../../dll/win32/kernel32/client/file/backup.c:34 is UNIMPLEMENTED!
WARNING:  BackupRead at ../../dll/win32/kernel32/client/file/backup.c:34 is UNIMPLEMENTED!
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41747, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 41747, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f7fb0000, count 200, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7fb0000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41747, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41747 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4174f, OrigWordsRequested 0x300, DevSize 0x3
IdeReadWrite (REQ): Starting sector is 4174f, Number of WORDS 0x300, DevSize 0x3
AtapiDmaSetup: mode 0x45, data f7fb0000, count 600, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7fb0000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4174f, Count 0x3(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4174f count 0x3 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 600, full size 600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41757, OrigWordsRequested 0x7200, DevSize 0x72
IdeReadWrite (REQ): Starting sector is 41757, Number of WORDS 0x7200, DevSize 0x72
AtapiDmaSetup: mode 0x45, data f7ff8000, count e400, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=1]=f7ffa000)
  get Phys(data[n=1]=f7ffb000)
  get Phys(data[n=1]=f7ffc000)
  get Phys(data[n=1]=f7ffd000)
  get Phys(data[n=2]=f7ffe000)
  get Phys(data[n=2]=f7fff000)
  get Phys(data[n=3]=f8000000)
  get Phys(data[n=3]=f8001000)
  get Phys(data[n=3]=f8002000)
  get Phys(data[n=3]=f8003000)
  get Phys(data[n=3]=f8004000)
  get Phys(data[n=3]=f8005000)
  get Phys(data[n=3]=f8006000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41757, Count 0x72(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41757 count 0x72 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e400, full size e400
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 417cf, OrigWordsRequested 0x700, DevSize 0x7
IdeReadWrite (REQ): Starting sector is 417cf, Number of WORDS 0x700, DevSize 0x7
AtapiDmaSetup: mode 0x45, data f7ff8000, count e00, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7ff8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x417cf, Count 0x7(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x417cf count 0x7 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e00, full size e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0ff0b50, CDB 0xb0ff0b80, AtaReq 0xb1298000, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0ff0b50
TopLevel (3), AtaReq 0xb1298000
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e2d0
** Ide: Command AtaReq 0xb1298000
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11e1f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 11e1f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f7fb0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1298058)
  get Phys(data[0]=f7fb0000)
  get Phys(data[n=1]=f7fb1000)
  get Phys(data[n=1]=f7fb2000)
  get Phys(data[n=2]=f7fb3000)
  get Phys(data[n=2]=f7fb4000)
  get Phys(data[n=2]=f7fb5000)
  get Phys(data[n=2]=f7fb6000)
  get Phys(data[n=2]=f7fb7000)
  get Phys(data[n=2]=f7fb8000)
  get Phys(data[n=2]=f7fb9000)
  get Phys(data[n=2]=f7fba000)
  get Phys(data[n=3]=f7fbb000)
  get Phys(data[n=3]=f7fbc000)
  get Phys(data[n=3]=f7fbd000)
  get Phys(data[n=3]=f7fbe000)
  get Phys(data[n=3]=f7fbf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x11e1f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x11e1f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0ff0b50
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0f31f68, CDB 0xb0f31f98, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=1
Non-empty queue
Try IDE prepare
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e2d0
** Ide: Command AtaReq 0xb1299018
** --- **
** Ide: Command continue prep
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11e9f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 11e9f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f7fc0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=f7fc0000)
  get Phys(data[n=1]=f7fc1000)
  get Phys(data[n=1]=f7fc2000)
  get Phys(data[n=2]=f7fc3000)
  get Phys(data[n=2]=f7fc4000)
  get Phys(data[n=2]=f7fc5000)
  get Phys(data[n=3]=f7fc6000)
  get Phys(data[n=3]=f7fc7000)
  get Phys(data[n=4]=f7fc8000)
  get Phys(data[n=4]=f7fc9000)
  get Phys(data[n=4]=f7fca000)
  get Phys(data[n=4]=f7fcb000)
  get Phys(data[n=4]=f7fcc000)
  get Phys(data[n=4]=f7fcd000)
  get Phys(data[n=4]=f7fce000)
  get Phys(data[n=4]=f7fcf000)
  set TERM
AtapiDmaSetup: OK
IdeSendCommand: SRB_STATUS_PENDING
AtapiStartIo: Already have 2 request(s)!
AtapiStartIo: next Srb b0f31f68
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a632e0, CDB 0xb0a63310, AtaReq 0xb129a030, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=2
Non-empty queue
Try IDE prepare
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb129a030
** --- **
** Ide: Command continue prep
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 417d7, OrigWordsRequested 0x2e00, DevSize 0x2e
IdeReadWrite (REQ): Starting sector is 417d7, Number of WORDS 0x2e00, DevSize 0x2e
AtapiDmaSetup: mode 0x45, data f7ff8000, count 5c00, lCh 0, dev 0
  get Phys(PRD=b129a088)
  get Phys(data[0]=f7ff8000)
  get Phys(data[n=1]=f7ff9000)
  get Phys(data[n=1]=f7ffa000)
  get Phys(data[n=1]=f7ffb000)
  get Phys(data[n=1]=f7ffc000)
  get Phys(data[n=1]=f7ffd000)
  set TERM
AtapiDmaSetup: OK
IdeSendCommand: SRB_STATUS_PENDING
AtapiStartIo: Already have 3 request(s)!
AtapiStartIo: next Srb b0a632e0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=3
Non-empty queue
Try IDE prepare
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e2d0
** Ide: Command AtaReq 0xb129b048
** --- **
** Ide: Command continue prep
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11f1f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 11f1f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f7fd0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=f7fd0000)
  get Phys(data[n=1]=f7fd1000)
  get Phys(data[n=1]=f7fd2000)
  get Phys(data[n=2]=f7fd3000)
  get Phys(data[n=3]=f7fd4000)
  get Phys(data[n=3]=f7fd5000)
  get Phys(data[n=3]=f7fd6000)
  get Phys(data[n=3]=f7fd7000)
  get Phys(data[n=3]=f7fd8000)
  get Phys(data[n=3]=f7fd9000)
  get Phys(data[n=3]=f7fda000)
  get Phys(data[n=3]=f7fdb000)
  get Phys(data[n=3]=f7fdc000)
  get Phys(data[n=4]=f7fdd000)
  get Phys(data[n=4]=f7fde000)
  get Phys(data[n=5]=f7fdf000)
  set TERM
AtapiDmaSetup: OK
IdeSendCommand: SRB_STATUS_PENDING
AtapiStartIo: Already have 4 request(s)!
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129c060, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=4
Non-empty queue
Try IDE prepare
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e2d0
** Ide: Command AtaReq 0xb129c060
** --- **
** Ide: Command continue prep
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11f9f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 11f9f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f7fe0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129c0b8)
  get Phys(data[0]=f7fe0000)
  get Phys(data[n=1]=f7fe1000)
  get Phys(data[n=1]=f7fe2000)
  get Phys(data[n=2]=f7fe3000)
  get Phys(data[n=2]=f7fe4000)
  get Phys(data[n=2]=f7fe5000)
  get Phys(data[n=2]=f7fe6000)
  get Phys(data[n=2]=f7fe7000)
  get Phys(data[n=2]=f7fe8000)
  get Phys(data[n=2]=f7fe9000)
  get Phys(data[n=2]=f7fea000)
  get Phys(data[n=2]=f7feb000)
  get Phys(data[n=2]=f7fec000)
  get Phys(data[n=3]=f7fed000)
  get Phys(data[n=3]=f7fee000)
  get Phys(data[n=4]=f7fef000)
  set TERM
AtapiDmaSetup: OK
IdeSendCommand: SRB_STATUS_PENDING
AtapiStartIo: Already have 5 request(s)!
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0ff0b50, status 1
AtapiInterrupt: RequestComplete, srb 0xb0ff0b50
AtapiInterrupt: NextRequest, srb=0xb0f31f68
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0f31f68, CDB 0xb0f31f98, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: qd=4
Send to device 28
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e1a4
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (ExecOnly):
IdeReadWrite: Lba 0x11e9f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x11e9f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0f31f68
AtapiStartIo: query PORT for next request
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0f31f68, status 1
AtapiInterrupt: RequestComplete, srb 0xb0f31f68
AtapiInterrupt: NextRequest, srb=0xb0a3ce18
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: qd=3
Send to device 28
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c9af8
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (ExecOnly):
IdeReadWrite: Lba 0x11f1f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x11f1f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0xb0a3cdd0
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129c060, SCmd 0x28
UniataNeedQueueing: qd=2
Send to device 28
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c9a2c
** Ide: Command AtaReq 0xb129c060
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (ExecOnly):
IdeReadWrite: Lba 0x11f9f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x11f9f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0xb0a632e0
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a632e0, CDB 0xb0a63310, AtaReq 0xb129a030, SCmd 0x28
UniataNeedQueueing: qd=1
Send to device 28
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88c9a2c
** Ide: Command AtaReq 0xb129a030
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (ExecOnly):
IdeReadWrite: Lba 0x417d7, Count 0x2e(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x417d7 count 0x2e feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a632e0
AtapiStartIo: query PORT for next request
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 5c00, full size 5c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a632e0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a632e0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e6cc
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11e1f, OrigWordsRequested 0x1000, DevSize 0x10
IdeReadWrite (REQ): Starting sector is 11e1f, Number of WORDS 0x1000, DevSize 0x10
AtapiDmaSetup: mode 0x45, data f820d000, count 2000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=f820d000)
  get Phys(data[n=1]=f820e000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x11e1f, Count 0x10(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x11e1f count 0x10 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2000, full size 2000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41807, OrigWordsRequested 0x700, DevSize 0x7
IdeReadWrite (REQ): Starting sector is 41807, Number of WORDS 0x700, DevSize 0x7
AtapiDmaSetup: mode 0x45, data f7ff8000, count e00, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=f7ff8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41807, Count 0x7(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41807 count 0x7 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e00, full size e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4180f, OrigWordsRequested 0x600, DevSize 0x6
IdeReadWrite (REQ): Starting sector is 4180f, Number of WORDS 0x600, DevSize 0x6
AtapiDmaSetup: mode 0x45, data f7ff8000, count c00, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=f7ff8000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4180f, Count 0x6(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4180f count 0x6 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered c00, full size c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b6d0
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 51367, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 51367, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85954000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85954000)
  get Phys(data[n=1]=85955000)
  get Phys(data[n=1]=85956000)
  get Phys(data[n=1]=85957000)
  get Phys(data[n=1]=85958000)
  get Phys(data[n=1]=85959000)
  get Phys(data[n=1]=8595a000)
  get Phys(data[n=1]=8595b000)
  get Phys(data[n=1]=8595c000)
  get Phys(data[n=1]=8595d000)
  get Phys(data[n=1]=8595e000)
  get Phys(data[n=1]=8595f000)
  get Phys(data[n=1]=85960000)
  get Phys(data[n=1]=85961000)
  get Phys(data[n=2]=85962000)
  get Phys(data[n=2]=85963000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x51367, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x51367 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b6d0
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 513e7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 513e7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85964000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85964000)
  get Phys(data[n=1]=85965000)
  get Phys(data[n=1]=85966000)
  get Phys(data[n=1]=85967000)
  get Phys(data[n=1]=85968000)
  get Phys(data[n=1]=85969000)
  get Phys(data[n=1]=8596a000)
  get Phys(data[n=1]=8596b000)
  get Phys(data[n=1]=8596c000)
  get Phys(data[n=1]=8596d000)
  get Phys(data[n=2]=8596e000)
  get Phys(data[n=2]=8596f000)
  get Phys(data[n=2]=85970000)
  get Phys(data[n=2]=85971000)
  get Phys(data[n=3]=85972000)
  get Phys(data[n=4]=85973000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x513e7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x513e7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=1
Non-empty queue
Try IDE prepare
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b6d0
** Ide: Command AtaReq 0xb129b048
** --- **
** Ide: Command continue prep
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 51467, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 51467, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85974000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=85974000)
  get Phys(data[n=1]=85975000)
  get Phys(data[n=2]=85976000)
  get Phys(data[n=2]=85977000)
  get Phys(data[n=2]=85978000)
  get Phys(data[n=2]=85979000)
  get Phys(data[n=2]=8597a000)
  get Phys(data[n=2]=8597b000)
  get Phys(data[n=3]=8597c000)
  get Phys(data[n=3]=8597d000)
  get Phys(data[n=3]=8597e000)
  get Phys(data[n=3]=8597f000)
  get Phys(data[n=3]=85980000)
  get Phys(data[n=3]=85981000)
  get Phys(data[n=4]=85982000)
  get Phys(data[n=4]=85983000)
  set TERM
AtapiDmaSetup: OK
IdeSendCommand: SRB_STATUS_PENDING
AtapiStartIo: Already have 2 request(s)!
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0xb0a3cdd0
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: qd=1
Send to device 28
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b5a4
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (ExecOnly):
IdeReadWrite: Lba 0x51467, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x51467 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=1
Non-empty queue
Try IDE prepare
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b6d0
** Ide: Command AtaReq 0xb1299018
** --- **
** Ide: Command continue prep
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 514e7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 514e7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85984000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85984000)
  get Phys(data[n=1]=85985000)
  get Phys(data[n=1]=85986000)
  get Phys(data[n=1]=85987000)
  get Phys(data[n=1]=85988000)
  get Phys(data[n=1]=85989000)
  get Phys(data[n=1]=8598a000)
  get Phys(data[n=1]=8598b000)
  get Phys(data[n=1]=8598c000)
  get Phys(data[n=1]=8598d000)
  get Phys(data[n=1]=8598e000)
  get Phys(data[n=1]=8598f000)
  get Phys(data[n=1]=85990000)
  get Phys(data[n=1]=85991000)
  get Phys(data[n=2]=85992000)
  get Phys(data[n=2]=85993000)
  set TERM
AtapiDmaSetup: OK
IdeSendCommand: SRB_STATUS_PENDING
AtapiStartIo: Already have 2 request(s)!
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0xb0a3ce18
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: qd=1
Send to device 28
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf856b5a4
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (ExecOnly):
IdeReadWrite: Lba 0x514e7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x514e7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41817, OrigWordsRequested 0xb00, DevSize 0xb
IdeReadWrite (REQ): Starting sector is 41817, Number of WORDS 0xb00, DevSize 0xb
AtapiDmaSetup: mode 0x45, data f7fb0000, count 1600, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=f7fb0000)
  get Phys(data[n=1]=f7fb1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41817, Count 0xb(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41817 count 0xb feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1600, full size 1600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41827, OrigWordsRequested 0x600, DevSize 0x6
IdeReadWrite (REQ): Starting sector is 41827, Number of WORDS 0x600, DevSize 0x6
AtapiDmaSetup: mode 0x45, data f7fb0000, count c00, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=f7fb0000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41827, Count 0x6(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41827 count 0x6 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered c00, full size c00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8026ed4
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d2867, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d2867, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85b54000, count 1000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=85b54000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d2867, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1d2867 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8026fcc
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 44b7, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 44b7, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85b94000, count 1000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=85b94000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x44b7, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x44b7 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4182f, OrigWordsRequested 0x1100, DevSize 0x11
IdeReadWrite (REQ): Starting sector is 4182f, Number of WORDS 0x1100, DevSize 0x11
AtapiDmaSetup: mode 0x45, data f7fb0000, count 2200, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=f7fb0000)
  get Phys(data[n=1]=f7fb1000)
  get Phys(data[n=1]=f7fb2000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4182f, Count 0x11(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4182f count 0x11 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 2200, full size 2200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41847, OrigWordsRequested 0x1800, DevSize 0x18
IdeReadWrite (REQ): Starting sector is 41847, Number of WORDS 0x1800, DevSize 0x18
AtapiDmaSetup: mode 0x45, data f7fb0000, count 3000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=f7fb0000)
  get Phys(data[n=1]=f7fb1000)
  get Phys(data[n=2]=f7fb2000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41847, Count 0x18(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41847 count 0x18 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 3000, full size 3000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4185f, OrigWordsRequested 0xf00, DevSize 0xf
IdeReadWrite (REQ): Starting sector is 4185f, Number of WORDS 0xf00, DevSize 0xf
AtapiDmaSetup: mode 0x45, data f7fb0000, count 1e00, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=f7fb0000)
  get Phys(data[n=1]=f7fb1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x4185f, Count 0xf(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4185f count 0xf feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1e00, full size 1e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf80276d0
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 25c37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 25c37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85b14000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=85b14000)
  get Phys(data[n=1]=85b15000)
  get Phys(data[n=1]=85b16000)
  get Phys(data[n=2]=85b17000)
  get Phys(data[n=2]=85b18000)
  get Phys(data[n=3]=85b19000)
  get Phys(data[n=4]=85b1a000)
  get Phys(data[n=5]=85b1b000)
  get Phys(data[n=5]=85b1c000)
  get Phys(data[n=5]=85b1d000)
  get Phys(data[n=5]=85b1e000)
  get Phys(data[n=6]=85b1f000)
  get Phys(data[n=6]=85b20000)
  get Phys(data[n=6]=85b21000)
  get Phys(data[n=7]=85b22000)
  get Phys(data[n=7]=85b23000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x25c37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x25c37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=1
Non-empty queue
Try IDE prepare
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf80276d0
** Ide: Command AtaReq 0xb1299018
** --- **
** Ide: Command continue prep
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 25cb7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 25cb7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85b24000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85b24000)
  get Phys(data[n=1]=85b25000)
  get Phys(data[n=1]=85b26000)
  get Phys(data[n=1]=85b27000)
  get Phys(data[n=1]=85b28000)
  get Phys(data[n=2]=85b29000)
  get Phys(data[n=2]=85b2a000)
  get Phys(data[n=2]=85b2b000)
  get Phys(data[n=3]=85b2c000)
  get Phys(data[n=4]=85b2d000)
  get Phys(data[n=4]=85b2e000)
  get Phys(data[n=4]=85b2f000)
  get Phys(data[n=4]=85b30000)
  get Phys(data[n=5]=85b31000)
  get Phys(data[n=5]=85b32000)
  get Phys(data[n=5]=85b33000)
  set TERM
AtapiDmaSetup: OK
IdeSendCommand: SRB_STATUS_PENDING
AtapiStartIo: Already have 2 request(s)!
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0xb0a3ce18
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: qd=1
Send to device 28
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf80275a4
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (ExecOnly):
IdeReadWrite: Lba 0x25cb7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x25cb7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=1
Non-empty queue
Try IDE prepare
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb129b048
** --- **
** Ide: Command continue prep
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 4186f, OrigWordsRequested 0x400, DevSize 0x4
IdeReadWrite (REQ): Starting sector is 4186f, Number of WORDS 0x400, DevSize 0x4
AtapiDmaSetup: mode 0x45, data f7fb0000, count 800, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=f7fb0000)
  set TERM
AtapiDmaSetup: OK
IdeSendCommand: SRB_STATUS_PENDING
AtapiStartIo: Already have 2 request(s)!
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0xb0a3cdd0
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: qd=1
Send to device 28
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad20c
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (ExecOnly):
IdeReadWrite: Lba 0x4186f, Count 0x4(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x4186f count 0x4 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 800, full size 800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf80276d0
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 25d37, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 25d37, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85b34000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85b34000)
  get Phys(data[n=1]=85b35000)
  get Phys(data[n=1]=85b36000)
  get Phys(data[n=1]=85b37000)
  get Phys(data[n=1]=85b38000)
  get Phys(data[n=2]=85b39000)
  get Phys(data[n=3]=85b3a000)
  get Phys(data[n=3]=85b3b000)
  get Phys(data[n=3]=85b3c000)
  get Phys(data[n=3]=85b3d000)
  get Phys(data[n=3]=85b3e000)
  get Phys(data[n=3]=85b3f000)
  get Phys(data[n=3]=85b40000)
  get Phys(data[n=3]=85b41000)
  get Phys(data[n=3]=85b42000)
  get Phys(data[n=3]=85b43000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x25d37, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x25d37 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf80276d0
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 25db7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 25db7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85b44000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85b44000)
  get Phys(data[n=1]=85b45000)
  get Phys(data[n=1]=85b46000)
  get Phys(data[n=2]=85b47000)
  get Phys(data[n=2]=85b48000)
  get Phys(data[n=3]=85b49000)
  get Phys(data[n=3]=85b4a000)
  get Phys(data[n=3]=85b4b000)
  get Phys(data[n=3]=85b4c000)
  get Phys(data[n=3]=85b4d000)
  get Phys(data[n=4]=85b4e000)
  get Phys(data[n=4]=85b4f000)
  get Phys(data[n=5]=85b50000)
  get Phys(data[n=5]=85b51000)
  get Phys(data[n=5]=85b52000)
  get Phys(data[n=6]=85b53000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x25db7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x25db7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41877, OrigWordsRequested 0xc00, DevSize 0xc
IdeReadWrite (REQ): Starting sector is 41877, Number of WORDS 0xc00, DevSize 0xc
AtapiDmaSetup: mode 0x45, data f7fb0000, count 1800, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=f7fb0000)
  get Phys(data[n=1]=f7fb1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41877, Count 0xc(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41877 count 0xc feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1800, full size 1800
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf86f5338
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41bff, OrigWordsRequested 0x8300, DevSize 0x83
IdeReadWrite (REQ): Starting sector is 41bff, Number of WORDS 0x8300, DevSize 0x83
AtapiDmaSetup: mode 0x45, data f7f70000, count 10600, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=f7f70000)
  get Phys(data[n=1]=f7f71000)
  get Phys(data[n=2]=f7f72000)
  get Phys(data[n=3]=f7f73000)
  get Phys(data[n=4]=f7f74000)
  get Phys(data[n=4]=f7f75000)
  get Phys(data[n=4]=f7f76000)
  get Phys(data[n=4]=f7f77000)
  get Phys(data[n=5]=f7f78000)
  get Phys(data[n=5]=f7f79000)
  get Phys(data[n=5]=f7f7a000)
  get Phys(data[n=6]=f7f7b000)
  get Phys(data[n=6]=f7f7c000)
  get Phys(data[n=6]=f7f7d000)
  get Phys(data[n=7]=f7f7e000)
  get Phys(data[n=7]=f7f7f000)
  get Phys(data[n=7]=f7f80000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41bff, Count 0x83(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41bff count 0x83 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10600, full size 10600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
(../../subsystems/win32/csrss/csrsrv/api/wapi.c:1114) Death from unknown thread, just continue
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 41887, OrigWordsRequested 0x2300, DevSize 0x23
IdeReadWrite (REQ): Starting sector is 41887, Number of WORDS 0x2300, DevSize 0x23
AtapiDmaSetup: mode 0x45, data f7fb0000, count 4600, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=f7fb0000)
  get Phys(data[n=1]=f7fb1000)
  get Phys(data[n=1]=f7fb2000)
  get Phys(data[n=2]=f7fb3000)
  get Phys(data[n=2]=f7fb4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x41887, Count 0x23(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x41887 count 0x23 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 4600, full size 4600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
CreateDirectory("C:\Documents and Settings\Administrator\Dane aplikacji\Microsoft")
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805dfcc
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 44bf, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 44bf, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85ad4000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85ad4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x44bf, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x44bf count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
CreateDirectory("C:\Documents and Settings\Administrator\Dane aplikacji\Microsoft\Internet Explorer")
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805dfcc
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 44c7, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 44c7, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85bd4000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85bd4000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x44c7, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x44c7 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 418af, OrigWordsRequested 0xb00, DevSize 0xb
IdeReadWrite (REQ): Starting sector is 418af, Number of WORDS 0xb00, DevSize 0xb
AtapiDmaSetup: mode 0x45, data f7fb0000, count 1600, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=f7fb0000)
  get Phys(data[n=1]=f7fb1000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x418af, Count 0xb(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x418af count 0xb feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1600, full size 1600
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 418bf, OrigWordsRequested 0x700, DevSize 0x7
IdeReadWrite (REQ): Starting sector is 418bf, Number of WORDS 0x700, DevSize 0x7
AtapiDmaSetup: mode 0x45, data f7fb0000, count e00, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=f7fb0000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x418bf, Count 0x7(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x418bf count 0x7 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered e00, full size e00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf82ad338
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 418c7, OrigWordsRequested 0x500, DevSize 0x5
IdeReadWrite (REQ): Starting sector is 418c7, Number of WORDS 0x500, DevSize 0x5
AtapiDmaSetup: mode 0x45, data f7fb0000, count a00, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=f7fb0000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x418c7, Count 0x5(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x418c7 count 0x5 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered a00, full size a00
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
CreateDirectory("C:\Documents and Settings\Administrator\Dane aplikacji\Microsoft\Internet Explorer\Quick Launch")
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805dfcc
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 44cf, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 44cf, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85c54000, count 1000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85c54000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x44cf, Count 0x8(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x44cf count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e01c
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1e21e7, OrigWordsRequested 0x100, DevSize 0x1
IdeReadWrite (REQ): Starting sector is 1e21e7, Number of WORDS 0x100, DevSize 0x1
AtapiDmaSetup: mode 0x45, data f7fb0000, count 200, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=f7fb0000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1e21e7, Count 0x1(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1e21e7 count 0x1 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 200, full size 200
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805de10
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11e1f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 11e1f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f7fb0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=f7fb0000)
  get Phys(data[n=1]=f7fb1000)
  get Phys(data[n=1]=f7fb2000)
  get Phys(data[n=1]=f7fb3000)
  get Phys(data[n=1]=f7fb4000)
  get Phys(data[n=1]=f7fb5000)
  get Phys(data[n=2]=f7fb6000)
  get Phys(data[n=3]=f7fb7000)
  get Phys(data[n=3]=f7fb8000)
  get Phys(data[n=3]=f7fb9000)
  get Phys(data[n=4]=f7fba000)
  get Phys(data[n=4]=f7fbb000)
  get Phys(data[n=4]=f7fbc000)
  get Phys(data[n=4]=f7fbd000)
  get Phys(data[n=4]=f7fbe000)
  get Phys(data[n=5]=f7fbf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x11e1f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x11e1f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805de10
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11e9f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 11e9f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f7fc0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=f7fc0000)
  get Phys(data[n=1]=f7fc1000)
  get Phys(data[n=1]=f7fc2000)
  get Phys(data[n=1]=f7fc3000)
  get Phys(data[n=2]=f7fc4000)
  get Phys(data[n=2]=f7fc5000)
  get Phys(data[n=2]=f7fc6000)
  get Phys(data[n=3]=f7fc7000)
  get Phys(data[n=4]=f7fc8000)
  get Phys(data[n=5]=f7fc9000)
  get Phys(data[n=6]=f7fca000)
  get Phys(data[n=6]=f7fcb000)
  get Phys(data[n=7]=f7fcc000)
  get Phys(data[n=8]=f7fcd000)
  get Phys(data[n=8]=f7fce000)
  get Phys(data[n=8]=f7fcf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x11e9f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x11e9f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805de10
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11f1f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 11f1f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f7fd0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=f7fd0000)
  get Phys(data[n=1]=f7fd1000)
  get Phys(data[n=2]=f7fd2000)
  get Phys(data[n=3]=f7fd3000)
  get Phys(data[n=4]=f7fd4000)
  get Phys(data[n=5]=f7fd5000)
  get Phys(data[n=6]=f7fd6000)
  get Phys(data[n=7]=f7fd7000)
  get Phys(data[n=7]=f7fd8000)
  get Phys(data[n=8]=f7fd9000)
  get Phys(data[n=9]=f7fda000)
  get Phys(data[n=10]=f7fdb000)
  get Phys(data[n=10]=f7fdc000)
  get Phys(data[n=11]=f7fdd000)
  get Phys(data[n=12]=f7fde000)
  get Phys(data[n=13]=f7fdf000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x11f1f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x11f1f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805de10
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 11f9f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 11f9f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data f7fe0000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=f7fe0000)
  get Phys(data[n=1]=f7fe1000)
  get Phys(data[n=2]=f7fe2000)
  get Phys(data[n=2]=f7fe3000)
  get Phys(data[n=2]=f7fe4000)
  get Phys(data[n=2]=f7fe5000)
  get Phys(data[n=3]=f7fe6000)
  get Phys(data[n=3]=f7fe7000)
  get Phys(data[n=3]=f7fe8000)
  get Phys(data[n=4]=f7fe9000)
  get Phys(data[n=5]=f7fea000)
  get Phys(data[n=6]=f7feb000)
  get Phys(data[n=6]=f7fec000)
  get Phys(data[n=6]=f7fed000)
  get Phys(data[n=6]=f7fee000)
  get Phys(data[n=6]=f7fef000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x11f9f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x11f9f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1261f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1261f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85cd4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85cd4000)
  get Phys(data[n=1]=85cd5000)
  get Phys(data[n=1]=85cd6000)
  get Phys(data[n=1]=85cd7000)
  get Phys(data[n=1]=85cd8000)
  get Phys(data[n=1]=85cd9000)
  get Phys(data[n=2]=85cda000)
  get Phys(data[n=3]=85cdb000)
  get Phys(data[n=3]=85cdc000)
  get Phys(data[n=3]=85cdd000)
  get Phys(data[n=4]=85cde000)
  get Phys(data[n=4]=85cdf000)
  get Phys(data[n=4]=85ce0000)
  get Phys(data[n=4]=85ce1000)
  get Phys(data[n=4]=85ce2000)
  get Phys(data[n=5]=85ce3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1261f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1261f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1269f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1269f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85ce4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85ce4000)
  get Phys(data[n=1]=85ce5000)
  get Phys(data[n=2]=85ce6000)
  get Phys(data[n=2]=85ce7000)
  get Phys(data[n=3]=85ce8000)
  get Phys(data[n=3]=85ce9000)
  get Phys(data[n=3]=85cea000)
  get Phys(data[n=4]=85ceb000)
  get Phys(data[n=5]=85cec000)
  get Phys(data[n=6]=85ced000)
  get Phys(data[n=7]=85cee000)
  get Phys(data[n=7]=85cef000)
  get Phys(data[n=8]=85cf0000)
  get Phys(data[n=9]=85cf1000)
  get Phys(data[n=9]=85cf2000)
  get Phys(data[n=9]=85cf3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1269f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1269f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1271f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1271f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85cf4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85cf4000)
  get Phys(data[n=1]=85cf5000)
  get Phys(data[n=2]=85cf6000)
  get Phys(data[n=3]=85cf7000)
  get Phys(data[n=4]=85cf8000)
  get Phys(data[n=5]=85cf9000)
  get Phys(data[n=6]=85cfa000)
  get Phys(data[n=7]=85cfb000)
  get Phys(data[n=7]=85cfc000)
  get Phys(data[n=8]=85cfd000)
  get Phys(data[n=9]=85cfe000)
  get Phys(data[n=10]=85cff000)
  get Phys(data[n=10]=85d00000)
  get Phys(data[n=11]=85d01000)
  get Phys(data[n=12]=85d02000)
  get Phys(data[n=13]=85d03000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1271f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1271f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1279f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1279f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85d04000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85d04000)
  get Phys(data[n=1]=85d05000)
  get Phys(data[n=2]=85d06000)
  get Phys(data[n=2]=85d07000)
  get Phys(data[n=2]=85d08000)
  get Phys(data[n=2]=85d09000)
  get Phys(data[n=3]=85d0a000)
  get Phys(data[n=3]=85d0b000)
  get Phys(data[n=3]=85d0c000)
  get Phys(data[n=4]=85d0d000)
  get Phys(data[n=5]=85d0e000)
  get Phys(data[n=6]=85d0f000)
  get Phys(data[n=6]=85d10000)
  get Phys(data[n=6]=85d11000)
  get Phys(data[n=6]=85d12000)
  get Phys(data[n=6]=85d13000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1279f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1279f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1201f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1201f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85d14000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85d14000)
  get Phys(data[n=1]=85d15000)
  get Phys(data[n=1]=85d16000)
  get Phys(data[n=1]=85d17000)
  get Phys(data[n=1]=85d18000)
  get Phys(data[n=1]=85d19000)
  get Phys(data[n=2]=85d1a000)
  get Phys(data[n=3]=85d1b000)
  get Phys(data[n=3]=85d1c000)
  get Phys(data[n=3]=85d1d000)
  get Phys(data[n=4]=85d1e000)
  get Phys(data[n=4]=85d1f000)
  get Phys(data[n=4]=85d20000)
  get Phys(data[n=4]=85d21000)
  get Phys(data[n=4]=85d22000)
  get Phys(data[n=5]=85d23000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1201f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1201f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1209f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1209f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85d24000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85d24000)
  get Phys(data[n=1]=85d25000)
  get Phys(data[n=2]=85d26000)
  get Phys(data[n=2]=85d27000)
  get Phys(data[n=3]=85d28000)
  get Phys(data[n=3]=85d29000)
  get Phys(data[n=3]=85d2a000)
  get Phys(data[n=4]=85d2b000)
  get Phys(data[n=5]=85d2c000)
  get Phys(data[n=6]=85d2d000)
  get Phys(data[n=7]=85d2e000)
  get Phys(data[n=7]=85d2f000)
  get Phys(data[n=8]=85d30000)
  get Phys(data[n=9]=85d31000)
  get Phys(data[n=9]=85d32000)
  get Phys(data[n=9]=85d33000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1209f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1209f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1211f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1211f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85d34000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85d34000)
  get Phys(data[n=1]=85d35000)
  get Phys(data[n=2]=85d36000)
  get Phys(data[n=3]=85d37000)
  get Phys(data[n=4]=85d38000)
  get Phys(data[n=5]=85d39000)
  get Phys(data[n=6]=85d3a000)
  get Phys(data[n=7]=85d3b000)
  get Phys(data[n=7]=85d3c000)
  get Phys(data[n=8]=85d3d000)
  get Phys(data[n=9]=85d3e000)
  get Phys(data[n=10]=85d3f000)
  get Phys(data[n=10]=85d40000)
  get Phys(data[n=11]=85d41000)
  get Phys(data[n=12]=85d42000)
  get Phys(data[n=13]=85d43000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1211f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1211f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1219f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1219f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85d44000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85d44000)
  get Phys(data[n=1]=85d45000)
  get Phys(data[n=2]=85d46000)
  get Phys(data[n=2]=85d47000)
  get Phys(data[n=2]=85d48000)
  get Phys(data[n=2]=85d49000)
  get Phys(data[n=3]=85d4a000)
  get Phys(data[n=3]=85d4b000)
  get Phys(data[n=3]=85d4c000)
  get Phys(data[n=4]=85d4d000)
  get Phys(data[n=5]=85d4e000)
  get Phys(data[n=6]=85d4f000)
  get Phys(data[n=6]=85d50000)
  get Phys(data[n=6]=85d51000)
  get Phys(data[n=6]=85d52000)
  get Phys(data[n=6]=85d53000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1219f, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x1219f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 36b47, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 36b47, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85c94000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85c94000)
  get Phys(data[n=1]=85c95000)
  get Phys(data[n=2]=85c96000)
  get Phys(data[n=3]=85c97000)
  get Phys(data[n=3]=85c98000)
  get Phys(data[n=3]=85c99000)
  get Phys(data[n=4]=85c9a000)
  get Phys(data[n=4]=85c9b000)
  get Phys(data[n=4]=85c9c000)
  get Phys(data[n=4]=85c9d000)
  get Phys(data[n=4]=85c9e000)
  get Phys(data[n=5]=85c9f000)
  get Phys(data[n=5]=85ca0000)
  get Phys(data[n=6]=85ca1000)
  get Phys(data[n=6]=85ca2000)
  get Phys(data[n=6]=85ca3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x36b47, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x36b47 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 36bc7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 36bc7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85ca4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85ca4000)
  get Phys(data[n=1]=85ca5000)
  get Phys(data[n=1]=85ca6000)
  get Phys(data[n=2]=85ca7000)
  get Phys(data[n=3]=85ca8000)
  get Phys(data[n=4]=85ca9000)
  get Phys(data[n=5]=85caa000)
  get Phys(data[n=5]=85cab000)
  get Phys(data[n=6]=85cac000)
  get Phys(data[n=7]=85cad000)
  get Phys(data[n=7]=85cae000)
  get Phys(data[n=7]=85caf000)
  get Phys(data[n=8]=85cb0000)
  get Phys(data[n=8]=85cb1000)
  get Phys(data[n=9]=85cb2000)
  get Phys(data[n=10]=85cb3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x36bc7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x36bc7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=1
Non-empty queue
Try IDE prepare
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb129b048
** --- **
** Ide: Command continue prep
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 36c47, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 36c47, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85cb4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=85cb4000)
  get Phys(data[n=1]=85cb5000)
  get Phys(data[n=2]=85cb6000)
  get Phys(data[n=3]=85cb7000)
  get Phys(data[n=3]=85cb8000)
  get Phys(data[n=4]=85cb9000)
  get Phys(data[n=5]=85cba000)
  get Phys(data[n=6]=85cbb000)
  get Phys(data[n=6]=85cbc000)
  get Phys(data[n=7]=85cbd000)
  get Phys(data[n=8]=85cbe000)
  get Phys(data[n=9]=85cbf000)
  get Phys(data[n=9]=85cc0000)
  get Phys(data[n=10]=85cc1000)
  get Phys(data[n=11]=85cc2000)
  get Phys(data[n=11]=85cc3000)
  set TERM
AtapiDmaSetup: OK
IdeSendCommand: SRB_STATUS_PENDING
AtapiStartIo: Already have 2 request(s)!
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0xb0a3cdd0
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: qd=1
Send to device 28
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e0e4
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (ExecOnly):
IdeReadWrite: Lba 0x36c47, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x36c47 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 36cc7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 36cc7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85cc4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85cc4000)
  get Phys(data[n=1]=85cc5000)
  get Phys(data[n=2]=85cc6000)
  get Phys(data[n=2]=85cc7000)
  get Phys(data[n=2]=85cc8000)
  get Phys(data[n=3]=85cc9000)
  get Phys(data[n=4]=85cca000)
  get Phys(data[n=5]=85ccb000)
  get Phys(data[n=5]=85ccc000)
  get Phys(data[n=5]=85ccd000)
  get Phys(data[n=5]=85cce000)
  get Phys(data[n=5]=85ccf000)
  get Phys(data[n=5]=85cd0000)
  get Phys(data[n=6]=85cd1000)
  get Phys(data[n=6]=85cd2000)
  get Phys(data[n=6]=85cd3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x36cc7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x36cc7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 34747, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 34747, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85cd4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85cd4000)
  get Phys(data[n=1]=85cd5000)
  get Phys(data[n=1]=85cd6000)
  get Phys(data[n=1]=85cd7000)
  get Phys(data[n=1]=85cd8000)
  get Phys(data[n=1]=85cd9000)
  get Phys(data[n=2]=85cda000)
  get Phys(data[n=2]=85cdb000)
  get Phys(data[n=2]=85cdc000)
  get Phys(data[n=2]=85cdd000)
  get Phys(data[n=2]=85cde000)
  get Phys(data[n=2]=85cdf000)
  get Phys(data[n=2]=85ce0000)
  get Phys(data[n=2]=85ce1000)
  get Phys(data[n=2]=85ce2000)
  get Phys(data[n=2]=85ce3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x34747, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x34747 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 347c7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 347c7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85ce4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85ce4000)
  get Phys(data[n=1]=85ce5000)
  get Phys(data[n=1]=85ce6000)
  get Phys(data[n=1]=85ce7000)
  get Phys(data[n=1]=85ce8000)
  get Phys(data[n=1]=85ce9000)
  get Phys(data[n=2]=85cea000)
  get Phys(data[n=2]=85ceb000)
  get Phys(data[n=2]=85cec000)
  get Phys(data[n=2]=85ced000)
  get Phys(data[n=2]=85cee000)
  get Phys(data[n=2]=85cef000)
  get Phys(data[n=2]=85cf0000)
  get Phys(data[n=2]=85cf1000)
  get Phys(data[n=2]=85cf2000)
  get Phys(data[n=2]=85cf3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x347c7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x347c7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=1
Non-empty queue
Try IDE prepare
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb129b048
** --- **
** Ide: Command continue prep
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 34847, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 34847, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85cf4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=85cf4000)
  get Phys(data[n=1]=85cf5000)
  get Phys(data[n=1]=85cf6000)
  get Phys(data[n=1]=85cf7000)
  get Phys(data[n=1]=85cf8000)
  get Phys(data[n=1]=85cf9000)
  get Phys(data[n=2]=85cfa000)
  get Phys(data[n=2]=85cfb000)
  get Phys(data[n=2]=85cfc000)
  get Phys(data[n=2]=85cfd000)
  get Phys(data[n=2]=85cfe000)
  get Phys(data[n=2]=85cff000)
  get Phys(data[n=2]=85d00000)
  get Phys(data[n=2]=85d01000)
  get Phys(data[n=2]=85d02000)
  get Phys(data[n=2]=85d03000)
  set TERM
AtapiDmaSetup: OK
IdeSendCommand: SRB_STATUS_PENDING
AtapiStartIo: Already have 2 request(s)!
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0xb0a3cdd0
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: qd=1
Send to device 28
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e0e4
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (ExecOnly):
IdeReadWrite: Lba 0x34847, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x34847 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 348c7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 348c7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85d04000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85d04000)
  get Phys(data[n=1]=85d05000)
  get Phys(data[n=1]=85d06000)
  get Phys(data[n=1]=85d07000)
  get Phys(data[n=1]=85d08000)
  get Phys(data[n=1]=85d09000)
  get Phys(data[n=2]=85d0a000)
  get Phys(data[n=2]=85d0b000)
  get Phys(data[n=2]=85d0c000)
  get Phys(data[n=2]=85d0d000)
  get Phys(data[n=3]=85d0e000)
  get Phys(data[n=3]=85d0f000)
  get Phys(data[n=3]=85d10000)
  get Phys(data[n=3]=85d11000)
  get Phys(data[n=3]=85d12000)
  get Phys(data[n=3]=85d13000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x348c7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x348c7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3ce18
TopLevel (3), AtaReq 0xb1299018
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 34347, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 34347, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85d14000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85d14000)
  get Phys(data[n=1]=85d15000)
  get Phys(data[n=1]=85d16000)
  get Phys(data[n=1]=85d17000)
  get Phys(data[n=1]=85d18000)
  get Phys(data[n=1]=85d19000)
  get Phys(data[n=1]=85d1a000)
  get Phys(data[n=1]=85d1b000)
  get Phys(data[n=2]=85d1c000)
  get Phys(data[n=2]=85d1d000)
  get Phys(data[n=2]=85d1e000)
  get Phys(data[n=2]=85d1f000)
  get Phys(data[n=2]=85d20000)
  get Phys(data[n=2]=85d21000)
  get Phys(data[n=2]=85d22000)
  get Phys(data[n=2]=85d23000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x34347, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x34347 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=1
Non-empty queue
Try IDE prepare
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb129b048
** --- **
** Ide: Command continue prep
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 343c7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 343c7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85d24000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=85d24000)
  get Phys(data[n=1]=85d25000)
  get Phys(data[n=1]=85d26000)
  get Phys(data[n=1]=85d27000)
  get Phys(data[n=1]=85d28000)
  get Phys(data[n=1]=85d29000)
  get Phys(data[n=1]=85d2a000)
  get Phys(data[n=1]=85d2b000)
  get Phys(data[n=2]=85d2c000)
  get Phys(data[n=2]=85d2d000)
  get Phys(data[n=2]=85d2e000)
  get Phys(data[n=2]=85d2f000)
  get Phys(data[n=3]=85d30000)
  get Phys(data[n=3]=85d31000)
  get Phys(data[n=3]=85d32000)
  get Phys(data[n=3]=85d33000)
  set TERM
AtapiDmaSetup: OK
IdeSendCommand: SRB_STATUS_PENDING
AtapiStartIo: Already have 2 request(s)!
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0xb0a3cdd0
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: qd=1
Send to device 28
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e0e4
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (ExecOnly):
IdeReadWrite: Lba 0x343c7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x343c7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=1
Non-empty queue
Try IDE prepare
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb1299018
** --- **
** Ide: Command continue prep
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 34447, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 34447, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85d34000, count 10000, lCh 0, dev 0
  get Phys(PRD=b1299070)
  get Phys(data[0]=85d34000)
  get Phys(data[n=1]=85d35000)
  get Phys(data[n=1]=85d36000)
  get Phys(data[n=1]=85d37000)
  get Phys(data[n=1]=85d38000)
  get Phys(data[n=1]=85d39000)
  get Phys(data[n=1]=85d3a000)
  get Phys(data[n=1]=85d3b000)
  get Phys(data[n=2]=85d3c000)
  get Phys(data[n=2]=85d3d000)
  get Phys(data[n=2]=85d3e000)
  get Phys(data[n=2]=85d3f000)
  get Phys(data[n=2]=85d40000)
  get Phys(data[n=2]=85d41000)
  get Phys(data[n=2]=85d42000)
  get Phys(data[n=2]=85d43000)
  set TERM
AtapiDmaSetup: OK
IdeSendCommand: SRB_STATUS_PENDING
AtapiStartIo: Already have 2 request(s)!
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0xb0a3ce18
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3ce18, CDB 0xb0a3ce48, AtaReq 0xb1299018, SCmd 0x28
UniataNeedQueueing: qd=1
Send to device 28
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e0e4
** Ide: Command AtaReq 0xb1299018
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (ExecOnly):
IdeReadWrite: Lba 0x34447, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x34447 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3ce18
AtapiStartIo: query PORT for next request
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 1)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  IDE status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3ce18, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3ce18
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 344c7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 344c7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85d44000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=85d44000)
  get Phys(data[n=1]=85d45000)
  get Phys(data[n=2]=85d46000)
  get Phys(data[n=2]=85d47000)
  get Phys(data[n=2]=85d48000)
  get Phys(data[n=2]=85d49000)
  get Phys(data[n=2]=85d4a000)
  get Phys(data[n=2]=85d4b000)
  get Phys(data[n=3]=85d4c000)
  get Phys(data[n=3]=85d4d000)
  get Phys(data[n=3]=85d4e000)
  get Phys(data[n=3]=85d4f000)
  get Phys(data[n=3]=85d50000)
  get Phys(data[n=3]=85d51000)
  get Phys(data[n=3]=85d52000)
  get Phys(data[n=4]=85d53000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x344c7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x344c7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 35547, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 35547, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85d54000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=85d54000)
  get Phys(data[n=1]=85d55000)
  get Phys(data[n=1]=85d56000)
  get Phys(data[n=1]=85d57000)
  get Phys(data[n=1]=85d58000)
  get Phys(data[n=1]=85d59000)
  get Phys(data[n=1]=85d5a000)
  get Phys(data[n=1]=85d5b000)
  get Phys(data[n=1]=85d5c000)
  get Phys(data[n=1]=85d5d000)
  get Phys(data[n=1]=85d5e000)
  get Phys(data[n=1]=85d5f000)
  get Phys(data[n=1]=85d60000)
  get Phys(data[n=2]=85d61000)
  get Phys(data[n=2]=85d62000)
  get Phys(data[n=2]=85d63000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x35547, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x35547 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 355c7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 355c7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85d64000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=85d64000)
  get Phys(data[n=1]=85d65000)
  get Phys(data[n=1]=85d66000)
  get Phys(data[n=1]=85d67000)
  get Phys(data[n=1]=85d68000)
  get Phys(data[n=1]=85d69000)
  get Phys(data[n=1]=85d6a000)
  get Phys(data[n=1]=85d6b000)
  get Phys(data[n=1]=85d6c000)
  get Phys(data[n=1]=85d6d000)
  get Phys(data[n=1]=85d6e000)
  get Phys(data[n=1]=85d6f000)
  get Phys(data[n=1]=85d70000)
  get Phys(data[n=2]=85d71000)
  get Phys(data[n=2]=85d72000)
  get Phys(data[n=2]=85d73000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x355c7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x355c7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 35647, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 35647, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85d74000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=85d74000)
  get Phys(data[n=1]=85d75000)
  get Phys(data[n=1]=85d76000)
  get Phys(data[n=1]=85d77000)
  get Phys(data[n=1]=85d78000)
  get Phys(data[n=1]=85d79000)
  get Phys(data[n=1]=85d7a000)
  get Phys(data[n=2]=85d7b000)
  get Phys(data[n=2]=85d7c000)
  get Phys(data[n=2]=85d7d000)
  get Phys(data[n=2]=85d7e000)
  get Phys(data[n=2]=85d7f000)
  get Phys(data[n=2]=85d80000)
  get Phys(data[n=3]=85d81000)
  get Phys(data[n=3]=85d82000)
  get Phys(data[n=3]=85d83000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x35647, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x35647 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 356c7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 356c7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85d84000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=85d84000)
  get Phys(data[n=1]=85d85000)
  get Phys(data[n=1]=85d86000)
  get Phys(data[n=1]=85d87000)
  get Phys(data[n=1]=85d88000)
  get Phys(data[n=2]=85d89000)
  get Phys(data[n=3]=85d8a000)
  get Phys(data[n=3]=85d8b000)
  get Phys(data[n=3]=85d8c000)
  get Phys(data[n=3]=85d8d000)
  get Phys(data[n=3]=85d8e000)
  get Phys(data[n=3]=85d8f000)
  get Phys(data[n=3]=85d90000)
  get Phys(data[n=4]=85d91000)
  get Phys(data[n=4]=85d92000)
  get Phys(data[n=4]=85d93000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x356c7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x356c7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf88657f8
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1d2867, OrigWordsRequested 0x800, DevSize 0x8
IdeReadWrite (REQ): Starting sector is 1d2867, Number of WORDS 0x800, DevSize 0x8
AtapiDmaSetup: mode 0x45, data 85b54000, count 1000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=85b54000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1d2867, Count 0x8(0x8)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1d2867 count 0x8 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 1000, full size 1000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 5f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 5f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c00000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=80c00000)
  get Phys(data[n=1]=80c01000)
  get Phys(data[n=2]=80c02000)
  get Phys(data[n=2]=80c03000)
  get Phys(data[n=2]=80c04000)
  get Phys(data[n=2]=80c05000)
  get Phys(data[n=2]=80c06000)
  get Phys(data[n=2]=80c07000)
  get Phys(data[n=3]=80c08000)
  get Phys(data[n=3]=80c09000)
  get Phys(data[n=3]=80c0a000)
  get Phys(data[n=3]=80c0b000)
  get Phys(data[n=3]=80c0c000)
  get Phys(data[n=3]=80c0d000)
  get Phys(data[n=3]=80c0e000)
  get Phys(data[n=3]=80c0f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x5f, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x5f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c10000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=80c10000)
  get Phys(data[n=1]=80c11000)
  get Phys(data[n=1]=80c12000)
  get Phys(data[n=1]=80c13000)
  get Phys(data[n=1]=80c14000)
  get Phys(data[n=1]=80c15000)
  get Phys(data[n=1]=80c16000)
  get Phys(data[n=1]=80c17000)
  get Phys(data[n=2]=80c18000)
  get Phys(data[n=2]=80c19000)
  get Phys(data[n=2]=80c1a000)
  get Phys(data[n=2]=80c1b000)
  get Phys(data[n=2]=80c1c000)
  get Phys(data[n=2]=80c1d000)
  get Phys(data[n=2]=80c1e000)
  get Phys(data[n=2]=80c1f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0xdf, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0xdf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 15f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 15f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c20000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=80c20000)
  get Phys(data[n=1]=80c21000)
  get Phys(data[n=1]=80c22000)
  get Phys(data[n=1]=80c23000)
  get Phys(data[n=1]=80c24000)
  get Phys(data[n=1]=80c25000)
  get Phys(data[n=1]=80c26000)
  get Phys(data[n=1]=80c27000)
  get Phys(data[n=2]=80c28000)
  get Phys(data[n=3]=80c29000)
  get Phys(data[n=4]=80c2a000)
  get Phys(data[n=4]=80c2b000)
  get Phys(data[n=4]=80c2c000)
  get Phys(data[n=5]=80c2d000)
  get Phys(data[n=5]=80c2e000)
  get Phys(data[n=5]=80c2f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x15f, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x15f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 1df, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 1df, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c30000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=80c30000)
  get Phys(data[n=1]=80c31000)
  get Phys(data[n=2]=80c32000)
  get Phys(data[n=2]=80c33000)
  get Phys(data[n=2]=80c34000)
  get Phys(data[n=2]=80c35000)
  get Phys(data[n=2]=80c36000)
  get Phys(data[n=2]=80c37000)
  get Phys(data[n=3]=80c38000)
  get Phys(data[n=3]=80c39000)
  get Phys(data[n=3]=80c3a000)
  get Phys(data[n=3]=80c3b000)
  get Phys(data[n=3]=80c3c000)
  get Phys(data[n=3]=80c3d000)
  get Phys(data[n=3]=80c3e000)
  get Phys(data[n=3]=80c3f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x1df, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x1df count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 204f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 204f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c00000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=80c00000)
  get Phys(data[n=1]=80c01000)
  get Phys(data[n=2]=80c02000)
  get Phys(data[n=2]=80c03000)
  get Phys(data[n=2]=80c04000)
  get Phys(data[n=2]=80c05000)
  get Phys(data[n=2]=80c06000)
  get Phys(data[n=2]=80c07000)
  get Phys(data[n=3]=80c08000)
  get Phys(data[n=3]=80c09000)
  get Phys(data[n=3]=80c0a000)
  get Phys(data[n=3]=80c0b000)
  get Phys(data[n=3]=80c0c000)
  get Phys(data[n=3]=80c0d000)
  get Phys(data[n=3]=80c0e000)
  get Phys(data[n=3]=80c0f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x204f, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x204f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 20cf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 20cf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c10000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=80c10000)
  get Phys(data[n=1]=80c11000)
  get Phys(data[n=1]=80c12000)
  get Phys(data[n=1]=80c13000)
  get Phys(data[n=1]=80c14000)
  get Phys(data[n=1]=80c15000)
  get Phys(data[n=1]=80c16000)
  get Phys(data[n=1]=80c17000)
  get Phys(data[n=2]=80c18000)
  get Phys(data[n=2]=80c19000)
  get Phys(data[n=2]=80c1a000)
  get Phys(data[n=2]=80c1b000)
  get Phys(data[n=2]=80c1c000)
  get Phys(data[n=2]=80c1d000)
  get Phys(data[n=2]=80c1e000)
  get Phys(data[n=2]=80c1f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x20cf, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x20cf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 214f, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 214f, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c20000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=80c20000)
  get Phys(data[n=1]=80c21000)
  get Phys(data[n=1]=80c22000)
  get Phys(data[n=1]=80c23000)
  get Phys(data[n=1]=80c24000)
  get Phys(data[n=1]=80c25000)
  get Phys(data[n=1]=80c26000)
  get Phys(data[n=1]=80c27000)
  get Phys(data[n=2]=80c28000)
  get Phys(data[n=3]=80c29000)
  get Phys(data[n=4]=80c2a000)
  get Phys(data[n=4]=80c2b000)
  get Phys(data[n=4]=80c2c000)
  get Phys(data[n=5]=80c2d000)
  get Phys(data[n=5]=80c2e000)
  get Phys(data[n=5]=80c2f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x214f, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x214f count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x2a
UniataNeedQueueing: TopLevel, qd=0
Send to device 2a
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf8865790
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_WRITE PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 21cf, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 21cf, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 80c30000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=80c30000)
  get Phys(data[n=1]=80c31000)
  get Phys(data[n=2]=80c32000)
  get Phys(data[n=2]=80c33000)
  get Phys(data[n=2]=80c34000)
  get Phys(data[n=2]=80c35000)
  get Phys(data[n=2]=80c36000)
  get Phys(data[n=2]=80c37000)
  get Phys(data[n=3]=80c38000)
  get Phys(data[n=3]=80c39000)
  get Phys(data[n=3]=80c3a000)
  get Phys(data[n=3]=80c3b000)
  get Phys(data[n=3]=80c3c000)
  get Phys(data[n=3]=80c3d000)
  get Phys(data[n=3]=80c3e000)
  get Phys(data[n=3]=80c3f000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x21cf, Count 0x80(0x80)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xca, lba 0x21cf count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: write on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=0, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 34947, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 34947, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85d94000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=85d94000)
  get Phys(data[n=1]=85d95000)
  get Phys(data[n=1]=85d96000)
  get Phys(data[n=1]=85d97000)
  get Phys(data[n=1]=85d98000)
  get Phys(data[n=1]=85d99000)
  get Phys(data[n=1]=85d9a000)
  get Phys(data[n=1]=85d9b000)
  get Phys(data[n=2]=85d9c000)
  get Phys(data[n=2]=85d9d000)
  get Phys(data[n=2]=85d9e000)
  get Phys(data[n=2]=85d9f000)
  get Phys(data[n=2]=85da0000)
  get Phys(data[n=2]=85da1000)
  get Phys(data[n=2]=85da2000)
  get Phys(data[n=2]=85da3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x34947, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x34947 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 349c7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 349c7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85da4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=85da4000)
  get Phys(data[n=1]=85da5000)
  get Phys(data[n=2]=85da6000)
  get Phys(data[n=2]=85da7000)
  get Phys(data[n=2]=85da8000)
  get Phys(data[n=2]=85da9000)
  get Phys(data[n=2]=85daa000)
  get Phys(data[n=2]=85dab000)
  get Phys(data[n=3]=85dac000)
  get Phys(data[n=3]=85dad000)
  get Phys(data[n=3]=85dae000)
  get Phys(data[n=3]=85daf000)
  get Phys(data[n=3]=85db0000)
  get Phys(data[n=3]=85db1000)
  get Phys(data[n=3]=85db2000)
  get Phys(data[n=3]=85db3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x349c7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x349c7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 34a47, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 34a47, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85db4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=85db4000)
  get Phys(data[n=1]=85db5000)
  get Phys(data[n=1]=85db6000)
  get Phys(data[n=1]=85db7000)
  get Phys(data[n=1]=85db8000)
  get Phys(data[n=1]=85db9000)
  get Phys(data[n=1]=85dba000)
  get Phys(data[n=1]=85dbb000)
  get Phys(data[n=2]=85dbc000)
  get Phys(data[n=2]=85dbd000)
  get Phys(data[n=2]=85dbe000)
  get Phys(data[n=2]=85dbf000)
  get Phys(data[n=2]=85dc0000)
  get Phys(data[n=2]=85dc1000)
  get Phys(data[n=2]=85dc2000)
  get Phys(data[n=2]=85dc3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x34a47, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x34a47 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
TopLevel
** AtapiStartIo: Function 0x0, PATH:LUN:TID = 0x0:0x0:0x0
   VendorID+DeviceID/Rev 0x269e8086/0x0
  SRB 0xb0a3cdd0, CDB 0xb0a3ce00, AtaReq 0xb129b048, SCmd 0x28
UniataNeedQueueing: TopLevel, qd=0
Send to device 28
TopLevel (2), srb 0xb0a3cdd0
TopLevel (3), AtaReq 0xb129b048
Try IDE send
** Ide: Command: entryway
** Ide: Command:

** Ide: Command &AtaReq 0xf805e210
** Ide: Command AtaReq 0xb129b048
** --- **
IdeSendCommand: SCSIOP_READ PATH:LUN:TID = 0x0:0x0:0x0
IdeReadWrite (Orig REQ): Starting sector 34ac7, OrigWordsRequested 0x8000, DevSize 0x80
IdeReadWrite (REQ): Starting sector is 34ac7, Number of WORDS 0x8000, DevSize 0x80
AtapiDmaSetup: mode 0x45, data 85dc4000, count 10000, lCh 0, dev 0
  get Phys(PRD=b129b0a0)
  get Phys(data[0]=85dc4000)
  get Phys(data[n=1]=85dc5000)
  get Phys(data[n=1]=85dc6000)
  get Phys(data[n=1]=85dc7000)
  get Phys(data[n=1]=85dc8000)
  get Phys(data[n=1]=85dc9000)
  get Phys(data[n=1]=85dca000)
  get Phys(data[n=1]=85dcb000)
  get Phys(data[n=2]=85dcc000)
  get Phys(data[n=3]=85dcd000)
  get Phys(data[n=3]=85dce000)
  get Phys(data[n=3]=85dcf000)
  get Phys(data[n=4]=85dd0000)
  get Phys(data[n=4]=85dd1000)
  get Phys(data[n=4]=85dd2000)
  get Phys(data[n=4]=85dd3000)
  set TERM
AtapiDmaSetup: OK
IdeReadWrite: Lba 0x34ac7, Count 0x80(0x0)
AtaCommand48: cntrlr 0x0:0x0 dev 0x0, cmd 0xc8, lba 0x34ac7 count 0x80 feature 0x0
  Status 0x0
AtapiDmaStart: read on 0x0:0x0
IdeSendCommand: SRB_STATUS_PENDING
IdeSendCommand: REQ_STATE_EXPECTING_INTR
AtapiStartIo: next Srb b0a3cdd0
AtapiStartIo: query PORT for next request
Intr: VendorID+DeviceID/Rev 0x269e8086/0x0 (ex 2)
AtapiInterrupt(base): cntrlr 0x0 chan 0x0
AtapiInterrupt(base): try lock
AtapiInterrupt(base): locked
AtapiCheckInterrupt__:
  cntrlr 0x0:0x0, lch 0x0 DmaTransfer = TRUE
  perform generic check
  getting status...
  ATAPI status 0x50
  base status 0x50
AtapiDmaDone: dev -1
AtapiCheckInterrupt__: exit with TRUE
AtapiInterrupt:
  cntrlr 0x0:0, irql 0xd, c 0
  DmaTransfer = TRUE
  dev_type IDE
  OldReqState = 40
AtapiInterrupt: Entered with status (0x50)
AtapiInterrupt: i-reason=2, status=0x58
AtapiInterrupt: CompleteRequest, srbstatus 1
   Transfered 10000, full size 10000
AtapiInterrupt: RequestComplete
AtapiInterrupt: set AutoSense
AtapiInterrupt: remove srb 0xb0a3cdd0, status 1
AtapiInterrupt: RequestComplete, srb 0xb0a3cdd0
AtapiInterrupt: NextRequest, srb=0x0
AtapiInterrupt: ReturnEnableIntr
AtapiInterrupt: exiting, UseDpc=1, NoStartIo=1
AtapiInterrupt(base): return status TRUE
AtapiInterrupt(base): exit with status 0x1
